# Paravision SX-1 External IDE

Paravision was formerly Microbotics.

(At the controller)

37 PIN D-SUB FEMALE at the controller.

Pin | Name | Description
--- | --- | ---
1 | /IDE-RESET | Drive Reset
2 | D0 | Data bit 0
3 | D2 | Data bit 2
4 | D4 | Data bit 4
5 | D6 | Data bit 6
6 | GND | Ground
7 | D8 | Data bit 8
8 | D10 | Data bit 10
9 | D12 | Data bit 12
10 | D14 | Data bit 14
11 | GND | Ground
12 | GND | Ground
13 | GND | Ground
14 | GND | Ground
15 | GND | Ground
16 | GND | Ground
17 | GND | Ground
18 | +5V | 5V Power
19 | +5V | 5V Power
20 | GND | Ground
21 | D1 | Data bit 1
22 | D3 | Data bit 3
23 | D5 | Data bit 5
24 | D7 | Data bit 7
25 | GND | Ground
26 | D9 | Data bit 9
27 | D11 | Data bit 11
28 | D13 | Data bit 13
29 | D15 | Data bit 15
30 | /IOW | I/O Write
31 | /IOR | I/O Read
32 | IDE-IRQ | Interrupt Request
33 | IDE-A2 | Address bit 2
34 | IDE-A1 | Address bit 1
35 | IDE-A0 | Address bit 0
36 | /BICS1 | Chip Select 1
37 | /BICS0 | Chip Select 0