# SCART

(At the video/TV)
(At the cable)

21 PIN SCART FEMALE at the Video/TV.
21 PIN SCART MALE at the Cable.

Pin | Name | Description | Signal Level | Impedance
--- | --- | --- | --- | ---
1 | AOR | Audio Out Right | 0.5 V rms | <1k ohm
2 | AIR | Audio In Right | 0.5 V rms | >10k ohm
3 | AOL | Audio Out Left + Mono | 0.5 V rms | <1k ohm
4 | AGND | Audio Ground |  |
5 | B GND | RGB Blue Ground |  |
6 | AIL | Audio In Left + Mono | 0.5 V rms | >10k ohm
7 | B | RGB Blue In | 0.7 V | 75 ohm
8 | SWTCH | Audio/RGB switch / 16:9 |  |
9 | G GND | RGB Green Ground |  |
10 | CLKOUT | Data 2: Clockpulse Out (Unavailble ??) |  |
11 | G | RGB Green In | 0.7 V | 75 ohm
12 | DATA | Data 1: Data Out (Unavailble ??) |  |
13 | R GND | RGB Red Ground |  |
14 | DATAGND | Data Ground |  |
15 | R | RGB Red In / Chrominance | 0.7 V (Chrom.: 0.3 V burst) | 75 ohm
16 | BLNK | Blanking Signal | 1-3 V=RGB, 0-0.4 V=Composite | 75 ohm
17 | VGND | Composite Video Ground |  |
18 | BLNKGND | Blanking Signal Ground |  |
19 | VOUT | Composite Video Out | 1 V | 75 ohm
20 | VIN | Composite Video In / Luminance | 1 V | 75 ohm
21 | SHIELD | Ground/Shield (Chassis) |  |