# GeekPort

The GeekPort is a connector availble at Be's BeBox computers.
This is a dream for all hobby engineers who like to connect the computer to the coffee machine.

(At the device)
(At the computer)

37 PIN D-SUB MALE CONNECTOR at the device.
37 PIN D-SUB FEMALE CONNECTOR at the computer.

Pin | Name | Description | Dir
--- | --- | --- | ---
1 | GND | Ground |
2 | A1 | Digital A 1 |
3 | A3 | Digital A 3 |
4 | A5 | Digital A 5 |
5 | A7 | Digital A 7 |
6 | GND | Ground |
7 | +5V | +5 VDC |
8 | GND | Ground |
9 | +12V | +12 VDC |
10 | GND | Ground |
11 | -12V | -12 VDC |
12 | GND | Ground |
13 | +5V | +5 VDC |
14 | GND | Ground |
15 | B0 | Digital B 0 |
16 | B2 | Digital B 2 |
17 | B4 | Digital B 4 |
18 | B6 | Digital B 6 |
19 | GND | Ground |
20 | A0 | Digital A 0 |
21 | A2 | Digital A 2 |
22 | A4 | Digital A 4 |
23 | A6 | Digital A 6 |
24 | AIref | Analog In Reference |
25 | A2D1 | Analog In 1 |
26 | A2D2 | Analog In 2 |
27 | A2D3 | Analog In 3 |
28 | A2D4 | Analog In 4 |
29 | D2A1 | Analog Out 1 |
30 | D2A2 | Analog Out 2 |
31 | D2A3 | Analog Out 3 |
32 | D2A4 | Analog Out 4 |
33 | AOref | Analog Out Reference |
34 | B1 | Digital B 1 |
35 | B3 | Digital B 3 |
36 | B5 | Digital B 5 |
37 | B7 | Digital B 7 |