# CompactPCI (Technical)

This section does not currently contain so much in depth information as I would like.

Since CompactPCI is based on PCI you should first refer to the PCI standard. This only explains the extensions CompactPCI specifies.

For a copy of the full CompactPCI standard, contact:

## Overview:

A CompactPCI system is composed of up to eight CompactPCI card locations:

- One System Slot
- Up to seven Peipherial Slots

The connector has 7 columns with 47 rows. They're divided into groups:

- Row 1-25: 32-bit PCI
- Row 26-47: Additional pins for 64-bit PCI (System Slot boards must use it).
- Row 26-28 and 40-42: Primarily implemented on System Slot boards.

The following signals must be terminated:

- AD0-31
- C/BE0#-C/BE3#
- PAR
- FRAME#
- IRDY#
- TRDY#
- STOP#
- LOCK#
- IDSEL
- DEVSEL#
- PERR#
- SERR#
- RST#

The following signals must be terminated if used:

- INTA#
- INTB#
- INTC#
- INTD#
- SB0#
- SDOBE
- AD32-AD63
- C/BE4#-C/BE7#
- REQ64#
- ACK64#
- PAR64#

The following signals do no require a stub termination:

- CLK
- REQ#
- GNT#
- TDI#
- TDO
- TCK
- TMS
- TRST#

The System Slot board must pullup the following signals (even if not used):

- REQ64#
- ACK64#

## Connector:

1 | GND | 5V | -12V | TRST# | 12V | 5V | GND
2 | GND | TCK | 5V | TMS | DO | TDI | GND
3 | GND | INTA# | INTB# | INTC# | 5V | INTD# | GND
4 | GND | BRSV | GND | V(I/O) | INTP | INTS | GND
5 | GND | BRSV | BRSV | RST | GND | GNT# | GND
6 | GND | REQ# | GND | 3.3V | CLK | AD(31) | GND
7 | GND | AD(30) | AD(29) | AD(28) | GND | AD(27) | GND
8 | GND | AD(26) | GND | V(I/O) | AD(25) | AD(24) | GND
9 | GND | C/BE(3)# | IDSEL | AD(23) | GND | AD(22) | GND
10 | GND | AD(21) | GND | 3.3V | AD(20) | AD(19) | GND
11 | GND | AD(18) | AS(17) | AD(16) | GND | C/BE(2)# | GND
12 | KEY | KEY | KEY | KEY | KEY | KEY | KEY
13 | KEY | KEY | KEY | KEY | KEY | KEY | KEY
14 | KEY | KEY | KEY | KEY | KEY | KEY | KEY
15 | GND | 3.3V | FRAME# | IRDY# | GND | TRDY# | GND
16 | GND | DEVSEL# | GND | V(I/O) | STOP# | LOCK# | GND
17 | GND | 3.3V | SDONE | SBO# | GND | PERR# | GND
18 | GND | SERR# | GND | 3.3V | PAR | C/BE(1)# | GND
19 | GND | 3.3V | AD(15) | AD(14) | GND | AD(13) | GND
20 | GND | AD(12) | GND | V(I/O) | AD(11) | AD(10) | GND
21 | GND | 3.3V | AD(9) | AD(8) | M66EN | C/BE(0)# | GND
22 | GND | AD(7) | GND | 3.3V | AD(6) | AD(5) | GND
23 | GND | 3.3V | AD(4) | AD(3) | 5V | AD(2) | GND
24 | GND | AD(1) | 5V | V(I/O) | AD(0) | ACK64# | GND
25 | GND | 5V | REQ64# | BRSV | 3.3V | 5V | GND
26 | GND | CLK1 | GND | REQ1# | GNT1# | REQ2# | GND
27 | GND | CLK2 | CLK3 | SYSEN# | GNT2# | REQ3# | GND
28 | GND | CLK4 | GND | GNT3# | REQ4# | GNT4# | GND
29 | GND | V(I/O) | BRSV | C/BE(7 ) | GND | C/BE(6)# | GND
30 | GND | C/BE(5)# | GND | V(I/O) | C/BE(4)# | PAR64 | GND
31 | GND | AD(63) | AD(62) | AD(61) | GND | AD(60) | GND
32 | GND | AD(59) | GND | V(I/O) | AD(58) | AD(57) | GND
33 | GND | AD(56) | AD(55) | AD(54) | GND | AD(53) | GND
34 | GND | AD(52) | GND | V(I/O) | AD(51) | AD(50) | GND
35 | GND | AD(49) | AD(48) | AD(47) | GND | AD(46) | GND
36 | GND | AD(45) | GND | V(I/O) | AD(44) | AD(43) | GND
37 | GND | AD(42) | AD(41) | AD(40) | GND | AD(39) | GND
38 | GND | AD(38) | GND | V(I/O) | AD(37) | AD(36) | GND
39 | GND | AD(35) | AD(34) | AD(33) | GND | AD(32) | GND
40 | GND | BRSV | GND | FAL# | REQ5# | GNT5# | GND
41 | GND | BRSV | BRSV | DEG# | GND | BRSV | GND
42 | GND | BRSV | GND | PRST# | REQ6# | GNT6# | GND
43 | GND | USR | USR | USR | USR | USR | GND
44 | GND | USR | USR | USR | USR | USR | GND
45 | GND | USR | USR | USR | USR | USR | GND
46 | GND | USR | USR | USR | USR | USR | GND
47 | GND | USR | USR | USR | USR | USR | GND
| Z | A | B | C | D | E | F
--- | --- | --- | --- | --- | --- | --- | ---

## Signal Descriptions:

### PRST

Push Button Reset.

### DEG

Power Supply Status DEG

### FAL

Power Supply Status FAL

### SYSEN

System Slot Identification