# Ethernet 10Base-T Crossover Cable

This cable can be used to cascade hubs, or for connecting two Ethernet stations back-to-back without a hub.

(To network interface card 1).
(To network interface card 1).

RJ45 MALE CONNECTOR to network interface card 1.
RJ45 MALE CONNECTOR to network interface card 2.

Name | Pin | Pin | Name
--- | --- | --- | ---
TX+ | 1 | 3 | RX+
TX- | 2 | 6 | RX-
RX+ | 3 | 1 | TX+
RX- | 6 | 2 | TX-