# Minuteman UPS

Is the directions right???

(At the UPS)

9 PIN D-SUB ??? at the UPS.

Pin | Description
--- | ---
1 | Unused
2 | Battery power
3 | Unused
4 | Common (same as 7)
5 | Low battery
6 | RS-232 level shutdown
7 | Common (same as 4)
8 | Ground level shutdown (A500 and above, reserved on >A500)
9 | Reserved

Pins 2 and 5 are connected to Common when they are true.
On pin 6, an rs-232 high level (>9V) will shutdown, when running off the battery.
On pin 8, shorting to ground will shutdown.