# MSX Joystick

(At the computer)
(At the joystick cable)

9 PIN D-SUB MALE at the computer.
9 PIN D-SUB FEMALE at the joystick cable.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | /FORWARD |  | Forward
2 | /BACK |  | Backward
3 | /LEFT |  | Left
4 | /RIGHT |  | Right
5 | +5V |  | +5 VDC (50mA max)
6 | /TRG1 |  | Trigger A / Output 1
7 | /TRG2 |  | Trigger A / Output 1
8 | OUTPUT |  | Output 3
9 | GND |  | Signal Ground