# Ethernet 10Base-T

(At the network interface cards/hubs)
(At the cables)

RJ45 FEMALE CONNECTOR at the network interface cards/hubs.
RJ45 MALE CONNECTOR at the cables.

Pin | Name | Description
--- | --- | ---
1 | TX+ | Trancieve Data+
2 | TX- | Trancieve Data-
3 | RX+ | Receive Data+
4 | n/c | Not connected
5 | n/c | Not connected
6 | RX- | Receive Data-
7 | n/c | Not connected
8 | n/c | Not connected