# Miniature Card

Developed by Intel.
Miniature Card is a memory-only expansion card.

(At the device)
(At the card)

UNKNOWN CONNECTOR at the device.
UNKNOWN CONNECTOR at the card.

Pin | Name | Description | Dir
--- | --- | --- | ---
1 | A18 | Address Bus |
2 | A16 | Address Bus |
3 | A14 | Address Bus |
4 | Vccr | Voltage Refresh |
5 | CEH# | Card Enable High Byte |
6 | A11 | Address Bus |
7 | A9 | Address Bus |
8 | A8 | Address Bus |
9 | A6 | Address Bus |
10 | A5 | Address Bus |
11 | A3 | Address Bus |
12 | A2 | Address Bus |
13 | A0 | Address Bus |
14 | RAS# | Row Address Strobe |
15 | A24 | Address Bus |
16 | A23 | Address Bus |
17 | A22 | Address Bus |
18 | OE# | Output Enable |
19 | D15 | Data Bus |
20 | D13 | Data Bus |
21 | D12 | Data Bus |
22 | D10 | Data Bus |
23 | D9 | Data Bus |
24 | D0 | Data Bus |
25 | D2 | Data Bus |
26 | D4 | Data Bus |
27 | RFU | Reserved for future use |
28 | D7 | Data Bus |
29 | SDA | Serial Data and Address |
30 | SCL | Serial Clock |
31 | A19 | Address Bus |
32 | A17 | Address Bus |
33 | A15 | Address Bus |
34 | A13 | Address Bus |
35 | A12 | Address Bus |
36 | RESET# | Reset |
37 | A10 | Address Bus |
38 | VS1# | Voltage Sense 1 |
39 | A7 | Address Bus |
40 | BS8# | Bus Size 8 |
41 | A4 | Address Bus |
42 | CEL# | Card Enable Low Byte |
43 | A1 | Address Bus |
44 | CASL# | Column Address Strobe Low Byte |
45 | CASH# | Column Address Strobe High Byte |
46 | CD# | Card Detect |
47 | A21 | Address Bus |
48 | BUSY# | Ready/Busy |
49 | WE# | Write Enable |
50 | D14 | Data Bus |
51 | RFU | Reserved for future use |
52 | D11 | Data Bus |
53 | VS2# | Voltage Sense 2 |
54 | D8 | Data Bus |
55 | D1 | Data Bus |
56 | D3 | Data Bus |
57 | D5 | Data Bus |
58 | D6 | Data Bus |
59 | RFU | Reserved for future use |
60 | A20 | Address Bus |

The following three is separate:

Name | Description | Dir
--- | --- | ---
GND | Ground |
VCC | Power |
CINS# | Card Insertion |

Contributor: Joakim Ögren