Getting started with the TVFS is a simple, two step process:

(i)   Extract the zip file to derive the set of TVFS executables.
      Note: the executables are valid for OS/2 2.x only.
(ii)  View the online help (aka the user's guide) via "view TVFS.INF".
      The user's guide provides detailed installation instructions
      and a command summary that should carry you through the rest
      of the way.

Change log:
-----------
2.09   February 23, 1995:
       o Added read only EA support for TVFS-local directories.
         You may now use TVFS drives with the OS/2 Drives Folder!
       o Added a "TvStatus" command to display the TvCtl status.
       o Added a "TvKill" command to terminate the TvCtl daemon.
       o Added a "default option setting" (-D) option to TVCTL.
       o Added a "reuse DOS search handles" (-h) option to TVCTL.
       o Added a "manually connect" (-m) option to TVCTL.
       o Added a "Zen movement" (-z) option to TVCTL.
       o Added a "display the device driver logo" (/LOGO) parameter to TVFS.IFS.
         The logo is now only displayed when requested.
       o The "TvCtl -w" option is now smarter about waiting for a TvCtl instance.
       o The "TvCtl -f" option now returns a more realistic free space value.
         An optional number of free space units (from 1 to 2048) may also be given.
       o Reduced the amount of information copied between Ring 0 and Ring 3.
       o Quadrupled the number of file handles available to TvCtl (256 -> 1024).
       o TVFS drives are automatically unmounted on TvCtl termination.
2.08   March  18, 1994:             
       o EWS Availability.

