      3Com NDIS 2.01 installation notes for Artisoft LANtastic/AI


 To install LANtastic AI version 5.0 as a DOS NDIS workstation, DOS must be
 installed on the target workstation C: drive, or you must have a bootable 
 DOS floppy.  Follow these steps:

 1. Insert the LANtastic/AI Disk # 1 of 2 diskette in drive A:.

 2. Type Install /DOS for a DOS client installation.

 3. A menu will appear.  One of the menu choices allows you to choose for
    which network adapter you want the driver installed.  Pick the default
    adapter.

 4. Copy all of the files from the NDIS Support for LANtastic diskette to the
    C:\LANTASTI subdirectory created in step 3 above.

 5. Copy the ELNK3.DOS driver from the EtherDisk's \NDIS\DOS subdirectory to
    the C:\LANTASTI subdirectory.

 6. Edit CONFIG.SYS to include the following two line anywhere in the file.

        DEVICE=C:\LANTASTI\PROTMAN.DOS /I:C:\LANTASTI
        DEVICE=C:\LANTASTI\ELNK3.DOS

 7. In the LANTASTI subdirectory, edit STARTNET.BAT and modify the adapter
 driver.

      3C503MM                  =====>   AI-NDIS BIND_TO=ETHERLINK3
      AILANBIO                          AILANBIO
      REDIR WS_NAME LOGINS=2            REDIR WS_NAME LOGINS=2


 8. In the LANTASTI subdirectory, edit PROTOCOL.INI to include a section
 for the EtherLink III:

        [PROTMAN]
          DRIVERNAME = PROTMAN$
          DYNAMIC = YES

        [ETHERLINK3]                    <==== ADD
          DRIVERNAME = ELNK3$           <==== ADD


 9. Reboot the machine and use LANtastic as normal.




 %VER LANTASTK.TXT - NDIS 2.01 Lantastic installation notes V 3.4b
