InS_StArT
3C5X9.COM
1.0
^3Com EtherLink III Parallel Tasking Family,3C5X9.COM,IEM
!OIE0 (INT) Interrupt       (ISA/EISA Only)
?You must assign a unique interrupt level for the EtherLink III LAN board.
3
5
7
9
10
11
12
15
!OIE0 (PORT) I/O Base        (ISA/EISA Only)
?You must select the option that matches your board's configuration.
200
210
220
230
240
250
260
270
280
290
2A0
2B0
2C0
2D0
2E0
2F0
300
310
320
330
340
350
360
370
380
390
3A0
3B0
3C0
3D0
3E0
!OIE0 (SLOT) EISA Slot       (ISA/EISA Only)
1
2
3
4
5
6
7
8
9
10
11
12
13
14
15
!O00M (SLOT) MCA Slot        (MCA Only)
1
2
3
4
5
6
7
8
!OIEM (FRAME) Frame Type      (ISA/EISA/MCA)
?Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
