AdapterId 0627Ch

AdapterName "3Com 3C529 Network Adapter"

NumBytes 4

NamedItem

Prompt  "Enable/Disable Adapter"

choice  " adapter enabled "   pos[0]=XXXXXXX1b
choice  " adapter disabled "  pos[0]=XXXXXXX0b

Help
"This controls whether the adapter is enabled or not.
Use the 'enabled' setting for normal use.  Use the
'disabled' setting if you are not using the adapter
and enabling it causes a conflict with another device."


NamedItem

Prompt  "I/O Address Range"

choice  " 200h to 20Fh "    pos[2]=000000XXb  io 0200h-020Fh
choice  " 600h to 60Fh "    pos[2]=000001XXb  io 0600h-060Fh
choice  " A00h to A0Fh "    pos[2]=000010XXb  io 0A00h-0A0Fh
choice  " E00h to E0Fh "    pos[2]=000011XXb  io 0E00h-0E0Fh
choice  " 1200h to 120Fh "  pos[2]=000100XXb  io 1200h-120Fh
choice  " 1600h to 160Fh "  pos[2]=000101XXb  io 1600h-160Fh
choice  " 1A00h to 1A0Fh "  pos[2]=000110XXb  io 1A00h-1A0Fh
choice  " 1E00h to 1E0Fh "  pos[2]=000111XXb  io 1E00h-1E0Fh
choice  " 2200h to 220Fh "  pos[2]=001000XXb  io 2200h-220Fh
choice  " 2600h to 260Fh "  pos[2]=001001XXb  io 2600h-260Fh
choice  " 2A00h to 2A0Fh "  pos[2]=001010XXb  io 2A00h-2A0Fh
choice  " 2E00h to 2E0Fh "  pos[2]=001011XXb  io 2E00h-2E0Fh
choice  " 3200h to 320Fh "  pos[2]=001100XXb  io 3200h-320Fh
choice  " 3600h to 360Fh "  pos[2]=001101XXb  io 3600h-360Fh
choice  " 3A00h to 3A0Fh "  pos[2]=001110XXb  io 3A00h-3A0Fh
choice  " 3E00h to 3E0Fh "  pos[2]=001111XXb  io 3E00h-3E0Fh
choice  " 4200h to 420Fh "  pos[2]=010000XXb  io 4200h-420Fh
choice  " 4600h to 460Fh "  pos[2]=010001XXb  io 4600h-460Fh
choice  " 4A00h to 4A0Fh "  pos[2]=010010XXb  io 4A00h-4A0Fh
choice  " 4E00h to 4E0Fh "  pos[2]=010011XXb  io 4E00h-4E0Fh

Help
"Determines the range of I/O addresses used by the
adapter.  The addresses in this range cannot be used
by another installed device."

NamedItem

Prompt  "Interrupt Request Level"

choice  " level 3 "   pos[3]=XXXX0011b  int 3
choice  " level 5 "   pos[3]=XXXX0101b  int 5
choice  " level 7 "   pos[3]=XXXX0111b  int 7
choice  " level 9 "   pos[3]=XXXX1001b  int 9
choice  " level 10 "  pos[3]=XXXX1010b  int 10
choice  " level 11 "  pos[3]=XXXX1011b  int 11
choice  " level 12 "  pos[3]=XXXX1100b  int 12
choice  " level 15 "  pos[3]=XXXX1111b  int 15

Help
"Determines the interrupt request level used by the
adapter.  This adapter's interrupt level can be shared
with another installed device.  You may be able to
improve performance by selecting a level that is not
used by any other installed device."

 NamedItem

 Prompt  "Boot ROM Address Range"

choice  " disabled "                pos[1]=000000XXb
choice  " C2000h to C3FFFh (8K) "   pos[1]=000001XXb  mem 0C2000h-0C3FFFh
choice  " C4000h to C5FFFh (8K) "   pos[1]=000010XXb  mem 0C4000h-0C5FFFh
choice  " C6000h to C7FFFh (8K) "   pos[1]=000011XXb  mem 0C6000h-0C7FFFh
choice  " C8000h to C9FFFh (8K) "   pos[1]=000100XXb  mem 0C8000h-0C9FFFh
choice  " CA000h to CBFFFh (8K) "   pos[1]=000101XXb  mem 0CA000h-0CBFFFh
choice  " CC000h to CDFFFh (8K) "   pos[1]=000110XXb  mem 0CC000h-0CDFFFh
choice  " CE000h to CFFFFh (8K) "   pos[1]=000111XXb  mem 0CE000h-0CFFFFh
choice  " D0000h to D1FFFh (8K) "   pos[1]=001000XXb  mem 0D0000h-0D1FFFh
choice  " D2000h to D3FFFh (8K) "   pos[1]=001001XXb  mem 0D2000h-0D3FFFh
choice  " D4000h to D5FFFh (8K) "   pos[1]=001010XXb  mem 0D4000h-0D5FFFh
choice  " D6000h to D7FFFh (8K) "   pos[1]=001011XXb  mem 0D6000h-0D7FFFh
choice  " D8000h to D9FFFh (8K) "   pos[1]=001100XXb  mem 0D8000h-0D9FFFh
choice  " DA000h to DBFFFh (8K) "   pos[1]=001101XXb  mem 0DA000h-0DBFFFh
choice  " DC000h to DDFFFh (8K) "   pos[1]=001110XXb  mem 0DC000h-0DDFFFh
choice  " DE000h to DFFFFh (8K) "   pos[1]=001111XXb  mem 0DE000h-0DFFFFh
choice  " C0000h to C3FFFh (16K) "  pos[1]=010001XXb  mem 0C0000h-0C3FFFh
choice  " C4000h to C7FFFh (16K) "  pos[1]=010010XXb  mem 0C4000h-0C7FFFh
choice  " C8000h to CBFFFh (16K) "  pos[1]=010100XXb  mem 0C8000h-0CBFFFh
choice  " CC000h to CFFFFh (16K) "  pos[1]=010110XXb  mem 0CC000h-0CFFFFh
choice  " D0000h to D3FFFh (16K) "  pos[1]=011000XXb  mem 0D0000h-0D3FFFh
choice  " D4000h to D7FFFh (16K) "  pos[1]=011010XXb  mem 0D4000h-0D7FFFh
choice  " D8000h to DBFFFh (16K) "  pos[1]=011100XXb  mem 0D8000h-0DBFFFh
choice  " DC000h to DFFFFh (16K) "  pos[1]=011110XXb  mem 0DC000h-0DFFFFh
choice  " C0000h to C7FFFh (32K) "  pos[1]=100001XXb  mem 0C0000h-0C7FFFh
choice  " C8000h to CFFFFh (32K) "  pos[1]=100100XXb  mem 0C0000h-0C7FFFh
choice  " D0000h to D7FFFh (32K) "  pos[1]=101000XXb  mem 0D0000h-0D7FFFh
choice  " D8000h to DFFFFh (32K) "  pos[1]=101100XXb  mem 0D0000h-0D7FFFh


Help
"Determines the range of addresses used by the boot
PROM installed on the adapter.  The addresses in this
range cannot be used by any other installed device
or software.  The size of the address range must
correspond with the size of the boot ROM.  Select
'disabled' if no boot ROM is installed."


NamedItem

Prompt  "Transceiver Type"

choice	" on-board (BNC) "   pos[2]=XXXXXX11b
choice	" external (AUI) "   pos[2]=XXXXXX01b

Help
"Determines the type of transceiver used by the
adapter.  If you wish to connect to the adapter's
BNC connector, select 'on-board'.  If you wish
to attach a drop cable from an external
transceiver to the adapter's 15-pin AUI connector,
select 'external'."

; %VER 3C529 MCA Configuration File v1.0a
