
SyntaxVersion: 1.00

  ; File: AHA1540.INF

    Driver AHA1540
    {
	Description:	$AHA1540_1

	Help:		$AHA1540_2

	File:		 AHA1540.DSK
	OFiles: 	 ASPITRAN.DSK



	PROMPT PORT REQUIRED
	{
	    Values:		330, 334, 234, 230, 134, 130
	    Default:		330
	    ReservedLength:	4
	}

    }


DLANG:	4
;English
	$AHA1540_1 = "Adaptec AHA-1540/42 SCSI & ASPI Module"
	$AHA1540_2 = "When you load the driver, you need to tell it which
			 host adapter you are loading the driver for.  This is
			 done with the command line option 'port=xxx'.  If the
			 option is not entered, you will be prompted to manually
			 enter a value.  The interrupt level and dma channel may
			 also be specified with a command line option.	If not,
			 the driver will read this information from the adapter
			 and pass it to the Netware operating system."

LANG:	6
;French
	$AHA1540_1 = "Adaptec AHA-1540/42 SCSI & ASPI Module"
	$AHA1540_2 = "When you load the driver, you need to tell it which
			 host adapter you are loading the driver for.  This is
			 done with the command line option 'port=xxx'.  If the
			 option is not entered, you will be prompted to manually
			 enter a value.  The interrupt level and dma channel may
			 also be specified with a command line option.	If not,
			 the driver will read this information from the adapter
			 and pass it to the Netware operating system."

LANG:	7
;German
	$AHA1540_1 = "Adaptec AHA-1540/42 SCSI & ASPI Module"
	$AHA1540_2 = "When you load the driver, you need to tell it which
			 host adapter you are loading the driver for.  This is
			 done with the command line option 'port=xxx'.  If the
			 option is not entered, you will be prompted to manually
			 enter a value.  The interrupt level and dma channel may
			 also be specified with a command line option.	If not,
			 the driver will read this information from the adapter
			 and pass it to the Netware operating system."

LANG:	8
;Italian
	$AHA1540_1 = "Adaptec AHA-1540/42 SCSI & ASPI Module"
	$AHA1540_2 = "When you load the driver, you need to tell it which
			 host adapter you are loading the driver for.  This is
			 done with the command line option 'port=xxx'.  If the
			 option is not entered, you will be prompted to manually
			 enter a value.  The interrupt level and dma channel may
			 also be specified with a command line option.	If not,
			 the driver will read this information from the adapter
			 and pass it to the Netware operating system."

LANG:	14
;Spanish
	$AHA1540_1 = "Adaptec AHA-1540/42 SCSI & ASPI Module"
	$AHA1540_2 = "When you load the driver, you need to tell it which
			 host adapter you are loading the driver for.  This is
			 done with the command line option 'port=xxx'.  If the
			 option is not entered, you will be prompted to manually
			 enter a value.  The interrupt level and dma channel may
			 also be specified with a command line option.	If not,
			 the driver will read this information from the adapter
			 and pass it to the Netware operating system."
