
SyntaxVersion: 1.00

  ; File: AIC7870.INF

    Driver AIC7870
    {
        Description:  $AIC7870_1

        Help:         $AIC7870_2

        File:         AIC7870.DSK
        OFiles:       ASPITRAN.DSK

    }


DLANG:	4
;English
	$AIC7870_1 = "Adaptec AIC-7870 ASPI & SCSI Module"
	$AIC7870_2 = "When you load the driver, you need to tell it which
                      host adapter you are loading the driver for. This is
                      done with the command line option 'slot=x'. If the
                      option is not entered, you will be prompted to manually
                      enter a value. The interrupt level will be determined 
                      from the PCI configuration."

LANG:	6
;French
	$AIC7870_1 = "Adaptec AIC-7870 ASPI & SCSI Module"
	$AIC7870_2 = "When you load the driver, you need to tell it which
                      host adapter you are loading the driver for. This is
                      done with the command line option 'slot=x'. If the
                      option is not entered, you will be prompted to manually
                      enter a value. The interrupt level will be determined 
                      from the PCI configuration."

LANG:	7
;German
	$AIC7870_1 = "Adaptec AIC-7870 ASPI & SCSI Module"
	$AIC7870_2 = "When you load the driver, you need to tell it which
                      host adapter you are loading the driver for. This is
                      done with the command line option 'slot=x'. If the
                      option is not entered, you will be prompted to manually
                      enter a value. The interrupt level will be determined 
                      from the PCI configuration."

LANG:	8
;Italian
	$AIC7870_1 = "Adaptec AIC-7870 ASPI & SCSI Module"
	$AIC7870_2 = "When you load the driver, you need to tell it which
                      host adapter you are loading the driver for. This is
                      done with the command line option 'slot=x'. If the
                      option is not entered, you will be prompted to manually
                      enter a value. The interrupt level will be determined 
                      from the PCI configuration."

LANG:	14
;Spanish
	$AIC7870_1 = "Adaptec AIC-7870 ASPI & SCSI Module"
	$AIC7870_2 = "When you load the driver, you need to tell it which
                      host adapter you are loading the driver for. This is
                      done with the command line option 'slot=x'. If the
                      option is not entered, you will be prompted to manually
                      enter a value. The interrupt level will be determined 
                      from the PCI configuration."
