;DrIvEr DeScRiPtIoN

SyntaxVersion: 1.00

  ; File: AHA1510.INF

    Driver AHA1510
    {
	Description:	"Adaptec AHA-1510/AIC-6x60 ASPI Manager & SCSI Disk Module"

	Help:		"When you load the driver, you need to tell it which
			 host adapter you are loading the driver for.  This is
			 done with the command line option 'port=xxx'.  The
			 interrupt level also may be specified with a command
			 line option, and the host adapter must be jumpered
			 accordingly for the interrupt selection. If either
			 are not specified, you will be prompted to manually
			 enter a value."


	File:		 AHA1510.DSK
	OFiles:		 ASPITRAN.DSK


	PROMPT PORT REQUIRED
	{
	    Values:		340, 140
	    Default:		340
	    ReservedLength:	8
	}

	PROMPT INT REQUIRED
	{
		Type:	DECIMAL(2)
	    Values:		9, 10, 11, 12
	    Default:		11
	}

    }

;DrIvEr DeScRiPtIoN EnD
