
SyntaxVersion: 1.00

  ; File: AIC7770.INF

    Driver AIC7770
    {
        Description:    $AIC7770_1

        Help:           $AIC7770_2

        File:            AIC7770.DSK
        OFiles:          ASPITRAN.DSK

        PROMPT SLOT REQUIRED
        {
            Values:             1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
        }

    }


DLANG:	4
;English
	$AIC7770_1 = "Adaptec AIC-7770 ASPI & SCSI Module"
	$AIC7770_2 = "When you load the driver, you need to tell it which
                        host adapter you are loading the driver for. This is
                        done with the command line option 'slot=x'. If the
                        option is not entered, you will be prompted to manually
                        enter a value. The interrupt level and dma channel will
                        be determined from the host adapter settings."

LANG:	6
;French
	$AIC7770_1 = "Adaptec AIC-7770 ASPI & SCSI Module"
	$AIC7770_2 = "When you load the driver, you need to tell it which
                        host adapter you are loading the driver for. This is
                        done with the command line option 'slot=x'. If the
                        option is not entered, you will be prompted to manually
                        enter a value. The interrupt level and dma channel will
                        be determined from the host adapter settings."

LANG:	7
;German
	$AIC7770_1 = "Adaptec AIC-7770 ASPI & SCSI Module"
	$AIC7770_2 = "When you load the driver, you need to tell it which
                        host adapter you are loading the driver for. This is
                        done with the command line option 'slot=x'. If the
                        option is not entered, you will be prompted to manually
                        enter a value. The interrupt level and dma channel will
                        be determined from the host adapter settings."

LANG:	8
;Italian
	$AIC7770_1 = "Adaptec AIC-7770 ASPI & SCSI Module"
	$AIC7770_2 = "When you load the driver, you need to tell it which
                        host adapter you are loading the driver for. This is
                        done with the command line option 'slot=x'. If the
                        option is not entered, you will be prompted to manually
                        enter a value. The interrupt level and dma channel will
                        be determined from the host adapter settings."

LANG:	14
;Spanish
	$AIC7770_1 = "Adaptec AIC-7770 ASPI & SCSI Module"
	$AIC7770_2 = "When you load the driver, you need to tell it which
                        host adapter you are loading the driver for. This is
                        done with the command line option 'slot=x'. If the
                        option is not entered, you will be prompted to manually
                        enter a value. The interrupt level and dma channel will
                        be determined from the host adapter settings."
