B)uffer       : Turn capture buffer 
C)onfigure    : Set up the com port parameters.
D)ial         : Dial a number.
E)xecute DOS  : Shell to DOS.
I)initialize  : Initialize the modem.
R)eceive      : Receive a file using an external protocol.
S)end         : Send a file using an external protocol.
T)erminal     : Terminal mode.
X)fer         : Transfer a file using DWXFER.
Q)uit         : Quit DWCOMM, and return to DOS.
(presently
OFF
ON
DWCOMM, at your service.
Enter one of the following valid commands:
Command:
DWCOMM Configuration Editor
COM PORT:
(LOCAL, COM:1-COM:4 or PORT:XXXX:Y)
Capture filename:
Opening Baud Rate:
Com port Locked?
Initialization String:
Number to Dial
Send HOST LPT1 to:
Send HOST LPT2 to:
Send HOST LPT3 to:
TONE:
PULSE:
Do you wish to Q)uit, E)xit or C)ontinue?
Quit without saving changes.
Exit and save the changes.
Continue editing the configuration file.
Enter filename (with path) to send:
Enter number to dial:
Dialing
Attempt
Modem:
Enter ESC to abort.
DWCOMM TERMINAL MODE
Press both shift keys at once to return to command mode.
