************************************************************************
*  This is version 1.0 of Telix.MDM, Modem Definitions dated 04/02/91  *
*  for Telix 3.15.    Please do not modify this file -- it is NOT a    *
*  text file and the program will not work properly if you try to make *
*  adjustments.   It will be updated often, so if you do think that a  *
*  setting might be in error, please contact Exis at 416-289-4641 by   *
*  voice, 416-439-9399 by modem (HST Dual Standard v.32), or by fax    *
*  at 416-289-4645.    Direct comments to Jeff Woods, Tech Support.    *
************************************************************************
÷Anchor
Anchor 2400i Internal Half-Card
240
"N"
8
1
On
Off
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL
40
ATZ^M~
ATE1Q0M1X4V1S7=60S11=60
AT&C1&D2S0=0
AT&W
0

Your Anchor 2400i Internal Half Card is now configured
for best performance with Telix 3.15.

Options might be to add M0 in your modem init string
to silence your speaker if you prefer.

÷AST
AST 2X9600
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL
40
ATZ^M
AT&FV1Q0
AT\J0\Q3\V1&C1&D2\N3
AT&W
10
See Ending Comments
Your AST modem is now configured for best performance with
Telix 3.15.    Set ALL dialing directory entries to 19,200
to get the most out of your modem.

Front Switches: 1 2 3 4 5 6 7 8   Rear: 1 2 3 4 5 6 7
                U D D U D U U D         D D D U D U U
÷AT&T
AT&T Model 4000
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL
30
ATV1E1Q0X2S7=45S0=0^M



0

Your AT&T modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷ATI
ATI 2400etc without v.42
960
"N"
8
1
On
On
Off
Off
Off
AT&Q5DT
AT&Q0DT
ATDT
NO DIALTONE
40
ATZ^M
AT&F1V1Q0
AT&C1&D2X4S11=60S7=60S9=10S10=18
AT&W
0

Your ATI modem is now set up for best perfomance with Telix
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 9600 bps for best performance.

Use Dialing Prefix 1 for calling error-correcting systems.
Use Dialing Prefix 2 for calling non-errorcorrecting systems.
ATI 2400etc with v.42
960
"N"
8
1
On
On
Off
Off
Off
AT&Q6DT
AT&Q0DT
ATDT
NO DIAL TONE
40
ATZ^M
AT&F2V1Q0
AT&C1&D2X4S11=60S7=60S9=10S10=18
AT&W
0

Your ATI modem is now set up for best perfomance with Telix
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 9600 bps for best performance.

Use Dialing Prefix 1 for calling error-correcting systems.
Use Dialing Prefix 2 for calling non-errorcorrecting systems.
ATI 9600etc/e v.32/v.42
3840
"N"
8
1
On
On
Off
Off
Off
AT&Q6DT
AT&Q0DT
ATDT
NO DIAL TONE
40
ATZ^M
AT&F2V1Q0
AT&C1&D2X4S11=60S7=60S9=10S10=18
AT&W
0

Your ATI modem is now set up for best perfomance with Telix
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 38400 bps for best performance.

Use Dialing Prefix 1 for calling error-correcting systems.
Use Dialing Prefix 2 for calling non-errorcorrecting systems.
÷Avatech
Avatech 2400E
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X4&C1&D2S7=55S11=60S0=0^M



0

Your Avatech modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷BSM
BSM Quick Comm 2400 MNP
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT\Q3\J0\N3%C1&C1&D2S7=55S0=0
AT&W
0

Your BSM modem is now set up for best perfomance with Telix
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 9600 bps for best performance.



÷Cardinal
Cardinal 2400 MNP-5
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT \Q3\N3\J0\C1S0=0&C1&D2\V1\K3&T5\C1
AT&W
0

Your Cardinal modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



÷Cermetek
Cermetek InfoMate 212a
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL
30
ATV1E1Q0X2S7=45S0=0^M



8
U D D U U D U D
Your Cermetek modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Cermetek R/2400 SPC
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
AT E1 Q0 V1 X4 S7=55 S11=60 S0=0^M



8
U D D U U D U D
Your Cermetek modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Cermetek 1200 SPC
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
AT E1 Q0 V1 X2 S7=55 S11=60 S0=0^M



8
U D D U U D U D
Your Cermetek modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Codex
Codex 2264
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
AT&C1&D2*FL3*XC1*PT0&R0
AT&W
0

Your Codex modem is now configured for best performance with
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 19200 bps for best performance.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.
÷CompuCom
CompuCom Speedmodem CSP
1920
"N"
8
1
Off
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&F2V1Q0
AT&C1&D3*H2
AT&W
0

Your CompuCom modem is now configured for best performance
with 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.
÷CTS
CTS Companion 212AH
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
Disconnect
40
ATE1Q0V1S7=55S11=60S0=0^M



0

Your CTS modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

CTS Datacomm 2424ADH
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT^C1&D2S0=0S2=255S10=30X4
AT&W
0

Your CTS modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Delta Gold
Delta Gold DM 1200
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X4 S7=55 S11=60 S0=0^M



0

Your Delta modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Digicom
DSI 9624LE (v.32 bis)
3840
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT&C1*F3&R0
AT&W
0

Your DigiCom modem is now configured for best performance
with 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 38400 bps for best performance.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.
DSI 9624PC (v.32 bis)
3840
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT&C1*F3&R0
AT&W
0

Your DigiCom modem is now configured for best performance
with 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 38400 bps for best performance.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.
÷Everex
Everex 12e External (EV-936)
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X1 S7=55 S11=60 S0=0^M



0

Your Everex modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Everex 24e External (EV-945)
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X4&C1&D2 S7=55 S11=60 S0=0^M



0

Your Everex modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Evercom 24+ (MNP)
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ0^M~~~AT S7=55 S11=60^M
AT&FV1Q0
AT Q0 V1 X4 &C1 &D2 \Q3 \C1 \N3 \J0 \V1
AT&W0
0

Your Everex modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



Everex Everfax 24/96
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ0^M~~~AT S7=55 S11=60^M
AT&FV1Q0
ATX4&C1&D2\Q3\C1\N3\J0\V1%C1&T5
AT&W0
0

Your Everex fax/modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



÷FastComm
FastComm FDX 2424 (MNP-5)
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
ATE1X4S7=60&C1&D2&B1&G0*H1&I1&M6
AT&W
8
All of them OFF
Your FastComm modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



FastComm 2496 Turbo
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
DATA TIME OUT
40
ATZ^M
AT&FV1Q0
ATE1X4S7=60&C1&D2&B1&G0*H1&I1&M6
AT&W
8
All of them OFF
Your FastComm modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



FastComm 9696 (v.32)
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
DATA TIME OUT
40
ATZ^M
AT&FV1Q0
ATE1X4S7=60&C1&D2&B1&G0*H1&I1&M6
AT&W
8
All of them OFF
Your FastComm fax/modem is now set up for best perfomance
with Telix 3.15.

Compression is enabled, so set ALL of your dialing directory
entries to 19200 bps for best performance.

÷Generic
1200 bps without switches
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X1S7=55S11=60S0=0^M



0

Your modem is now configured for best performance with Telix.


An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

1200 bps with switches
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X1S7=55S11=60S0=0^M



8
U U D U D U U D
Your modem is now configured for best performance with Telix.


An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

2400 bps without switches
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
AT&C1&D2E1Q0V1X1S7=55S11=60S0=0^M



0

Your modem is now configured for best performance with Telix.


An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

2400 bps with switches
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X1S7=55S11=60S0=0^M



8
U U D U D U U D
Your modem is now configured for best performance with Telix.


An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷GVC
GVC 9600 v.42
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
AT&C1&D2%C1\Q3\J0\N3\V1
AT&W
0

Your GVC modem is now configured for best performance with
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 19200 bps for best performance.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.
÷Hayes
Smartmodem 1200 External
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
 
40
AT E1 Q0 V1 X1 S7=55 S11=60 S0=0^M



10
U U D U D U U D U U
Your Hayes modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Smartmodem 1200B Half Card
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
 
40
AT E1 Q0 V1 X1 S7=55 S11=60 S0=0^M



8
X X U U X X X X
Your Hayes modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Smartmodem 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
AT E1Q0V1X4&C1&D2 S7=55 S11=60 S0=0^M



0

Your Hayes modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Hayes Personal Modem 1200
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
AT E1 Q0 V1 X4 &C1 &D2 S0=0^M



0

Your Hayes modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Hayes Personal Modem 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
AT E1 Q0 V1 X4 &C1 &D2 S0=0^M



0

Your Hayes modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Hayes V-Series 2400
480
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ0^M AT &Q5 S36=3^M
AT&FV1Q0
AT &C1 &D2 &K3 S7=55 S11=60
AT&W0
0

Your Hayes modem is now set up for best perfomance with Telix
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 4800 bps for best performance.



Hayes V-Series 9600
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
AT &C1&D2S7=55S11=60
AT&W
0

Your Hayes modem is now set up for best perfomance with Telix
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 19200 bps for best performance.



Hayes V-Series 9600 with v.42
3840
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ0^M AT &Q5 S36=3^M
AT&FV1Q0
AT &C1&D2&K3S7=55S11=60
AT&W0
0

Your Hayes modem is now set up for best perfomance with Telix
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 38400 bps for best performance.



Hayes Ultra-Smartmodem
3840
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ0^M
AT&FV1Q0
AT &C1&D2S7=55S11=60
AT&W0
0

Your Hayes modem is now set up for best perfomance with Telix
3.15.   Compression is enabled, so set ALL of your dialing
directory entries to 38400 bps for best performance.



÷IBM
IBM Model 5841 (1200)
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
 
40
ATE1Q0V1S7=55S11=60S0=0^M



0

Your IBM modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

IBM PC 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X4&C1&D2 S7=55 S11=60 S0=0^M



0

Your IBM modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

IBM PCjr Internal
30
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
^NF 4^M



0

Your IBM modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Infomate
Infomate 212/A PC
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL
40
ATE1V1Q0 S7=55 S11=60 S0=0^M



0

Your Infomate modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Infomate 212/X PC
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1 S7=55 S11=60 S0=0^M



0

Your Infomate modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Intel
Intel 2400EX
480
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
AT\Q3\N3\J0\V1\C1 S11=60
AT&W
0

Your Intel modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Intel 9600EX (v.32/v.42bis)
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
AT \Q3\N3\J0\V1\C1S11=60
AT&W
0

Your Intel modem is now set up for best perfomance with
Telix 3.15.

Compression is enabled, so set ALL of your dialing directory
entries to 19200 bps for best performance.

Intel SatisFAXion
480
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ0^M
AT&F
AT \C1 S11=60
AT&W0
0

Your Intel modem/fax is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 4800 bps for best performance.



÷Maxwell
Maxwell Modem 300/V
30
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
 
40
AT E1 Q0 V1 S0=0^M



0

Your Maxwell modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Maxwell Modem 1200VP
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
AT E1 Q0 V1 X4 &C1 &D2 S7=55 S0=0^M



0

Your Maxwell modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Maxwell Modem 2400PC
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
AT E1 Q0 V1 S7=30 S0=0^M



0

Your Maxwell modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Megahertz
MHz EasyTalk 1200
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
AT E1 Q0 V1 S7=55 S11=60 S0=0^M



0

Your Megahertz modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

MHz EasyTalk 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
AT E1Q0V1X4&C1&D2S7=55S11=60S0=0^M



0

Your Megahertz modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Microcom
Microcom AX1200/AX2400
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT\J0\Q3\N3S0=0%C1
AT&W
10
See Ending Comments
Your MicroCom modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.

Rear Switches:  1 2 3 4 5 6 7 8  Front: 1 2 3 4 5 6 7 8 9 10
                D D D U D U D D         U D D D D U U D U U
Microcom AX9612c/AX9624c
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT\J0\Q3\N3S0=0
AT&W
10
See Ending Comments
Your MicroCom modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.

Rear Switches:  1 2 3 4 5 6 7 8  Front: 1 2 3 4 5 6 7 8 9 10
                D D D U D U D D         U D D D D U U D U U
Microcom QXv.32c/4232hs
3840
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT\J0\Q3\N3%C3Q2S7=55S0=0
AT&W
10
See Ending Comments
Your MicroCom modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 38400 bps for best performance.

Rear Switches:  1 2 3 4 5 6 7 8  Front: 1 2 3 4 5 6 7 8 9 10
                D D D U D U D D         U D D U D U U D   U
÷MultiTech
MultiModem 224 PC
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X4&C1&D2 S7=55 S11=60 S0=0^M



0

Your MultiTech modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

MultiModem 224 EC (MNP)
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
ATQ0&E1&E4&E7&E13&E15
AT$SB9600$BA0$A1$I1$R1&W
0

Your Multitech modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



MultiModem MT224EH5/EH7
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
ATQ0&E1&E4&E7&E13&E15
AT$SB9600$BA0$A1$I1$R1&W
10
See Ending Comments
Your Multitech modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.

4 Switch set : 1 2 3 4   8 Switch Set:  1 2 3 4 5 6 7 8
               D U D D                  U U D U D U U D
MultiModem v.32
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
ATB0&E1&E4&E7&E13
ATX4$SB19200$BA0$A1S7=55S11=60S0=0&W
10
See Ending Comments
Your Multitech modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.

4 Switch set : 1 2 3 4   8 Switch Set:  1 2 3 4 5 6 7 8
               D U D D                  U U D U D U U D
MultiModem 696E
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0&D2$EP1$F1&Q0&E15&E10
AT&B0&E1&E4&E8&E13$MB9600&BS0$D0&C1
ATX4$SB19200$BA0$A1S7=55S11=60S0=0&W0
0

Your Multitech modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.



MultiModem 932EC
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&F
ATB0&E1&E4&E8&E10&E13&E15
ATX4$SB19200$MB9600$BA0&W
0

Your Multitech modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.



÷NEC
NEC 2431c
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT&C1&D2&E1S7=55S11=60
AT&W
0

Your NEC 2431c modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



NEC N9631 v.32
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&F2V1Q0
AT&T5\Q3\X1\V1*FT1
AT&W
0

Your NEC 9631c modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.



÷Novation
Novation Professional 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO TONE
40
ATE1Q0V1X3YC0YF1YT0 S7=45 S0=0^M



0

Your Novation modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Okidata
OkiTel 2400 Plus
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ0^M
AT&FV1Q0
AT &C1&D2 \V1 \N3 \Q3 \J0 \C1
ATS7=55S11=60&W0&Y0
0

Your Okidata modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



OkiTel 1200
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1 S7=55 S11=60 S0=0^M



0

Your Okidata modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

OkiTel 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X4&C1&D2 S7=55 S11=60 S0=0^M



0

Your Okidata modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

OkiTel 9600
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
AT&C1&D2
AT&W
0

Your Okidata modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.



÷Penrill Alliance
Penrill Alliance v.32
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
AT&C1&D2\Q1,1
AT&W
0

Your Penrill modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.



÷Practical Periph'l
Practical PM 1200
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1 S7=55 S11=60 S0=0^M



0

Your Practical modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Practical PM 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X4&C1&D2 S11=60 S0=0 S7=55^M



0

Your Practical modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Practical PM 2400 SA
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ0^M ATS7=55 S11=60^M
AT&FV1Q0E1X4
AT&C1&D2\Q3\N3\J0\V1
AT&W0
0

Your Practical modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



Practical PM 9600 SA v.32
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ0^M
AT&FV1Q0
AT&C1&D2
AT&W0&Y0
0

Your Practical modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.



÷Prometheus
Prometheus Pro 1200
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1 S7=55 S11=60 S0=0^M



0

Your Prometheus modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Prometheus MCT-24I Half Card
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X4&C1&D2 S7=55 S11=60 S0=0^M



0

Your Prometheus modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Prometheus 9600
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
AT&F^M~~~AT*F3^M



0

Your Prometheus modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.



÷Racal Vadic
Racal Milgo RMD 3221
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
AT&F^M ATX9&C1&D2*F2 S7=55 S11=60 S0=0^M



0

Your Racal-Vadic modem is now set up for best perfomance
with Telix 3.15.

Compression is enabled, so set ALL of your dialing directory
entries to 9600 bps for best performance.

Racal Vadic 1200 PA
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
AT&F^M~~~AT &C1&D2^M



0

Your Racal-Vadic modem is now set up for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Racal Vadic 2400 PS
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ0^M~~~AT S7=55 S11=60^M
AT&FV1Q0
AT*F2&C1&D2*E1
AT&W0
0

Your Racal-Vadic is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Racal Vadic 2400 LC
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ0^M~~~AT S7=55 S11=60^M
AT&FV1Q0
AT &C1&D2 *E1*F2*P1S7=55S11=60
AT&W0
0

Your Racal-Vadic is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Racal Vadic LC2400 PC
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M~~~ATS7=55S11=60



0

Your Racal-Vadic is now set up for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Racal Vadic 2400 PA Model 2
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M~~~AT S7=55 S11=60^M
AT&FV1Q0
AT &C1&D2 X4 *E1*L1*Q1*F2*P1
AT&W
0

Your Racal-Vadic is now set up for best performance with
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Racal Vadic 2400 VP
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT &C1*C1&D2*E1*F2Y1S7=55*Q1S11=60
AT&W
0

Your Racal-Vadic modem is now set up for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Racal Vadic 9600 PA
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M~~~ATS7=55^M
AT&FV1Q0
AT&C1*C1&D2*F2Y1*Q1
AT&W
0

Your Prometheus modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



÷Supra
Supra Modem 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X4 &C1&D2 S7=55 S11=60 S0=0^M



0

Your Supra modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Sysdyne
Sysdyne MDM 24H
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X4&C1&D2S7=55S11=60S0=0^M



0

Your Sysdyne modem is now configured for best performance
with Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

÷Telebit
Telebit T1500
960
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
ATS51=4S0=0S52=1S131=1
ATS58=2S66=1S68=2&W
0

Your Telebit modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



Telebit T2000
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
ATS11=55S52=1S53=1S58=2S66=1S68=2
ATS95=2S110=1&W
0

Your Telebit modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.

Note that this assumed you were in Enhanced command mode. If
you were not, please refer to your manual and redo MODEMCFG.
Telebit T2500
19200
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
AT&C1&D2&G0&J0&K3&L0&P0&Q5
AT&W
0

Your Telebit modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.

Note that this assumed you were in Conventional command
mode. If not, please refer to your manual and redo MODEMCFG.
Telebit Trailblazer Plus
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
ATS11=55S52=1S53=1S58=2S66=1S68=2
ATS95=2S110=1&W
0

Your Telebit modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.

Note that this assumed you were in Enhanced command mode. If
you were not, please refer to your manual and redo MODEMCFG.
÷UDS
UDS Fast Talk 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X4&C1&D2 S7=55 S0=0^M



0

Your UDS modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

UDS v.32
1920
"N"
8
1
On
On
Off
Off
Off
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT&C1&D2&R&T5\Q3\V1%C1
AT&W
0

Your UDS modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.



÷US Robotics
USR 1200 PC Internal
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X1S7=55S11=60S0=0^M



0

Your USR modem is now configured for best performance with
Telix 3.15.  Set the jumpers as:  J1: Up  J2: Up  J3: Down
and J14:  Up      All switches should be off.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.
USR Password 1200
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATE1Q0V1X1S7=55S11=60S0=0^M



0

Your USR modem is now configured for best performance with
Telix 3.15.  Set the jumpers as:  J1: Up  J2: Up  J3: Right
and J5:  Down      All switches should be Up.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.
USR Sportster 1200
120
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X2 S7=55 S11=60 S0=0^M



10
U U D U D U U D
Your USR modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

USR Sportster 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X6&C1&D2 S7=55 S11=60 S0=0^M



8
U U D U D U U D
Your USR modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

USR MicroLink 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X6&C1&D2 S7=55 S11=60 S0=0^M



10
U U D U D U U D D D
Your USR modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

USR VARmodem 2400
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1Q0V1X6&C1&D2 S7=55 S11=60 S0=0^M



10
U U D U D U U D D D
Your USR modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

USR Courier HST 9600
1920
"N"
8
1
On
On
Off
Off
Off
AT&M4DT
AT&M0DT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
AT&K0X6&B1&H1&R2S7=55S11=60
AT&W
10
U U D U D U U D D D
Your USR modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.

Use Dialing prefix 1 for calling MNP-equipped systems.
Use Dialing prefix 2 for calling non-MNP systems.
USR Courier HST 14400
1920
"N"
8
1
On
On
Off
Off
Off
AT&M5DT
AT&M0DT
ATDT
NO DIAL TONE
40
ATZ^M
AT&F
ATX6&K0&B1&H1&R2S7=55S11=60
AT&W
10
U U D U D U U D D D
Your USR modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.

Use Dialing prefix 1 for calling MNP-equipped systems.
Use Dialing prefix 2 for calling non-MNP systems.
USR Courier HST 14400 v.42
3840
"N"
8
1
On
On
Off
Off
Off
AT&M4DT
AT&M0DT
ATDT
NO DIAL TONE
40
ATZ^M
AT&F
ATX6&B1&H1&R2&M4&A3S7=55S11=60
AT&W
10
U U D U D U U D D D
Your USR modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 38400 bps for best performance.

Use Dialing prefix 1 for calling MNP-equipped systems.
Use Dialing prefix 2 for calling non-MNP systems.
USR Courier HST Dual Standard
3840
"N"
8
1
On
On
Off
Off
Off
AT&M5DT
AT&M0DT
ATDT
NO DIAL TONE
40
ATZ^M
AT&F
ATX6&B1&H1&R2S7=55S11=60
AT&W
10
U U D U D U U D D D
Your USR modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 38400 bps for best performance.

Use Dialing prefix 1 for calling MNP-equipped systems.
Use Dialing prefix 2 for calling non-MNP systems.
USR Courier v.32bis
1920
"N"
8
1
On
On
Off
Off
Off
AT&M4DT
AT&M0DT
ATDT
NO DIAL TONE
40
ATZ^M
AT&F
ATX6&H1&R2&B7
AT S7=55S0=0
10
U U D U D U U D D D
Your USR modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 19200 bps for best performance.

Use Dialing prefix 1 for calling MNP-equipped systems.
Use Dialing prefix 2 for calling non-MNP systems.
÷Ventel
Ventel 2400 Internal
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATE1 Q0 V1 X4 S7=30 S0=0^M



0

Your Ventel modem is now configured for best performance
with Telix 3.15.


If there are four switches, see your manual to set the comm
port.   If there are six, set 1 and 5 open, and 2 closed.
Ventel 2400-33
960
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT %A13B1\C1&C1\D3&D2E1F1V1Q0\G0&G0
AT &L0&M0\N3Q0\Q3&R1\T0&T4V1
AT \V1X4\X1T0&W
10
See Ending Comments
Your Ventel modem is now configured for best performance
with Telix 3.15.  Set all dialing directory entries to 9600
for best performance as compression is enabled.

Switch Block:  1   2   3   4   5   6   7   8   9   10
              OFF OFF OFF OFF OFF OFF ON  ON  ON  OFF
Ventel Pathfinder
1920
"N"
8
1
On
On
Off
Off
On
ATDT
ATDT
ATDT
NO DIAL TONE
40
ATZ^M
AT&FV1Q0
ATS51-5S54=3S58=2S66=1S68=2S92=1
ATS95=2S111=0&W
0

Your Ventel modem is now set up for best performance with
Telix 3.15.  An option might be to add M0 to the modem
initial string to silence your modem if you prefer.

Compression is enabled so set all dialing directory entries
to 19200 for best performance.
÷Zoom
Zoom 2400 w/ optional fax
240
"N"
8
1
On
Off
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
ATE1X1S7=55S11=60S0=0&C1&D2^M
AT&W

0

Your Zoom modem is now configured for best performance with
Telix 3.15.

An option might be to add M0 to the modem initial string to
silence your modem if you prefer.

Zoom HC2400R with v.42bis
960
"N"
8
1
On
On
Off
Off
On
ATDT
ATDT
ATDT
NO DIALTONE
40
ATZ^M
AT&FV1Q0
ATS11=60S0=0&C1&D2S36=7S38=0S95=44^M
AT&W

0

Your Zoom modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 9600 bps for best performance.



÷ZyXEL
ZyXEL U-1496 MODELS
3840
"N"
8
1
Off
On
Off
Off
Off
ATDP
ATDP
ATDP
NO DIAL TONE
90
ATZ^M
AT&F
ATE1X6&B1&H3&K4&D2S7=60S11=60
AT&W
10

Your ZyXEL modem is now set up for best perfomance with
Telix 3.15.   Compression is enabled, so set ALL of your
dialing directory entries to 38400 bps for best performance.
If you have 16550 UART installed please set to 57600 bps.
Use Dialing prefix 1 for calling MNP-equipped systems.
Use Dialing prefix 2 for calling non-MNP systems.

