;                       SWI file for MYCALBK Version 3.xx
;       Any line with a ; are considered comments
;       All switches MUST be on a line by themselves with NO ; on the line!
;       Removal of all ; lines will speed up loading process
;       Any blank line MUST be a ;!
;       Here we go!
;       ==========================================================
;       Use this switch for extended logging in your .LOG file.
;       once you have the system up and running, you will probably
;       want to comment this out to save some HD space in your .LOG
;       file.
;DEBUG
;      Use one of these (not both!) to force the use or non use of your
;      FOSSIL driver.
;      This is more a lessa kludge, but some folks requested it, so...
;      Not needed if your RBBS is passing the FOSSIL info correctly!
;FOSSIL=OFF
;FOSSIL=ON
;       This is used in case MYCALBK just DOESN'T seem to want
;       to talk to your modem!  Use ONLY if you are NOT using a FOSSIL!
;USE_ALTERNATE_PORT_PARMS
;       Use this if MYCALBK seems to have trouble dialing out during a
;       busy time of day
BUSY
;       Number of retries to re-dial on NO CARRIER or BUSY for a
;       LOCAL call!
LOCAL_RETRIES=7
;       Number of retries to re-dial on NO CARRIER or BUSY
;       on a LONG DISTANCE call!
LONG_DISTANCE_RETRIES=3
;       This is more or less a command line switch but it's here anyway!
;       If you this, MYCALBK does NOT check for carrier!
;LOCAL
;       When it has been determined that this user is calling from a
;       duplicate number, use this to just hang up on them!
DUMP
;       If you do not need to dial a 1 in your areacode, use this!
;NO-1
;       I know, I know, but some folks still have pulse dialing in thier
;       area!
;PULSE
;       This is if you are REALLY in a wierd phone area and you HAVE to
;       dial your areacode to dial Long Distance
;NEED-AC
;       Sets how long between calls MYCALBK will re-dial
;       Set this to 1 or 2 and use the BUSY switch on a busy system!
REDIALTIME=5
;       Used if you want to call back with your calling card
;       Replace the #'s with your card number.
;PREFIX=###-#######-###
;       Same as above but allows it at the end of the number
;SUFFIX=###-#######
;       Number of seconds to wait after hanging up on caller to start
;       dialing back
WAIT=7
;       Sometimes HST's are REAL stubborn!
;HST
;       If you want to print out what happens during a callback session.
;       Can be network printer, doesn't matter!
;LPT=
;       If you are running COM3 on IRQ 5 or any other intterrupt OTHER
;       than "the standard" COM1,COM3 COM2,COM4 setup, put the IRQ here!
;IRQ=3
;       The following switches are so you can control passage or
;       failures depending on the situation.
;
;       -1 means failed to verify.
;        0 means ignore.
;        1 means pass verification.
;
;       If you are not calling thier areacode, consider it failed.
Bad.Ac=-1
;       The number they entered was already verified.
Verified.Number=-1
;       Didn't answer the phone.
No.Answer=-1
;       They dropped carrier.
Hang.Up=-1
;       They aborted the callback.
Aborted=-1
;       Not the specified time to call them back long distance.
Not.Time=-1
;       They entered 911, 976, 900 or 555!
Entered.911=-1
;       How long they can sit without pressing a key in seconds
Inactivity.Timeout=120
;       If they fall asleep, pass or fail (Default = Fail)
Fell.Asleep=-1
;
; Please refer to the DOCS for your BBS type!
;
BBS.Type=1
;
;User.Info.Path=c:\rbbs\node4\
;
;Pass.Name=Verified
;
;LD.Pass.Name=LDVerified
;
;Fail.Name=unverified
;
;LD.Fail.Name=LDUnVerified
;
