10
Z110Zmodem with Resume Capability - Still the Best!
DSZ handshake slow port %1 pB4096 sz -s -m
DSZ handshake slow port %1 pB4096 rz -s -m -r
P110Puma Protocol with Resume Capability
Puma Lc:\fnet\dszlog p%1 x+ s
Puma Lc:\fnet\dszlog p%1 x+ r+ r
G010Ymodem-G Batch (Error Correcting Modems ONLY!!)
DSZ handshake slow port %1 sb -k -g
DSZ handshake slow port %1 rb -g -p
Y010Ymodem Batch
DSZ handshake slow port %1 sb -k
DSZ handshake slow port %1 rb -k
O000Xmodem-1k (Old Ymodem)
DSZ handshake slow port %1 sx -ks
DSZ handshake slow port %1 rx -c -k -y
C000Xmodem CRC and Checksum (Slow and painful!)
DSZ handshake slow port %1 sx
DSZ handshake slow port %1 rx -c
J000Jmodem (Fast)
Jmodem S%1
Jmodem R%1
N000Nmodem (Turbo Pascal Fast! Protocol)
Nmodem S%1
Nmodem R%1
B111Bimodem Bi-Directional Transfers + Chat
CALL h:\bim\Bimodem /CH:\bim\bimodem2.cfg /U
CALL H:\bim\Bimodem /CH:\bim\bimodem2.cfg /D
H111HS/Link (Bi-Directional / Start 2-Way Transfers as D/L!)
C:\HSLINK -p%1 -@G:\FNET\NODE1.CFG
C:\HSLINK -p%1 -@G:\FNET\NODE1.CFG


This is the protocol data file used on node #1 of "The Programmer's Inn".
It utilizes serial port #1.  If you do not have an error correcting modem,
do not use Ymodem-G Protocol as there is NO built-in error checking with
that protocol.

A new parameter has been added to each protocol definition to specify that
a protocol supports bi-directional transfers or not.
A sample entry of the fnetprot.dat file for HS/Link Protocol is:

1
H111HS/Link (Bi-Directional / Start 2-Way Transfers as D/L!)
C:\TELIX\HSLINK -P%1 @G:\QB3\NODE1.CFG
C:\TELIX\HSLINK -P%1 @G:\QB3\NODE1.CFG

Line 1: Still the number of protocols configured.  Why do I still place a
        number here?  You may make notes or add anything you wish after the
        last prootcol entry in the file.

Line 2: "Z" is the key letter for this protocol (Zmodem)
     1st "1"  - Use a 1 if the protocol can resume an aborted upload.
     2nd "1"  - Enter a 1 if the protocol supports batch transfers (or a "0")
** NEW **  "0"  - Enter a 0 if the protocol doesn't support bi-directional
                  transfers.  Enter a 1 if it DOES support this type of
                  transfer.

 The rest of line 2 is a description of the protocol (40 characters max):
        "Zmodem with Resume Capability"

Line 3: "DSZ handshake slow port %1  pB4096 sz -s -m"

        A command line for sending files (user download) with this protocol.
        If this is a bi-directional protocol you must ensure the protocol
        receives files in the NODE work directory either by including
        the protocol's command to do this on the command line or in a
        configuration or sequence file the protocol uses.
        For HS/Link I use a separate configuration file for each node. Here
        is my NODE1.CFG file.  Note that my HSLink.EXE file is located
        in the C:\TELIX directory. My bbs node directory is G:\QB3
-------------------------------------------------


