á
 7
    Description:  Anchor 2400i (Internal)                   
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 116                             
    Description:  Anchor 9600i (Internal)                   
  Port Selected:
  Opening Speed:  9600                                      
                                                            
       Comments:  None
                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255                      
                  AT\K5\N3\Q3\V2\X1                         
                  AT%C1&C1&D2&W                             
á
 57                              
    Description:  DM424 v.32                                
  Port Selected:
  Opening Speed:  9600                                      

       Comments:  Lock in Opening Baud Rate at 9600         
                                                            
  NRAM Settings:  ATE0M0X4&C1&D2*F3*M1*S0&W                 
á
 36                              
    Description:  ATI2400ETC Modem                          
  Port Selected:
  Opening Speed:  9600                                      

       Comments:  "Don't `lock' modem!"                     
                  "No 300 baud support in `lock' mode."
                                                            
  NRAM Settings:  ATM0N1Q0V1&C1&D2&G0&I0&J0&B1              
                  AT&K3&L0&P0&Q5&R0&S1&T4&X0                
                  ATS2=255S0=0&E1X4&W0&Y0                   
á
 44
    Description:  ATI2400ETC w/V.42                                   
  Port Selected:
  Opening Speed:  9600                                                
  Using Factory:  &F2                                                 
                                                                      
       Comments:  Lock Modem at 9600

                                                                      
                                                                      
  NRAM Settings:  AT&C1&D2&B1                                         
                  ATS2=255E0M0W1&W0                                   
á
 48                              
    Description:  ATI 9600 etc/e                            
  Port Selected:
  Opening Speed:  38400                                     
  Using Factory:  &F2                                       


  NRAM Settings:  ATE0Q0V1X4M0W2&C1&D2&Q6&B1                
                  AT&K3&O1&R1&S0S0=0S2=255                  
                  AT&T5&T10&U1&W0                           
á
 53                              
    Description:  Atrie 2400MNP                             
  Port Selected:
  Opening Speed:  9600                                      

       Comments:  None                                      
                                                            
  NRAM Settings:  ATE0Q0V1X4\G0\N3\J0
                  AT\Q3\X1\K5\V1&C1&D2                      
                  AT&M0&R0&G0B1\T0%A13&W                    
á
 132                             
    Description:  Atrie 9600MNP                             
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  None                                      

  NRAM Settings:  ATB1E0Q0V1X4%A13%C1\J0                    
                  AT&C1&D2&M0&R0&G0                         
                  AT\G0\K5\N3\Q3\T0\X1\V1&W                 
á
 111                             
    Description:  AT&T Paradyne Comsphere 3810              
  Port Selected:
  Opening Speed:  57600                                     

       Comments:  None                                      

  NRAM Settings:  ATE0Q0V1X6S0=0S2=255                      
                  AT&C1&D2&R1&S0                            
                  AT\N5\Q3\X1%C1&W                          
á
 8                         
      Seconds to wait:  15                                  
        Port Selected:
   Port Opening Speed:  1200                                
Lock In Opening Speed:  N                                   
Initialization String:  ATS0=0S2=255C1M0Q0E0V1X1H0          
    'Off-Hook' String:  ATM0H1                              
             Comments:  None                                
á
 9                         
      Seconds to wait:  15                                  
        Port Selected:
   Port Opening Speed:  2400                                
Lock In Opening Speed:  N                                   
Initialization String:  ATS0=0S2=255S7=60S11=60C1M0Q0E0V1X1H
    'Off-Hook' String:  ATM0H1                              
             Comments:  None                                
á
 127                             
    Description:  Boca FAXModem (14400)                     
  Port Selected:
  Opening Speed:  57600                                     

       Comments:  None                                      

  NRAM Settings:  ATE0Q0V1X4S0=0S2=255S46=138               
                  AT&C1&D2&K3&Q5S95=43                      
                  AT%C1%E1\N3\K5&W                          
á
 69                              
    Description:  QuikKomm 2400 MNP                         
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

  NRAM Settings:  ATE0M0X4&C1&D2S0=0S2=255                  
                  AT&W                                      
á
 43                              
    Description:  Cardinal 2400 MNP-5                       
  Port Selected:
  Opening Speed:  4800                                      
                                                            
  NRAM Settings:  AT&C1&D2S0=0\J0                           
                  AT\N3\V1\Q3\C1%C1&W                       
á
 72                              
    Description:  Cardinal 9650 v.32                        
  Port Selected:
  Opening Speed:  4800                                      
                                                            
  NRAM Settings:  ATS0=0Q0V1X4&C1&D2&B1                     
                  AT&B1&M6&N0S46=0&W                        
á
 83                              
    Description:  Cardinal 9600 v.42                        
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  None                                      
                                                            
  NRAM Settings:  ATS0=0Q0V1W1X4&C1&D2&Y0                   
                  ATS48=7%C1\N3&W                           
á
 65                              
    Description:  Codex 2264                                
  Port Selected:
  Opening Speed:  19200                                     
                                                            
       Comments:  None                                      
                                                            
  NRAM Settings:  ATS0=0Q0&C1&D2&R0&S1                      
                  AT*AA0*FL3*ML5*MR0*SM3*XC1                
                  AT&W                                      
á
 107                             
    Description:  Complete Communicator                     
  Port Selected:
  Opening Speed:  38400                                     
                                                            
       Comments:  None                                      
                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255\J0                   
                  AT&C1&D2&K3&Q5                            
                  AT\N3\Q3%C1&W                             
á
 56                        
      Seconds to wait:  20                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  19200                               
Lock In Opening Speed:  Y                                   
Initialization String:  AAAT&F2*H2M0S10=30S2=255&D2H0       
    'Off-Hook' String:  ATM0H1                              
             Comments:  None                                
á
 122                             
    Description:  CompuCom STAR                             
  Port Selected:
  Opening Speed:  19200                                     
  Using Factory:  &F2                                       
                                                            
       Comments:  None                                      
                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255\J0                   
                  AT\N3\Q3\V1\X1                            
                  AT%C1&C1&D2&W0                            
á
 10                              
    Description:  CTS Datacom 2424ADH                       
  Port Selected:
  Opening Speed:  2400                                      
                                                            
       Comments:  None                                      
                                                            
  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 55                              
    Description:  DigiCom 9624LE/9624PC/9624E w/o v.42bis   
  Port Selected:
  Opening Speed:  19200                                     
                                                            
       Comments:  None                                      
                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255*S0                   
                  AT&C1&D3*E1*F3*M1&W                       
á
 54                              
    Description:  DigiCom 9624LE+/9624PC+/9624E+/9624LR+/962
  Port Selected:
  Opening Speed:  38400                                     
                                                            
       Comments:  None                                      
                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255&C1&D3*S0             
                  AT*E9*F3*M2&W                             
á
 131                             
    Description:  DigiCom Scout v.32/Scout Plus v.32bis     
  Port Selected:
  Opening Speed:  57600                                     

       Comments:  None                                      

  NRAM Settings:  ATE0Q0V1X4S0=0S2=255*S1                   
                  AT&C1&D3*E9*F3*M2&W                       
á
 11                        
      Seconds to wait:  15                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  2400                                
Lock In Opening Speed:  N                                   
Initialization String:  ATE0V1Q0S11=55S2=255X4&D2M0H0       
    'Off-Hook' String:  ATM0H1                              
             Comments:  None                                
á
 12                        
      Seconds to wait:  15                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  2400                                
Lock In Opening Speed:  N                                   
Initialization String:  ATS0=0S2=255S10=25&C1M0Q0E0V1X2&D2H0
    'Off-Hook' String:  ATM0H1                              
             Comments:  Do *not* turn on speaker with M1 command
                        as the modem will not function properly!
á
 59                        
      Seconds to wait:  15                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  2400                                
Lock In Opening Speed:  N                                   
Initialization String:  ATS0=0S2=255S10=25&C1M0Q0E0V1X2&D2H0
    'Off-Hook' String:  ATM0H1                              
             Comments:  Do *not* turn on speaker with M1 command
                        as the modem will not function properly!
á
 42                              
    Description:  Everex Evercom 24E+                       
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  Do *not* turn on speaker with M1 command  
                  as the modem will not function properly!  

  NRAM Settings:  ATS0=0S2=255&C1E0V1X4&D2Q0\J0             
                  AT%C1\C1\N3\V1                            
                  AT&W                                      
á
 84                              
    Description:  EverFax 24/96                             
  Port Selected:
  Opening Speed:  4800                                      

       Comments:  None                                      

  NRAM Settings:  ATY&D2\N3\V1\X1&C1\Q3\J0                  
                  AT&W                                      
á
 73                              
    Description:  Everex Evercom 96+                        
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  None                                      

  NRAM Settings:  ATS0=0S2=255&C1E0V1X4&D2Q0\J1             
                  AT%C1\C1\N3\V1&W1                         
á
 88                              
    Description:  Everex EverFAX  24/96 v.32                
  Port Selected:
  Opening Speed:  2400                                      
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATY0&D2&C1\N3\V1\X1\Q3%C1\J0              
                  AT&W                                      
á
 40                              
    Description:  FastComm 9696                             
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  None                                      
                                                            
                                                            
                                                            
  NRAM Settings:  ATS46=3S0=0&S0S69=2&I1S10=4&M6            
                  AT&W                                      
á
 71                              
    Description:  FastComm 9696 (v.32/v.42bis)              
  Port Selected:
  Opening Speed:  38400                                     
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATS0=0E0M0H0S46=10                        
                  AT&H1&I1&M4&Q5&U0&W                       
á
 50                              
    Description:  FORVAL IM14400                            
  Port Selected:
  Opening Speed:  115200                                    
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATM0&C1&D2\J1\V2\N6\Q3S2=63H0&W           
á
 105                             
    Description:  Forval SA14400                            
  Port Selected:
  Opening Speed:  38400                                     
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATM0V1E0N1X4S0=0S2=255\J0                 
                  AT\N6\Q3\V2%C1%E-J1                       
                  AT&C1&D2&W                                
á
 101                             
    Description:  Galaxy UFO v.32bis                        
  Port Selected:
  Opening Speed:  38400                                     
                                                            
                                                            
       Comments:  None                                      
                                                            
                                                            
                                                            
  NRAM Settings:  ATE0Q0V1W1X4S0=0S2=255\J0                 
                  AT&C1&D2%C1                               
                  AT\N3\Q3\V1&W                             
á
 134                             
    Description:  TelePath FAXModem                         
  Port Selected:
  Opening Speed:  38400                                     
                                                            
                                                            
       Comments:  None                                      
                                                            
                                                            
                                                            
  NRAM Settings:  ATE0Q0V1W1X4S0=0S2=255S48=7               
                  AT&C1&D2&K5&Q5%C1%E1S36=7                 
                  ATS46=138S95=44\N3&Y0&W0                  
á
 30                        
      Seconds to wait:  15                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  1200                                
Lock In Opening Speed:  N                                   
Initialization String:  ATS0=0S2=255C1M0Q0E0V1X1H0          
    'Off-Hook' String:  ATM0H1                              
             Comments:  None                                
á
 31                              
    Description:  'Generic' 2400 EEPROM Modem               
  Port Selected:
  Opening Speed:  2400                                      
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 32                        
      Seconds to wait:  18                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  2400                                
Lock In Opening Speed:  N                                   
Initialization String:  ATE0V1X1Q0&C1&D2S2=255S0=0S10=30M0H0
    'Off-Hook' String:  ATM0H1                              
             Comments:  None                                
á
 58                              
    Description:  GVC 9600                                  
  Port Selected:
  Opening Speed:  38400                                     
  Using Factory:  &F2                                       
                                                            
       Comments:  Some GVC modems need the \H0 in the Init String
                  If found in your manual, place \H0 in your
                  String in FNCFG (Modem / Node / Subscription Information)
                                                            
  NRAM Settings:  ATB0X4&C1&D2\J0                           
                  AT%C1\N6\Q3\V1\C1&W                       
á
 81                              
    Description:  GVC v.42bis                               
  Port Selected:
  Opening Speed:  38400                                     
  Using Factory:  &F2                                       
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATW1&W2                                   
á
 124                             
    Description:  GVC v.32 non-MNP                          
  Port Selected:
  Opening Speed:  9600                                      
                                                            
                                                            
       Comments:  Sporadic Problems with MNP Connectiions.


                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255                      
                  AT&C1&D2&W                                
á
 82                              
    Description:  GVC v.32/v.42bis                          
  Port Selected:
  Opening Speed:  38400                                     
                                                            
                                                            
       Comments:  None
                                                            
                                                            
                                                            
  NRAM Settings:  ATS0=0S2=255S7=45E0M0Q0V1X4               
                  AT&C1&D2%C1\Q3\N3\V1&W                    
á
 13                        
      Seconds to wait:  15                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  1200                                
Lock In Opening Speed:  N                                   
Initialization String:  ATS0=0S2=255C1M0Q0E0V1X1H0          
    'Off-Hook' String:  ATM0H1                              
             Comments:  "                1 2 3 4 5 6 7 8 9 0
                        " Switches (8):  U U D D D U U D"   
                        "Switches (10):  U U D D D U U D U U
á
 1                               
    Description:  Hayes 2400 without V.42 Chip              
  Port Selected:
  Opening Speed:  2400                                      
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 115                             
    Description:  Hayes Optima 2400                         
  Port Selected:
  Opening Speed:  9600                                      
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1W1X4S0=0S2=255                    
                  AT&C1&D2&Q5&W                             
á
 115                             
    Description:  Hayes Optima 2400                         
  Port Selected:
  Opening Speed:  9600                                      
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATE0Q0V1W1X4S0=0S2=255                    
                  AT&C1&D2&Q5&W                             
á
 119                             
    Description:  Hayes Optima 9600                         
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATE0M0Q0V1W1X4S0=0S2=255                  
                  ATS36=7S46=138S48=7S95=44                 
                  AT&C1&D2&K3&R1&S0&Q5&W                    
á
 4                               
    Description:  Hayes V-Series without V.42               
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATQ0V1&L0&G0&J0&P0Y0N1S10=30              
                  ATM0L2X4W1&C1&D2&S0&K3E0                  
                  ATS2=255S0=0S36=1S37=0S38=2&W             
á
 5                               
    Description:  Hayes V-Series with V.42                  
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATQ0V1&L0&G0&J0&P0Y0N1&K3&Q5              
                  ATM0L2X4W1&C1&D2&S0&X0E0                  
                  ATS2=255S0=0S36=5S37=0S38=2&W             
á
 41                              
    Description:  Hayes ULTRA Smartmodem 9600/14400         
  Port Selected:
  Opening Speed:  38400                                     
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATQ0V1N1&K3&Q5&T5                         
                  ATX4W1&C1&D2E0                            
                  ATS2=255S0=0S36=5S95=44&W                 
á
 77                              
    Description:  IBM 7855 Model 10                         
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATE0Q0V1X4Y0&B8N1%G1%H1%F1                
                  AT&I0&M0\K0\M14\Q2\R2%C1                  
                  ATC1S0=0&W                                
á
 103                             
    Description:  Identity 2400E-5                          
  Port Selected:
  Opening Speed:  9600                                      
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATQ0V1X4S0=0S2=255\J0                     
                  AT&C1&D2%C1\N3\Q3\V1&W                    
á
 130                             
    Description:  Identity ID-2400I or ID-2400E             
  Port Selected:
  Opening Speed:  2400                                      
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATB0E0Q0V1X4S0=0S2=255                    
                  AT&C1&D2&W                                
á
 110                             
    Description:  Identity 9600 v.32                        
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATE0Q0V1X4S0=0S2=255\J0                   
                  AT&C1&D2%C1\N3\Q3\V1&W                    
á
 110                             
    Description:  Identity 9600 v.32                        
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255\J0                   
                  AT&C1&D2%C1\N3\Q3\V1&W                    
á
 96                              
    Description:  Incomm Turbo 2400                         
  Port Selected:
  Opening Speed:  2400                                      
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATE0Q0V1X4&C1&D2                          
                  ATS0=0S2=255&W                            
á
 14                        
      Seconds to wait:  15                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  2400                                
Lock In Opening Speed:  N                                   
Initialization String:  ATS2=255E0M0X4Q0V1&D2&C1\K3\N3\Q3H0 
    'Off-Hook' String:  ATM0H1                              
             Comments:  None                                
á
 63                        
      Seconds to wait:  35                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  4800                                
Lock In Opening Speed:  Y                                   
Initialization String:  AT&FM0H0E0L0X4V1\D3\K3\Q3\J0\N3     
    'Off-Hook' String:  ATM0H1                              
             Comments:  Lock Comport at 4800                
                        Use \J1 if you are NOT LOCKING Comport
á
 85                              
    Description:  Infinity 2400                             
  Port Selected:
  Opening Speed:  2400                                      
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  AT&C1&D2X4                                
                  AT&W                                      
á
 112                             
    Description:  InfoTel 9600 v.32                         
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATE0Q0V1X4S0=0S2=255                      
                  AT\N3                                     
                  AT&C1&D2&K5&R1&S0&W                       
á
 66                              
    Description:  Intel 24EX                                
  Port Selected:
  Opening Speed:  2400                                      
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0L0M0Q0V1X4&C1&D2                      
                  ATS0=0S2=255                              
                  AT&W                                      
á
 39                              
    Description:  Intel 2400EX                              
  Port Selected:
  Opening Speed:  4800                                      
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  AT\J0\N3\Q3\V1%C1&W                       
á
 52                              
    Description:  Intel 9600EX                              
  Port Selected:
  Opening Speed:  38400                                     
                                                            
                                                            
       Comments:  None                                      
                                                            
                                                            
  NRAM Settings:  ATE0L0M0Q0V1X4&C1&D2&R0\J0                
                  ATS0=0S2=255\C1                           
                  AT&W                                      
á
 95                              
    Description:  Intel 14.4EX                              
  Port Selected:
  Opening Speed:  57600                                     
                                                            
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  AT\J0                                     
                  AT&W                                      
á
 15                        
      Seconds to wait:  15                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  1200                                
Lock In Opening Speed:  N                                   
Initialization String:  ATS0=0S2=255C1M0Q0E0V1X1H0          
    'Off-Hook' String:  ATM0H1                              
á
 145                             
    Description:  Lightning LightCom96                      
  Port Selected:
  Opening Speed:  38400                                     


       Comments:  None                                      
                                                            

  NRAM Settings:  ATW1&C1&D2%E1                             
                  ATS0=0S2=255&Y0&W0                        
á
 129                             
    Description:  Lightning LightCom 14.4k                  
  Port Selected:
  Opening Speed:  38400                                     
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATW1&C1&D2%E1                             
                  ATS0=0S2=255&Y0                           
                  ATS95=44S48=75S46=138S36=5&W0             
á
 75                              
    Description:  LightSpeed 9624E                          
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATS0=0*Q2L3&W*S1                          
á
 16                              
    Description:  Maxum SM 2400                             
  Port Selected:
  Opening Speed:  2400                                      
                                                            
                                                            
       Comments:  None                                      
                                                            
                                                            
                                                            
  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 121                             
    Description:  MicroCom QX/3296c                         
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9"       
                  "       Front -> U D D U D U U D U"       
                  "        Back -> D U D U D U D U  "       
                                                            
  NRAM Settings:  ATS0=0Q0V1X4&C1&D2\J0                     
                  AT%C1\C1\N3\Q3\V1\X0                      
                  AT&W                                      
á
 17                        
      Seconds to wait:  20                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  9600                                
Lock In Opening Speed:  N                                   
Initialization String:  AT\G0\Q3\V1\J0\T0%C1\A3\C2%A13\L0\N3
    'Off-Hook' String:  ATM0H1                              
             Comments:  "Switches: 1 2 3 4 5 6 7 8 9"       
                        "   Front: U D D D D D U U D"       
                        "    Rear: D D D U D U D D"         
á
 2                               
    Description:  Microcom AX9624c                          
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8"         
                  "       Front -> U D D D D U U D"         
                  "        Rear -> D D D U D U D  "         
                                                            
  NRAM Settings:  AT\G0\N3S0=0\Q3\X0\K5E0Q0V1\V1&L0&M0&R0\J0
                  AT\E0\T0%E1%C1%P2%M0\A3\C2%A13X1&P0&G0    
                  AT\H0S8=2S2=255&D2&C1\D0\R1M0&W           
á
 97                              
    Description:  MicroCom QX/4232hs                        
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  AT\G0\N3S0=0\Q3\X0\K5E0Q0V1\V1&L0&M0&R0\J0
                  AT\E0\T0%E1%C1%P2%M0\A3\C2%A13X1&P0&G0    
                  AT\H0S8=2S2=255&D2&C1\D0\R1M0&W           
á
 104                             
    Description:  MicroCom QX/4232bis                       
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255\J0                   
                  AT\D3\G0\K5\N3\Q3\V1\X0                   
                  AT%C1&C1&D2&R0&S1&X0&W                    
á
 18                              
    Description:  Mitac 2400BD                              
  Port Selected:
  Opening Speed:  2400                                      
                                                            
  NRAM Settings:  ATQ0V1&C1&D2&T5S2=255                     
                  ATE0M0X1S10=60S0=0C1&W                    
á
 136                             
    Description:  MultiTech 224BA                           
  Port Selected:
  Opening Speed:  2400                                      
                                                            
       Comments:  None
                                                            
                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255%C1&W                 
á
 19                              
    Description:  Multitech 224EH                           
  Port Selected:
  Opening Speed:  9600                                      
                                                            
                                                            
       Comments:  "Switches: I:UUDD  E: UUDDDUUD"           
                  Open at 9600 bps

                                                            
  NRAM Settings:  ATE0M0Q0V1X1&E1&E4&E7&E8&E10&R0$BA0       
                  AT&E13&E15&Q0$MB2400$SB9600&T5&V1$R1&S0   
                  AT&A0$A1&B0&BS1&C1$D0$F1&G0&I0$MI0&W0     
á
 35                              
    Description:  MultiTech MultiModem V.32                 
  Port Selected:
  Opening Speed:  19200                                     
                                                            
                                                            
       Comments:  "`Lock' modem if running at 9600."        
                   Set Switch #1 UP                         
                                                            
                                                            
  NRAM Settings:  ATM0Q0V1X1&Q0S0=0S2=255&E1&E4$BA0$SB19200 
                  AT&E8&E10&E12&E15$MB9600&S1&T5E0$R1&V1&R1&
                  AT&A0$A1&B0&BS1&C1&D2$D0$F0#F0&G0$MI0S7=30
á
 38                              
    Description:  MultiTech MultiModem 696E                 
  Port Selected:
  Opening Speed:  19200                                     
                                                            
       Comments:  8-Position DIP-Switch & 4-Position DIP-Swi
                    8) #1-U  #2-U  #3-D  #4-D  #5-D  #6-U  #
                    4) #1-D  #2-U  #3-U  #4-D               
                                                            
  NRAM Settings:  ATM0&R0$SB19200$A1$BA0&C1&D2&E1&W$SB19200 
á
 126                             
    Description:  MultiTech MT 1432                         
  Port Selected:
  Opening Speed:  57600                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1X4&C1&D2$SB57600$MB14400$BA0      
                  ATS0=0S2=255&W                            
á
 64                              
    Description:  NEC 9635E                                 
  Port Selected:
  Opening Speed:  9600                                      

       Comments:  Do NOT LOCK comport.  Problems will arise!

                                                            
  NRAM Settings:  ATE0M0Y1S0=0&C1&D2&R2&T5                  
                  AT%E2%P0%P4%B6%G1                         
                  AT\D0\G2\Q3\V1&Y1&W                       
á
 89                              
    Description:  NEC N9631 v.32                            
  Port Selected:
  Opening Speed:  9600                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATX4Q0S0=0\N3&W\J0                        
á
 98                              
    Description:  OkiTel 9600                               
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1W1X4&C1&D2\J0                     
                  ATS0=0\N3\V1&W0                           
á
 20                              
    Description:  Packard Bell IS/EM                        
  Port Selected:
  Opening Speed:  2400                                      

  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 21                              
    Description:  Packard Bell Smartmodem                   
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 144                             
    Description:  PB 9600 MNP                               
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  None                                      

  NRAM Settings:  ATB0Q0V1X4                                
                  AT&C1&D2\C2%C1                            
                  ATS0=0S2=255S7=30&W                       
á
 99                              
    Description:  Penril v.32                               
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1X1                                
                  AT&C1&D2&R0&S1                            
                  AT\K5\N3\V1\X1&W                          
á
 22                              
    Description:  Practical Peripherals 2400                
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  Turn modem off for 30 seconds before      
                  running this program.                     

  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 62                              
    Description:  Practical Peripherals 2400 V.42 bis       
  Port Selected:
  Opening Speed:  9600                                      
                                                            
       Comments:  Lock Comport At 9600

                                                            
  NRAM Settings:  ATS0=0S2=255&C1&D2W1E0&Q5                 
                  ATL0M0&W                                  
á
 37                              
    Description:  Practical Peripherals MNP-5               
  Port Selected:
  Opening Speed:  9600                                      
                                                            
       Comments:  May need to add \J0 to init string in FNCFG.

                                                            
  NRAM Settings:  AT\N3\Q3\V1\J0\G0\J0                      
                  AT&C1&D2&W                                
á
 51                              
    Description:  Practical 9600SA                          
  Port Selected:
  Opening Speed:  38400                                     

                                                            
  NRAM Settings:  ATS95=44S48=7S46=138S36=7                 
                  AT&C1&D2&K3W1X4E0&W                       
á
 120                             
    Description:  Practical Peripherals PM9600 v.32         
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0M0Q0V1W1X4S0=0S2=255                  
                  ATS36=7S46=138S48=7S95=44                 
                  AT&B1&C1&D2&K3&S0&Q5&W                    
á
 128                             
    Description:  Practical Peripherals 14400FXSA v.32bis   
  Port Selected:
  Opening Speed:  57600                                     
  Using Factory:  &F1                                       
                                                            
       Comments:  None                                      
                                                            

  NRAM Settings:  ATE0W1S0=0S2=255S48=7&T5&Q5               
                  ATS10=7S36=7S46=2S95=44&W                 
á
 23                              
    Description:  Qubie 2400E                               
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 87                              
    Description:  QuickTel 9600 v.32/v.42bis                
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  AT\A3%C1&D2%E1\G0&K3&L0\N3                
                  ATE1V1N1X4S0=0                            
                  AT&W                                      
á
 24                              
    Description:  Racal Vadic 2400VP                        
  Port Selected:
  Opening Speed:  2400                                      
                                                            
       Comments:  None
                                                            

  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 25                              
    Description:  Small Talk 2400                           
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 133                             
    Description:  SmartLink 2400                            
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255                      
                  AT&C1&D2&W                                
á
 94                              
    Description:  SmartOne 2400                             
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATQ0V1X4&C1&D2                            
                  ATS0=0S2=255&W                            
á
 90                              
    Description:  SmartOne 2400 w/MNP                       
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATQ0V1X4&C1&D2\J0                         
                  AT\N3S0=0S2=255&W                         
á
 74                              
    Description:  SupraModem 2400 MNP/Plus                  
  Port Selected:
  Opening Speed:  9600                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATQ0V1X4S0=0S2=255\J0                     
                  AT&C1&D2&K3&R0&S1                         
                  AT\G0\N3\Q3\V2%C1&W                       
á
 125                             
    Description:  SupraFAX v.32bis                          
  Port Selected:
  Opening Speed:  38400                                     
  Using Factory:  &F2                                       
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATW1%C1\N3&Q5S0=0S2=255S95=32&W           
á
 49                              
    Description:  TELEBIT T2500 v.32                        
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  Open at 19200 Baud                        
                  To make PEP tones last in the carrier searh, set S92=1.
                                                            
                                                            
  NRAM Settings:  ATM0                                      
                  ATM0                                      
á
 109                             
    Description:  TELEBIT T3000 v.32 w/o PEP                
  Port Selected:
  Opening Speed:  57600                                     
  Using Factory:  &F9                                       
                                                            
       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0L1M3X2S48=1S46=0                      
                  ATS0=0S2=255S51=252&D2&W                  
á
 67                              
    Description:  Trailblazer                               
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE1Q0V1X3                                
                  ATS0=0S51=5S58=2S68=2S66=1                
                  ATS52=1S53=1S67=0S95=2S104=0&W            
á
 92                              
    Description:  TELEBIT QBlazer                           
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1X2&C1&D2                          
                  ATS0=0S2=255S58=2S59=11&W                 
á
 80                              
    Description:  TwinCom 96/42i                            
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATS0=0Q0V1X4&C1&D2                        
                  ATW1&K3&Q6%C1%E1\N3&W                     
á
 114                             
    Description:  TwinCom 144/DF                            
  Port Selected:
  Opening Speed:  57600                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1W1X4S0=0S2=255S48=7               
                  AT&C1&D2&K3&Q5S36=5S46=138S95=44          
                  AT\N3%C1%E1&W                             
á
 68                              
    Description:  UDS FastTalk 2400/5                       
  Port Selected:
  Opening Speed:  19200                                     

                                                            
  NRAM Settings:  ATB2X4&C1&D2&R0&S1\J0                     
                  AT&T5\C1%C1\N3\Q0&W                       
á
 91                              
    Description:  UDS Fastalk v.32/v.42bis                  
  Port Selected:
  Opening Speed:  9600                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1X4&C1&D2\J0                       
                  AT\N3\V1%C1                               
                  ATS0=0S2=255&W                            
á
 106                             
    Description:  UDS v3224/5                               
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  None                                      

                                                            
  NRAM Settings:  ATE0Q0V1X4S0=0S2=255\J0                   
                  AT%C1&C1&D2&R0&S1&X0                      
                  AT\K5\N3\Q3\V1&W                          
á
 45                              
    Description:  FastTalk V.32                             
  Port Selected:
  Opening Speed:  19200                                     

                                                            
  NRAM Settings:  ATB2X4&C1&D2&R0&S1\J0                     
                  AT&T5\C1%C1\N3&W                          
á
 86                              
    Description:  Unisys v.32                               
  Port Selected:
  Opening Speed:  9600                                      

       Comments:  None                                      

                                                            
  NRAM Settings:  ATM0&C1&D2\G1\N3\Q3\V1\X1%F1\J0           
                  AT&W0                                     
á
 6                               
    Description:  USRobotics Dual Standard V.32/V.32bis     
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9 0"     
                  "        Rear -> U U D D D U U D D U"     
                                                            
                                                            
  NRAM Settings:  ATB0C1F1M1Q0V1X4S2=255&B1&K3&A3
                  AT&A3&H1&I0&M4&N0&P0&C1S15=73S10=15
                  AT&R2&S0&Y1S7=60S0=0S11=45&D2&W
á
 118                             
    Description:  USRobotics Dual 16800 Standard v32/v32bis 
  Port Selected:
  Opening Speed:  57600                                     

       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9 0"     
                  "        Rear -> U U D D D U U D D U"     
                                                            
                                                            
  NRAM Settings:  ATB0C1F1M0Q0V1X4S2=255&B1                 
                  AT&A3&H1&I0&K3&M4&N0&P0&C1                
                  AT&R2&S0&Y1S7=60S0=0&D2&W                 
á
 47                              
    Description:  USR Dual Standard V.32/V.32bis (Rackmount)
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9 0"     
                  "        Rear -> U U D D D U U D D U"     

                                                            
  NRAM Settings:  ATB0C1F1Q0V1X4S2=255&B1&K3&A3             
                  AT&A1&H1&I0&M4&N0&P0&C1                   
                  AT&R2&S0&Y1S7=60S0=0&D2&W                 
á
 3                               
    Description:  USRobotics HST (9600 model)               
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9 0"     
                  "        Rear -> U U D D D U U D D U"     
                                                            
                                                            
  NRAM Settings:  ATC1F1M0Q0V1X4S2=255&B1                   
                  AT&A1&H1&I0&M4&N0                         
                  AT&R2&S0&Y1S7=60S0=0&W                    
á
 33                              
    Description:  USRobotics HST (14400 model)              
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9 0"     
                  "        Rear -> U U D D D U U D D U"     
                                                            
                                                            
  NRAM Settings:  ATC1F1M0Q0V1X4S2=255S15=8&B1&K3&A3        
                  AT&A1&H1&I0&M4&N0                         
                  AT&R2&S0&Y1S7=60S0=0&W                    
á
 117                             
    Description:  USRobotics HST (16800 model)              
  Port Selected:
  Opening Speed:  57600                                     
                                                            
       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9 0"
                  "        Rear -> U U D D D U U D D U"     
                                                            
                                                            
  NRAM Settings:  ATC1F1M0Q0V1X4S2=255S15=8&B1              
                  AT&A3&H1&I0&K3&M4&N0                      
                  AT&R2&S0&Y1S7=60S0=0&W                    
á
 60                              
    Description:  USRobotics HST (9600 Rackmount)           
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9 0"     
                  "        Rear -> U U D D D U U D D U"     


  NRAM Settings:  ATC1F1Q0V1X4S2=255&B1&K3&A3               
                  AT&A1&H1&I0&M4&N0                         
                  AT&R2&S0&Y1S7=60S0=0&W                    
á
 61                              
    Description:  USRobotics HST (14400 Rackmount)          
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9 0"     
                  "        Rear -> U U D D D U U D D U"     
                                                            

  NRAM Settings:  ATC1F1Q0V1X4S2=255S15=8&B1&K3&A3
                  AT&A1&H1&I0&M4&N0                         
                  AT&R2&S0&Y1S7=60S0=0&W                    
á
 93                        
      Seconds to wait:  30                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  2400                                
Lock In Opening Speed:  N                                   
Initialization String:  ATE0Q0V1X4S0=0S2=255M0H0            
    'Off-Hook' String:  ATM0H1                              
             Comments:  None                                
á
 140                             
    Description:  Courier 2400/FAX                          
  Port Selected:
  Opening Speed:  57600                                     
                                                            
       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8 9 0"
                  "        Rear -> U U D U D U U D D U"     
                                                            
                                                            
  NRAM Settings:  ATB0C1F1M0Q0V1X4S2=255%R0&B1&K3&A3        
                  AT&A1&H1&I0&M4&N0&P0&C1                   
                  AT&R2&S0&Y1S7=60S0=0&D2&W                 
á
 34                              
    Description:  USRobotics Sportster 2400                 
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255
                  ATS10=30E0M0X1&W                          
á
 108                             
    Description:  USRobotics Sportster v.32/PC              
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  None                                      

  NRAM Settings:  ATE0Q0V1X4S0=0S2=255&B1                   
                  AT&A1&C1&D2&H1&K3&M4&R0&S1&W              
á
 142                             
    Description:  USRobotics Sportster 14400                
  Port Selected:
  Opening Speed:  57600                                     

       Comments:  "Set Switches -> 1 2 3 4 5 6 7 8"         
                  "        Rear -> U U D D D U U D"         

                                                            
  NRAM Settings:  ATB0F1M0Q0V1X4S2=255&B1                   
                  AT&A1&H1&I0&K3&M4&N0                      
                  AT&R2&S0&Y1S7=60S0=0&W                    
á
 26                        
      Seconds to wait:  20                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  9600                                
Lock In Opening Speed:  Y                                   
Initialization String:  ATS2=255C1E0X1M0&H1I0H0             
    'Off-Hook' String:  ATM0H1                              
             Comments:  "May require locking in DTE speed." 

                        "Switches: U U D U D U U D D U"     
á
 27                        
      Seconds to wait:  20                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  2400                                
Lock In Opening Speed:  N                                   
Initialization String:  ATS2=255C1E0X1V1M0H0                
    'Off-Hook' String:  ATM0H1                              
             Comments:  Switches all up except #2 which sele
                        the proper COM port #.              
á
 28                              
    Description:  Ventel Trailblazer                        
  Port Selected:
  Opening Speed:  19200                                     
                                                            
       Comments:  None

  NRAM Settings:  ATQ0V1S50=0S51=5S58=2                     
                  ATE0S66=1S111=255X1&W                     
á
 46                              
    Description:  Ventel 9600 Plus                          
  Port Selected:
  Opening Speed:  38400                                     

       Comments:  Switch SW2 on Modem HardWare should be like so:
                   1-OFF 2-OFF 3-OFF 4-OFF 5-OFF 6-OFF      
                  A 16550AFN chip is needed for port locking at 38400.
                                                            
  NRAM Settings:  AT&C1&D2\N3\Q3%F2S0=0S2=255               
                  ATM0&W1&Y1                                
á
 123                             
    Description:  Viva 24im                                 
  Port Selected:
  Opening Speed:  9600                                      

       Comments:  None                                      

  NRAM Settings:  ATE0Q0V1X4S0=0S2=255\J0                   
                  AT\N3\Q3\V1\X1                            
                  AT%C1&C1&D2&W                             
á
 100                             
    Description:  Viva 9642e v.32/v.42bis                   
  Port Selected:
  Opening Speed:  19200                                     

       Comments:  None                                      

  NRAM Settings:  ATE0Q0V1X4S0=0S2=255                      
                  AT\N3                                     
                  AT&C1&D2&K3&R0&S1&W                       
á
 78                              
    Description:  WorldPort 9600                            
  Port Selected:
  Opening Speed:  9600                                      
                                                            
       Comments:  None

  NRAM Settings:  ATS0=0X4\V1\Q0\N3&W\J0                    
á
 70                              
    Description:  Zenith 2M-2401                            
  Port Selected:
  Opening Speed:  2400                                      

       Comments:  None                                      

  NRAM Settings:  ATQ0V1&C1&D2S0=0S2=255                    
                  ATS10=30E0M0X1&W                          
á
 29                        
      Seconds to wait:  15                                  
    COM Port Selected:  1                                   
   Port Opening Speed:  2400                                
Lock In Opening Speed:  N                                   
Initialization String:  ATE0Q0V1X4&C1&D2&S1S2=255M0H0       
    'Off-Hook' String:  ATM0H1                              
             Comments:  None                                
á
 76                              
    Description:  Zoom/Modem v.42bis                        
  Port Selected:
  Opening Speed:  9600                                      
                                                            
       Comments:  None

  NRAM Settings:  ATQ0V1W1X4S0=0S95=44                      
                  AT&C1&D2&Q5\G0\N3%C1&W                    
á
 102                             
    Description:  Zoom v.32bis                              
  Port Selected:
  Opening Speed:  38400                                     
                                                            
       Comments:  None                                      
                                                            
  NRAM Settings:  ATE0Q0V1W1X4S0=0S2=255                    
                  AT&C1&D2&K3&Q5S36=5S46=13                 
                  AT%C1S95=44S48=7&W                        
á
 113                             
    Description:  ZyXel U-1496 v.32bis                      
  Port Selected:
  Opening Speed:  57600                                     
                                                            
       Comments:  None

  NRAM Settings:  ATE0Q0V1X6S0=0S2=255&B1                   
                  AT*E0&B1&C1&D2&H3&K4&M0&W                 
á
 141
    Description:  USRobotics Sportster 9600
  Port Selected:
  Opening Speed:  38400
  
      Comments:  "Set Switches -> 1 2 3 4 5 6 7 8"
                 "        Rear -> U U D U D U U D"
  

  NRAM Settings:  ATB0E1F1M0Q0V1X4S2=255
                  AT&A3&B2&H1&I0&K3&M4&N0&B1
                  AT&R2&S0&Y1S7=60S0=0&W
á
 139
    Description:  Viva 14.4/FAX
  Port Selected:
  Opening Speed:  38400

       Comments:  None


  NRAM Settings:  ATE0Q0V1X4S0=0S2=255
                  AT&C1&D2&K3&R0&S1
                  AT\N3S95=44S48=7S36=7S46=138&W
á
 146
    Description:  Viva 24i
  Port Selected:
  Opening Speed:  2400

       Comments:  None


  NRAM Settings:  ATB0E1M0Q0V1X4S0=0S2=255
                  AT&C1&D2&Y0&W0
á
 147
    Description:  QuickComm Sprit/Spirit II
  Port Selected:
  Opening Speed:  38400

       Comments:  None


  NRAM Settings:  ATE1M0Q0V1X4S0=0S2=255
                  AT&C1&D2&M0*E5*E9*F3&W
á
 144
    Description:  InfoTel 14.4 v.32bis
  Port Selected:
  Opening Speed:  38400

       Comments:  Using B6 instead of B1 sometimes
                  results in better reliability.


  NRAM Settings:  ATB1E0Q0V1X4
                  AT&C1&D2&K3&R1&S0
                  ATS0=0S2=255&Y0&W0
á
 143
    Description:  InfoTel 9600 w/o v.42bis
  Port Selected:
  Opening Speed:  19200

       Comments:  None


  NRAM Settings:  ATE0Q0V1X4S0=0S2=255
                  AT&C1&D2&K5&R1&S0&W
á
 145
    Description:  Cardinal 14400 v.42bis
  Port Selected:
  Opening Speed:  57600

       Comments:  None


  NRAM Settings:  ATB0E1M0Q0V1W1X4&C1&D2&Y0
                  AT&K3&Q9\G0\N3S36=7S46=138
                  ATS0=0S2=255S7=60S48=7&W0
á
