  +------------------------------------------------------------------------+
  |    This report is created by ASTRA v.5.46     Jun-21-2010 23:18:10     |
  +------------------------------------------------------------------------+

     Registered To:            Sysinfo Lab
     License Type:             Professional for 1 computer

                  +-----------------------------------------+
                  |              System Summary             |
                  +-----------------------------------------+
  Processor
     Processor:                AMD Phenom II X4 710
     CPU Clock:                3445.1 MHz (13.0 x 265.0 MHz)
     Level 1 Cache:            4 x 64+64 kB (data+instr.)
     Level 2 Cache:            4 x 512 kB
     Level 3 Cache:            1 x 6144 kB
  Motherboard
     System Name:              Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
     Motherboard Vendor:       Gigabyte Technology Co., Ltd.
     Board Model:              Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
     BIOS Version:             Award Modular BIOS v6.00PG
     Chipset Name:             AMD 770/780FX/790FX
     Chipset Vendor:           ATI Technologies Inc
     Chipset:                  RX790 GFX Single Slot
     Southbridge Vendor:       ATI Technologies Inc
     Southbridge:              SB700 LPC host controller
     PCI Bus Version:          3.0
     PnP BIOS Version:         1.0
     DMI/SMBIOS Version:       2.4
  Memory
     Base Memory:              640 kB (604 kB free)
     Extended Memory:          2094976 kB (2045.88 MB)
     System Memory:            2048 MB
     Memory Module:            1024MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
     Memory Module:            1024MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
  Storage
     Floppy Drive:             A: 1.44 MB (3.5")
     HDD Model:                WDC WD1001FALS-00J7B0
     HDD Size:                 953869 MB (931.51 GB)
     CD/DVD Model:             _NEC DVD_RW ND-3550A
     CD/DVD Speed:             48x (Write: 48x)
     CD/DVD Model:             CD-W540E
     CD/DVD Speed:             48x (Write: 40x)
  Video
     Monitor Vendor:           LG Electronics Inc.
     Monitor Model:            LG FLATRON F920P
     Video Chip Vendor:        ATI Technologies Inc
     Video Chip:               RV770 [Radeon HD 4870]
     VESA OEM String:          ATI ATOMBIOS
     Video Memory Size:        16 MB
  Sound
     Sound Chip Vendor:        ATI Technologies Inc
     Sound Chip:               IXP SB600 High Definition Audio Controller
     Sound Chip Vendor:        ATI Technologies Inc
     Sound Chip:               HD48x0 audio
     AC'97/HDA Codec Name:     ATI R600 HDMI
     Sound Chip Vendor:        Creative Labs
     Sound Chip:               EMU10K2 Audio Chipset (SB Audigy Series)
  Operating System
     DOS Version:              Microsoft DOS 6.22 rev.0 in HMA
     Windows Version:          Not Found
  Network
     Adapter Vendor:           Realtek Semiconductor
     Adapter Name:             RTL8168/8111 PCI-E Gigabit Ethernet NIC
  Ports
     Mouse Type:               PS/2 (version 7.00)
     LPT Ports:                LPT1(0378h)
     COM Ports:                COM1(03F8h)
     Joystick:                 Present

                  +-----------------------------------------+
                  |               Motherboard               |
                  +-----------------------------------------+
  System
     System Vendor:            Gigabyte Technology Co., Ltd.
     Product Name:             GA-MA770T-UD3P
     Version:
     Serial Number:
     UUID:                     303032343144383931353430FFFFFFFF
     Wake-up Type:             Power Switch
     SKU Number:
     Family:
  Motherboard
     Motherboard Vendor:       Gigabyte Technology Co., Ltd.
     Vendor URL:               www.gigabyte.com.tw
     Board Model:              Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
     Version:
     Serial Number:
     BIOS Version:             Award Modular BIOS v6.00PG
     BIOS Date:                06/24/09
     Chipset Name:             AMD 770/780FX/790FX
     Chipset Vendor:           ATI Technologies Inc
     Chipset:                  RX790 GFX Single Slot
     Southbridge Vendor:       ATI Technologies Inc
     Southbridge:              SB700 LPC host controller
  System Enclosure
     Manufacturer:             Gigabyte Technology Co., Ltd.
     Type:                     Desktop
     Version:
     Serial Number:
     Asset Tag:
     Boot-up State:            Unknown
     Power Supply State:       Unknown
     Thermal State:            Unknown
     Security Status:          Unknown
     OEM-defined:              00000000h

                  +-----------------------------------------+
                  |                  CPU                    |
                  +-----------------------------------------+
  CPU
     Processor:                AMD Phenom II X4 710
     Coprocessor:              Internal
     CPU Clock:                3445.1 MHz
     Level 1 Cache:            4 x 64+64 kB (data+instr.)
     Level 2 Cache:            4 x 512 kB
     Level 3 Cache:            1 x 6144 kB
     FSB Clock:                265.0 MHz
     Multiplier:               13.0
     Platform ID:              Socket AM2+
     Vendor:                   AuthenticAMD
     Processor Name:           AMD Phenom(tm) II X4 10 Processor
     Processor Type:           Original OEM Processor
     CPUID:                    Family: 15, Model: 4, Stepping: 2
     Ext. Family/Model:        Family: 1, Model: 0
     CPU Signature:            00100F42h
     Brand ID:                 Phenom II X4 710 (40A6h)
     Number of Cores:          4
     Logical CPU Count:        HTT Not Supported
     Max CPUID Level:          5
     Max ExtCPUID Level:       8000001Bh
     Code Name:                Deneb (0.045mk)
     Core Stepping:            RB-C2
     MSR C0010064h:            800001FDh:3800240Ah
     MSR C0010065h:            800001EBh:38003403h
     MSR C0010066h:            800001DEh:3800444Ch
     MSR C0010067h:            80000187h:38005040h
     MSR C0010071h:            30B40093h:3800240Ah
  Instruction Set
     Floating-Point Unit On-Chip:         [X]
     IA MMX Technology:                   [X]
     SSE Instruction Set:                 [X]
     SSE2 Instruction Set:                [X]
     SSE3 Instruction Set:                [X]
     Supplemental SSE3 Instruction Set:   [ ]
     SSE4.1 Instruction Set:              [ ]
     SSE4.2 Instruction Set:              [ ]
     Advanced Vector Extensions (AVX):    [ ]
     FMA Instructions Set:                [ ]
     AES Instructions Set:                [ ]
     Intel Extended Memory 64 Tech.:      [ ]
     Intel Architecture - 64 (IA-64):     [ ]
     AMD MMX Instruction Extensions:      [X]
     AMD 3DNow! Instructions:             [X]
     AMD 3DNow! Extensions:               [X]
     AMD 3DNow! Prefetch:                 [X]
     AMD SSE4A Extensions:                [X]
     AMD SSE5 Extensions:                 [ ]
     AMD Misaligned SSE:                  [X]
     AMD64 Architecture:                  [X]
     Cyrix Extended MMX:                  [ ]
     CMPXCHG8 Instruction Supported:      [X]
     CMPXCHG16 Instruction Supported:     [X]
     Fast System Call:                    [X]
     Conditional Move Instruction:        [X]
     CLFLUSH Insruction Supported:        [X]
     Fast Save and Restore:               [X]
     Monitor/MWAIT Instructions:          [X]
     SYSCALL/SYSRET Instructions:         [X]
     LAHF/SAHF Instructions:              [X]
     POPCNT Insruction Supported:         [X]
     XSAVE Insructions Supported:         [ ]
     OS Supports XSAVE Instructions:      [ ]
     PCLMULQDQ Instruction Supported:     [ ]
     MOVBE Insruction Supported:          [ ]
     AMD RDTSCP Insruction Supported:     [X]
     AMD Fast Save and Restore:           [X]
     AMD SKINIT, STGI, DEV Supported:     [X]
  Processor Features
     Virtual Mode Extension:              [X]
     Debugging Extension:                 [X]
     Page Size Extension:                 [X]
     Time Stamp Counter:                  [X]
     Model Specific Registers:            [X]
     Physical Address Extension:          [X]
     Machine Check Exception:             [X]
     On-chip APIC Hardware Supported:     [X]
     Memory Type Range Registers:         [X]
     Page Global Enable:                  [X]
     Machine Check Architecture:          [X]
     Page Attribute Table:                [X]
     36-bit Page Size Extension:          [X]
     Processor Serial Number:             [ ]
     Debug Store:                         [ ]
     64-bit Debug Store:                  [ ]
     Self-Snoop:                          [ ]
     Hyper-Threading Technology:          [ ]
     Pending Break Enable:                [ ]
     CPL-Qualified Debug Store:           [ ]
     L1 Context ID:                       [ ]
     Send Task Priority Messages:         [ ]
     Direct Cache Access:                 [ ]
     Performance Capabilities MSR:        [ ]
     x2APIC Architecture:                 [ ]
     Advanced Bit Manipulation:           [X]
     OS Visible Workaround:               [X]
     Instruction Based Sampling:          [X]
     Intel Virtualization Technology:     [ ]
     Intel Trusted Execution Technology:  [ ]
     Intel Turbo Boost Technology:        [ ]
     AMD No-execute Page Protection:      [X]
     AMD Secure Virtual Machine:          [X]
     AMD Model-Specific Registers:        [X]
     AMD Multiprocessing Capable:         [ ]
     AMD CMP Legacy Mode:                 [X]
     AMD CR8 in Legacy Mode:              [X]
     AMD Ext. APIC Register Space:        [X]
     AMD Watchdog Timer:                  [X]
     AMD 1-GB Large Page:                 [X]
  Power Management
     ACPI Supported:                      [ ]
     Thermal Monitor Supported:           [ ]
     Thermal Monitor 2:                   [ ]
     Enhanced SpeedStep Technology:       [ ]
     Digital Thermal Sensor:              [ ]
     Operating Point Protection:          [ ]
     AMD Temperature Sensor:              [X]
     AMD Frequency ID Control:            [ ]
     AMD Voltage ID Control:              [ ]
     AMD Thermal Trip:                    [X]
     AMD Thermal Monitoring:              [X]
     AMD Software Thermal Control:        [X]
     AMD Invariant TSC:                   [X]
     AMD 100MHz Multiplier Steps:         [X]
     AMD Hardware P-State Control:        [X]

                  +-----------------------------------------+
                  |                CPU Cache                |
                  +-----------------------------------------+
  Level 1 Instruction Cache
     Size:                     4 x 64 kB
     Associativity:            2-way
     Lines per Tag:            1
     Line Size:                64 byte
     TLB 4K Pages:
       Number of Entries:      32
       Associativity:          full
     TLB 2/4M Pages:
       Number of Entries:      16
       Associativity:          full
  Level 1 Data Cache
     Size:                     4 x 64 kB
     Associativity:            2-way
     Lines per Tag:            1
     Line Size:                64 byte
     TLB 4K Pages:
       Number of Entries:      48
       Associativity:          full
     TLB 2/4M Pages:
       Number of Entries:      48
       Associativity:          full
  Level 2 Cache
     Size:                     4 x 512 kB
     Associativity:            16-way
     Lines per Tag:            1
     Line Size:                64 byte
     Instr. TLB 4K Pages:
       Number of Entries:      512
       Associativity:          4-way
     Data TLB 4K Pages:
       Number of Entries:      512
       Associativity:          4-way
     Instr. TLB 2/4M Pages:
       Number of Entries:      0
       Associativity:          off
     Data TLB 2/4M Pages:
       Number of Entries:      128
       Associativity:          2-way
  Level 3 Cache
     Size:                     1 x 6144 kB
     Associativity:            48-way
     Line Size:                64 byte

                  +-----------------------------------------+
                  |              CPU (SMBIOS)               |
                  +-----------------------------------------+
  Processor
     Processor Vendor:         AMD
     Processor Version:        AMD Phenom(tm) II X4 10 Processor
     Current Speed:            3445 MHz
     External Clock:           265 MHz
     Voltage:                  1.3 V
     Processor Upgrade:        ZIF Socket
     Processor Status:         CPU Enabled
     Socket Designation:       Socket M2
     Processor Type:           Central Processor
     Processor Family:         AMD Athlon
     Processor ID1:            00100F42h
     Processor ID2:            178BFBFFh
     Max Speed:                3200 MHz
     Socket Status:            CPU Socket Populated
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         23h

                  +-----------------------------------------+
                  |            CPU (SMBIOS) Cache           |
                  +-----------------------------------------+
  Level 1 Cache
     Installed Size:           128 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Synchronous
     Status:                   Enabled
     Socket Designation:       Internal Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       128 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h
  Level 1 Cache
     Installed Size:           128 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Synchronous
     Status:                   Enabled
     Socket Designation:       Internal Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       128 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h
  Level 3 Cache
     Installed Size:           512 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Synchronous
     Status:                   Enabled
     Socket Designation:       External Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       512 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h
  Level 2 Cache
     Installed Size:           0 kB
     Operational Mode:         Write Through
     Current SRAM Type:        Synchronous
     Status:                   Disabled
     Socket Designation:       External Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       1024 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h

                  +-----------------------------------------+
                  |                  BIOS                   |
                  +-----------------------------------------+
  BIOS
     Motherboard Vendor:       Gigabyte Technology Co., Ltd.
     Vendor URL:               www.gigabyte.com.tw
     BIOS Version:             Award Modular BIOS v6.00PG
     BIOS Model:               Model: FCh  SubModel: 01h  Revision: 00h
     BIOS Date:                06/24/09
     BIOS Copyright:           Award Software Inc. - 04/23/90
     Motherboard ID:           AMD 770 BIOS for GA-MA770T-UD3P F2
     BIOS ID:                  06/24/2009-RX780-SB710-7A66AG05C-00
     BIOS Type:                Unknown (7)
     Bus Type:                 ISA/PCI
     Processor:                686
     Chipset:                  AMD 790FX
     Chipset ID:               RX780-SB710
     BIOS Revision:            00
     MP Specification Ver.:    1.4
     MP Table Address:         000Fh:1100h
     Number of CPU/Cores:      4
     DMI/SMBIOS Version:       2.4
     DMI/SMBIOS Structures:    55
     DMI/SMBIOS Address:       000Fh:0100h
     APM Version:              1.2
  SMBIOS
     BIOS Vendor:              Award Software International, Inc.
     BIOS Version:             F2
     BIOS Date:                06/24/2009
     BIOS ROM Size:            1024 kB
     Starting Segment:         E000h
     Current Language:         n|US|iso8859-1
     Number of Languages:      3
     Structure Length:         18h
  Bus Supported
     PCI is Supported:                    [X]
     AGP is Supported:                    [ ]
     USB is Supported:                    [X]
     ISA is Supported:                    [X]
     VLBus is Supported:                  [ ]
     MCA is Supported:                    [ ]
     EISA is Supported:                   [ ]
     PC Card is Supported:                [ ]
  Boot Options
     Selectable Boot:                     [X]
     Boot From CD:                        [X]
     ATAPI ZIP Drive Boot:                [X]
     LS-120 Boot:                         [X]
     BIOS Boot Specification:             [X]
     Boot From PC Card:                   [ ]
     Network Service Boot Supported:      [ ]
     I2O Boot:                            [ ]
     1394 Boot:                           [ ]
  BIOS Features
     BIOS Characteristics:                [X]
     ACPI Supported:                      [X]
     PnP is Supported:                    [X]
     APM is Supported:                    [X]
     ESCD Support:                        [ ]
     Enhanced Disk Drive (EDD):           [X]
     BIOS is Upgradeable (Flash):         [X]
     BIOS ROM is Socketed:                [X]
     BIOS Shadowing is Allowed:           [X]
     Smart Battery Supported:             [ ]
     Targeted Content Distribution:       [X]
     Int 13h - 5.25"/360kB Floppy:        [X]
     Int 13h - 5.25"/1.2MB Floppy:        [X]
     Int 13h - 3.5"/720kB Floppy:         [X]
     Int 13h - 3.5"/2.88MB Floppy:        [X]
     Int 5h, Print Screen Service:        [X]
     Int 9h, 8042 Keyboard Services:      [X]
     Int 14h, Serial Services:            [X]
     Int 17h, Printer Services:           [X]
     Int 10h, CGA/Mono Video Services:    [X]
     Int 13h - Floppy for NEC 9800:       [ ]
     Int 13h - Floppy for Toshiba:        [ ]
     NEC PC-98:                           [ ]
  Advanced Power Management Features
     16-bit PM Interface Support:         [X]
     32-bit PM Interface Support:         [X]
     CPU Idle Call:                       [X]
     BIOS Power Management Disabled:      [ ]
     BIOS Power Management Disengaged:    [ ]
  Other SMBIOS Structures
     Memory Array Mapped Address (19)
     Memory Device Mapped Address (20)
     Memory Device Mapped Address (20)
     Memory Device Mapped Address (20)
     Memory Device Mapped Address (20)
     System Boot Information (32)
     Unknown (188)
     Unknown (190)
     Unknown (192)
     Unknown (194)
     Unknown (196)
     Unknown (198)

                  +-----------------------------------------+
                  |             PCI/AGP Devices             |
                  +-----------------------------------------+
  PCI/AGP
     PCI Bus Version:          3.0
     Number of PCI Buses:      4

  Bus: 00h, Device: 00h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (5957h):           RX790 GFX Single Slot
     Subsys Vendor (1002h):    ATI Technologies Inc
     Subsystem ID (5957h):     Unknown
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           E0000000h - FFFFFFFFh

  Bus: 00h, Device: 02h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (5978h):           RD790 PCI to PCI bridge (external gfx0 port A)
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            E000h - EFFFh
     Memory Address:           FDF00000h - FDFFFFFFh
     Memory Address:           D0000000h - DFFFFFFFh
     System IRQ:               10
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               5.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0

  Bus: 00h, Device: 0Ah, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (597Fh):           RD790 PCI to PCI bridge (PCIe gpp port F)
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            D000h - DFFFh
     Memory Address:           FDE00000h - FDEFFFFFh
     Memory Address:           FDB00000h - FDBFFFFFh
     System IRQ:               10
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               5.0 GB/s (Current: 2.5 GB/s)
     Link Width:               x1 (Current: x1)
     Link Port Number:         5
     Physical Slot Number:     1

  Bus: 00h, Device: 11h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (4390h):           SB700 SATA Controller [IDE mode]
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (B002h):     Unknown
     Class (01h):              Storage
     SubClass (01h):           IDE
     Revision:                 00h
     Interface:                8Fh
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            0000FF00h - 0000FF07h
     Base I/O Port:            0000FE00h - 0000FE03h
     Base I/O Port:            0000FD00h - 0000FD07h
     Base I/O Port:            0000FC00h - 0000FC03h
     Base I/O Port:            0000FB00h - 0000FB0Fh
     Memory Address:           FE02F000h - FE02F3FFh
     System IRQ:               11
     Interrupt Pin:            INTA#

  Bus: 00h, Device: 12h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (4397h):           SB700 USB OHCI0 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02E000h - FE02EFFFh
     System IRQ:               3
     Interrupt Pin:            INTA#

  Bus: 00h, Device: 12h, Function: 01h
     Vendor (1002h):           ATI Technologies Inc
     Device (4398h):           SB700 USB OHCI1 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02D000h - FE02DFFFh
     System IRQ:               3
     Interrupt Pin:            INTA#

  Bus: 00h, Device: 12h, Function: 02h
     Vendor (1002h):           ATI Technologies Inc
     Device (4396h):           SB700 USB EHCI Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                20h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02C000h - FE02C0FFh
     System IRQ:               10
     Interrupt Pin:            INTB#

  Bus: 00h, Device: 13h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (4397h):           SB700 USB OHCI0 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02B000h - FE02BFFFh
     System IRQ:               10
     Interrupt Pin:            INTA#

  Bus: 00h, Device: 13h, Function: 01h
     Vendor (1002h):           ATI Technologies Inc
     Device (4398h):           SB700 USB OHCI1 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE02A000h - FE02AFFFh
     System IRQ:               10
     Interrupt Pin:            INTA#

  Bus: 00h, Device: 13h, Function: 02h
     Vendor (1002h):           ATI Technologies Inc
     Device (4396h):           SB700 USB EHCI Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                20h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE029000h - FE0290FFh
     System IRQ:               11
     Interrupt Pin:            INTB#

  Bus: 00h, Device: 14h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (4385h):           IXP SB600 SMBUS Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (4385h):     Unknown
     Class (0Ch):              Serial
     SubClass (05h):           SMBus Controller
     Revision:                 3Ch
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [ ]
     66 MHz Speed Support:     [X]
  Device Resources
     SMBus Port:               0B00h

  Bus: 00h, Device: 14h, Function: 01h
     Vendor (1002h):           ATI Technologies Inc
     Device (439Ch):           SB700 IDE
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5002h):     Unknown
     Class (01h):              Storage
     SubClass (01h):           IDE
     Revision:                 00h
     Interface:                8Ah
  Device Properties
     Device Timing:            Medium
     Memory Access:            [ ]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            0000FA00h - 0000FA0Fh

  Bus: 00h, Device: 14h, Function: 02h
     Vendor (1002h):           ATI Technologies Inc
     Device (4383h):           IXP SB600 High Definition Audio Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (A022h):     Unknown
     Class (04h):              Multimedia
     SubClass (03h):           Hi-definition Audio
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Slow
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           FE024000h - FE027FFFh
     System IRQ:               3
     Interrupt Pin:            INTA#

  Bus: 00h, Device: 14h, Function: 03h
     Vendor (1002h):           ATI Technologies Inc
     Device (439Dh):           SB700 LPC host controller
     Subsys Vendor (1002h):    ATI Technologies Inc
     Subsystem ID (439Dh):     Unknown
     Class (06h):              Bridge
     SubClass (01h):           PCI/ISA
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources

  Bus: 00h, Device: 14h, Function: 04h
     Vendor (1002h):           ATI Technologies Inc
     Device (4384h):           IXP SB600 PCI to PCI Bridge
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 00h
     Interface:                01h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            C000h - CFFFh
     Memory Address:           FDD00000h - FDDFFFFFh
     Memory Address:           FDC00000h - FDCFFFFFh

  Bus: 00h, Device: 14h, Function: 05h
     Vendor (1002h):           ATI Technologies Inc
     Device (4399h):           SB700 USB OHCI2 Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (5004h):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           FE028000h - FE028FFFh
     System IRQ:               10
     Interrupt Pin:            INTC#

  Bus: 00h, Device: 18h, Function: 00h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1200h):           K10 [Opteron, Athlon64, Sempron] HyperTransport Configuration
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources

  Bus: 00h, Device: 18h, Function: 01h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1201h):           K10 [Opteron, Athlon64, Sempron] Address Map
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources

  Bus: 00h, Device: 18h, Function: 02h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1202h):           K10 [Opteron, Athlon64, Sempron] DRAM Controller
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources

  Bus: 00h, Device: 18h, Function: 03h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1203h):           K10 [Opteron, Athlon64, Sempron] Miscellaneous Control
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources

  Bus: 00h, Device: 18h, Function: 04h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1204h):           K10 [Opteron, Athlon64, Sempron] Link Control
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources

  Bus: 01h, Device: 00h, Function: 00h
     Vendor (1002h):           ATI Technologies Inc
     Device (9440h):           RV770 [Radeon HD 4870]
     Subsys Vendor (1787h):    Hightech Information System Ltd (Medion??)
     Subsystem ID (2267h):     Unknown
     Class (03h):              Display
     SubClass (00h):           VGA
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           D0000000h - DFFFFFFFh
     Memory Address:           FDFE0000h - FDFEFFFFh
     Base I/O Port:            0000EE00h - 0000EEFFh
     System IRQ:               10
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               2.5 GB/s (Current: 2.5 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0

  Bus: 01h, Device: 00h, Function: 01h
     Vendor (1002h):           ATI Technologies Inc
     Device (AA30h):           HD48x0 audio
     Subsys Vendor (1787h):    Hightech Information System Ltd (Medion??)
     Subsystem ID (AA30h):     Unknown
     Class (04h):              Multimedia
     SubClass (03h):           Hi-definition Audio
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           FDFFC000h - FDFFFFFFh
     System IRQ:               10
     Interrupt Pin:            INTB#
  AC'97/HDA Capabilities
     AC'97/HDA Codec Name:     ATI R600 HDMI
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               2.5 GB/s (Current: 2.5 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0

  Bus: 02h, Device: 00h, Function: 00h
     Vendor (10ECh):           Realtek Semiconductor
     Device (8168h):           RTL8168/8111 PCI-E Gigabit Ethernet NIC
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (E000h):     GA-EP45-DS5 Motherboard
     Class (02h):              Network
     SubClass (00h):           Ethernet
     Revision:                 02h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            0000DE00h - 0000DEFFh
     Memory Address:           FDBFF000h - FDBFFFFFh
     Memory Address:           FDBE0000h - FDBEFFFFh
     System IRQ:               10
     Interrupt Pin:            INTA#
  PCI-E Capabilities
     PCI Express Version:      1
     Link Speed:               2.5 GB/s (Current: 2.5 GB/s)
     Link Width:               x1 (Current: x1)
     Link Port Number:         0
     Physical Slot Number:     0

  Bus: 03h, Device: 06h, Function: 00h
     Vendor (1102h):           Creative Labs
     Device (0004h):           EMU10K2 Audio Chipset (SB Audigy Series)
     Subsys Vendor (1102h):    Creative Labs
     Subsystem ID (2005h):     Unknown
     Class (04h):              Multimedia
     SubClass (01h):           Audio
     Revision:                 04h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [ ]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            0000CF00h - 0000CF3Fh
     System IRQ:               5
     Interrupt Pin:            INTA#

  Bus: 03h, Device: 0Eh, Function: 00h
     Vendor (104Ch):           Texas Instruments (TI)
     Device (8024h):           TSB43AB23 1394a-2000 OHCI PHY/link-layer Controller
     Subsys Vendor (1458h):    Giga-Byte Technology
     Subsystem ID (1000h):     GA-EP45-DS5 Motherboard
     Class (0Ch):              Serial
     SubClass (00h):           Firewire
     Revision:                 00h
     Interface:                10h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Memory Address:           FDDFF000h - FDDFF7FFh
     Memory Address:           FDDF8000h - FDDFBFFFh
     System IRQ:               11
     Interrupt Pin:            INTA#

                  +-----------------------------------------+
                  |              Memory Modules             |
                  +-----------------------------------------+
  Memory Slot 1
     Memory Type:              1024MB DDR3-1333 (PC3-10600) SDRAM
     Manufacturer:             Kingston
     Module Type:              Unbuffered DIMM
     Number of Ranks/Banks:    1 Ranks, 8 Banks
     Module Attributes:        Unbuffered
     Error Checking:           None
     CAS# Latency:             9.0 (Cycle Time: 1.500ns/686MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 9.0-9-9-24)
                               (tWR-tRC: 10-33)
     CAS# Latency:             8.0 (Cycle Time: 1.371ns/610MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 8.0-8-8-22)
                               (tWR-tRC: 10-30)
     CAS# Latency:             7.0 (Cycle Time: 1.200ns/533MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 7.0-7-7-20)
                               (tWR-tRC: 8-27)
     CAS# Latency:             6.0 (Cycle Time: 1.029ns/457MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 6.0-6-6-17)
                               (tWR-tRC: 7-23)
     Refresh Rate:             7.8 us (2X 85-95 C)
     Data Width:               64 bits
     SDRAM Width:              x8
     Voltage Interface:        1.5 V
     Max Case Temperature:     95 C (203 F)
     SPD Revision:             1.0
     Part Number:              9905402-015.A03LF
     Manufacturing Location:   China
     Manufacture Date:         September 2009 (0926h)
     Serial Number:            14CC41B4h
     Revision Code:            None
     EPP is Supported:         [ ]

  Memory Slot 2
     Memory Type:              1024MB DDR3-1333 (PC3-10600) SDRAM
     Manufacturer:             Kingston
     Module Type:              Unbuffered DIMM
     Number of Ranks/Banks:    1 Ranks, 8 Banks
     Module Attributes:        Unbuffered
     Error Checking:           None
     CAS# Latency:             9.0 (Cycle Time: 1.500ns/686MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 9.0-9-9-24)
                               (tWR-tRC: 10-33)
     CAS# Latency:             8.0 (Cycle Time: 1.371ns/610MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 8.0-8-8-22)
                               (tWR-tRC: 10-30)
     CAS# Latency:             7.0 (Cycle Time: 1.200ns/533MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 7.0-7-7-20)
                               (tWR-tRC: 8-27)
     CAS# Latency:             6.0 (Cycle Time: 1.029ns/457MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 6.0-6-6-17)
                               (tWR-tRC: 7-23)
     Refresh Rate:             7.8 us (2X 85-95 C)
     Data Width:               64 bits
     SDRAM Width:              x8
     Voltage Interface:        1.5 V
     Max Case Temperature:     95 C (203 F)
     SPD Revision:             1.0
     Part Number:              9905402-015.A03LF
     Manufacturing Location:   China
     Manufacture Date:         September 2009 (0926h)
     Serial Number:            16CC37B4h
     Revision Code:            None
     EPP is Supported:         [ ]

                  +-----------------------------------------+
                  |             Memory (SMBIOS)             |
                  +-----------------------------------------+
  Physical Memory Array 1
     Maximum Capacity:         2048 MB
     Location:                 System Board or Motherboard
     Use:                      System Memory
     Memory Error Correct.:    None
     Memory Devices:           4
     Structure Length:         0Fh
  Memory Device 1
     Size:                     1024 MB
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    1066 MHz
     Device Locator:           A0
     Bank Locator:             Bank0/1
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         1Bh
  Memory Device 2
     Size:                     1024 MB
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    1066 MHz
     Device Locator:           A1
     Bank Locator:             Bank2/3
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         1Bh
  Memory Device 3
     Size:                     Not Installed
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    1066 MHz
     Device Locator:           A2
     Bank Locator:             Bank4/5
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         1Bh
  Memory Device 4
     Size:                     Not Installed
     Form Factor:              DIMM
     Memory Type:              Unknown
     Speed:                    1066 MHz
     Device Locator:           A3
     Bank Locator:             Bank6/7
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Manufacturer:
     Serial Number:
     Asset Tag:
     Part Number:
     Structure Length:         1Bh

                  +-----------------------------------------+
                  |                   HDD                   |
                  +-----------------------------------------+
  Tertiary/Master HDD
     HDD Model:                WDC WD1001FALS-00J7B0
     HDD Size:                 953869 MB (931.51 GB)
     Interface Type:           Serial ATA II
     Geometry:                 Heads: 16, Sectors: 63, Tracks: 16383
     Compatibility:            ATA/ATAPI-7
     Serial Number:            WD-WMATV0357962
     Controller Revision:      05.00K05
     HDD Marketing Size:       1000204 MB (1000.20 GB)
     Buffer Size:              32767.5 kB
     Buffer Type:              Not Specified
     HDD Temperature:          50 C (122 F)
     Reallocated Sectors:      0
     HDD Health Status:        Good
     ECC bytes:                50
     Security Erase Time:      194 min
     Enh. Security Erase:      194 min
     Current APM Value:        None
     Acoustic Management:      FEh (80h Recommended) - Disabled
     ATA Controller Vendor:    ATI Technologies Inc
     ATA Controller Name:      SB700 SATA Controller [IDE mode]
     Device Location:          Tertiary/Master
  Transfer Modes
     PIO Mode Support:         4
     SW DMA Mode Support:      Not Supported
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        6 (UltraDMA/133), Active: 6 (UltraDMA/133)
     Sectors per Interrupt:    16, Active: 16
  HDD Features
     SATA NCQ Command:                    [X]
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [X]
     Double Word I/O:                     [ ]
     Standard Standby Timer:              [X]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     S.M.A.R.T.:                          [X] enabled
     S.M.A.R.T. Self-test:                [X] enabled
     S.M.A.R.T. Error Logging:            [X] enabled
     Security Mode Feature Set:           [X] disabled
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [ ]
     Write Cache:                         [X] enabled
     Look-ahead:                          [X] enabled
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [ ]
     Host Protected Area:                 [X] enabled
     Write Verify Command:                [ ]
     Write Buffer Command:                [X] enabled
     Read Buffer Command:                 [X] enabled
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [X] enabled
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [X] disabled
     Set Features Req. to Spinup:         [X] enabled
     Set Max Security Extension:          [X] disabled
     Automatic Acoustic Management:       [X] disabled
     48-bit Address:                      [X] enabled
     Device Configuration Overlay:        [X] enabled
     Flush Cache Command:                 [X] enabled
     Flush Cache Ext Command:             [X] enabled
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [X] enabled
     Write DMA/Multiple FUA EXT:          [ ]
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [X] enabled
  S.M.A.R.T.
     ID  | Attribute Name            |Threshold|Worst|Value| Raw Value
     ----+---------------------------+---------+-----+-----+-----------
     1   | Raw Read Error Rate       |       51|  200|  200|          0
     3   | Spin-up Time              |       21|  253|  253|       4350
     4   | Start/Stop Count          |        0|   99|   99|       1275
     5   | Reallocated Sectors Count |      140|  200|  200|          0
     7   | Seek Error Rate           |       51|  200|  200|          0
     9   | Power On Hours Count      |        0|   96|   96|       3124
     10  | Spin-up Retry Count       |       51|  100|  100|          0
     11  | Recalibration Retries     |       51|  100|  100|          0
     12  | Drive Power Cycle Count   |        0|   99|   99|       1257
     192 | Power-Off Retract Cycle   |        0|  199|  199|        883
     193 | Load/Unload Cycle Count   |        0|  200|  200|       1275
     194 | Drive Temperature         |        0|   94|  100|         50
     196 | Reallocation Event Count  |        0|  200|  200|          0
     197 | Current Pending Sectors   |        0|  200|  200|          0
     198 | Uncorrectable Sectors     |        0|  200|  200|          0
     199 | UltraDMA CRC Error Rate   |        0|  200|  200|          0
     200 | Write Error Rate          |       51|  200|  200|          0

                  +-----------------------------------------+
                  |                  ATAPI                  |
                  +-----------------------------------------+
  Primary/Master ATAPI
     ATAPI Model:              _NEC DVD_RW ND-3550A
     ATAPI Type:               DVD+-RW DL/CD-RW
     Interface Type:           Parallel ATA
     Physical Interface:       ATAPI
     ATAPI Name:               _NEC DVD_RW ND-3550A
     Vendor Specific:          05093000
     CD Read Speed:            48x (Current: 48x)
     CD Write Speed:           48x (Current: 48x)
     DVD Read Speed:           Current: 6x
     DVD Write Speed:          Current: 6x
     Buffer Size:              2048 kB
     Loading Mechanism:        Tray Type
     Rotation Control:         CLV
     Read Retry Count:         15
     Write Retry Count:        0
     Compatibility:            Unknown
     Serial Number:            63E1J06S211
     Controller Revision:      1.05
     Command DRQ Type:         Microprocessor DRQ
     Command Packet Size:      12 bytes
     ATA Controller Vendor:    ATI Technologies Inc
     ATA Controller Name:      SB700 IDE
     Device Location:          Primary/Master
  Transfer Modes
     PIO Mode Support:         4
     SW DMA Mode Support:      Not Supported
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        2 (UltraDMA/33), Active: 2 (UltraDMA/33)
  Reading Features
     CD-R Disk Read:                      [X]
     CD-RW Disk Read:                     [X]
     DVD-ROM Disk Read:                   [X]
     DVD-RAM Disk Read:                   [ ]
     DVD-R Disk Read:                     [X]
     DVD-R DL Disk Read:                  [X]
     DVD-RW Disk Read:                    [X]
     DVD-RW DL Disk Read:                 [ ]
     DVD+R Disk Read:                     [X]
     DVD+R DL Disk Read:                  [X]
     DVD+RW Disk Read:                    [X]
     DVD+RW DL Disk Read:                 [ ]
     BD-ROM Disk Read:                    [ ]
     BD-R Disk Read:                      [ ]
     BD-RE Disk Read:                     [ ]
     HD DVD-ROM Disk Read:                [ ]
     HD DVD-RAM Disk Read:                [ ]
     HD DVD-R Disk Read:                  [ ]
     HD DVD-R DL Disk Read:               [ ]
     HD DVD-RW Disk Read:                 [ ]
     HD DVD-RW DL Disk Read:              [ ]
     Read Packet Using Method 2:          [X]
     Read Mode2 Form1 Sectors:            [X]
     Read Mode2 Form2 Sectors:            [X]
     Multisession Disk Read:              [X]
     READ-CD Command on AudioCD:          [X]
     Read Bar Code Capable:               [ ]
     Read Lead-in (CD-Text):              [X]
  Writing Features
     CD-R Disk Write:                     [X]
     CD-RW Disk Write:                    [X]
     DVD-RAM Disk Write:                  [ ]
     DVD-R Disk Write:                    [X]
     DVD-R DL Disk Write:                 [X]
     DVD-RW Disk Write:                   [X]
     DVD+R Disk Write:                    [X]
     DVD+R DL Disk Write:                 [X]
     DVD+RW Disk Write:                   [X]
     DVD+RW DL Disk Write:                [ ]
     BD-R Disk Write:                     [ ]
     BD-RE Disk Write:                    [ ]
     HD DVD-R Disk Write:                 [ ]
     HD DVD-R DL Disk Write:              [ ]
     HD DVD-RAM Disk Write:               [ ]
     HD DVD-RW Disk Write:                [ ]
     HD DVD-RW DL Disk Write:             [ ]
     Test Write Mode Support:             [X]
     Buffer Underrun Protection:          [X]
  Other Features
     Audio Play Support:                  [X]
     CD-DA Stream is Accurate:            [X]
     Composite Audio/Video:               [ ]
     Digital Output on Port 1:            [ ]
     Digital Output on Port 2:            [ ]
     Support Subcode R-W:                 [X]
     Support Subcode R-W D&C:             [ ]
     C2 Pointers Supported:               [X]
     ISRC Supported:                      [X]
     UPC Supported:                       [X]
  ATAPI Features
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [ ]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [ ]
     ATA Software Reset:                  [ ]
     Overlap Operation:                   [ ]
     Command Queuing:                     [ ]
     Interleaving DMA:                    [ ]

  Primary/Slave ATAPI
     ATAPI Model:              CD-W540E
     ATAPI Type:               CD-RW
     Interface Type:           Parallel ATA
     Physical Interface:       ATAPI
     ATAPI Name:               TEAC CD-W540E
     Vendor Specific:          09/30/02
     CD Read Speed:            48x (Current: 48x)
     CD Write Speed:           40x (Current: 40x)
     Buffer Size:              8192 kB
     Loading Mechanism:        Tray Type
     Rotation Control:         CLV
     Read Retry Count:         5
     Write Retry Count:        3
     Compatibility:            ATA/ATAPI-5 revision 19
     Serial Number:
     Controller Revision:      1.0H
     Command DRQ Type:         Accelerated DRQ
     Command Packet Size:      12 bytes
     ATA Controller Vendor:    ATI Technologies Inc
     ATA Controller Name:      SB700 IDE
     Device Location:          Primary/Slave
  Transfer Modes
     PIO Mode Support:         4
     SW DMA Mode Support:      2, Active: None
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        2 (UltraDMA/33), Active: 2 (UltraDMA/33)
  Reading Features
     CD-R Disk Read:                      [X]
     CD-RW Disk Read:                     [X]
     DVD-ROM Disk Read:                   [ ]
     DVD-RAM Disk Read:                   [ ]
     DVD-R Disk Read:                     [ ]
     DVD-R DL Disk Read:                  [ ]
     DVD-RW Disk Read:                    [ ]
     DVD-RW DL Disk Read:                 [ ]
     DVD+R Disk Read:                     [ ]
     DVD+R DL Disk Read:                  [ ]
     DVD+RW Disk Read:                    [ ]
     DVD+RW DL Disk Read:                 [ ]
     BD-ROM Disk Read:                    [ ]
     BD-R Disk Read:                      [ ]
     BD-RE Disk Read:                     [ ]
     HD DVD-ROM Disk Read:                [ ]
     HD DVD-RAM Disk Read:                [ ]
     HD DVD-R Disk Read:                  [ ]
     HD DVD-R DL Disk Read:               [ ]
     HD DVD-RW Disk Read:                 [ ]
     HD DVD-RW DL Disk Read:              [ ]
     Read Packet Using Method 2:          [X]
     Read Mode2 Form1 Sectors:            [X]
     Read Mode2 Form2 Sectors:            [X]
     Multisession Disk Read:              [X]
     READ-CD Command on AudioCD:          [X]
     Read Bar Code Capable:               [ ]
     Read Lead-in (CD-Text):              [X]
  Writing Features
     CD-R Disk Write:                     [X]
     CD-RW Disk Write:                    [X]
     DVD-RAM Disk Write:                  [ ]
     DVD-R Disk Write:                    [ ]
     DVD-R DL Disk Write:                 [ ]
     DVD-RW Disk Write:                   [ ]
     DVD+R Disk Write:                    [ ]
     DVD+R DL Disk Write:                 [ ]
     DVD+RW Disk Write:                   [ ]
     DVD+RW DL Disk Write:                [ ]
     BD-R Disk Write:                     [ ]
     BD-RE Disk Write:                    [ ]
     HD DVD-R Disk Write:                 [ ]
     HD DVD-R DL Disk Write:              [ ]
     HD DVD-RAM Disk Write:               [ ]
     HD DVD-RW Disk Write:                [ ]
     HD DVD-RW DL Disk Write:             [ ]
     Test Write Mode Support:             [X]
     Buffer Underrun Protection:          [X]
  Other Features
     Audio Play Support:                  [X]
     CD-DA Stream is Accurate:            [X]
     Composite Audio/Video:               [ ]
     Digital Output on Port 1:            [ ]
     Digital Output on Port 2:            [ ]
     Support Subcode R-W:                 [X]
     Support Subcode R-W D&C:             [ ]
     C2 Pointers Supported:               [X]
     ISRC Supported:                      [X]
     UPC Supported:                       [X]
  ATAPI Features
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [ ]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     ATA Software Reset:                  [ ]
     Overlap Operation:                   [ ]
     Command Queuing:                     [ ]
     Interleaving DMA:                    [ ]
     S.M.A.R.T.:                          [ ]
     S.M.A.R.T. Self-test:                [ ]
     S.M.A.R.T. Error Logging:            [ ]
     Security Mode Feature Set:           [ ]
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [X] enabled
     Write Cache:                         [ ]
     Look-ahead:                          [ ]
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [X] enabled
     Host Protected Area:                 [ ]
     Write Verify Command:                [ ]
     Write Buffer Command:                [ ]
     Read Buffer Command:                 [ ]
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [ ]
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [ ]
     Set Features Req. to Spinup:         [ ]
     Set Max Security Extension:          [ ]
     Automatic Acoustic Management:       [ ]
     48-bit Address:                      [ ]
     Device Configuration Overlay:        [ ]
     Flush Cache Command:                 [ ]
     Flush Cache Ext Command:             [ ]
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [ ]
     Write DMA/Multiple FUA EXT:          [ ]
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [ ]

                  +-----------------------------------------+
                  |              Storage (ASPI)             |
                  +-----------------------------------------+
     ASPI manager not found

                  +-----------------------------------------+
                  |                  Drives                 |
                  +-----------------------------------------+
  BIOS Drives
     INT 13h Extensions:       Not Supported
  A:
     Drive Letter:             A:
     Drive Size:               1.44 MB
     Drive Type:               Floppy 1.44 MB (3.5")
     Cylinders:                80
     Heads:                    2
     Sectors:                  18

  Local Drives
  A:
     Drive Letter:             A:
     Drive Type:               Floppy 1.44 MB (3.5")
  C:[SYSTEM]
     Drive Letter:             C:
     Drive Type:               Fixed Disk
     Volume Label:             SYSTEM
     File System:              FAT16
     Volume Serial Number:     2255-1BEA
     Total Size:               2047.0 MB
     Free Space:               1017.9 MB (49.7%)
  D:[KINGSTON]
     Drive Letter:             D:
     Drive Type:               Fixed Disk
     Volume Label:             KINGSTON
     File System:              FAT16
     Volume Serial Number:     94C6-CB33
     Total Size:               491.2 MB
     Free Space:               351.0 MB (71.4%)
  E:[UTILITIES]
     Drive Letter:             E:
     Drive Type:               Fixed Disk
     Volume Label:             UTILITIES
     File System:              FAT16
     Volume Serial Number:     2E4A-1BEB
     Total Size:               2047.1 MB
     Free Space:               42.2 MB (2.1%)
  F:[GAMES]
     Drive Letter:             F:
     Drive Type:               Fixed Disk
     Volume Label:             GAMES
     File System:              FAT16
     Volume Serial Number:     2D54-1BEC
     Total Size:               2047.1 MB
     Free Space:               709.7 MB (34.7%)

                  +-----------------------------------------+
                  |               USB Devices               |
                  +-----------------------------------------+
     USB devices not found

                  +-----------------------------------------+
                  |              Plug and Play              |
                  +-----------------------------------------+
  Plug and Play
     PnP Version:              1.0
     Number of PnP Devices:    14

  Device Number 1
     PnP Device Name:          AT Interrupt Controller
     PnP Device ID:            PNP0000
     Base Type (08h):          System Peripheral
     SubType (00h):            Interrupt controller
     Node Size:                37 byte
  Device Resources
     I/O Port:                 0020h-0021h
     I/O Port:                 00A0h-00A1h
     System IRQ:               2 - High True Edge

  Device Number 2
     PnP Device Name:          AT DMA Controller
     PnP Device ID:            PNP0200
     Base Type (08h):          System Peripheral
     SubType (01h):            DMA controller
     Node Size:                69 byte
  Device Resources
     I/O Port:                 0000h-000Fh
     I/O Port:                 0081h-0083h
     I/O Port:                 0087h-0087h
     I/O Port:                 0089h-008Bh
     I/O Port:                 008Fh-0091h
     I/O Port:                 00C0h-00DFh
     DMA Channel:              4 - Type 8237 (8-bit)

  Device Number 3
     PnP Device Name:          AT Timer
     PnP Device ID:            PNP0100
     Base Type (08h):          System Peripheral
     SubType (02h):            System timer
     Node Size:                29 byte
  Device Resources
     I/O Port:                 0040h-0043h
     System IRQ:               0 - High True Edge

  Device Number 4
     PnP Device Name:          AT Real-Time Clock
     PnP Device ID:            PNP0B00
     Base Type (08h):          System Peripheral
     SubType (03h):            Real Time Clock
     Node Size:                29 byte
  Device Resources
     I/O Port:                 0070h-0071h
     System IRQ:               8 - High True Edge

  Device Number 5
     PnP Device Name:          IBM Enhanced keyboard controller (101/2-key)
     PnP Device ID:            PNP0303
     Base Type (09h):          Input Device
     SubType (00h):            Keyboard Controller
     Node Size:                37 byte
  Device Resources
     I/O Port:                 0060h-0060h
     I/O Port:                 0064h-0064h
     System IRQ:               1 - High True Edge

  Device Number 6
     PnP Device Name:          AT standard speaker sound
     PnP Device ID:            PNP0800
     Base Type (08h):          System Peripheral
     SubType (80h):            Other System device
     Node Size:                26 byte
  Device Resources
     I/O Port:                 0061h-0061h

  Device Number 7
     PnP Device Name:          Math Coprocessor
     PnP Device ID:            PNP0C04
     Base Type (0Bh):          CPU Type
     SubType (01h):            486 CPU
     Node Size:                29 byte
  Device Resources
     I/O Port:                 00F0h-00FFh
     System IRQ:               13 - High True Edge

  Device Number 8
     PnP Device Name:          System Board
     PnP Device ID:            PNP0C01
     Base Type (05h):          Memory
     SubType (00h):            RAM Memory
     Node Size:                90 byte
  Device Resources
     Memory Address:           00000000h-FFFFFFFFh RAM 8-bit Cacheble
     Memory Address:           FFFE0000h-FFFDFFFFh ROM 8/16-bit Cacheble
     Memory Address:           FFF80000h-FFF7FFFFh ROM 8/16-bit Cacheble
     Memory Address:           FEC00000h-FEBFFFFFh ROM 8/16-bit Cacheble
     Memory Address:           FEE00000h-FEDFFFFFh ROM 8/16-bit Cacheble
     Memory Address:           00100000h-7F0FFFFFh RAM 8-bit Cacheble

  Device Number 9
     PnP Device Name:          Motherboard registers
     PnP Device ID:            PNP0C02
     Base Type (08h):          System Peripheral
     SubType (80h):            Other System device
     Node Size:                66 byte
  Device Resources
     Memory Address:           000F0000h-000F3FFFh ROM 8/16-bit Cacheble Shadow
     Memory Address:           000F4000h-000F7FFFh ROM 8/16-bit Cacheble Shadow
     Memory Address:           000F8000h-000FFFFFh ROM 8/16-bit Cacheble Shadow
     Memory Address:           000CF800h-000CFFFFh ROM 8/16-bit Cacheble Shadow

  Device Number 10
     PnP Device Name:          PCI Bus
     PnP Device ID:            PNP0A03
     Base Type (06h):          Bridge Controller
     SubType (04h):            PCI Bridge
     Node Size:                42 byte
  Device Resources
     I/O Port:                 0290h-029Fh
     I/O Port:                 04D0h-04D1h
     I/O Port:                 0CF8h-0CFFh

  Device Number 11
     PnP Device Name:          PS/2 Port for PS/2-style Mice
     PnP Device ID:            PNP0F13
     Base Type (09h):          Input Device
     SubType (02h):            Mouse Controller
     Node Size:                26 byte
  Device Resources
     System IRQ:               12 - High True Edge

  Device Number 12
     PnP Device Name:          16550A-compatible COM port
     PnP Device ID:            PNP0501
     Base Type (07h):          Communications
     SubType (00h):            RS-232 Serial port
     Node Size:                69 byte
  Device Resources
     I/O Port:                 03F8h-03FFh
     System IRQ:               4 - High True Edge

  Device Number 13
     PnP Device Name:          PC standard floppy disk controller
     PnP Device ID:            PNP0700
     Base Type (01h):          Mass Storage
     SubType (02h):            Floppy Controller
     Node Size:                64 byte
  Device Resources
     I/O Port:                 03F0h-03F5h
     I/O Port:                 03F7h-03F7h
     System IRQ:               6 - High True Edge
     DMA Channel:              2 - Type 8237 (8-bit)

  Device Number 14
     PnP Device Name:          Standard LPT printer port
     PnP Device ID:            PNP0400
     Base Type (07h):          Communications
     SubType (01h):            AT Parallel port
     Node Size:                92 byte
  Device Resources
     I/O Port:                 0378h-037Fh
     I/O Port:                 0778h-077Fh
     System IRQ:               7 - High True Edge

                  +-----------------------------------------+
                  |            Physical Printers            |
                  +-----------------------------------------+
     LPT/PnP or USB printer not found

                  +-----------------------------------------+
                  |              Slots (SMBIOS)             |
                  +-----------------------------------------+
  Slot PCI
     Slot Type:                PCI
     Current Usage:            Available
     Data Bus Width:           32 bit
     Slot Designation:         PCI
     Slot Length:              Long Length
     Slot ID:                  7
  Slot PCI
     Slot Type:                PCI
     Current Usage:            In Use
     Data Bus Width:           32 bit
     Slot Designation:         PCI
     Slot Length:              Long Length
     Slot ID:                  6
  Slot PCI Express
     Slot Type:                PCI Express
     Current Usage:            Unknown
     Data Bus Width:           16x or x16
     Slot Designation:         PCI Express x16
     Slot Length:              Other
     Slot ID:                  0

                  +-----------------------------------------+
                  |              Ports (SMBIOS)             |
                  +-----------------------------------------+
  Port 1 Other
     Int. Connector Type:      On Board IDE
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          PRIMARY IDE
     Ext. Designator:
  Port 2 8251 FIFO Compatible
     Int. Connector Type:      On Board Floppy
     Ext. Connector Type:      None
     Port Type:                8251 FIFO Compatible
     Int. Designator:          FDD
     Ext. Designator:
  Port 3 Serial Port 16450 Compatible
     Int. Connector Type:      9 Pin Dual Inline (pin 10 cut)
     Ext. Connector Type:      DB-9 pin male
     Port Type:                Serial Port 16450 Compatible
     Int. Designator:          COM1
     Ext. Designator:
  Port 4 Serial Port 16450 Compatible
     Int. Connector Type:      9 Pin Dual Inline (pin 10 cut)
     Ext. Connector Type:      DB-9 pin male
     Port Type:                Serial Port 16450 Compatible
     Int. Designator:          COM2
     Ext. Designator:
  Port 5 Parallel Port ECP/EPP
     Int. Connector Type:      DB-25 pin female
     Ext. Connector Type:      DB-25 pin female
     Port Type:                Parallel Port ECP/EPP
     Int. Designator:          LPT1
     Ext. Designator:
  Port 6 Keyboard Port
     Int. Connector Type:      Other
     Ext. Connector Type:      PS/2
     Port Type:                Keyboard Port
     Int. Designator:          Keyboard
     Ext. Designator:
  Port 7 Mouse Port
     Int. Connector Type:      PS/2
     Ext. Connector Type:      PS/2
     Port Type:                Mouse Port
     Int. Designator:          PS/2 Mouse
     Ext. Designator:          Detected
  Port 8 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 9 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 10 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 11 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 12 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 13 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 14 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 15 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 16 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 17 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 18 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:
  Port 19 USB
     Int. Connector Type:      None
     Ext. Connector Type:      USB
     Port Type:                USB
     Int. Designator:          USB
     Ext. Designator:

                  +-----------------------------------------+
                  |                 Monitor                 |
                  +-----------------------------------------+
  Monitor
     Monitor Vendor:           LG Electronics Inc.
     Monitor Model:            LG FLATRON F920P
     Viewable Size:            17.7" (45.0 sm)
     Serial Number:            319823
     Manufacture Date:         March 2005
     EDID Version:             1.3
     Monitor ID:               GSM4A88
     Aspect Ratio:             4:3
     Horizontal Size:          36 sm
     Vertical Size:            27 sm
     Gamma Factor:             2.910
     Display Type:             RGB Color
     Input Signal:             Analog
     Internal Model:           F920P
     Vertical Frequency:       50-160 Hz
     Horizontal Frequency:     30-111 kHz
  DPMS Features
     Active Off:               [X]
     Suspend:                  [X]
     Standby:                  [X]
  Supported Modes
     Mode 1:                   720x400   @ 70 Hz (VGA)
     Mode 2:                   720x400   @ 88 Hz (XGA2)
     Mode 3:                   640x480   @ 60 Hz (VGA)
     Mode 4:                   640x480   @ 67 Hz (Mac II)
     Mode 5:                   640x480   @ 72 Hz (VESA)
     Mode 6:                   640x480   @ 75 Hz (VESA)
     Mode 7:                   800x600   @ 56 Hz (VESA)
     Mode 8:                   800x600   @ 60 Hz (VESA)
     Mode 9:                   800x600   @ 72 Hz (VESA)
     Mode 10:                  800x600   @ 75 Hz (VESA)
     Mode 11:                  832x624   @ 75 Hz (Mac II)
     Mode 12:                  1024x768  @ 87 Hz (interlaced)
     Mode 13:                  1024x768  @ 60 Hz (VESA)
     Mode 14:                  1024x768  @ 70 Hz (VESA)
     Mode 15:                  1024x768  @ 75 Hz (VESA)
     Mode 16:                  1280x1024 @ 75 Hz (VESA)
     Mode 17:                  1920x1440 @ 70 Hz
     Mode 18:                  2048x1536 @ 60 Hz
     Mode 19:                  1024x768  @ 85 Hz
     Mode 20:                  1280x1024 @ 75 Hz
     Mode 21:                  1280x1024 @ 85 Hz
     Mode 22:                  1600x1200 @ 75 Hz
     Mode 23:                  1600x1200 @ 85 Hz
     Mode 24:                  1152x864  @ 75 Hz

                  +-----------------------------------------+
                  |                  Video                  |
                  +-----------------------------------------+
  Video
     Video Chip Vendor:        ATI Technologies Inc
     Video Chip:               RV770 [Radeon HD 4870]
     Subsystem Vendor:         Hightech Information System Ltd (Medion??)
     Video Memory Size:        16 MB
     Bus Type:                 PCI-E
     VESA OEM String:          ATI ATOMBIOS
     VESA Version:             3.0
     Vendor Name:              (C) 1988-2005, ATI Technologies Inc.
     Product Name:             RV770 01.00
     OEM Software Version:     11.10
  VESA Power Management
     VESA PM Version:          1.0
     Standby:                  [ ]
     Suspend:                  [ ]
     Off:                      [X]
     Reduced On:               [ ]
  PCI-E Capabilities
     PCI Express Version:      2
     Link Speed:               2.5 GB/s (Current: 2.5 GB/s)
     Link Width:               x16 (Current: x16)
     Link Port Number:         0
     Physical Slot Number:     0
  VESA Modes
     Number | Mode  |Resolution|Colors| bpp| Features
     -------+-------+----------+------+----+----------
       100h | Graph |   640x400|   256|   8| Bank + LFB
       101h | Graph |   640x480|   256|   8| Bank + LFB
       103h | Graph |   800x600|   256|   8| Bank + LFB
       105h | Graph |  1024x768|   256|   8| Bank + LFB
       107h | Graph | 1280x1024|   256|   8| Bank + LFB
       110h | Graph |   640x480|   64k|  16| Bank + LFB
       111h | Graph |   640x480|   64k|  16| Bank + LFB
       113h | Graph |   800x600|   64k|  16| Bank + LFB
       114h | Graph |   800x600|   64k|  16| Bank + LFB
       116h | Graph |  1024x768|   64k|  16| Bank + LFB
       117h | Graph |  1024x768|   64k|  16| Bank + LFB
       119h | Graph | 1280x1024|   64k|  16| Bank + LFB
       11Ah | Graph | 1280x1024|   64k|  16| Bank + LFB
       10Dh | Graph |   320x200|   64k|  16| Bank + LFB
       10Eh | Graph |   320x200|   64k|  16| Bank + LFB
       120h | Graph |   320x200|   16M|  32| Bank + LFB
       193h | Graph |   320x240|   256|   8| Bank + LFB
       195h | Graph |   320x240|   64k|  16| Bank + LFB
       196h | Graph |   320x240|   16M|  32| Bank + LFB
       1B3h | Graph |   512x384|   256|   8| Bank + LFB
       1B5h | Graph |   512x384|   64k|  16| Bank + LFB
       1B6h | Graph |   512x384|   16M|  32| Bank + LFB
       1C3h | Graph |   640x350|   256|   8| Bank + LFB
       1C5h | Graph |   640x350|   64k|  16| Bank + LFB
       1C6h | Graph |   640x350|   16M|  32| Bank + LFB
       133h | Graph |   720x400|   256|   8| Bank + LFB
       135h | Graph |   720x400|   64k|  16| Bank + LFB
       136h | Graph |   720x400|   16M|  32| Bank + LFB
       153h | Graph |  1152x864|   256|   8| Bank + LFB
       155h | Graph |  1152x864|   64k|  16| Bank + LFB
       156h | Graph |  1152x864|   16M|  32| Bank + LFB
       163h | Graph |  1280x960|   256|   8| Bank + LFB
       165h | Graph |  1280x960|   64k|  16| Bank + LFB
       166h | Graph |  1280x960|   16M|  32| Bank + LFB
       121h | Graph |   640x480|   16M|  32| Bank + LFB
       122h | Graph |   800x600|   16M|  32| Bank + LFB
       123h | Graph |  1024x768|   16M|  32| Bank + LFB
       124h | Graph | 1280x1024|   16M|  32| Bank + LFB
       143h | Graph | 1400x1050|   256|   8| Bank + LFB
       145h | Graph | 1400x1050|   64k|  16| Bank + LFB
       146h | Graph | 1400x1050|   16M|  32| Bank + LFB
       173h | Graph | 1600x1200|   256|   8| Bank + LFB
       175h | Graph | 1600x1200|   64k|  16| Bank + LFB
       176h | Graph | 1600x1200|   16M|  32| Bank + LFB
       183h | Graph | 1792x1344|   256|   8| Bank + LFB
       185h | Graph | 1792x1344|   64k|  16| Bank + LFB
       186h | Graph | 1792x1344|   16M|  32| Bank + LFB
       1D3h | Graph | 1856x1392|   256|   8| Bank + LFB
       1D5h | Graph | 1856x1392|   64k|  16| Bank + LFB
       1D6h | Graph | 1856x1392|   16M|  32| Bank + LFB
       1E3h | Graph | 1920x1440|   256|   8| Bank + LFB
       1E5h | Graph | 1920x1440|   64k|  16| Bank + LFB
       1E6h | Graph | 1920x1440|   16M|  32| Bank + LFB

                                [End of Report]
