Quick Navigation

| Background
| System Summary
| Motherboard
| Processor
| BIOS
| PCI/AGP Devices
| Memory Modules
| Memory (SMBIOS)
| HDD
| ATAPI
| Storage (ASPI)
| Drives
| USB Devices
| Plug and Play
| Printers
| Slots (SMBIOS)
| Ports (SMBIOS)
| Monitor
| Video
Background

| Background
| Version | ASTRA v.5.46
| URL | www.sysinfolab.com
| Report Date | June 21, 2010
| Report Time | 23:18:10
| OS Version | Microsoft DOS 6.22 rev.0 in HMA
| Registered To | Sysinfo Lab
| License Type | Professional for 1 computer
System Summary

| Processor
| Processor | AMD Phenom II X4 710
| CPU Clock | 3445.1 MHz (13.0 x 265.0 MHz)
| Level 1 Cache | 4 x 64+64 kB (data+instr.)
| Level 2 Cache | 4 x 512 kB
| Level 3 Cache | 1 x 6144 kB
| Motherboard
| System Name | Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
| Motherboard Vendor | Gigabyte Technology Co., Ltd.
| Board Model | Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
| BIOS Version | Award Modular BIOS v6.00PG
| Chipset Name | AMD 770/780FX/790FX
| Chipset Vendor | ATI Technologies Inc
| Chipset | RX790 GFX Single Slot
| Southbridge Vendor | ATI Technologies Inc
| Southbridge | SB700 LPC host controller
| PCI Bus Version | 3.0
| PnP BIOS Version | 1.0
| DMI/SMBIOS Version | 2.4
| Memory
| Base Memory | 640 kB (604 kB free)
| Extended Memory | 2094976 kB (2045.88 MB)
| System Memory | 2048 MB
| Memory Module | 1024MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
| Memory Module | 1024MB DDR3-1333 (PC3-10600) SDRAM (Kingston)
| Storage
| Floppy Drive | A: 1.44 MB (3.5")
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Size | 953869 MB (931.51 GB)
| CD/DVD Model | _NEC DVD_RW ND-3550A
| CD/DVD Speed | 48x (Write: 48x)
| CD/DVD Model | CD-W540E
| CD/DVD Speed | 48x (Write: 40x)
| Video
| Monitor Vendor | LG Electronics Inc.
| Monitor Model | LG FLATRON F920P
| Video Chip Vendor | ATI Technologies Inc
| Video Chip | RV770 [Radeon HD 4870]
| VESA OEM String | ATI ATOMBIOS
| Video Memory Size | 16 MB
| Sound
| Sound Chip Vendor | ATI Technologies Inc
| Sound Chip | IXP SB600 High Definition Audio Controller
| Sound Chip Vendor | ATI Technologies Inc
| Sound Chip | HD48x0 audio
| AC'97/HDA Codec Name | ATI R600 HDMI
| Sound Chip Vendor | Creative Labs
| Sound Chip | EMU10K2 Audio Chipset (SB Audigy Series)
| Operating System
| DOS Version | Microsoft DOS 6.22 rev.0 in HMA
| Windows Version | Not Found
| Network
| Adapter Vendor | Realtek Semiconductor
| Adapter Name | RTL8168/8111 PCI-E Gigabit Ethernet NIC
| Ports
| Mouse Type | PS/2 (version 7.00)
| LPT Ports | LPT1(0378h)
| COM Ports | COM1(03F8h)
| Joystick | Present
Motherboard

| System
| System Vendor | Gigabyte Technology Co., Ltd.
| Product Name | GA-MA770T-UD3P
| Version |
| Serial Number |
| UUID | 303032343144383931353430FFFFFFFF
| Wake-up Type | Power Switch
| SKU Number |
| Family |
| Motherboard
| Motherboard Vendor | Gigabyte Technology Co., Ltd.
| Vendor URL | www.gigabyte.com.tw
| Board Model | Gigabyte Technology Co., Ltd. GA-MA770T-UD3P
| Version |
| Serial Number |
| BIOS Version | Award Modular BIOS v6.00PG
| BIOS Date | 06/24/09
| Chipset Name | AMD 770/780FX/790FX
| Chipset Vendor | ATI Technologies Inc
| Chipset | RX790 GFX Single Slot
| Southbridge Vendor | ATI Technologies Inc
| Southbridge | SB700 LPC host controller
| System Enclosure
| Manufacturer | Gigabyte Technology Co., Ltd.
| Type | Desktop
| Version |
| Serial Number |
| Asset Tag |
| Boot-up State | Unknown
| Power Supply State | Unknown
| Thermal State | Unknown
| Security Status | Unknown
| OEM-defined | 00000000h
CPU

| CPU
| Processor | AMD Phenom II X4 710
| Coprocessor | Internal
| CPU Clock | 3445.1 MHz
| Level 1 Cache | 4 x 64+64 kB (data+instr.)
| Level 2 Cache | 4 x 512 kB
| Level 3 Cache | 1 x 6144 kB
| FSB Clock | 265.0 MHz
| Multiplier | 13.0
| Platform ID | Socket AM2+
| Vendor | AuthenticAMD
| Processor Name | AMD Phenom(tm) II X4 10 Processor
| Processor Type | Original OEM Processor
| CPUID | Family: 15, Model: 4, Stepping: 2
| Ext. Family/Model | Family: 1, Model: 0
| CPU Signature | 00100F42h
| Brand ID | Phenom II X4 710 (40A6h)
| Number of Cores | 4
| Logical CPU Count | HTT Not Supported
| Max CPUID Level | 5
| Max ExtCPUID Level | 8000001Bh
| Code Name | Deneb (0.045mk)
| Core Stepping | RB-C2
| MSR C0010064h | 800001FDh:3800240Ah
| MSR C0010065h | 800001EBh:38003403h
| MSR C0010066h | 800001DEh:3800444Ch
| MSR C0010067h | 80000187h:38005040h
| MSR C0010071h | 30B40093h:3800240Ah
| Instruction Set
| Floating-Point Unit On-Chip | Supported
| IA MMX Technology | Supported
| SSE Instruction Set | Supported
| SSE2 Instruction Set | Supported
| SSE3 Instruction Set | Supported
| Supplemental SSE3 Instruction Set | Not Supported
| SSE4.1 Instruction Set | Not Supported
| SSE4.2 Instruction Set | Not Supported
| Advanced Vector Extensions (AVX) | Not Supported
| FMA Instructions Set | Not Supported
| AES Instructions Set | Not Supported
| Intel Extended Memory 64 Tech. | Not Supported
| Intel Architecture - 64 (IA-64) | Not Supported
| AMD MMX Instruction Extensions | Supported
| AMD 3DNow! Instructions | Supported
| AMD 3DNow! Extensions | Supported
| AMD 3DNow! Prefetch | Supported
| AMD SSE4A Extensions | Supported
| AMD SSE5 Extensions | Not Supported
| AMD Misaligned SSE | Supported
| AMD64 Architecture | Supported
| Cyrix Extended MMX | Not Supported
| CMPXCHG8 Instruction Supported | Supported
| CMPXCHG16 Instruction Supported | Supported
| Fast System Call | Supported
| Conditional Move Instruction | Supported
| CLFLUSH Insruction Supported | Supported
| Fast Save and Restore | Supported
| Monitor/MWAIT Instructions | Supported
| SYSCALL/SYSRET Instructions | Supported
| LAHF/SAHF Instructions | Supported
| POPCNT Insruction Supported | Supported
| XSAVE Insructions Supported | Not Supported
| OS Supports XSAVE Instructions | Not Supported
| PCLMULQDQ Instruction Supported | Not Supported
| MOVBE Insruction Supported | Not Supported
| AMD RDTSCP Insruction Supported | Supported
| AMD Fast Save and Restore | Supported
| AMD SKINIT, STGI, DEV Supported | Supported
| Processor Features
| Virtual Mode Extension | Supported
| Debugging Extension | Supported
| Page Size Extension | Supported
| Time Stamp Counter | Supported
| Model Specific Registers | Supported
| Physical Address Extension | Supported
| Machine Check Exception | Supported
| On-chip APIC Hardware Supported | Supported
| Memory Type Range Registers | Supported
| Page Global Enable | Supported
| Machine Check Architecture | Supported
| Page Attribute Table | Supported
| 36-bit Page Size Extension | Supported
| Processor Serial Number | Not Supported
| Debug Store | Not Supported
| 64-bit Debug Store | Not Supported
| Self-Snoop | Not Supported
| Hyper-Threading Technology | Not Supported
| Pending Break Enable | Not Supported
| CPL-Qualified Debug Store | Not Supported
| L1 Context ID | Not Supported
| Send Task Priority Messages | Not Supported
| Direct Cache Access | Not Supported
| Performance Capabilities MSR | Not Supported
| x2APIC Architecture | Not Supported
| Advanced Bit Manipulation | Supported
| OS Visible Workaround | Supported
| Instruction Based Sampling | Supported
| Intel Virtualization Technology | Not Supported
| Intel Trusted Execution Technology | Not Supported
| Intel Turbo Boost Technology | Not Supported
| AMD No-execute Page Protection | Supported
| AMD Secure Virtual Machine | Supported
| AMD Model-Specific Registers | Supported
| AMD Multiprocessing Capable | Not Supported
| AMD CMP Legacy Mode | Supported
| AMD CR8 in Legacy Mode | Supported
| AMD Ext. APIC Register Space | Supported
| AMD Watchdog Timer | Supported
| AMD 1-GB Large Page | Supported
| Power Management
| ACPI Supported | Not Supported
| Thermal Monitor Supported | Not Supported
| Thermal Monitor 2 | Not Supported
| Enhanced SpeedStep Technology | Not Supported
| Digital Thermal Sensor | Not Supported
| Operating Point Protection | Not Supported
| AMD Temperature Sensor | Supported
| AMD Frequency ID Control | Not Supported
| AMD Voltage ID Control | Not Supported
| AMD Thermal Trip | Supported
| AMD Thermal Monitoring | Supported
| AMD Software Thermal Control | Supported
| AMD Invariant TSC | Supported
| AMD 100MHz Multiplier Steps | Supported
| AMD Hardware P-State Control | Supported
CPU Cache

| Level 1 Instruction Cache
| Size | 4 x 64 kB
| Associativity | 2-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 32
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 16
| Associativity | full
| Level 1 Data Cache
| Size | 4 x 64 kB
| Associativity | 2-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 48
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 48
| Associativity | full
| Level 2 Cache
| Size | 4 x 512 kB
| Associativity | 16-way
| Lines per Tag | 1
| Line Size | 64 byte
| Instr. TLB 4K Pages |
| Number of Entries | 512
| Associativity | 4-way
| Data TLB 4K Pages |
| Number of Entries | 512
| Associativity | 4-way
| Instr. TLB 2/4M Pages |
| Number of Entries | 0
| Associativity | off
| Data TLB 2/4M Pages |
| Number of Entries | 128
| Associativity | 2-way
| Level 3 Cache
| Size | 1 x 6144 kB
| Associativity | 48-way
| Line Size | 64 byte
CPU (SMBIOS)

| Processor
| Processor Vendor | AMD
| Processor Version | AMD Phenom(tm) II X4 10 Processor
| Current Speed | 3445 MHz
| External Clock | 265 MHz
| Voltage | 1.3 V
| Processor Upgrade | ZIF Socket
| Processor Status | CPU Enabled
| Socket Designation | Socket M2
| Processor Type | Central Processor
| Processor Family | AMD Athlon
| Processor ID1 | 00100F42h
| Processor ID2 | 178BFBFFh
| Max Speed | 3200 MHz
| Socket Status | CPU Socket Populated
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 23h
CPU (SMBIOS) Cache

| Level 1 Cache
| Installed Size | 128 kB
| Operational Mode | Write Back
| Current SRAM Type | Synchronous
| Status | Enabled
| Socket Designation | Internal Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 128 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
| Level 1 Cache
| Installed Size | 128 kB
| Operational Mode | Write Back
| Current SRAM Type | Synchronous
| Status | Enabled
| Socket Designation | Internal Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 128 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
| Level 3 Cache
| Installed Size | 512 kB
| Operational Mode | Write Back
| Current SRAM Type | Synchronous
| Status | Enabled
| Socket Designation | External Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 512 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
| Level 2 Cache
| Installed Size | 0 kB
| Operational Mode | Write Through
| Current SRAM Type | Synchronous
| Status | Disabled
| Socket Designation | External Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 1024 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
BIOS

| BIOS
| Motherboard Vendor | Gigabyte Technology Co., Ltd.
| Vendor URL | www.gigabyte.com.tw
| BIOS Version | Award Modular BIOS v6.00PG
| BIOS Model | Model: FCh SubModel: 01h Revision: 00h
| BIOS Date | 06/24/09
| BIOS Copyright | Award Software Inc. - 04/23/90
| Motherboard ID | AMD 770 BIOS for GA-MA770T-UD3P F2
| BIOS ID | 06/24/2009-RX780-SB710-7A66AG05C-00
| BIOS Type | Unknown (7)
| Bus Type | ISA/PCI
| Processor | 686
| Chipset | AMD 790FX
| Chipset ID | RX780-SB710
| BIOS Revision | 00
| MP Specification Ver. | 1.4
| MP Table Address | 000Fh:1100h
| Number of CPU/Cores | 4
| DMI/SMBIOS Version | 2.4
| DMI/SMBIOS Structures | 55
| DMI/SMBIOS Address | 000Fh:0100h
| APM Version | 1.2
| SMBIOS
| BIOS Vendor | Award Software International, Inc.
| BIOS Version | F2
| BIOS Date | 06/24/2009
| BIOS ROM Size | 1024 kB
| Starting Segment | E000h
| Current Language | n|US|iso8859-1
| Number of Languages | 3
| Structure Length | 18h
| Bus Supported
| PCI is Supported | Supported
| AGP is Supported | Not Supported
| USB is Supported | Supported
| ISA is Supported | Supported
| VLBus is Supported | Not Supported
| MCA is Supported | Not Supported
| EISA is Supported | Not Supported
| PC Card is Supported | Not Supported
| Boot Options
| Selectable Boot | Supported
| Boot From CD | Supported
| ATAPI ZIP Drive Boot | Supported
| LS-120 Boot | Supported
| BIOS Boot Specification | Supported
| Boot From PC Card | Not Supported
| Network Service Boot Supported | Not Supported
| I2O Boot | Not Supported
| 1394 Boot | Not Supported
| BIOS Features
| BIOS Characteristics | Supported
| ACPI Supported | Supported
| PnP is Supported | Supported
| APM is Supported | Supported
| ESCD Support | Not Supported
| Enhanced Disk Drive (EDD) | Supported
| BIOS is Upgradeable (Flash) | Supported
| BIOS ROM is Socketed | Supported
| BIOS Shadowing is Allowed | Supported
| Smart Battery Supported | Not Supported
| Targeted Content Distribution | Supported
| Int 13h - 5.25"/360kB Floppy | Supported
| Int 13h - 5.25"/1.2MB Floppy | Supported
| Int 13h - 3.5"/720kB Floppy | Supported
| Int 13h - 3.5"/2.88MB Floppy | Supported
| Int 5h, Print Screen Service | Supported
| Int 9h, 8042 Keyboard Services | Supported
| Int 14h, Serial Services | Supported
| Int 17h, Printer Services | Supported
| Int 10h, CGA/Mono Video Services | Supported
| Int 13h - Floppy for NEC 9800 | Not Supported
| Int 13h - Floppy for Toshiba | Not Supported
| NEC PC-98 | Not Supported
| Advanced Power Management Features
| 16-bit PM Interface Support | Supported
| 32-bit PM Interface Support | Supported
| CPU Idle Call | Supported
| BIOS Power Management Disabled | Not Supported
| BIOS Power Management Disengaged | Not Supported
| Other SMBIOS Structures
| Memory Array Mapped Address (19)
| Memory Device Mapped Address (20)
| Memory Device Mapped Address (20)
| Memory Device Mapped Address (20)
| Memory Device Mapped Address (20)
| System Boot Information (32)
| Unknown (188)
| Unknown (190)
| Unknown (192)
| Unknown (194)
| Unknown (196)
| Unknown (198)
PCI/AGP Devices

| PCI/AGP
| PCI Bus Version | 3.0
| Number of PCI Buses | 4
| Bus: 00h, Device: 00h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (5957h) | RX790 GFX Single Slot
| Subsys Vendor (1002h) | ATI Technologies Inc
| Subsystem ID (5957h) | Unknown
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | E0000000h - FFFFFFFFh
| Bus: 00h, Device: 02h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (5978h) | RD790 PCI to PCI bridge (external gfx0 port A)
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | E000h - EFFFh
| Memory Address | FDF00000h - FDFFFFFFh
| Memory Address | D0000000h - DFFFFFFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Bus: 00h, Device: 0Ah, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (597Fh) | RD790 PCI to PCI bridge (PCIe gpp port F)
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | D000h - DFFFh
| Memory Address | FDE00000h - FDEFFFFFh
| Memory Address | FDB00000h - FDBFFFFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2
| Link Speed | 5.0 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 5
| Physical Slot Number | 1
| Bus: 00h, Device: 11h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (4390h) | SB700 SATA Controller [IDE mode]
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (B002h) | Unknown
| Class (01h) | Storage
| SubClass (01h) | IDE
| Revision | 00h
| Interface | 8Fh
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | 0000FF00h - 0000FF07h
| Base I/O Port | 0000FE00h - 0000FE03h
| Base I/O Port | 0000FD00h - 0000FD07h
| Base I/O Port | 0000FC00h - 0000FC03h
| Base I/O Port | 0000FB00h - 0000FB0Fh
| Memory Address | FE02F000h - FE02F3FFh
| System IRQ | 11
| Interrupt Pin | INTA#
| Bus: 00h, Device: 12h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (4397h) | SB700 USB OHCI0 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02E000h - FE02EFFFh
| System IRQ | 3
| Interrupt Pin | INTA#
| Bus: 00h, Device: 12h, Function: 01h
| Vendor (1002h) | ATI Technologies Inc
| Device (4398h) | SB700 USB OHCI1 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02D000h - FE02DFFFh
| System IRQ | 3
| Interrupt Pin | INTA#
| Bus: 00h, Device: 12h, Function: 02h
| Vendor (1002h) | ATI Technologies Inc
| Device (4396h) | SB700 USB EHCI Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 20h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02C000h - FE02C0FFh
| System IRQ | 10
| Interrupt Pin | INTB#
| Bus: 00h, Device: 13h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (4397h) | SB700 USB OHCI0 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02B000h - FE02BFFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| Bus: 00h, Device: 13h, Function: 01h
| Vendor (1002h) | ATI Technologies Inc
| Device (4398h) | SB700 USB OHCI1 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE02A000h - FE02AFFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| Bus: 00h, Device: 13h, Function: 02h
| Vendor (1002h) | ATI Technologies Inc
| Device (4396h) | SB700 USB EHCI Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 20h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE029000h - FE0290FFh
| System IRQ | 11
| Interrupt Pin | INTB#
| Bus: 00h, Device: 14h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (4385h) | IXP SB600 SMBUS Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (4385h) | Unknown
| Class (0Ch) | Serial
| SubClass (05h) | SMBus Controller
| Revision | 3Ch
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Supported
| Device Resources
| SMBus Port | 0B00h
| Bus: 00h, Device: 14h, Function: 01h
| Vendor (1002h) | ATI Technologies Inc
| Device (439Ch) | SB700 IDE
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5002h) | Unknown
| Class (01h) | Storage
| SubClass (01h) | IDE
| Revision | 00h
| Interface | 8Ah
| Device Properties
| Device Timing | Medium
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | 0000FA00h - 0000FA0Fh
| Bus: 00h, Device: 14h, Function: 02h
| Vendor (1002h) | ATI Technologies Inc
| Device (4383h) | IXP SB600 High Definition Audio Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (A022h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | Hi-definition Audio
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Slow
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FE024000h - FE027FFFh
| System IRQ | 3
| Interrupt Pin | INTA#
| Bus: 00h, Device: 14h, Function: 03h
| Vendor (1002h) | ATI Technologies Inc
| Device (439Dh) | SB700 LPC host controller
| Subsys Vendor (1002h) | ATI Technologies Inc
| Subsystem ID (439Dh) | Unknown
| Class (06h) | Bridge
| SubClass (01h) | PCI/ISA
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Bus: 00h, Device: 14h, Function: 04h
| Vendor (1002h) | ATI Technologies Inc
| Device (4384h) | IXP SB600 PCI to PCI Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | 00h
| Interface | 01h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | C000h - CFFFh
| Memory Address | FDD00000h - FDDFFFFFh
| Memory Address | FDC00000h - FDCFFFFFh
| Bus: 00h, Device: 14h, Function: 05h
| Vendor (1002h) | ATI Technologies Inc
| Device (4399h) | SB700 USB OHCI2 Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (5004h) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | FE028000h - FE028FFFh
| System IRQ | 10
| Interrupt Pin | INTC#
| Bus: 00h, Device: 18h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1200h) | K10 [Opteron, Athlon64, Sempron] HyperTransport Configuration
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1201h) | K10 [Opteron, Athlon64, Sempron] Address Map
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 02h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1202h) | K10 [Opteron, Athlon64, Sempron] DRAM Controller
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1203h) | K10 [Opteron, Athlon64, Sempron] Miscellaneous Control
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 04h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1204h) | K10 [Opteron, Athlon64, Sempron] Link Control
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 01h, Device: 00h, Function: 00h
| Vendor (1002h) | ATI Technologies Inc
| Device (9440h) | RV770 [Radeon HD 4870]
| Subsys Vendor (1787h) | Hightech Information System Ltd (Medion??)
| Subsystem ID (2267h) | Unknown
| Class (03h) | Display
| SubClass (00h) | VGA
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | D0000000h - DFFFFFFFh
| Memory Address | FDFE0000h - FDFEFFFFh
| Base I/O Port | 0000EE00h - 0000EEFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 2
| Link Speed | 2.5 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Bus: 01h, Device: 00h, Function: 01h
| Vendor (1002h) | ATI Technologies Inc
| Device (AA30h) | HD48x0 audio
| Subsys Vendor (1787h) | Hightech Information System Ltd (Medion??)
| Subsystem ID (AA30h) | Unknown
| Class (04h) | Multimedia
| SubClass (03h) | Hi-definition Audio
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FDFFC000h - FDFFFFFFh
| System IRQ | 10
| Interrupt Pin | INTB#
| AC'97/HDA Capabilities
| AC'97/HDA Codec Name | ATI R600 HDMI
| PCI-E Capabilities
| PCI Express Version | 2
| Link Speed | 2.5 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| Bus: 02h, Device: 00h, Function: 00h
| Vendor (10ECh) | Realtek Semiconductor
| Device (8168h) | RTL8168/8111 PCI-E Gigabit Ethernet NIC
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (E000h) | GA-EP45-DS5 Motherboard
| Class (02h) | Network
| SubClass (00h) | Ethernet
| Revision | 02h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000DE00h - 0000DEFFh
| Memory Address | FDBFF000h - FDBFFFFFh
| Memory Address | FDBE0000h - FDBEFFFFh
| System IRQ | 10
| Interrupt Pin | INTA#
| PCI-E Capabilities
| PCI Express Version | 1
| Link Speed | 2.5 GB/s (Current: 2.5 GB/s)
| Link Width | x1 (Current: x1)
| Link Port Number | 0
| Physical Slot Number | 0
| Bus: 03h, Device: 06h, Function: 00h
| Vendor (1102h) | Creative Labs
| Device (0004h) | EMU10K2 Audio Chipset (SB Audigy Series)
| Subsys Vendor (1102h) | Creative Labs
| Subsystem ID (2005h) | Unknown
| Class (04h) | Multimedia
| SubClass (01h) | Audio
| Revision | 04h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000CF00h - 0000CF3Fh
| System IRQ | 5
| Interrupt Pin | INTA#
| Bus: 03h, Device: 0Eh, Function: 00h
| Vendor (104Ch) | Texas Instruments (TI)
| Device (8024h) | TSB43AB23 1394a-2000 OHCI PHY/link-layer Controller
| Subsys Vendor (1458h) | Giga-Byte Technology
| Subsystem ID (1000h) | GA-EP45-DS5 Motherboard
| Class (0Ch) | Serial
| SubClass (00h) | Firewire
| Revision | 00h
| Interface | 10h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Memory Address | FDDFF000h - FDDFF7FFh
| Memory Address | FDDF8000h - FDDFBFFFh
| System IRQ | 11
| Interrupt Pin | INTA#
Memory Modules

| Memory Slot 1
| Memory Type | 1024MB DDR3-1333 (PC3-10600) SDRAM
| Manufacturer | Kingston
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 8 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| CAS# Latency | 9.0 (Cycle Time: 1.500ns/686MHz)
| CAS# Latency | 8.0 (Cycle Time: 1.371ns/610MHz)
| CAS# Latency | 7.0 (Cycle Time: 1.200ns/533MHz)
| CAS# Latency | 6.0 (Cycle Time: 1.029ns/457MHz)
| Refresh Rate | 7.8 us (2X 85-95 C)
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.5 V
| Max Case Temperature | 95 C (203 F)
| SPD Revision | 1.0
| Part Number | 9905402-015.A03LF
| Manufacturing Location | China
| Manufacture Date | September 2009 (0926h)
| Serial Number | 14CC41B4h
| Revision Code | None
| EPP is Supported | Not Supported
| Memory Slot 2
| Memory Type | 1024MB DDR3-1333 (PC3-10600) SDRAM
| Manufacturer | Kingston
| Module Type | Unbuffered DIMM
| Number of Ranks/Banks | 1 Ranks, 8 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| CAS# Latency | 9.0 (Cycle Time: 1.500ns/686MHz)
| CAS# Latency | 8.0 (Cycle Time: 1.371ns/610MHz)
| CAS# Latency | 7.0 (Cycle Time: 1.200ns/533MHz)
| CAS# Latency | 6.0 (Cycle Time: 1.029ns/457MHz)
| Refresh Rate | 7.8 us (2X 85-95 C)
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | 1.5 V
| Max Case Temperature | 95 C (203 F)
| SPD Revision | 1.0
| Part Number | 9905402-015.A03LF
| Manufacturing Location | China
| Manufacture Date | September 2009 (0926h)
| Serial Number | 16CC37B4h
| Revision Code | None
| EPP is Supported | Not Supported
Memory (SMBIOS)

| Physical Memory Array 1
| Maximum Capacity | 2048 MB
| Location | System Board or Motherboard
| Use | System Memory
| Memory Error Correct. | None
| Memory Devices | 4
| Structure Length | 0Fh
| Memory Device 1
| Size | 1024 MB
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | 1066 MHz
| Device Locator | A0
| Bank Locator | Bank0/1
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer |
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 1Bh
| Memory Device 2
| Size | 1024 MB
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | 1066 MHz
| Device Locator | A1
| Bank Locator | Bank2/3
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer |
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 1Bh
| Memory Device 3
| Size | Not Installed
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | 1066 MHz
| Device Locator | A2
| Bank Locator | Bank4/5
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer |
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 1Bh
| Memory Device 4
| Size | Not Installed
| Form Factor | DIMM
| Memory Type | Unknown
| Speed | 1066 MHz
| Device Locator | A3
| Bank Locator | Bank6/7
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Manufacturer |
| Serial Number |
| Asset Tag |
| Part Number |
| Structure Length | 1Bh
HDD

| Tertiary/Master HDD
| HDD Model | WDC WD1001FALS-00J7B0
| HDD Size | 953869 MB (931.51 GB)
| Interface Type | Serial ATA II
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ATA/ATAPI-7
| Serial Number | WD-WMATV0357962
| Controller Revision | 05.00K05
| HDD Marketing Size | 1000204 MB (1000.20 GB)
| Buffer Size | 32767.5 kB
| Buffer Type | Not Specified
| HDD Temperature | 50 C (122 F)
| Reallocated Sectors | 0
| HDD Health Status | Good
| ECC bytes | 50
| Security Erase Time | 194 min
| Enh. Security Erase | 194 min
| Current APM Value | None
| Acoustic Management | FEh (80h Recommended) - Disabled
| ATA Controller Vendor | ATI Technologies Inc
| ATA Controller Name | SB700 SATA Controller [IDE mode]
| Device Location | Tertiary/Master
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 6 (UltraDMA/133)
| Sectors per Interrupt | 16, Active: 16
| HDD Features
| SATA NCQ Command | Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Not Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Not Supported
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Supported, Disabled
| Set Features Req. to Spinup | Supported, Enabled
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Supported, Disabled
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Supported, Enabled
| S.M.A.R.T.

| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 1 | Raw Read Error Rate | 51 | 200 | 200 | 0
| 3 | Spin-up Time | 21 | 253 | 253 | 4350
| 4 | Start/Stop Count | 0 | 99 | 99 | 1275
| 5 | Reallocated Sectors Count | 140 | 200 | 200 | 0
| 7 | Seek Error Rate | 51 | 200 | 200 | 0
| 9 | Power On Hours Count | 0 | 96 | 96 | 3124
| 10 | Spin-up Retry Count | 51 | 100 | 100 | 0
| 11 | Recalibration Retries | 51 | 100 | 100 | 0
| 12 | Drive Power Cycle Count | 0 | 99 | 99 | 1257
| 192 | Power-Off Retract Cycle | 0 | 199 | 199 | 883
| 193 | Load/Unload Cycle Count | 0 | 200 | 200 | 1275
| 194 | Drive Temperature | 0 | 94 | 100 | 50
| 196 | Reallocation Event Count | 0 | 200 | 200 | 0
| 197 | Current Pending Sectors | 0 | 200 | 200 | 0
| 198 | Uncorrectable Sectors | 0 | 200 | 200 | 0
| 199 | UltraDMA CRC Error Rate | 0 | 200 | 200 | 0
| 200 | Write Error Rate | 51 | 200 | 200 | 0

ATAPI

| Primary/Master ATAPI
| ATAPI Model | _NEC DVD_RW ND-3550A
| ATAPI Type | DVD+-RW DL/CD-RW
| Interface Type | Parallel ATA
| Physical Interface | ATAPI
| ATAPI Name | _NEC DVD_RW ND-3550A
| Vendor Specific | 05093000
| CD Read Speed | 48x (Current: 48x)
| CD Write Speed | 48x (Current: 48x)
| DVD Read Speed | Current: 6x
| DVD Write Speed | Current: 6x
| Buffer Size | 2048 kB
| Loading Mechanism | Tray Type
| Rotation Control | CLV
| Read Retry Count | 15
| Write Retry Count | 0
| Compatibility | Unknown
| Serial Number | 63E1J06S211
| Controller Revision | 1.05
| Command DRQ Type | Microprocessor DRQ
| Command Packet Size | 12 bytes
| ATA Controller Vendor | ATI Technologies Inc
| ATA Controller Name | SB700 IDE
| Device Location | Primary/Master
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 2 (UltraDMA/33), Active: 2 (UltraDMA/33)
| Reading Features
| CD-R Disk Read | Supported
| CD-RW Disk Read | Supported
| DVD-ROM Disk Read | Supported
| DVD-RAM Disk Read | Not Supported
| DVD-R Disk Read | Supported
| DVD-R DL Disk Read | Supported
| DVD-RW Disk Read | Supported
| DVD-RW DL Disk Read | Not Supported
| DVD+R Disk Read | Supported
| DVD+R DL Disk Read | Supported
| DVD+RW Disk Read | Supported
| DVD+RW DL Disk Read | Not Supported
| BD-ROM Disk Read | Not Supported
| BD-R Disk Read | Not Supported
| BD-RE Disk Read | Not Supported
| HD DVD-ROM Disk Read | Not Supported
| HD DVD-RAM Disk Read | Not Supported
| HD DVD-R Disk Read | Not Supported
| HD DVD-R DL Disk Read | Not Supported
| HD DVD-RW Disk Read | Not Supported
| HD DVD-RW DL Disk Read | Not Supported
| Read Packet Using Method 2 | Supported
| Read Mode2 Form1 Sectors | Supported
| Read Mode2 Form2 Sectors | Supported
| Multisession Disk Read | Supported
| READ-CD Command on AudioCD | Supported
| Read Bar Code Capable | Not Supported
| Read Lead-in (CD-Text) | Supported
| Writing Features
| CD-R Disk Write | Supported
| CD-RW Disk Write | Supported
| DVD-RAM Disk Write | Not Supported
| DVD-R Disk Write | Supported
| DVD-R DL Disk Write | Supported
| DVD-RW Disk Write | Supported
| DVD+R Disk Write | Supported
| DVD+R DL Disk Write | Supported
| DVD+RW Disk Write | Supported
| DVD+RW DL Disk Write | Not Supported
| BD-R Disk Write | Not Supported
| BD-RE Disk Write | Not Supported
| HD DVD-R Disk Write | Not Supported
| HD DVD-R DL Disk Write | Not Supported
| HD DVD-RAM Disk Write | Not Supported
| HD DVD-RW Disk Write | Not Supported
| HD DVD-RW DL Disk Write | Not Supported
| Test Write Mode Support | Supported
| Buffer Underrun Protection | Supported
| Other Features
| Audio Play Support | Supported
| CD-DA Stream is Accurate | Supported
| Composite Audio/Video | Not Supported
| Digital Output on Port 1 | Not Supported
| Digital Output on Port 2 | Not Supported
| Support Subcode R-W | Supported
| Support Subcode R-W D&C | Not Supported
| C2 Pointers Supported | Supported
| ISRC Supported | Supported
| UPC Supported | Supported
| ATAPI Features
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Not Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Not Supported
| ATA Software Reset | Not Supported
| Overlap Operation | Not Supported
| Command Queuing | Not Supported
| Interleaving DMA | Not Supported
| Primary/Slave ATAPI
| ATAPI Model | CD-W540E
| ATAPI Type | CD-RW
| Interface Type | Parallel ATA
| Physical Interface | ATAPI
| ATAPI Name | TEAC CD-W540E
| Vendor Specific | 09/30/02
| CD Read Speed | 48x (Current: 48x)
| CD Write Speed | 40x (Current: 40x)
| Buffer Size | 8192 kB
| Loading Mechanism | Tray Type
| Rotation Control | CLV
| Read Retry Count | 5
| Write Retry Count | 3
| Compatibility | ATA/ATAPI-5 revision 19
| Serial Number |
| Controller Revision | 1.0H
| Command DRQ Type | Accelerated DRQ
| Command Packet Size | 12 bytes
| ATA Controller Vendor | ATI Technologies Inc
| ATA Controller Name | SB700 IDE
| Device Location | Primary/Slave
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | 2, Active: None
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 2 (UltraDMA/33), Active: 2 (UltraDMA/33)
| Reading Features
| CD-R Disk Read | Supported
| CD-RW Disk Read | Supported
| DVD-ROM Disk Read | Not Supported
| DVD-RAM Disk Read | Not Supported
| DVD-R Disk Read | Not Supported
| DVD-R DL Disk Read | Not Supported
| DVD-RW Disk Read | Not Supported
| DVD-RW DL Disk Read | Not Supported
| DVD+R Disk Read | Not Supported
| DVD+R DL Disk Read | Not Supported
| DVD+RW Disk Read | Not Supported
| DVD+RW DL Disk Read | Not Supported
| BD-ROM Disk Read | Not Supported
| BD-R Disk Read | Not Supported
| BD-RE Disk Read | Not Supported
| HD DVD-ROM Disk Read | Not Supported
| HD DVD-RAM Disk Read | Not Supported
| HD DVD-R Disk Read | Not Supported
| HD DVD-R DL Disk Read | Not Supported
| HD DVD-RW Disk Read | Not Supported
| HD DVD-RW DL Disk Read | Not Supported
| Read Packet Using Method 2 | Supported
| Read Mode2 Form1 Sectors | Supported
| Read Mode2 Form2 Sectors | Supported
| Multisession Disk Read | Supported
| READ-CD Command on AudioCD | Supported
| Read Bar Code Capable | Not Supported
| Read Lead-in (CD-Text) | Supported
| Writing Features
| CD-R Disk Write | Supported
| CD-RW Disk Write | Supported
| DVD-RAM Disk Write | Not Supported
| DVD-R Disk Write | Not Supported
| DVD-R DL Disk Write | Not Supported
| DVD-RW Disk Write | Not Supported
| DVD+R Disk Write | Not Supported
| DVD+R DL Disk Write | Not Supported
| DVD+RW Disk Write | Not Supported
| DVD+RW DL Disk Write | Not Supported
| BD-R Disk Write | Not Supported
| BD-RE Disk Write | Not Supported
| HD DVD-R Disk Write | Not Supported
| HD DVD-R DL Disk Write | Not Supported
| HD DVD-RAM Disk Write | Not Supported
| HD DVD-RW Disk Write | Not Supported
| HD DVD-RW DL Disk Write | Not Supported
| Test Write Mode Support | Supported
| Buffer Underrun Protection | Supported
| Other Features
| Audio Play Support | Supported
| CD-DA Stream is Accurate | Supported
| Composite Audio/Video | Not Supported
| Digital Output on Port 1 | Not Supported
| Digital Output on Port 2 | Not Supported
| Support Subcode R-W | Supported
| Support Subcode R-W D&C | Not Supported
| C2 Pointers Supported | Supported
| ISRC Supported | Supported
| UPC Supported | Supported
| ATAPI Features
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Not Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| ATA Software Reset | Not Supported
| Overlap Operation | Not Supported
| Command Queuing | Not Supported
| Interleaving DMA | Not Supported
| S.M.A.R.T. | Not Supported
| S.M.A.R.T. Self-test | Not Supported
| S.M.A.R.T. Error Logging | Not Supported
| Security Mode Feature Set | Not Supported
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Supported, Enabled
| Write Cache | Not Supported
| Look-ahead | Not Supported
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Supported, Enabled
| Host Protected Area | Not Supported
| Write Verify Command | Not Supported
| Write Buffer Command | Not Supported
| Read Buffer Command | Not Supported
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Not Supported
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Not Supported
| Set Features Req. to Spinup | Not Supported
| Set Max Security Extension | Not Supported
| Automatic Acoustic Management | Not Supported
| 48-bit Address | Not Supported
| Device Configuration Overlay | Not Supported
| Flush Cache Command | Not Supported
| Flush Cache Ext Command | Not Supported
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Not Supported
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Not Supported
Storage (ASPI)

| ASPI manager not found
Drives

| BIOS Drives
| INT 13h Extensions | Not Supported
| A:
| Drive Letter | A:
| Drive Size | 1.44 MB
| Drive Type | Floppy 1.44 MB (3.5")
| Cylinders | 80
| Heads | 2
| Sectors | 18
| Local Drives
| A:
| Drive Letter | A:
| Drive Type | Floppy 1.44 MB (3.5")
| C:[SYSTEM]
| Drive Letter | C:
| Drive Type | Fixed Disk
| Volume Label | SYSTEM
| File System | FAT16
| Volume Serial Number | 2255-1BEA
| Total Size | 2047.0 MB
| Free Space | 1017.9 MB (49.7%)
| D:[KINGSTON]
| Drive Letter | D:
| Drive Type | Fixed Disk
| Volume Label | KINGSTON
| File System | FAT16
| Volume Serial Number | 94C6-CB33
| Total Size | 491.2 MB
| Free Space | 351.0 MB (71.4%)
| E:[UTILITIES]
| Drive Letter | E:
| Drive Type | Fixed Disk
| Volume Label | UTILITIES
| File System | FAT16
| Volume Serial Number | 2E4A-1BEB
| Total Size | 2047.1 MB
| Free Space | 42.2 MB (2.1%)
| F:[GAMES]
| Drive Letter | F:
| Drive Type | Fixed Disk
| Volume Label | GAMES
| File System | FAT16
| Volume Serial Number | 2D54-1BEC
| Total Size | 2047.1 MB
| Free Space | 709.7 MB (34.7%)
USB Devices

| USB devices not found
Plug and Play

| Plug and Play
| PnP Version | 1.0
| Number of PnP Devices | 14
| Device Number 1
| PnP Device Name | AT Interrupt Controller
| PnP Device ID | PNP0000
| Base Type (08h) | System Peripheral
| SubType (00h) | Interrupt controller
| Node Size | 37 byte
| Device Resources
| I/O Port | 0020h-0021h
| I/O Port | 00A0h-00A1h
| System IRQ | 2 - High True Edge
| Device Number 2
| PnP Device Name | AT DMA Controller
| PnP Device ID | PNP0200
| Base Type (08h) | System Peripheral
| SubType (01h) | DMA controller
| Node Size | 69 byte
| Device Resources
| I/O Port | 0000h-000Fh
| I/O Port | 0081h-0083h
| I/O Port | 0087h-0087h
| I/O Port | 0089h-008Bh
| I/O Port | 008Fh-0091h
| I/O Port | 00C0h-00DFh
| DMA Channel | 4 - Type 8237 (8-bit)
| Device Number 3
| PnP Device Name | AT Timer
| PnP Device ID | PNP0100
| Base Type (08h) | System Peripheral
| SubType (02h) | System timer
| Node Size | 29 byte
| Device Resources
| I/O Port | 0040h-0043h
| System IRQ | 0 - High True Edge
| Device Number 4
| PnP Device Name | AT Real-Time Clock
| PnP Device ID | PNP0B00
| Base Type (08h) | System Peripheral
| SubType (03h) | Real Time Clock
| Node Size | 29 byte
| Device Resources
| I/O Port | 0070h-0071h
| System IRQ | 8 - High True Edge
| Device Number 5
| PnP Device Name | IBM Enhanced keyboard controller (101/2-key)
| PnP Device ID | PNP0303
| Base Type (09h) | Input Device
| SubType (00h) | Keyboard Controller
| Node Size | 37 byte
| Device Resources
| I/O Port | 0060h-0060h
| I/O Port | 0064h-0064h
| System IRQ | 1 - High True Edge
| Device Number 6
| PnP Device Name | AT standard speaker sound
| PnP Device ID | PNP0800
| Base Type (08h) | System Peripheral
| SubType (80h) | Other System device
| Node Size | 26 byte
| Device Resources
| I/O Port | 0061h-0061h
| Device Number 7
| PnP Device Name | Math Coprocessor
| PnP Device ID | PNP0C04
| Base Type (0Bh) | CPU Type
| SubType (01h) | 486 CPU
| Node Size | 29 byte
| Device Resources
| I/O Port | 00F0h-00FFh
| System IRQ | 13 - High True Edge
| Device Number 8
| PnP Device Name | System Board
| PnP Device ID | PNP0C01
| Base Type (05h) | Memory
| SubType (00h) | RAM Memory
| Node Size | 90 byte
| Device Resources
| Memory Address | 00000000h-FFFFFFFFh RAM 8-bit Cacheble
| Memory Address | FFFE0000h-FFFDFFFFh ROM 8/16-bit Cacheble
| Memory Address | FFF80000h-FFF7FFFFh ROM 8/16-bit Cacheble
| Memory Address | FEC00000h-FEBFFFFFh ROM 8/16-bit Cacheble
| Memory Address | FEE00000h-FEDFFFFFh ROM 8/16-bit Cacheble
| Memory Address | 00100000h-7F0FFFFFh RAM 8-bit Cacheble
| Device Number 9
| PnP Device Name | Motherboard registers
| PnP Device ID | PNP0C02
| Base Type (08h) | System Peripheral
| SubType (80h) | Other System device
| Node Size | 66 byte
| Device Resources
| Memory Address | 000F0000h-000F3FFFh ROM 8/16-bit Cacheble Shadow
| Memory Address | 000F4000h-000F7FFFh ROM 8/16-bit Cacheble Shadow
| Memory Address | 000F8000h-000FFFFFh ROM 8/16-bit Cacheble Shadow
| Memory Address | 000CF800h-000CFFFFh ROM 8/16-bit Cacheble Shadow
| Device Number 10
| PnP Device Name | PCI Bus
| PnP Device ID | PNP0A03
| Base Type (06h) | Bridge Controller
| SubType (04h) | PCI Bridge
| Node Size | 42 byte
| Device Resources
| I/O Port | 0290h-029Fh
| I/O Port | 04D0h-04D1h
| I/O Port | 0CF8h-0CFFh
| Device Number 11
| PnP Device Name | PS/2 Port for PS/2-style Mice
| PnP Device ID | PNP0F13
| Base Type (09h) | Input Device
| SubType (02h) | Mouse Controller
| Node Size | 26 byte
| Device Resources
| System IRQ | 12 - High True Edge
| Device Number 12
| PnP Device Name | 16550A-compatible COM port
| PnP Device ID | PNP0501
| Base Type (07h) | Communications
| SubType (00h) | RS-232 Serial port
| Node Size | 69 byte
| Device Resources
| I/O Port | 03F8h-03FFh
| System IRQ | 4 - High True Edge
| Device Number 13
| PnP Device Name | PC standard floppy disk controller
| PnP Device ID | PNP0700
| Base Type (01h) | Mass Storage
| SubType (02h) | Floppy Controller
| Node Size | 64 byte
| Device Resources
| I/O Port | 03F0h-03F5h
| I/O Port | 03F7h-03F7h
| System IRQ | 6 - High True Edge
| DMA Channel | 2 - Type 8237 (8-bit)
| Device Number 14
| PnP Device Name | Standard LPT printer port
| PnP Device ID | PNP0400
| Base Type (07h) | Communications
| SubType (01h) | AT Parallel port
| Node Size | 92 byte
| Device Resources
| I/O Port | 0378h-037Fh
| I/O Port | 0778h-077Fh
| System IRQ | 7 - High True Edge
Physical Printers

| LPT/PnP or USB printer not found
Slots (SMBIOS)

| Slot PCI
| Slot Type | PCI
| Current Usage | Available
| Data Bus Width | 32 bit
| Slot Designation | PCI
| Slot Length | Long Length
| Slot ID | 7
| Slot PCI
| Slot Type | PCI
| Current Usage | In Use
| Data Bus Width | 32 bit
| Slot Designation | PCI
| Slot Length | Long Length
| Slot ID | 6
| Slot PCI Express
| Slot Type | PCI Express
| Current Usage | Unknown
| Data Bus Width | 16x or x16
| Slot Designation | PCI Express x16
| Slot Length | Other
| Slot ID | 0
Ports (SMBIOS)

| Port 1 Other
| Int. Connector Type | On Board IDE
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | PRIMARY IDE
| Ext. Designator |
| Port 2 8251 FIFO Compatible
| Int. Connector Type | On Board Floppy
| Ext. Connector Type | None
| Port Type | 8251 FIFO Compatible
| Int. Designator | FDD
| Ext. Designator |
| Port 3 Serial Port 16450 Compatible
| Int. Connector Type | 9 Pin Dual Inline (pin 10 cut)
| Ext. Connector Type | DB-9 pin male
| Port Type | Serial Port 16450 Compatible
| Int. Designator | COM1
| Ext. Designator |
| Port 4 Serial Port 16450 Compatible
| Int. Connector Type | 9 Pin Dual Inline (pin 10 cut)
| Ext. Connector Type | DB-9 pin male
| Port Type | Serial Port 16450 Compatible
| Int. Designator | COM2
| Ext. Designator |
| Port 5 Parallel Port ECP/EPP
| Int. Connector Type | DB-25 pin female
| Ext. Connector Type | DB-25 pin female
| Port Type | Parallel Port ECP/EPP
| Int. Designator | LPT1
| Ext. Designator |
| Port 6 Keyboard Port
| Int. Connector Type | Other
| Ext. Connector Type | PS/2
| Port Type | Keyboard Port
| Int. Designator | Keyboard
| Ext. Designator |
| Port 7 Mouse Port
| Int. Connector Type | PS/2
| Ext. Connector Type | PS/2
| Port Type | Mouse Port
| Int. Designator | PS/2 Mouse
| Ext. Designator | Detected
| Port 8 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 9 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 10 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 11 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 12 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 13 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 14 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 15 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 16 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 17 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 18 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
| Port 19 USB
| Int. Connector Type | None
| Ext. Connector Type | USB
| Port Type | USB
| Int. Designator | USB
| Ext. Designator |
Monitor

| Monitor
| Monitor Vendor | LG Electronics Inc.
| Monitor Model | LG FLATRON F920P
| Viewable Size | 17.7" (45.0 sm)
| Serial Number | 319823
| Manufacture Date | March 2005
| EDID Version | 1.3
| Monitor ID | GSM4A88
| Aspect Ratio | 4:3
| Horizontal Size | 36 sm
| Vertical Size | 27 sm
| Gamma Factor | 2.910
| Display Type | RGB Color
| Input Signal | Analog
| Internal Model | F920P
| Vertical Frequency | 50-160 Hz
| Horizontal Frequency | 30-111 kHz
| DPMS Features
| Active Off | Supported
| Suspend | Supported
| Standby | Supported
| Supported Modes
| Mode 1 | 720x400 @ 70 Hz (VGA)
| Mode 2 | 720x400 @ 88 Hz (XGA2)
| Mode 3 | 640x480 @ 60 Hz (VGA)
| Mode 4 | 640x480 @ 67 Hz (Mac II)
| Mode 5 | 640x480 @ 72 Hz (VESA)
| Mode 6 | 640x480 @ 75 Hz (VESA)
| Mode 7 | 800x600 @ 56 Hz (VESA)
| Mode 8 | 800x600 @ 60 Hz (VESA)
| Mode 9 | 800x600 @ 72 Hz (VESA)
| Mode 10 | 800x600 @ 75 Hz (VESA)
| Mode 11 | 832x624 @ 75 Hz (Mac II)
| Mode 12 | 1024x768 @ 87 Hz (interlaced)
| Mode 13 | 1024x768 @ 60 Hz (VESA)
| Mode 14 | 1024x768 @ 70 Hz (VESA)
| Mode 15 | 1024x768 @ 75 Hz (VESA)
| Mode 16 | 1280x1024 @ 75 Hz (VESA)
| Mode 17 | 1920x1440 @ 70 Hz
| Mode 18 | 2048x1536 @ 60 Hz
| Mode 19 | 1024x768 @ 85 Hz
| Mode 20 | 1280x1024 @ 75 Hz
| Mode 21 | 1280x1024 @ 85 Hz
| Mode 22 | 1600x1200 @ 75 Hz
| Mode 23 | 1600x1200 @ 85 Hz
| Mode 24 | 1152x864 @ 75 Hz
Video

| Video
| Video Chip Vendor | ATI Technologies Inc
| Video Chip | RV770 [Radeon HD 4870]
| Subsystem Vendor | Hightech Information System Ltd (Medion??)
| Video Memory Size | 16 MB
| Bus Type | PCI-E
| VESA OEM String | ATI ATOMBIOS
| VESA Version | 3.0
| Vendor Name | (C) 1988-2005, ATI Technologies Inc.
| Product Name | RV770 01.00
| OEM Software Version | 11.10
| VESA Power Management
| VESA PM Version | 1.0
| Standby | Not Supported
| Suspend | Not Supported
| Off | Supported
| Reduced On | Not Supported
| PCI-E Capabilities
| PCI Express Version | 2
| Link Speed | 2.5 GB/s (Current: 2.5 GB/s)
| Link Width | x16 (Current: x16)
| Link Port Number | 0
| Physical Slot Number | 0
| VESA Modes

| Number | Mode | Resolution | Colors | bpp | Features
| 100h | Graph | 640x400 | 256 | 8 | Bank + LFB
| 101h | Graph | 640x480 | 256 | 8 | Bank + LFB
| 103h | Graph | 800x600 | 256 | 8 | Bank + LFB
| 105h | Graph | 1024x768 | 256 | 8 | Bank + LFB
| 107h | Graph | 1280x1024 | 256 | 8 | Bank + LFB
| 110h | Graph | 640x480 | 64k | 16 | Bank + LFB
| 111h | Graph | 640x480 | 64k | 16 | Bank + LFB
| 113h | Graph | 800x600 | 64k | 16 | Bank + LFB
| 114h | Graph | 800x600 | 64k | 16 | Bank + LFB
| 116h | Graph | 1024x768 | 64k | 16 | Bank + LFB
| 117h | Graph | 1024x768 | 64k | 16 | Bank + LFB
| 119h | Graph | 1280x1024 | 64k | 16 | Bank + LFB
| 11Ah | Graph | 1280x1024 | 64k | 16 | Bank + LFB
| 10Dh | Graph | 320x200 | 64k | 16 | Bank + LFB
| 10Eh | Graph | 320x200 | 64k | 16 | Bank + LFB
| 120h | Graph | 320x200 | 16M | 32 | Bank + LFB
| 193h | Graph | 320x240 | 256 | 8 | Bank + LFB
| 195h | Graph | 320x240 | 64k | 16 | Bank + LFB
| 196h | Graph | 320x240 | 16M | 32 | Bank + LFB
| 1B3h | Graph | 512x384 | 256 | 8 | Bank + LFB
| 1B5h | Graph | 512x384 | 64k | 16 | Bank + LFB
| 1B6h | Graph | 512x384 | 16M | 32 | Bank + LFB
| 1C3h | Graph | 640x350 | 256 | 8 | Bank + LFB
| 1C5h | Graph | 640x350 | 64k | 16 | Bank + LFB
| 1C6h | Graph | 640x350 | 16M | 32 | Bank + LFB
| 133h | Graph | 720x400 | 256 | 8 | Bank + LFB
| 135h | Graph | 720x400 | 64k | 16 | Bank + LFB
| 136h | Graph | 720x400 | 16M | 32 | Bank + LFB
| 153h | Graph | 1152x864 | 256 | 8 | Bank + LFB
| 155h | Graph | 1152x864 | 64k | 16 | Bank + LFB
| 156h | Graph | 1152x864 | 16M | 32 | Bank + LFB
| 163h | Graph | 1280x960 | 256 | 8 | Bank + LFB
| 165h | Graph | 1280x960 | 64k | 16 | Bank + LFB
| 166h | Graph | 1280x960 | 16M | 32 | Bank + LFB
| 121h | Graph | 640x480 | 16M | 32 | Bank + LFB
| 122h | Graph | 800x600 | 16M | 32 | Bank + LFB
| 123h | Graph | 1024x768 | 16M | 32 | Bank + LFB
| 124h | Graph | 1280x1024 | 16M | 32 | Bank + LFB
| 143h | Graph | 1400x1050 | 256 | 8 | Bank + LFB
| 145h | Graph | 1400x1050 | 64k | 16 | Bank + LFB
| 146h | Graph | 1400x1050 | 16M | 32 | Bank + LFB
| 173h | Graph | 1600x1200 | 256 | 8 | Bank + LFB
| 175h | Graph | 1600x1200 | 64k | 16 | Bank + LFB
| 176h | Graph | 1600x1200 | 16M | 32 | Bank + LFB
| 183h | Graph | 1792x1344 | 256 | 8 | Bank + LFB
| 185h | Graph | 1792x1344 | 64k | 16 | Bank + LFB
| 186h | Graph | 1792x1344 | 16M | 32 | Bank + LFB
| 1D3h | Graph | 1856x1392 | 256 | 8 | Bank + LFB
| 1D5h | Graph | 1856x1392 | 64k | 16 | Bank + LFB
| 1D6h | Graph | 1856x1392 | 16M | 32 | Bank + LFB
| 1E3h | Graph | 1920x1440 | 256 | 8 | Bank + LFB
| 1E5h | Graph | 1920x1440 | 64k | 16 | Bank + LFB
| 1E6h | Graph | 1920x1440 | 16M | 32 | Bank + LFB