XMS/EMS RAM disk installable and
resizable from command line.

You can choose the drive letter.
Up to 2 Gbytes supported.

Compatible with:
- MSDOS 3 to 7 (Win95), DosEmu (Linux),
  NWDOS 7 (OpenDOS/DR-DOS 7), PCDOS 7.
- DBLSPACE/DRVSPACE, GUEST/GUEST95,
  Stacker 4.
  
Include a little helper for HIMEM 3.09+
to let it use more than 64MB.

Freeware by Franck Uberto.
