                                 Example 1
                                 ÄÄÄÄÄÄÄÄÄ

     System Analyser     (C) 2009  Hans Niekus     V5.3w     Registered
 *****************************************************************************
             Computer : AT  (ID=FCh / Subm=01h / Vers=0)
    BIOS  date / name : 09/09/97   Award Modular BIOS v4.51PG
                      : i440LX-<P2L97>-00   (#401A0-0102)
                      : Asustek Flash Bios
          DOS version : 7.10  Rev=0  OEM=FFh
                      : Virtual 8086 mode
   OEM version string : Windows 95 [Version 4.00.1111]
                      : (Windows 95 OSR 2 / 2.1)
Adv. Power Management : Version=1.2   (enabled)
                 ACPI : Version=1.0   OEM=ASUS
   Plug and Play BIOS : Version=1.0
             PCI BIOS : Version=2.10
----------------------+--------------------------------------------------------
              Network : Novell Netware v3.12a   (max 100 users)
                      : Server name=SOYO   User name=SUPERVISOR
                      : Shell v4.00a in Extended memory
                      : IPX/SPX v3.30   TCP/IP v2.11   Netbios
         Node address : 00 80 29 69 55 EF
                 Card : SMC LAN Adapter MLID
                      : Frame=ETHERNET_802.3
                      : Port=0280h   IRQ=12

              Network : Microsoft LAN manager
                      : Computer=DEFAULT   User=GEBRUIKER   Domain=GROUP

     ISA Network Card : Port=0280h   (NE2000 or compatible)
         Node address : 00 80 29 69 55 EF
----------------------+--------------------------------------------------------
         Windows path : C:\WINDOWS\
             Computer : Standard PC
              Display : Diamond Viper V330
             Keyboard : Standard 101/102-Key or Microsoft Natural Keyboard
                Mouse : Microsoft IntelliPoint
              Printer : HP DeskJet 870 (Color),HPDSKJTB,LPT1:
              Country : United States
      Swap file drive : D:
----------------------+--------------------------------------------------------
           DOS config : Files=100   Fcbs=4,0   Buffers=50,0   Stacks=0,0
                      : Dos in HMA   Last Drive=`:   Break=on   Verify=off
          Environment : 2064 Bytes   Used=243 Bytes
         Country code : 31   Date=DMY   Time=24h
            Code page : Active=850   Default=437
         System start : Cold-reset   Boot-drive=C:   Boot-menu=EMM 
----------------------+--------------------------------------------------------
                 APIC : Enabled (More than one processor present?)
             CPU type : Intel Pentium II
                CPUID : Family=06h   Model=03h   Stepping=03h
  Feature flags (EDX) : Feature flags=00000000 10000000 11111011 11111111
                      : Internal bus width=64 bit
     Math Coprocessor : Integrated   (Dan-0411 bug)
          Multi Media : MMX
          Clock speed : 301.6 MHz   Multiplier=4.5   FSB=66 MHz   (67 MHz)
        Level 1 Cache : Code=16 kB   4 Way   Cache-line=32 Byte             
                      : Data=16 kB   4 Way   Cache-line=32 Byte
                      : Write back
        Level 2 Cache : 512 kB   4 Way   Cache-line=32 Byte
                      : Write back   ECC=on

    Memory efficiency : Code=10.3-0.0ws   DataR=7.4-0.0ws   DataW=1.0ws
   Prim. / Sec. cache : Code=1.9-0.0ws   DataR=0.2-0.0ws
    Prim. cache speed : Code=2256.4 Mb/s   DataR=292.2 Mb/s
     Sec. cache speed : Code=396.5 Mb/s    DataR=288.8 Mb/s
         Memory speed : Code=102.0 Mb/s    DataR=101.2 Mb/s
    PC-relative speed : CPU=54867%   FPU=105246%   (Cache hit speed)
----------------------+--------------------------------------------------------
   Main memory (CMOS) : 640 kB  (A0000h)
   Main memory (DOS)  : 639 kB  (9FC00h)   Used=46832 Bytes   Free=593 kB
   Main memory (PSP)  : 639 kB  (9FBF0h)
 Program load address : 0B6F0h
        Ram above 1MB : 64512 kB
         Total memory : 64 MB
 
              DIMM 0 : SDRAM   32 MB   PC100   10.0ns (100MHz)
                      : Banks=2   Rows=2x11   Colomn=9   Width=64b
                      : ErrorT/C=None   Unbuffered   SPD-ver=1.2
                      : THMY6440A1AEG-10   ver=?   Date=97-44   sn=?   
		      : Company=?   Level=LVTTL
                      : CL=2,3  Trcd=20 ns  Trp=20 ns  Tras=50 ns  Tac=8.0
               DIMM 1 : SDRAM   32 MB   PC100   8.0ns (125MHz)
                      : Banks=2   Rows=2x11   Colomn=9   Width=64b
                      : ErrorT/C=None   Unbuffered   SPD-ver=1.2
                      : name=?   ver=?   date=?   sn=?
                      : Company=?   Level=LVTTL
                      : CL=2  Trcd=18 ns  Trp=18 ns  Tras=45 ns  Tac=6.0

              LIM-EMS : version=4.0   Page frame=NONE   (EMM386-version=4.95)
               Memory : 33152 kB   Used=384 kB   Free=32768 kB
              Handles : Base=384 kB

           XMS driver : XMS-version=3.00   HIMEM-version=3.5F
    (639h..1024h) UMB : 140 kB   Used=118 kB   Free=21840 Bytes
   (1024h..1088h) HMA : 64 kB   Used=57 kB   Free=7 kB   A20=Enabled
                      : Handler=1 (AT)   Switch speed=medium
         (>1088h) EMB : 64448 kB   Free=64036 kB  (Largest free block=64036 kB)
              Handles :  EMB_D47E=4 kB  EMB_D488=408 kB

          Virtual DMA : VDS-version=1.0   buffer=64 kB   (EMM386)
----------------------+--------------------------------------------------------
          VESA VBE/DC : Supported (Display Data Channel)
              Monitor : EIZ1004 = EIZO FlexScan F56
                      : Year=1997   Week=8   Sn=28189   EDID-version=1.1
                      : Horizontal=31 cm   Vertical=23 cm   (Diagonal=15.20")
                      : Vertical=50-160 Hz   Horizontal=27-86 kHz

          VESA VBE/PM : Version=1.0   (State=On)
     Supported states : Standby  Suspend  Off

       3D accelerator : 3DFX VooDoo

       AGP controller : Version=1.0   Rate=x1/x2 (used=?x)   Queue=32
                      : >4GB=no   SBA=no
    AGP Video adapter : Version=1.0   Rate=x1 (used=?x)   Queue=5
                      : >4GB=no   SBA=no

      Display adapter : VGA in mode 03h
                 Chip : NVidia Riva 128
          Bios / Card : Diamond Multimedia Systems, Inc. Viper V330 Version 1.
                      : 49
                  DAC : TrueColor 24 bit
                      : (EGA switches=0110   Feature bits=0000)

         VESA version : 3.0   OEM=NVidia
VESA Software version : 81.1   OEM=NVidia
  VESA Poduct version : Rev B1   OEM=Riva 128 Eval Card
           VESA modes : 0100, 0101, 0102, 0103, 0104, 0105, 0106, 0107, 0108
                      : 0109, 010A, 010B, 010C, 010E, 010F, 0111, 0112, 0114
                      : 0115, 0117, 0118, 011A, 0130, 0131, 0132, 0133, 0134
                      : 0135, 0136, 0137, 0138, 0139, 013A, 013B, 013C, 013D
                      : 013E, 0141, 0142, 0143, 0145, 0146, 0147, 0148, 0149
                      : 014A, 014B, 014C

   Memory (Vesa info) : 4096 kB     Type=SGRAM
  Monitor (PS/2 info) : VGA Color display   (Vert=70.0 Hz / Horiz=31.45 kHz)
      Video-speed RAM : 8bit=8315 kB/s   16bit=16688 kB/s   32bit=33611 kB/s
Video-speed BIOS, DOS : 112 KC/s  Scroll=0.73ms,   65380 C/s  Scroll=0.74ms
----------------------+--------------------------------------------------------
     Disk compression : Stacker  version=4.02

     Logical drive(s) : 11  named  A: to K:

  Floppy disk control : BIOS=Multirate   Controller=Enhanced   IRQ=6   DMA=3
 Floppy disk drive(s) : 2   0/A:1.44 MB  (80T 2H 18S) NEC 3mode
                      :     1/B:1.2 MB   (80T 2H 15S)

 Logical Hard disk(s) : 80a/C:13457 MB  (11278 MB)  MAXTOR100 A  Fat32  Active 
                      : 81a/D: 1028 MB  (  983 MB)  IBM A 1      Fat16  Active
                      : 82a/E: 1539 MB  ( 1023 MB)  IBM B 1      Fat32  Active
                      : 80c/F:17547 kB  (  657 kB)  Compressed
                      : 80d/G: 6622 MB  ( 4826 MB)  MAXTOR100 D  Fat32  
                      : 81b/H: 1173 MB  (  642 MB)  IBM A 2      Fat16
                      : 82d/I: 5548 MB  ( 3272 MB)  IBM B 4      Fat32
                      : 80a/K:13457 MB  (  234 MB)  SUBST  C:\TALEN\ASM

 Non DOS partition(s) : 80b    8482 MB  (HPFS / NTFS)
                      : 82b    1655 MB  (Linux extd)
                      : 82c     201 MB  (Linux swap)

        Hard disk 80h : (30015MB 59554T 16H 63S) E-IDE   Mode=LBA   Type=47
             ATA info : (30015MB / 8257MB 16383T 16H 63S) Maxtor 53073H6      
            seek (ms) : T-T=1.3   Average=9.1   Full=13.6   Overhead=0.3
         speed (kB/s) : Max=9360   64kB=9017   4kB=7203   512B=2890
             Rotation : +/-7103 rpm   half-revolution=4.2ms
             ATA info : Buffer=2048kB   Sn=K60ECBZC               Rev=DAC10SC0
                      : LBA=yes  LBA48bit=no  DMA=yes  IORDY=yes (sw)
                      : DwordIO=no  PIOmode=4  DMAmode=0  MultiSec=16 sectors
                      : ATA 6  MultiW-DMA=2 (used=no)  Ultra-DMA=5 (used=2)
                      : SMART=off  Look-ahead=on  Write cache=on  APM=no
  Acoustic management : Disabled   (Current=FEh   Recommended=C0h)
           Controller : IRQ=14   port=01F0h   Master
               INT 13 : extension V2.1

        Hard disk 81h : (2201MB 274T 255H 63S) SCSI
            ASPI info : (2201MB 274T 255H 63S) IBM DFRSS2W
            seek (ms) : T-T=3.6   Average=8.7   Full=15.7   Overhead=0.7
         speed (kB/s) : Max=7237   64kB=7237   4kB=4559   512B=601
             Rotation : +/-7120 rpm   half-revolution=4.2ms
           Controller : IRQ=10
               INT 13 : extension V1.0

        Hard disk 82h : (8217MB 1023T 255H 63S) SCSI
            ASPI info : (8958MB 1115T 255H 63S) IBM DGHS09V
            seek (ms) : T-T=2.1   Average=7.9   Full=13.2   Overhead=0.6
         speed (kB/s) : Max=35222   64kB=15033   4kB=14181   512B=2561
             Rotation : +/-7201 rpm   Average-latency=4.2ms
           Controller : IRQ=10             
               INT 13 : extension V1.0

    Hard disk found ? : port=01F0h   Slave   Address=83h
                      : (4209MB 524T 255H 63S Novell NetWr) Part. table info
             ATA info : (4209MB 14848T 9H 63S) QUANTUM FIREBALL ST4.3A        
                      : Buffer=81kB   Sn=154709841715           Rev=A0F.0400
                      : LBA=yes  LBA48bit=no  DMA=yes  IORDY=yes (sw)
                      : DwordIO=no  PIOmode=4  DMAmode=2  MultiSec=16 sectors
                      : ATA 3  MultiW-DMA=2 (used=no)  Ultra-DMA=2 (used=2)

ATAPI magnetic device : port=0170h   Slave    Name=IOMEGA  ZIP 100       ATAPI
           ATAPI info : Buffer=0kB   Sn=                       Rev=23.D
----------------------+--------------------------------------------------------
               MSCDEX : version=2.25

               CD-ROM : K:396 MB   PC-WELT 01/2002     
               Driver : ASPICD   Divice=ASPICD0
                 Type : SCSI
         Capabilities : 00000796  ->  Raw_mode   Audio+Video   Prefetching
                      : Audio_manip.   Red-book
    Measured CD speed : Inner=1459 kB/s  (x10)   -   Outer=2993 kB/s  (x20)
                      : Average access=153ms
           Controller : IRQ=10

 ATAPI CD-ROM found ? : port=01F0h   Master   Name=PLEXTOR CD-R   PX-W2410A
                 Type : ATAPI (IDE)
                 Read : CD-R, CD-RW
                Write : CD-R, CD-RW
           ATAPI info : Buffer=4096kB   Sn=              717256   Rev=1.02
                      : LBA=yes  DMA=yes  IORDY=yes (sw)
                      : DwordIO=no  PIOmode=4  DMAmode=2  MultiSec=no
                      : ATA 6  MultiW-DMA=2 (used=no)  Ultra-DMA=2 (used=2)
         Capabilities : Composite   XA   Mode 2 Form 2   Multi-session   
                      : CD DA stream   ISRC   UPC   
Supported raw CDspeed : Maximum=7056 kB/s (x40)   Current=7056 kB/s (x40)
  Writing raw CDspeed : Maximum=4234 kB/s (x24)
----------------------+--------------------------------------------------------
       Parallel ports : 1) Lpt1=0378h  IRQ=7    ECP   DMA=3   Fifo=16 Byte
                      : 2) Lpt2=0278h  IRQ=5    Bi-directional  (off)
         Serial ports : 1) Com1=03F8h  IRQ=4    Chip=16550A        2400,N,8,1
                      : 2) Com2=02F8h  IRQ=3    Chip=16550A        1200,N,7,1
                      : 3) Com4=02E8h  IRQ=3    Chip=16550A        2400,N,8,1
                      :    Com?=03E0h  IRQ=4    Chip=16550         9600,E,7,1
         Serial mouse : 2 buttons  Com1  IRQ=4  Dr-Vers=08.20  (.COM/.EXE)
                      : LOGITECH MOUSE DRIVER V7.00
                      : ID=MZ@   PnP-ID=MSH0001   Vers=1.00
                      : Serial#=00040200   Class=MOUSE   DeviceID=PNP0F0A
                      : UserName=MICROSOFT INTELLIMOUSE - SERIAL VERSION
            Game port : 0 Joystick(s)
             Keyboard : BIOS=101/102 key   Keyboard=AT-MF2
                      : 8042 Controller: yes   Intercept: yes   INT16/9: no
  Keyboard controller : (C)1996  HOLTEK
----------------------+--------------------------------------------------------
 Parallel port device : Lpt1  IRQ=7    Printer
              VSTATUS : $H00118001$M00008EC1,ff,UP,IDLE
                  MFG : HEWLETT-PACKARD
                  MDL : DESKJET 870C
                  CMD : PCL,MLC,PML
                CLASS : PRINTER
          DESCRIPTION : Hewlett-Packard Deskjet 870C
----------------------+--------------------------------------------------------
                Modem : Com4   IRQ=3
                Class : 0 1 2.0 80   (Fax-Voice-modem)   Current class=0
        Maximum speed : 56000 bps
      Supported modes : V.21, V.22, V.22bis, V.23, V.32, V.32bis, V.34,
                      : K56flex, BELL 103, BELL 212
  Fax/modem Manufact. : ROCKWELL
      Fax/modem Model : AC/V34
    Fax/modem version : V1.002-K56_DLS
           Model info : RCV56DPF L8570A Rev 30.0/30.0
        Plug and Play : PnP-ID=ETT0003   Vers=1.00
                      : Serial#=12345678   Class=MODEM   DeviceID=ETT0003
                      : UserName=E56K
----------------------+--------------------------------------------------------
      Common ISDN API : version=1.1 and 2.0
         Manufacturer : TELES GmbH, Berlin
                      : Version 1.1, Profil A, Release 3.17
            Adapter 1 : number of B channels=1
          B1 protocol : 64k bps with HDLC framing
                      : 64k bps bit transparent with network byte framing
                      : V.110 asynchronous with start/stop byte framing
                      : 56k bps bit transparent with network framing
          B2 protocol : ISO 7776 (X.75 SLP)
                      : transparant
                      : SDLC
          B3 protocol : transparent
                      : T.90NL with T70NL compatibility
                      : ISO 8208 (X.25 DTE-DTE)
----------------------+--------------------------------------------------------
                Adlib : Port=0388h
        Sound Blaster : port=0220h   DSP-version=4.16   IRQ=5   DMA=1,5
        DSP Copyright : COPYRIGHT (C) CREATIVE TECHNOLOGY LTD, 1992.
Wavetablechip EMU8000 : port=0620h   Memory=4096 kb
                 Type : Sound Blaster AWE 32 (or compatible)
                Mixer : CT1745 (or compatible)
 Environment BLASTER= : SB=220h  IRQ=5  DMA8=1  DMA16=5  MIDI=330h  Wave=620h
                      : Type=6  ->  Sound Blaster 16 (or compatible)
                 MIDI : port=0330h
    Environment MIDI= : SYNTH=Intern  MAP=Extended  MODE=Standard
----------------------+--------------------------------------------------------
         SCSI adapter : Adaptec   AHA-2940 /U /W /UW
		      : IRQ=10

               Driver : ASPI   Name=DOS SCSIMGR 1.24   Adapter=ADAPTEC AIC-7870
                      : Wide 16 bit

            Device(s) : 0) Disk drive
                      :    IBM      DGHS09V           Rev=03E0
                      :    SCSI-3   Wide-16   Synchronous   Linking   Queuing
                      :    (8958MB 8152T 10H)   Bytes/Sect=512   Address=82h
                      :    Rotation=7200 rpm   Write cache=Enabled

                      : 1) Disk drive         
                      :    IBM      DFRSS2W           R=4B4B 
                      :    SCSI-2   Wide-16   Synchronous   Linking   Queuing
                      :    Capacity=2202 MB     Bytes/sect=512   Address=81h

                      : 2) Tape drive
                      :    HP       C1533A            R=9406
                      :    SCSI-2   Synchronous   Linking

                      : 4) CD-ReWritable
                      :    YAMAHA   CRW4416S          Rev=1.0e   Date=25/11/98
                      :    SCSI-2   Synchronous
                      :    Capacity=454 MB      Bytes/Sect=2048  Buffer=2048 kB

                      : 7) Host adapter   (IRQ=10)
----------------------+--------------------------------------------------------
             Bus type : ISA / PCI
  CMOS clock / memory : yes / 128 Bytes
Equipment list INT 11 : (LLxxRRRx FFVVxxCF)  01000110 01100011
Sys. config. INT15/C0 : FCh  01h  00h  dICKwBmx  00h  00h  00h  00h
----------------------+--------------------------------------------------------
  Main RAM on address : 00000 -  A0000  640 kB (32 bit  8.4-1.2)
 Video RAM on address : B8000 -  BC000   32 kB (32 bit  45)

 32 kB BIOS extension : VGA Compatible
       ROM on address : C0000 -  C8000   32 kB (32 bit  47.8-49.2)

 18 kB BIOS extension : Copyright Adaptec, Inc. 1998PCIR
       ROM on address : C8000 -  CC800   18 kB (32 bit  47.8-49.2)

   UMB RAM on address : CD000 -  F0000  140 kB (32 bit  8.4-0.0)

       ROM on address : F0000 -  F5C00   23 kB (32 bit  47.8-49.2)
       ROM on address : F6000 -  FDC00   31 kB (32 bit  48.4-49.2)
       ROM on address : FE000 - 100000    8 kB (32 bit  48.4-49.8)
----------------------+--------------------------------------------------------
  Ext. RAM on address : 00100000 - 04000000   64512 kB

 Device drivers
 *****************************************************************************
  Address    Strat  Inter  Attr  T  Device    Addr    Name      Size
  =========  =====  =====  ====  =  ========  ======  ========  ============
  00C9:0048  :0DCD  :0DD3  8004  C  NUL
  D7E5:0000  :001E  :0029  8000  C  SETVERXX  D7E4:0  SETVER       832 Bytes
  D732:0000  :040B  :03A8  D000  C  IFS$HLP$  D731:0  IFSHLP      2848 Bytes
  D415:0000  :025E  :0269  C800  C  ASPICD0   D414:0  ASPICD     12736 Bytes
  CE5E:0000  :3434  :343F  C000  C  SCSIMGR$  CE5D:0  ASPI8DOS   23392 Bytes
  EAB7:0000  :0124  :012F  8000  C  _STAC_HI  EAB6:0  STACHIGH   16272 Bytes
  037D:0000  :0016  :0021  C840  C  DblBuff$  037C:0  DBLBUFF     2432 Bytes
  026F:003A  :004C  :007E  C000  C  $MMXXXX0  026E:0  EMM386      4304 Bytes
  026F:0000  :004C  :007E  C000  C  EMMQXXX0  026E:0  EMM386      4304 Bytes
  0226:0000  :0047  :0052  A000  C  XMSXXXX0  0225:0  HIMEM       1152 Bytes
  0070:0016  :027A  :0285  8013  C  CON
  0070:0028  :027A  :02A6  8000  C  AUX
  0070:003A  :027A  :028A  A0C0  C  PRN
  0070:004C  :027A  :00EE  8008  C  CLOCK$
  0070:005E  :027A  :00F3  08C2  B  10
  0070:006A  :027A  :02A6  8000  C  COM1
  0070:007C  :027A  :0291  A0C0  C  LPT1
  0070:008E  :027A  :0298  A0C0  C  LPT2
  0070:00A0  :027A  :029F  A0C0  C  LPT3
  0070:012D  :027A  :02BE  C000  C  CONFIG$
  0070:00B8  :027A  :02AC  8000  C  COM2
  0070:00CA  :027A  :02B2  8000  C  COM3
  0070:00DC  :027A  :02B8  8000  C  COM4

 Environment
 *****************************************************************************
 TMP        = C:\WINDOWS\TEMP
 TEMP       = C:\WINDOWS\TEMP
 CONFIG     = EMM
 PROMPT     = $p$g
 winbootdir = C:\WINDOWS
 COMSPEC    = C:\COMMAND.COM
 BLASTER    = A220 I5 D1 H5 P330 E620 T6
 MIDI       = SYNTH:1 MAP:E MODE:0
 PATH       = C:\WINDOWS;C:\WINDOWS\COMMAND;D:\NC;C:\AUTO;D:\ARC;C:\PBDLL10
 CMDLINE    = sa51

 E:\TALEN\ASM\AA\SA\SA51.COM

 Memory Control Blocks
 *****************************************************************************
  Address          T  Own   Name      Size          Type
  ===============  =  ====  ========  ============  ==========
  0224:0 - 0459:0  M  0008  SD          9024 Bytes  Device(s):

  0225:0 - 026E:0  D  0226  HIMEM       1152 Bytes  XMSXXXX0
  026E:0 - 037C:0  D  026F  EMM386      4304 Bytes  EMMQXXX0
  037C:0 - 0415:0  D  037D  DBLBUFF     2432 Bytes  DblBuff$
  0415:0 - 0438:0  I  0416               544 Bytes  IFS driver
  0438:0 - 0459:0  B  0439               512 Bytes  BUFFERS=50,0

  0459:0 - 045E:0  M  0008  SC            64 Bytes
  045E:0 - 0470:0  M  2B70               272 Bytes  Environment
  0470:0 - 0B5B:0  M  0471  MOUSE      28320 Bytes  Program
  0B5B:0 - 0B6E:0  M  0B6F  SA51         288 Bytes  Environment
  0B6E:0 - 9FBF:0  Z  0B6F  SA51      607488 Bytes  Program
------------------------------------------------------------- UMBs NOT linked -
  9FBF:0 - CE5C:0  M  0008  SC        190912 Bytes  Not used

  CD00:0 - CE5B:0  M  CD01  UMB         5536 Bytes  UMB Control block
  CE5B:0 - F000:0  Z  CE5C  UMB       137792 Bytes  UMB Program(s):

  CE5C:0 - E1E7:0  M  0008  SD         80032 Bytes  Device(s):

  CE5D:0 - D414:0  D  CE5E  ASPI8DOS   23392 Bytes  SCSIMGR$
  D414:0 - D731:0  D  D415  ASPICD     12736 Bytes  ASPICD0
  D731:0 - D7E4:0  D  D732  IFSHLP      2848 Bytes  IFS$HLP$
  D7E4:0 - D819:0  D  D7E5  SETVER       832 Bytes  SETVERXX
  D819:0 - D878:0  I  D81A              1504 Bytes  IFS driver
  D878:0 - D9D8:0  F  D879              5616 Bytes  FILES=100
  D9D8:0 - D9E9:0  X  D9D9               256 Bytes  FCBS=4,0
  D9E9:0 - E075:0  B  D9EA             26800 Bytes  BUFFERS=50,0
  E075:0 - E126:0  L  E076              2816 Bytes  LASTDRIVE=`:
  E126:0 - E1E7:0  S  E127              3072 Bytes  STACKS=9,256

  E1E7:0 - E34D:0  M  E1E8  COMMAND     5712 Bytes  Program
  E34D:0 - E3CF:0  M  E1E8  COMMAND     2064 Bytes  Environment
  E3CF:0 - E3DE:0  M  0000  -free-       224 Bytes
  E3DE:0 - EAB6:0  M  E3DF  MSCDEX     28016 Bytes  Program
  EAB6:0 - EEB0:0  D  EAB7  STACHIGH   16272 Bytes  _STAC_HI
  EEB0:0 - F000:0  Z  0000  -free-      5360 Bytes
------------------------------------------------------------------------- HMA -
  FFFF:0030           FFFF             53072 Bytes
  FFFF:CF90           0C30              9760 Bytes
  FFFF:F5C0           FFFB               736 Bytes
  FFFF:F8B0           0000  -free-      1856 Bytes

 CMOS memory
 *****************************************************************************
    1999-2000 rollover : Cmos=01-01-1900   Bios=01-01-2000   Ok
 Set century byte Cmos : Cmos=01-01-2000   Bios=01-01-2000   Ok
   Set 01-01-2000 Bios : Cmos=01-01-2000   Bios=01-01-2000   Ok
        Leap year 2000 : Cmos=29-02-2000   Bios=29-02-2000   Ok
            Conclusion : Millennium proof

       DOS Time  : 21:04:20                    DOS Date : 01/01/2003 Wednesday

(04 02 00) Time  : 21:03:00       (07 08 32 09 06) Date : 01/01/2003 Monday
(05 03 01) Alarm : 15:18:46

(10) (0100 ....)  Type of diskette drive 0  : 1.44MB
     (.... 0010)  Type of diskette drive 1  : 1.2MB

(14) (01.. ....)  Number of diskette drives : 2
     (..00 ....)  Primary display           : EGA / VGA
     (.... 11..)  Reserved
     (.... ..1.)  Coprocessor               : Yes
     (.... ...1)  Diskette drive installed  : Yes

(16 15) Main memory      : 640 kB          (12) (x.) fixed disk type 0 : 15
(18 17) Expansion memory : 64512 kB             (.x) fixed disk type 1 : 0
(31 30) Actual Exp. mem. : 64512 kB        (19)      fixed disk type 0 : 47 <-
                                           (1A)      fixed disk type 1 : 47
(0A) Status A : 0010 0110  (0010 0110) ok
(0B) Status B : 0000 0010  (0000 0010) ok
(0C) Status C : 0101 0000  (010x 0000) ok
(0D) Status D : 1000 0000  Power ok        (0F) Shutdown Status  : 0000 0000
(0E) POST     : 0000 0000                  (33) Information flag : 1000 0000

(2E 2F) Checksum 10h-2Dh : 09AAh ok

Hard disk user types :
(26-2D) 0 : Cyl= 14848   Head=  9   Precomp= 65535   Landz= 14847   Sector= 63
(1E-25) 1 : Cyl=     0   Head=  0   Precomp=     0   Landz=     0   Sector=  0
(68-6F) 2 : Cyl=  1654   Head= 16   Precomp= 65535   Landz=  1655   Sector= 63
(71-78) 3 : Cyl=     0   Head=  0   Precomp=     0   Landz=     0   Sector=  0

      Bytes from the CMOS RAM
      =======================
      00  01  02  03  04  05  06  07  08  09  0A  0B  0C  0D  0E  0F
      --  --  --  --  --  --  --  --  --  --  --  --  --  --  --  --
 00 | 00  46  03  18  21  15  02  01  01  03  26  02  50  80  00  00
 10 | 42  65  F0  02  4F  80  02  00  FC  2F  2F  30  FF  FF  00  00
 20 | 00  00  00  00  00  00  00  3A  09  FF  FF  FF  39  3F  09  AA
 30 | 00  FC  20  80  FF  FF  BF  FF  FF  DF  FF  0F  78  9B  F8  19
 40 | 88  FC  F1  FC  88  88  FD  00  7F  AF  2F  F1  4F  DE  FF  FF
 50 | 90  7F  00  00  FF  F7  F8  F7  00  00  20  80  C0  C0  FF  FF
 60 | FF  FF  FE  74  FF  FF  FF  2F  00  00  00  00  00  00  FF  00
 70 | 2F  00  00  00  00  00  00  00  00  FF  17  54  FF  FF  1E  D9

 PCI   +   PCMCIA   +   Plug & Play
 *****************************************************************************
 PCI BIOS version=2.10      Last bus number=0

 Bus 0   Devices:
 ================
  00:Intel             7180h=82443LX Pentium(r) II PCI bridge          Rev=03h
     Class=06h/00h     Class=Host bridge                              RLPI=00h
     No PCI-INT
     Busmaster=Yes   Mem space=Yes   I/O space=No    66MHz=No
     AGP version=1.0

  10:Intel             7181h=82443LX Pentium(r) II AGP Controller      Rev=03h
     Class=06h/04h     Class=PCI bridge                               RLPI=00h
     No PCI-INT
     Busmaster=Yes   Mem space=Yes   I/O space=Yes   66MHz=Yes
     Mem Base address=E2D0E180h

  40:Intel             7110h=82371AB PIIX4 ISA Bridge                  Rev=01h
     Class=06h/01h     Class=ISA bridge                               RLPI=00h
     No PCI-INT
     Busmaster=Yes   Mem space=Yes   I/O space=Yes   66MHz=No

  41:Intel             7111h=82371AB PIIX4 EIDE Controller             Rev=01h
     Class=01h/01h     Class=IDE bus controller                       RLPI=80h
     No PCI-INT
     Busmaster=Yes   Mem space=No    I/O space=Yes   66MHz=No
     I/O Base address=0000D800h

  42:Intel             7112h=82371AB PIIX4 USB Universal Host Contr.   Rev=01h
     Class=0Ch/03h     Class=USB (Universal Serial Bus)               RLPI=00h
     PCI-INTD -> IRQ 9                                                        
     Busmaster=Yes   Mem space=No    I/O space=Yes   66MHz=No
     I/O Base address=0000D400h

     USB-version=1.0   Status=No errors   IRQ=Enabled    Frame time=1.0 ms
     Port 1 status : Device(s) Present   Enabled    Low-speed    Normal cond.
     Port 2 status : Device(s) Not present

  43:Intel             7113h=82371AB PIIX4 Power management controller Rev=01h
     Class=06h/80h     Class=Other bridge controller                  RLPI=00h
     No PCI-INT
     Busmaster=No    Mem space=Yes   I/O space=Yes   66MHz=No

 110:3Dfx              0001h=VooDoo 3D Video processor                 Rev=02h
     Class=04h/00h     Class=Video device                             RLPI=00h
     No PCI-INT
     Busmaster=No    Mem space=Yes   I/O space=No    66MHz=No

 120:Adaptec           8178h=AHA-2940 /U /W /UW SCSI Controller        Rev=00h
     Class=01h/00h     Class=SCSI bus controller                      RLPI=00h
     PCI-INTA -> IRQ 10
     Busmaster=Yes   Mem space=Yes   I/O space=Yes   66MHz=No
     ROM=C8000-CC800h   (18 kB)

 Bus 1   Devices:
 ================
  00:NVidia            0018h=Riva 128 2D/3D Video adapter              Rev=10h
     Class=03h/00h     Class=VGA controller                           RLPI=00h
     PCI-INTA -> IRQ 11
     Subsys: Diamond           1092h=Viper V330 (Turbo) Video adapter
     Busmaster=Yes   Mem space=Yes   I/O space=Yes   66MHz=Yes
     AGP version=1.0
     ROM=C0000-C8000h   (32 kB)
-------------------------------------------------------------------------------

 PCMCIA Card Services (c) 1993 Phoenix Technologies Ltd
 PCMCIA Card Service version=2.0A      Vendor-version=2.15      Socket(s)=1

 Sockets:
 ========
  0: Xircom 
     CreditCard 10Base-T
     CE-10BC
     2.0/0008071478-033194
     Device = Function specific (13h)
-------------------------------------------------------------------------------

 Plug and Play BIOS : version=1.0   (PNP0C00)
                 CM : not present

 Number of ISA/EISA PnP card(s) = 1   (Read Port=020Bh)

 PnP Card(s):
 ============
  1: CTL009C : Creative SB32 PnP
     CTL0041 : Audio                                                  Enabled
         IRQ : 5
         DMA : 1, 5
        Port : 0220, 0330, 0388
     CTL7002 : Game                                                   Enabled
        Port : 0200
     CTL0021 : WaveTable                                              Enabled
        Port : 0620, 0A20, 0E20
     CTL2011 : IDE                                                    Disabled

 PnP ROM(s):
 ===========
     Segment : C800h   Length=18 kB
     D@D7881 : Adaptec   2940U/UW
       Class : SCSI bus controller

 Nodes: (PnP BIOS)
 ======
  0: PNP0401 : ECP printer port
       Class : 07h/01h/00h   Paralell Port
         DMA : 3
         IRQ : 7
        Port : 0378-037Fh, 0778-077Fh

  1: PNP0401 : ECP printer port
       Class : 07h/01h/00h   Paralell Port
         DMA : 3
         IRQ : 7
        Port : 0378-037Fh, 0778-077Fh

  2: PNP0501 : 16550A compatible COM port
       Class : 07h/00h/02h   RS-232 device (16550 compatible)
         IRQ : 4
        Port : 03F8-03FFh

  3: PNP0501 : 16550A compatible COM port
       Class : 07h/00h/02h   RS-232 device (16550 compatible)
         IRQ : 3
        Port : 02F8-02FFh

  4: PNP0700 : PC standard floppy disk controller
       Class : 01h/02h/00h   Floppy disk controller
         IRQ : 6
         DMA : 2
        Port : 03F2-03F5h

  6: PNP0C01 : System Board
       Class : 05h/00h/00h   RAM controller
         Mem : 00000000-0009FFFFh  RAM  32bit  Cacheable
               00100000-03FFFFFFh  RAM  32bit  Cacheable
               000E8000-000FFFFFh  ROM  32bit  Cacheable  Shadowable
               FFFE0000-FFFFFFFFh  RAM  32bit  Cacheable

  7: PNP0000 : AT Interrupt Controller
       Class : 08h/00h/01h   ISA Programable Interrupt Controller
         IRQ : 2
        Port : 0020-0021h, 00A0-00A1h, 04D0-04D1h

  8: PNP0100 : AT Timer
       Class : 08h/02h/01h   ISA System Timer
         IRQ : 0
        Port : 0040-0043h

  9: PNP0B00 : AT Real Time Clock
       Class : 08h/03h/01h   ISA Real Time Clock
         IRQ : 8
        Port : 0070-0071h

 10: PNP0303 : IBM Enhanced (101/102-key  PS/2 mouse support)
       Class : 09h/00h/00h   Keyboard controller
         IRQ : 1
        Port : 0060h, 0064h

 11: PNP0C04 : Math Coprocessor
       Class : 0Bh/01h/00h   486-based processor
         IRQ : 13
        Port : 00F0h

 12: PNP0200 : AT DMA Controller
       Class : 08h/01h/01h   ISA DMA controller
         DMA : 4  (Master)
        Port : 0000-000Fh, 0080-0090h, 0094-009Fh, 00C0-00DEh

 13: PNP0800 : AT style speaker sound
       Class : 08h/80h/00h   Other System Peripheral
        Port : 0061h

 APM Devices:
 ===========
     PNP0C01 : DeviceID = 0101h
-------------------------------------------------------------------------------
 
 ESCD : Size=4096 bytes   Address=FFFF0000h    version=2.1
 
 ESCD Info:
 ==========

 ======= Slot 01h == ISA/EISA ================================================
     IRQ : 5
     DMA : 1, 5
    Port : 0220h-022Fh, 0330h-0331h, 0388h-038Bh
    Port : 0200h-0207h
    Port : 0620h-0623h ,0A20h-0A23h ,0E20h-0E23h
    Type : PnPISA
         : PnP-ID=CTL009C   Serial Number=E2B91008h

 ======= Slot 0Eh == ISA/EISA ================================================
    Port : 02E8h-02EFh

 ======= Slot 0Fh == ISA/EISA ================================================
    Port : 02E0h-03E7h
    Port : 0278h-027Fh

 ======= System Board Devices ================================================
     IRQ : 7
    Port : 0378h-037Fh, 0778h-077Fh
     IRQ : 4
    Port : 03F8h-03FFh
     IRQ : 3
    Port : 02F8h-02FFh
     IRQ : 6
     DMA : 2
    Port : 03F2h-03F5h
  Memory : 00000000h-000A0000h, 00100000h-040F0000h, 000E8000h-00100000h
         : FFFE0000h-00000000h
     IRQ : 2
    Port : 0020h-0021h, 00A0h-00A1h, 04D0h-04D1h
     IRQ : 0
    Port : 0040h-0043h
     IRQ : 8
    Port : 0070h-0071h
     IRQ : 1
    Port : 0060h, 0064h
     IRQ : 13
    Port : 00F0h
     DMA : 4
    Port : 0000h-000Fh, 0080h, 0094h-009Fh, 00C0h-00CEh
    Port : 0061h
    Port : 0CF8h-0CFFh
    Port : 0290h-0297h, E400h-E40Fh, E420h-E42Fh, E800h-E80Fh, E820h-E82Fh

 ======= Slot 10h == PCI =====================================================
     IRQ : 14, 15
    Port : 01F0h-01F7h, 03F6h, 0170h-0177h, 0376h, D800h-D80Fh
     IRQ : 9
    Port : D400h-D40Fh
    Type : PCI
         : Bus=0   Device=40   Vendor=8086h   Type=7110h
         : Intel   82371AB PIIX4 Function 0: ISA Bridge
    Type : PCI
         : Bus=0   Device=41   Vendor=8086h   Type=7111h
         : Intel   82371AB PIIX4 EIDE Controller
    Type : PCI
         : Bus=0   Device=42   Vendor=8086h   Type=7112h
         : Intel   82371AB PIIX4 USB Universal Host Contr.
    Type : PCI
         : Bus=0   Device=43   Vendor=8086h   Type=7113h
         : Intel   82371AB PIIX4 Function 3: IýC Bus Bridge

 ======= Slot 11h == PCI =====================================================
  Memory : E4000000h-E5000000h, E6000000h-E7000000h, 000A0000h-000B0000h
         : 000B0000h-000C0000h, 000C0000h-000C8000h
     IRQ : 11
    Port : 03B4h-03B5h, 03BAh, 03C0h-03CAh, 03CCh, 03CEh-03CFh, 03D4h-03D5h
         : 03DAh
    Type : PCI
         : Bus=1   Device=00   Vendor=12D2h   Type=0018h
         : NVidia   Riva 128/ZX  2D/3D Video adapter 

 ======= Slot 12h == PCI =====================================================
    Type : PCI bridge
         : Bus=0   Device=10   Vendor=8086h   Type=7181h
         : Intel   82443LX Pentium(r) II AGP Controller

 ======= Slot 13h == PCI =====================================================
  Memory : E7800000h-E8000000h
    Type : PCI
         : Bus=0   Device=00   Vendor=8086h   Type=7180h
         : Intel   82443LX Pentium(r) II PCI bridge

 ======= Slot 14h == PCI =====================================================
  Memory : E8000000h-E8001000h
     IRQ : 10
    Port : 7000h-7003h
    Type : PCI
         : Bus=0   Device=120   Vendor=9004h   Type=8178h
         : Adaptec   AHA-2940 /U /W /UW SCSI Controller

 DMI
 *****************************************************************************

 DMI : Size=1020 bytes   Address=000F585Ah   version=2.2

 ============== BIOS ========================================================= 
         Vendor : Award Software, Inc.
        Version : #401A0-0102
           BIOS : Start-address=F000h   Size=128 kb   Date=09/09/97
Characteristics : ISA \ PCI \ PnP \ APM \ Flash BIOS \ Shadowing \ ESCD
                : CD boot \ Boot select \ Rom in socket \ EDD \ NEC9800 floppy
                : 360 kB floppy \ 1.2MB floppy \ 720kB floppy \ 2.88MB floppy
                : Print screen Int5 \ 8042 Int9 \ Int14 \ Int17
                : Int10 CGA/Mono \ USB \ AGP
 ============== System ======================================================= 
   Manufacturer : System Manufacturer
           Name : System Name
        Version : System Version
  Serial Number : SYS-1234567890
           UUID : Currently not present
   Wake-up Type : Power Switch
 ============== Base Board =================================================== 
   Manufacturer : ASUSTeK Computer INC.
        Product : P2L97
        Version : REV 1.xx
  Serial Number : MB-1234567890
 ============== System Enclosure ============================================= 
   Manufacturer : Chassis Manufacture
        Version : Chassis Version
           Type : Unknown
  Serial Number : Chassis Serial Number
      Asset Tag : Asset-1234567890
          State : Bootup=Safe                   Power Supply=Safe
                : Thermal=Safe                  Security=None
 ============== Processor ==================================================== 
   Manufacturer : Intel Corporation
        Version : Intel Pentium II Processor
           Type : Central Processor   Family=Pentium II  Voltage=2.9 Volt
             ID : 0633h   Feature flags=0080F9FFh
          Clock : Current=300 MHz   Maximum=366 MHz   External=66 MHz
         Socket : SLOT 1   Upgade=Slot 1
 Cache Present : L1, L2
 ============== Memory Controller ============================================ 
        Modules : Max size=64 MB   Number of slots=6   Voltage=3.3 Volt
          Types : EDO \ Parity \ DIMM
         Speeds : 70ns \ 60ns \ 50ns
          Error : Detection=None   Correction=None
     Interleave : Current=1 Way Interleave   Supported=1 Way Interleave
 ============== Memory Module ================================================ 
         Socket : DIMM1-1        Type=Other \ DIMM               Speed=70 ns
           Size : Installed=16 MB           Enabled=16 MB           RAS=0&1

         Socket : DIMM1-2        Type=Other \ DIMM               Speed=70 ns
           Size : Installed=16 MB           Enabled=16 MB           RAS=0&1

         Socket : DIMM2-1        Type=Other \ DIMM               Speed=70 ns
           Size : Installed=16 MB           Enabled=16 MB           RAS=2&3

         Socket : DIMM2-2        Type=Other \ DIMM               Speed=70 ns
           Size : Installed=16 MB           Enabled=16 MB           RAS=2&3

         Socket : DIMM3-1        Type=SIMM                       Speed=70 ns
           Size : Installed=Not installed   Enabled=Not installed   RAS=4&5

         Socket : DIMM3-2        Type=SIMM                       Speed=70 ns
           Size : Installed=Not installed   Enabled=Not installed   RAS=4&5
 ============== Cache ======================================================== 
         Socket : L1 Cache   Internal   Enabled   Mode=Write Back
           Size : Installed=32 KB   Maximum=32 KB

         Socket : L2 Cache   Internal   Enabled   Mode=Write Back
                : 15 ns   4 way   Type=Unified
    Error Corr. : None
           Size : Installed=512 KB   Maximum=512 KB
   Current Type : Burst
 Supported Type : Burst
 ============== Port Connectors ============================================== 
       Internal : COM1            9 Pin Dual Inline            16550A Comp.
       External : COM A           DB-9 pin male

       Internal : COM2            9 Pin Dual Inline            16550A Comp.
       External : COM B           DB25 pin male

       Internal : PRINTER         25 Pin Dual Inline           ECP/EPP
       External : LPT             DB25 pin female

       Internal : KEY             None                         Keyboard
       External : KEYBOARD        Micro-DIN

       Internal : PRIMARY IDE     On Board IDE
       External : IDE-1           None

       Internal : SECONDARY IDE   On Board IDE
       External : IDE-2           None

       Internal : FLOPPY          On Board Floppy
       External : FLOPPY          None

       Internal : PS/2            none                         Mouse
       External :                 Mini-DIN

       Internal : USB             none                         USB
       External :                 Access Bus (USB)

       Internal : IrDA            none                         Other
       External :                 Infrared
 ============== System Slots ================================================= 
           Slot : PCI Slot1       Long     PCI               32 bit   In Use
Characteristics : 5.0 Volt

           Slot : PCI Slot2       Long     PCI               32 bit   In Use
Characteristics : 5.0 Volt

           Slot : PCI Slot3       Long     PCI               32 bit   Available
Characteristics : 5.0 Volt

           Slot : PCI Slot4       Long     PCI               32 bit   Available
Characteristics : 5.0 Volt

           Slot : PCI Slot5       Long     PCI               32 bit   Available
Characteristics : 5.0 Volt \ Shared opening

           Slot : ISA Slot1       Long     ISA               16 bit   Unknown  
Characteristics : 5.0 Volt \ Shared opening

           Slot : ISA Slot2       Long     ISA               16 bit   Unknown  
Characteristics : 5.0 Volt
 ============== Cooling Device================================================ 
    Device type : Fan   Status=OK
 ============== Temperatuur Probe============================================= 
    Description : CPU Internal Temperature
       Location : Processor   Status=OK
    Temperature : Minimum=0.0 øC   Maximum=128.0 øC
                : Resolution=1.0 øC   Tolerance=0.5 øC   Accuracy=Unknown
 ============== OEM Strings ================================================== 
                : OEM String
 ============== System Configuration Options ================================= 
                : System String
 ============== BIOS language ================================================ 
      Available : 1 Language(s)
        Current : ENGLISH
 ============== System Event Log ============================================= 
  Log data Area : Header start=0000h   Data start=0010h   Length=4096
                : Area valid=No    Area full=No    Change token=00000000
    Area access : Memory mapped

 IRQ + DMA
 *****************************************************************************
 IRQ  Address    Owner      IRQ  S  Devices                           PnP
 ===  =========  ========   ===  =  =======                           =======
  8   E127:001F  STACKS       0  e  Timer                             PNP0100
  9   E127:0028  STACKS       1  e  Keyboard                          PNP0303
 10   F000:EF6F  bios         2  e  [Cascade]                         PNP0000
 11   F000:EF6F  bios         3  e  Com2  Com4  Modem                 PNP0501
 12   0481:3E22  MOUSE        4     Com1  Com?  Mouse                 PNP0501
 13   F000:EF6F  bios         5     Lpt2  Sound                       CTL0041
 14   E127:009A (bios)        6  e  Floppy                            PNP0700
 15   0070:0465  dos          7     Lpt1                     PNP0401  PNP0401
 70   E127:0035  STACKS       8  e  Clock                             PNP0B00
 71   F000:ECF3  bios      (2)9  e  PCI: Serial
 72   E127:00B2 (ASPI8DOS)   10  e  SCSI  CD_Rom  PCI: Storage 
 73   F000:EF6F  bios        11     PCI: Display
 74   E127:00E2 (bios)       12     Network
 75   F000:F0FC  bios        13  e  FPU                               PNP0C04
 76   E127:00FA (bios)       14  e  Hard_Disk
 77   F000:EF6F  bios        15  e  ?

                     e = Enabled    ? = Measured

                            DMA     Devices                           PnP
                            ===     =======                           ======= 
                              0
                              1     Sound                             CTL0041
                              2     Floppy                            PNP0700
                              3     Lpt1                     PNP0401  PNP0401
                              4     [Cascade]                         PNP0200
                              5     Sound                             CTL0041
                              6
                              7
