                                 Example 2
                                 ÄÄÄÄÄÄÄÄÄ

     System Analyser     (C) 2009  Hans Niekus     V5.3w     Registered
 *****************************************************************************
             Computer : AT  (ID=FCh / Subm=01h / Vers=0)
    BIOS  date / name : 06/10/96   Award Modular BIOS v4.50G
                      : SIS-85C471B/E/G-2C4I9S23-00   (REV .G2.)
                      : Vendor=Soyo
                      : Award Flash Bios
          DOS version : 7.00  Rev=0  OEM=00h
                      : Virtual 8086 mode
   OEM version string : PC DOS Version 7.0
                      : Revision 0
Adv. Power Management : Version=1.2   (enabled)
   Plug and Play BIOS : Version=1.0
----------------------+--------------------------------------------------------
           DOS config : Files=40   Fcbs=4,0   Buffers=25,0   Stacks=0,0
                      : Dos in HMA   Last Drive=H:   Break=Off   Verify=Off
          Environment : 256 Bytes   Used=112 Bytes
         Country code : 31   Date=DMY   Time=24h
            Code page : Active=850   Default=437
          Sytem start : Warm-reset   Boot-drive=C:   Boot-menu=QEMM
----------------------+--------------------------------------------------------
             CPU type : Intel 80486dx2-sl
                CPUID : Family=04h   Model=03h   Stepping ID=05h
        Feature flags : 0000000 00000011
                      : Internal bus width=32 bit   Que-length=32 Byte
     Math Coprocessor : Integrated
          Clock speed : 66.8 MHz   External Clock probable=33.4 MHz
        Primary Cache : 8 kB   4 Way   Cache-line=16 Byte
                      : Write trough
      Secondary Cache : 256 kB   Direct mapped   Cache-line=16 Byte
                      : Write back   !! No Dirty Tag !!            

    Memory efficiency : Code=12.7-0.0ws   DataR=13.0-0.0ws   DataW=0.0ws
   Prim. / Sec. cache : Code=1.5-0.0ws   DataR=2.0-0.0ws
                      : Code burst=2-1-1-1   Data burst=3-1-1-1
    Prim. cache speed : Code=254.7 MB/s    DataR=65187 kB/s
     Sec. cache speed : Code=101.7 MB/s    DataR=43647 kB/s
         Memory speed : Code=19057 kB/s    DataR=15326 kB/s
    PC-relative speed : CPU=8795%   FPU=11382%   (Cache hit speed)
----------------------+--------------------------------------------------------
   Main memory (DOS)  : 640 kB  (A0000h)   Used=77 kB   Free=562 kB
   Main memory (PSP)  : 640 kB  (9FFF0h)
 Program load address : 137F0h
        Ram above 1MB : CMOS=7168 kB   Dos=0 kB

                 DPMI : version=0.90   OEM=Quarterdeck   (32 bit)

                 VCPI : version=1.0   (Max address=8196 kB)

              LIM-EMS : version=4.0   Page frame=E0000h   (QEMM386)
               Memory : 7472 kB   Used=2912 kB   Free=4560 kB
              Handles : Base=624 kB  HMA=64 kB

 DPMS (dr/tsr in EMB) : DPMS-version=1.0   Novell-version=1.20

           XMS driver : XMS-version=3.00   QEMM386-version=7.50
    (640h..1024h) UMB : 112 kB   Used=86 kB   Free=26544 Bytes
   (1024h..1088h) HMA : 64 kB   Used=52 kB   Free=12 kB   A20=Enabled
         (>1088h) EMB : 6608 kB   Free=4560 kB   (Largest free block=4496 kB)
              Handles :  EMB_0003=2048 kB

          Virtual DMA : VDS-version=1.0   buffer=12 kB   (QEMM386)
----------------------+--------------------------------------------------------
          VESA VBE/DC : Supported (Display Data Channel)
              Monitor : Compaq V70
                      : Year=1996   Week=23   EDID-version=1.1
                      : Horizontal=31 cm   Vertical=23 cm   (Diagonal=15.20")
                      : Vertical=50-150 Hz   Horizontal=30-69 kHz

          VESA VBE/PM : Version=1.0   (State=on)
     Supported states : Standby  Suspend  Off

      Display adapter : VGA in mode 03h
                 Chip : Tseng  ET4000W32P  (version=2)
          Bios / Card : Stealth 32 VLB  Vers. 1.15A  (c) Diamond
                      : Tseng
                  DAC : TrueColor 24 bit
                      : (EGA switches=0110   Feature bits=1111)

         VESA version : 1.20   OEM=Diamond Stealth 32
           VESA modes : 0100, 0101, 0102, 0103, 0104, 0105, 0106, 0107, 0108
                      : 0109, 010C, 22, 24, 2A, 2D, 010D, 5D, 0110, 5F, 0113
                      : 010E, 6D, 0111, 6F, 0114, 0112, 0116, 0117, 0115

   Memory (Vesa info) : 2048 kB   Memory type=DRAM
  Monitor (PS/2 info) : VGA Color display   (Vert=70.0 Hz / Horiz=31.43 kHz)
      Video-speed RAM : 8bit=8257 kB/s   16bit=16688 kB/s   32bit=29829 kB/s
Video-speed BIOS, DOS : 84 KC/s  Scroll=0.44ms,   24729 C/s  Scroll=0.45ms
----------------------+--------------------------------------------------------
           Disk cache : Smartdrive   version=5.10   Size=2048 kB
     Disk compression : Stacker  version=4.02

     Logical drive(s) : 7  named  A: to H:

  Floppy disk control : BIOS=Multirate   Controller=Enhanced   IRQ=6   DMA=2
 Floppy disk drive(s) : 2   0/A:1.44 MB  (80T 2H 18S)
                      :     1/B:1.2 MB   (80T 2H 15S)

 Logical Hard disk(s) : 80a/C:  452 MB  (  237 MB)  Compressed
                      : 81a/D:  519 MB  (  224 MB)  THOSH 1      Fat16  Active
                      : 81b/E:  519 MB  (  123 MB)  THOSH 2      Fat16
                      : 80a/F:  209 MB  (   98 MB)  QUANTUM 1    Fat16  Active
                      : 81b/H:  519 MB  (  123 MB)  SUBST  E:\TALEN\ASM

 Non DOS partition(s) : 80b     502 MB  (OS/2 FAT hid)
                      : 80c    1072 kB  (OS/2 Boot mgr)

        Hard disk 80h : (712MB 707T 32H 63S) E-IDE   Mode=LBA   Type=46
 Partition table info : (713MB 708T 32H 63S)
             ATA info : (714MB 1416T 16H 63S) QUANTUM LIGHTNING 730A
            seek (ms) : T-T=3.2   Average=11.9   Full=19.7   Overhead=0.6
         speed (kB/s) : Max=1661   64kB=1658   4kB=1287   512b=472
             Rotation : 4496 rpm   Average-latency=6.7ms
             ATA info : Buffer=96kB   Sn=32742935               Rev=A24.1C00
                      : LBA=yes  LBA48bit=no  DMA=yes  IORDY=yes (sw)
                      : DwordIO=no  PIOmode=3  DMAmode=2  Multi-sector=8 sec
           Controller : IRQ=14   Port=1F0h   Master
 > 516.096 kB support : LBA (INT 13 extension V2.0)

        Hard disk 81h : (1038MB 1014T 64H 32S) SCSI  TOSHIBA MK537FB
            seek (ms) : T-T=5.6   Average=17.5   Full=30.1   Overhead=3.8
         speed (kB/s) : Max=2699   64kB=2354   4kB=827   512b=135
             Rotation : +/-3607 rpm   Average-latency=8.3ms
           Controller : IRQ=11   DMA=5

    Hard disk found ? : port=01F0h   Slave   Address=82h
                      : (4209MB 524T 255H 63S Novell NetWr) Part. table info
           ATA info   : (4209MB 14848T 9H 63S) QUANTUM FIREBALL ST4.3A        
                      : Buffer=81kB   Sn=154709841715           Rev=A0F.0400
                      : LBA=yes  LBA48bit=no  DMA=yes  IORDY=yes (sw)
                      : DwordIO=no  PIOmode=4  DMAmode=2  MultiSec=16 sectors
                      : ATA 3  MultiW-DMA=2 (used=no)  Ultra-DMA=2 (used=2)
----------------------+--------------------------------------------------------
               MSCDEX : version=2.25

               CD-ROM : G:3929  MB
               Driver : MTMIDE01   Device=CD-ROM
                 Type : ATAPI (IDE)
                 Read : CD-R, CD-RW, DVD-ROM, DVD-R
                Write : None
             RPC info : Region=1
                      : Type Code=Set   Scheme=RPC Phase II
                      : Vendor resets left=4   User changes left=3
           ATAPI Info : Name=TOSHIBA DVD-ROM SD-M1402
                      : Buffer=128kB   Sn=6000504622             Rev=1010
                      : LBA=yes  DMA=yes  IORDY=yes (sw)
                      : DwordIO=no  PIOmode=4  DMAmode=2  MultiSec=no
                      : MultiW-DMA=2 (used=no)  Ultra-DMA=2 (used=2)
       Capabilities 1 : 00001F96  ->  Raw_mode   Audio+Video   Prefetching   
                      : Audio_manip.   Red-book   Sub_channel   
       Capabilities 2 : 1F0075772923  ->  Digtal output   XA   
                      : Mode 2 Form 2   Multi-session   CD DA stream   ISRC   
                      : UPC   
Supported raw CDspeed : Maximum=7056 kB/s (x40)   Current=7056 kB/s (x40)
   Measured DVD speed : Inner=2795 kB/s  (x2)   -   Outer=4624 kB/s  (x3.5)
                      : Average access=99ms
           Controller : port=0170h   Master
----------------------+--------------------------------------------------------
       Parallel ports : 1) Lpt1=0378h  IRQ=7    Bi-directional  (off)
                      : 2) Lpt2=0278h  IRQ=5    ECP   DMA=3   Fifo=16 Byte
         Serial ports : 1) Com1=03F8h  IRQ=4    Chip=8250A/16450   1200,N,7,1
                      : 2) Com2=02F8h  IRQ=3    Chip=8250A/16450   2400,N,8,1
                      : 3) Com4=02E8h  IRQ=3    Chip=16550A        2400,N,8,1
                      :    Com?=03E0h  IRQ=10   Chip=16550         9600,E,7,1
         Serial mouse : 2 buttons  Com1  IRQ=4  Dr-Vers=08.20  (.COM)      
                      : LOGITECH MOUSE DRIVER V6.44
                      : ID=MZ@   PnP-ID=MSH0001   Vers=1.00
                      : Serial#=00040200   Class=MOUSE   DeviceID=PNP0F0A
                      : UserName=MICROSOFT INTELLIMOUSE - SERIAL VERSION
            Game port : 1 Joystick(s)
             Keyboard : BIOS=101/102 key   Keyboard=AT-MF2   Intercept=yes
                      : 8042 Controller: yes   Intercept: yes   INT16/9: no
  Keyboard controller : (C)1990 AMERICAN MEGATRENDS INC
----------------------+--------------------------------------------------------
 Parallel port device : Lpt1  IRQ=7    Printer
                  MFG : HEWLETT-PACKARD
                  MDL : DESKJET 660C
                  CMD : MLC,PCL,PML
                CLASS : PRINTER
          DESCRIPTION : Hewlett-Packard DeskJet 660C
              VSTATUS : $CB0$RC0,ff,DN,IDLE
----------------------+--------------------------------------------------------
                Modem : Com4   IRQ=3
                Class : 0 1 2 80   (Fax-Voice-modem)   Current class=0
        Maximum speed : 33600 bps
      Supported modes : V.21, V.22, V.22bis, V.23, V.32, V.32bis, V.34,
                      : BELL 103, BELL 212                            
  Fax/modem Manufact. : ROCKWELL
      Fax/modem Model : AC/V34
    Fax/modem version : V1.510-V34_DP
           Model info : FM-288PC   V1.51 08/02/96
----------------------+--------------------------------------------------------
                Adlib : port=0338h
        Sound Blaster : port=0220h   DSP-version=4.16   IRQ=7   DMA=1,6
        DSP Copyright : COPYRIGHT (C) CREATIVE TECHNOLOGY LTD, 1992.
Wavetablechip EMU8000 : port=0620h   Memory=512 kb
                 Type : Sound Blaster AWE 32 (or compatible)
                Mixer : CT1745 (or compatible)
 Environment BLASTER= : SB=220h  IRQ=7  DMA8=1  DMA16=5  MIDI=330h  Type=6
                      : Wave=620h
                      : Type=6  ->  Sound Blaster 16
                 MIDI : port=0330h
    Environment MIDI= : SYNTH=Intern  MAP=Extended  MODE=Standard
----------------------+--------------------------------------------------------
         SCSI adapter : Adaptec AHA-1540CF/AHA-1542CF   Revision=C.0
                      : Host-ID=7   Port=0330h   DMA=5   IRQ=11

               Driver : ASPI   Name=DOS SCSIMGR 3.3   Adapter=ADAPTEC AHA-1x4x

            Device(s) : 0) Disk drive
                      :    TOSHIBA  MK537FB           R=6261
                      :    SCSI-2   Synchronous
                      :    Capacity=1038 MB     Bytes/sect=512   Address=81h

                      : 2) Tape drive         
                      :    EXABYTE  EXB-4200c         R=149 
                      :    SCSI-2   Synchronous   Linking

                      : 7) Host adapter   (IRQ=11  DMA=5)
----------------------+--------------------------------------------------------
             Bus type : ISA
  CMOS clock / memory : yes / 128 Bytes
Equipment list INT 11 : (LLxxRRRx FFVVxxCF)  10000110 01100011
Sys. config. INT15/C0 : FCh  01h  00h  dICKWbmx  00h  00h  00h  00h
----------------------+--------------------------------------------------------
  Main RAM on address : 00000 -  A0000  640 kB (32 bit  12.8-0.0)
   UMB RAM on address : B0000 -  B8000   32 kB (32 bit  12.7-0.0)
 Video RAM on address : B8000 -  C0000   32 kB (32 bit  24.5)                 

 32 kB BIOS extension : Copyright(c)1988 Tseng Laboratories, Inc. 10/05/93 V8.0
       ROM on address : C0000 -  C8000   32 kB (32 bit  12.8-0.0)             

 16 kB BIOS extension : (c) 1993 Adaptec, Inc. All Rights Reserved.
       ROM on address : C8000 -  CAC00   11 kB ( 8 bit  58.1-58.4)
       ROM on address : CBC00 -  CC000    1 kB ( 8 bit  58.4-58.1)

   UMB RAM on address : CC000 -  E0000   80 kB (32 bit  12.8-0.0)
   EMS RAM on address : E0000 -  EC000   48 kB (32 bit  12.8-0.0)

       ROM on address : EC000 -  F0000   16 kB (32 bit  4.1-4.0)              
       ROM on address : F0000 -  FC000   48 kB (32 bit  4.0-4.0)              
       ROM on address : FC000 - 100000   16 kB (32 bit  4.1-4.0)  EC000-F0000
----------------------+--------------------------------------------------------
  Ext. RAM on address : 00100000 - 00800000    7168 kB

 Device drivers
 *****************************************************************************
  Address    Attr  T  Device    Addr    Name      Size
  =========  ====  =  ========  ======  ========  ============
  B010:0048  8004  C  NUL       B00F:0  DOSDATA     5136 Bytes
  D8B2:1FDE  4842  B  1         D8A1:0  SMARTDRV   29824 Bytes
  D8B2:1FF0  48C2  B  5         D8A1:0  SMARTDRV   29824 Bytes
  D0AE:0000  C000  C  SCSIMGR$  D0AD:0  ASPI4DOS    8096 Bytes
  CCB4:0000  8000  C  _STAC_HI  CCB3:0  STACHIGH   16272 Bytes
  0235:0000  C800  C  MTMIDE01  0234:0  MTMCDAI    38256 Bytes
  01C4:0000  8000  C  DPMSXXX0  01C3:0  DPMS        1792 Bytes
  0140:0000  8000  C  QDPMI$$$  013F:0  QDPMI       2096 Bytes
  010F:0000  C000  C  QEMM386$  010E:0  QEMM386      768 Bytes
  CC01:0000  C000  C  EMMXXXX0  CC00:0  QEMM386     2816 Bytes
  0103:0000  4842  B  1         0102:0               160 Bytes
  0070:0023  8013  C  CON
  0070:0035  8000  C  AUX
  0070:0047  A0C0  C  PRN
  0070:0059  8008  C  CLOCK$
  0070:006B  48C2  B  5
  0070:007B  8000  C  COM1
  0070:008D  A0C0  C  LPT1
  0070:009F  A0C0  C  LPT2
  0070:00B8  A0C0  C  LPT3
  0070:00CA  8000  C  COM2
  0070:00DC  8000  C  COM3
  0070:00EE  8000  C  COM4

 Environment
 *****************************************************************************
 CONFIG  = UMBDRV
 COMSPEC = C:\DOS\COMMAND.COM
 PROMPT  = $p$g
 PATH    = C:\QEMM;C:\DOS;C:\;C:\STACKER;C:\AUTO;
 BLASTER = A220 I7 D1 H6 P330 T6 E620
 MIDI    = SYNTH:1 MAP:E MODE:0                                             
 TEMP    = C:\TEMP

 E:\TALEN\ASM\SA51.COM

 Memory Control Blocks
 *****************************************************************************
  Address          T  Own   Name      Size          Type
  ===============  =  ====  ========  ============  ==========
  010D:0 - 0C19:0  M  0008  SD         45232 Bytes  Device(s):

  010E:0 - 013F:0  D  010F  QEMM386      768 Bytes  QEMM386$
  013F:0 - 01C3:0  D  0140  QDPMI       2096 Bytes  QDPMI$$$
  01C3:0 - 0234:0  D  01C4  DPMS        1792 Bytes  DPMSXXX0
  0234:0 - 0B8C:0  D  0235  MTMCDAI    38256 Bytes  MTMIDE01

  0B8C:0 - 0C0F:0  F  0B8D              2080 Bytes  FILES=40
  0C0F:0 - 0C19:0  T  0C10               144 Bytes  INSTALL

  0C19:0 - 0C1A:0  M  0008  SC            00 Bytes  
  0C1A:0 - 0C1F:0  M  0008  SC            64 Bytes  
  0C1F:0 - 0C26:0  M  0C20  LOADHI        96 Bytes  Program
  0C26:0 - 0C37:0  M  D2BA  COMMAND      256 Bytes  Environment
  0C37:0 - 0C3C:0  M  0C3D  NDE           64 Bytes  Environment
  0C3C:0 - 0D0E:0  M  0C3D  NDE         3344 Bytes  Program
  0D0E:0 - 0D13:0  M  0000  -free-        64 Bytes  
  0D13:0 - 1373:0  M  0D14  MOUSE      26096 Bytes  Program
  1373:0 - 137E:0  M  137F  SA50         160 Bytes  Environment
  137E:0 - 9FFF:0  Z  137F  SA50      575488 Bytes  Program
------------------------------------------------------------- UMBs NOT linked -
  9FFF:0 - B001:0  M  0008  SC         65552 Bytes  Not used

  B000:0 - B7FF:0  M  B001  UMB        32736 Bytes  UMB Program(s):

  B001:0 - B00F:0  M  B002  DOS-UP       208 Bytes  Program
  B00F:0 - B151:0  M  B010  DOSDATA     5136 Bytes  Program
  B151:0 - B172:0  M  B152  WKBUFFER     512 Bytes  Program
  B172:0 - B19F:0  M  B173  LASTDRIV     704 Bytes  Program
  B19F:0 - B7FE:0  M  0000  -free-     26080 Bytes  
  B7FE:0 - CCB2:0  M  0008  SC         84784 Bytes  Not used

  B7FF:0 - CC00:0  M  010F             81920 Bytes  Not used
  CC00:0 - CCB1:0  M  CC01  QEMM386     2816 Bytes  UMB Control block
  CCB1:0 - E000:0  Z  CCB2  UMB        79072 Bytes  UMB Program(s):

  CCB2:0 - D2A8:0  M  0008  SD         24400 Bytes  Device(s):

  CCB3:0 - D0AD:0  D  CCB4  STACHIGH   16272 Bytes  _STAC_HI
  D0AD:0 - D2A8:0  D  D0AE  ASPI4DOS    8096 Bytes  SCSIMGR$

  D2A8:0 - D2B9:0  M  D2A9  FCBS         256 Bytes  Program
  D2B9:0 - D34E:0  M  D2BA  COMMAND     2368 Bytes  Program
  D34E:0 - D353:0  M  0000  -free-        64 Bytes  
  D353:0 - D358:0  M  0000  -free-        64 Bytes  
  D358:0 - D8A1:0  M  D359  MSCDEX     21632 Bytes  Program
  D8A1:0 - DFEA:0  M  D8A2  SMARTDRV   29824 Bytes  Program
  DFEA:0 - E000:0  Z  0000  -free-       336 Bytes  
------------------------------------------------------------------------- HMA -
  FFFF:0030           FFFF             53072 Bytes
  FFFF:CF90           0C30              9760 Bytes
  FFFF:F5C0           FFFB               736 Bytes
  FFFF:F8B0           0000  -free-      1856 Bytes

 CMOS memory
 *****************************************************************************
    1999-2000 rollover : Cmos=01-01-1900   Bios=01-01-1900   Bad
 Set century byte Cmos : Cmos=01-01-2000   Bios=01-01-2000   Ok
   Set 01-01-2000 Bios : Cmos=01-01-2000   Bios=01-01-2000   Ok
        Leap year 2000 : Cmos=29-02-2000   Bios=29-02-2000   Ok
            Conclusion : Set the date once after 2000
                         Check if it still Ok when it has been switched off

       DOS Time  : 19:50:20                    DOS Date : 01/01/2003 Wednesday

(04 02 00) Time  : 19:51:32       (07 08 32 09 06) Date : 01/01/2003 Monday
(05 03 01) Alarm : 00:00:00

(10) (0100 ....)  Type of diskette drive 0  : 1.44MB
     (.... 0010)  Type of diskette drive 1  : 1.2MB

(14) (01.. ....)  Number of diskette drives : 2
     (..00 ....)  Primary display           : EGA / VGA
     (.... 00..)  Reserved
     (.... ..1.)  Coprocessor               : Yes
     (.... ...1)  Diskette drive installed  : Yes

(16 15) Main memory      : 640 kB          (12) (x.) fixed disk type 0 : 15
(18 17) Expansion memory : 7168 kB              (.x) fixed disk type 1 : 0
(31 30) Actual Exp. mem. : 7168 kB         (19)      fixed disk type 0 : 47 <-
                                           (1A)      fixed disk type 1 : 0
(0A) Status A : 0010 0110  (0010 0110) ok
(0B) Status B : 0000 0010  (0000 0010) ok
(0C) Status C : 0101 0000  (010x 0000) ok
(0D) Status D : 1000 0000  Power ok        (0F) Shutdown Status  : 0000 0000
(0E) POST     : 0000 0000                  (33) Information flag : 1110 1111

(2E 2F) Checksum 10h-2Dh : 04A3h ok

Hard disk user types :
(26-2D) 0 : Cyl=  1416   Head= 16   Precomp= 65535   Landz=  1417   Sector= 63
(1E-25) 1 : Cyl=     0   Head=  0   Precomp=     0   Landz=     0   Sector=  0
(68-6F) 2 : Cyl=  1654   Head=  0   Precomp= 65535   Landz=  1655   Sector= 63
(71-78) 3 : Cyl=     0   Head=  0   Precomp=     0   Landz=     0   Sector=  0

      Bytes from the CMOS RAM
      =======================
      00  01  02  03  04  05  06  07  08  09  0A  0B  0C  0D  0E  0F
      --  --  --  --  --  --  --  --  --  --  --  --  --  --  --  --
 00 | 32  00  51  00  19  00  02  01  01  03  26  02  50  80  00  00
 10 | 42  00  F0  00  43  80  02  00  1C  2F  00  00  1C  44  00  9C
 20 | E8  3B  00  40  00  00  00  00  00  00  00  00  00  00  04  A3
 30 | 00  1C  20  EF  AE  A9  AB  EA  80  02  AA  A3  2A  AB  AA  81
 40 | 40  2F  08  00  00  9B  BF  DC  00  00  05  25  56  3F  00  B0
 50 | 50  04  04  60  00  00  C4  90  01  00  00  00  00  00  00  20
 60 | 00  00  00  00  00  00  00  00  FF  07  00  FF  07  00  00  20
 70 | 13  10  01  99  C4  3B  AA  BB  A3  14  45  F0  51  00  60  40

 PCI   +   PCMCIA   +   Plug & Play
 *****************************************************************************
 No PCI
-------------------------------------------------------------------------------
 No PCMCIA
-------------------------------------------------------------------------------
 Plug and Play BIOS : version=1.0
          ACFG BIOS : version=2.10
                 CM : Not present
               ESCD : Size=4096 bytes   Address=FFFFD000h
                DMI : Size=4096 bytes   Address=FFFFC000h

 Number of ISA/EISA PnP card(s) = 1   (Read Port=0227h)

 PnP Card(s):
 ============
  1: CTL009C : Creative SB32 PnP
     CTL0041 : Audio                                                  Enabled
         IRQ : 5
         DMA : 1, 6
        Port : 0220, 0330, 0388
     CTL7002 : Game                                                   Enabled
        Port : 0200
     CTL0021 : WaveTable                                              Enabled
        Port : 0620, 0A20, 0E20
     CTL2011 : IDE                                                    Disabled

 Nodes: (PnP BIOS)
 ======
  0: PNP0400 : Standard LPT printer port
       Class : 07h/01h/01h   Paralell Port (Bi-dirirectional)
         IRQ : 7
        Port : 0378-037Bh

  1: PNP0500 : Standard PC COM port
       Class : 07h/00h/02h   RS-232 device (16550 compatible)
         IRQ : 4
        Port : 03F8-03FFh

  2: PNP0500 : Standard PC COM port
       Class : 07h/00h/02h   RS-232 device (16550 compatible)
         IRQ : 3
        Port : 02F8-02FFh

  3: PNP0700 : PC standard floppy disk controller
       Class : 01h/02h/00h   Floppy disk controller
         IRQ : 6
        Port : 03F2-03F5h, 3F7h
         DMA : 2

  4: PNP0C01 : System Board
       Class : 05h/00h/00h   RAM controller
         Mem : 000E8000-000FFFFFh  ROM  8/16bit  Cacheable  Shadowable

  5: PNP0000 : AT Interrupt Controller
       Class : 08h/00h/01h   ISA Programable Interrupt Controller
         IRQ : 2
        Port : 0020-0021h, 00A0-00A1h

  6: PNP0100 : AT Timer
       Class : 08h/02h/01h   ISA System Timer
         IRQ : 0
        Port : 0040-0043h

  7: PNP0B00 : AT Real Time Clock
       Class : 08h/03h/01h   ISA Real Time Clock
         IRQ : 8
        Port : 0070-0071h

  8: PNP0303 : IBM Enhanced (101/102-key  PS/2 mouse support)
       Class : 09h/00h/00h   Keyboard controller
         IRQ : 1
        Port : 0060h, 0064h

  9: PNP0C04 : Math Coprocessor
       Class : 0Bh/01h/00h   486-based processor
         IRQ : 13
        Port : 00F0h

 10: PNP0200 : AT DMA Controller
       Class : 08h/01h/01h   ISA DMA controller
         DMA : 4  (Master)
        Port : 0000-000Fh, 0080-0090h, 0094-009Fh, 00C0-00DEh

 11: PNP0800 : AT style speaker sound
       Class : 08h/80h/00h   Other System Peripheral
        Port : 0061h

 APM Devices:                                                                  
 ===========                                                                   
     PNP0C01 : DeviceID = 0101h                                                
 
 IRQ + DMA
 *****************************************************************************
 IRQ  Address    Owner      IRQ  S  Devices                           PnP
 ===  =========  ========   ===  =  =======                           =======
  8   D8B2:173E  SMARTDRV     0  e  Timer                             PNP0100
  9   D8B2:17E7  SMARTDRV     1  e  Keyboard                          PNP0303
 10   F000:FF7C  bios         2  e  [Cascade]                         PNP0000
 11   F000:FF7C  bios         3     Com2  Com4  Modem                 PNP0500
 12   0D24:3B37  MOUSE        4  e  Com1  Mouse                       PNP0500
 13   F000:FF7C  bios         5     Lpt1  Sound               CTL0031 PNP0400
 14   F000:603E  bios         6  e  Floppy                            PNP0700
 15   0070:05B0  dos          7     Lpt2
 70   F000:6C28  bios         8  e  Clock                             PNP0B00
 71   F000:F589  bios      (2)9  e  Video
 72   F000:FF7C  bios        10     Com?
 73   D0AE:09DB  ASPI4DOS    11  e  Hard_Disk  SCSI
 74   F000:EEC5  bios        12  e                                    CTL2011
 75   F000:F592  bios        13  e  FPU                               PNP0C04
 76   F000:6664  bios        14  e  Hard_Disk 
 77   0B8C:012F  MTMCDAI     15  e  CD_ROM

                     e = Enabled    ? = Measured

                            DMA     Devices                           PnP
                            ===     =======                           =======
                              0     
                              1     Sound                             CTL0031
                              2     Floppy                            PNP0700
                              3     Lpt2
                              4     [Cascade]                         PNP0200
                              5     Hard_Disk  SCSI
                              6     Sound                             CTL0031
                              7
 Remark
 *****************************************************************************
