# Library test apps

On a PI-hosted dev system, test the SPI driver:

	~/2065-Z80-programmer/pi/flash < spi_test.bin

To test the SD driver:

	~/2065-Z80-programmer/pi/flash < sd_test.bin

A suitable executable program to use with sd_test.asm can be found in: [../hello](../hello).
