
# 2063-Z80.sch

## Tue Mar 28 20:43:38 2023

## Eeschema 5.1.5+dfsg1-2build2

## Component Count:86

Ref | Qty | Value | Digikey | Datasheet | Description
----|-----|-------|---------|-----------|------------
C1, C11, C12, C20 | 4 | .47 | 399-14039-1-ND | https://api.kemet.com/component-edge/download/datasheet/C315C474K5R5TA7303.pdf | Unpolarized capacitor, small symbol
C2, C3, C4, C5, C6, C7, C8, C9, C10, C13, C14, C15, C16, C21, C22, C23 | 16 | .1 | 399-9859-1-ND | https://api.kemet.com/component-edge/download/specsheet/C315C104M5U5TA7303.pdf | Unpolarized capacitor, small symbol
C17 | 1 | .1 | 1276-1935-1-ND | https://www.mouser.com/datasheet/2/585/MLCC-1837944.pdf | Unpolarized capacitor, small symbol
C18 | 1 | 10uF | 1276-1298-1-ND | https://media.digikey.com/pdf/Data%20Sheets/Samsung%20PDFs/CL21A106MQFNNNE_Spec.pdf | Polarized capacitor, small US symbol
C19 | 1 | 10uF | P975-ND | https://industrial.panasonic.com/cdbs/www-data/pdf/RDF0000/ABA0000C1059.pdf | Polarized capacitor, small US symbol
C24 | 1 | .1 | 1276-1935-1-ND | https://www.mouser.com/datasheet/2/585/MLCC-1837944.pdf | Unpolarized capacitor, small symbol
D1, D2 | 2 | LED_ALT | 1080-1122-ND | https://media.digikey.com/PDF/Data%20Sheets/Everlight%20PDFs/ds300034.pdf | Light emitting diode, filled shape
D3 | 1 | 1N914 | 1N4148FSCT-ND | http://www.vishay.com/docs/85622/1n914.pdf | 100V 0.3A Small Signal Fast Switching Diode, DO-35
H1, H2, H3, H4 | 4 | MountingHole |  |  | Mounting Hole without connection
J1, J8 | 2 | Conn_01x05 | S1011EC-05-ND | https://media.digikey.com/PDF/Data%20Sheets/Sullins%20PDFs/xRxCzzzSxxN-RC_ST_11635-B.pdf | Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)
J2 | 1 | DM3D-SF(41) | H126097CT-ND (alternate: 114-00841-68-1-ND) | https://www.hirose.com/product/document?clcode=CL0609-0033-6-00&productname=DM3AT-SF-PEJ2M5&series=DM3&documenttype=Catalog&lang=en&documentid=D49662_en | Micro SD Card Socket with card detection pins
J3 | 1 | Conn_02x20 | S2011EC-20-ND | https://drawings-pdf.s3.amazonaws.com/11636.pdf | Generic connector, double row, 02x20, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)
J4, J5 | 2 | Conn_02x05 | 1849-1002-ND |  | Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)
J6 | 1 | 0548190519 | A135698-ND | https://www.molex.com/pdm_docs/sd/548190519_sd.pdf | CONN RCPT USB2.0 MINI B 5P R/A
J7 | 1 | Conn_02x13 | S2011EC-13-ND | https://drawings-pdf.s3.amazonaws.com/11636.pdf | Generic connector, double row, 02x13, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)
J9, J12 | 2 | Conn_01x02 | S1011EC-02-ND | https://media.digikey.com/PDF/Data%20Sheets/Sullins%20PDFs/xRxCzzzSxxN-RC_ST_11635-B.pdf | Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)
J10 | 1 | Conn_01x07 | S1011EC-07-ND | https://media.digikey.com/PDF/Data%20Sheets/Sullins%20PDFs/xRxCzzzSxxN-RC_ST_11635-B.pdf | Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)
J11 | 1 | Conn_02x03 | 2057-PH2-06-UA-ND | https://app.adam-tech.com/products/download/data_sheet/202065/ph2-xx-ua-data-sheet.pdf | Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)
LOGO1 | 1 | OSHW_Logo |  |  | Open Hardware logo, small
LOGO2 | 1 | OSHW_Logo |  |  | Open Hardware logo, small
NT1, NT2 | 2 | Net-Tie_2 |  | ~ | Net tie, 2 pins
Q1 | 1 | PN2222 | 1514-PN2222APBFREE-ND | https://my.centralsemi.com/datasheets/PN2221-2222A.PDF | NPN transistor, emitter/base/collector
R1, R3, R5 | 3 | 2K7 | CF18JT2K70CT-ND | https://www.seielect.com/catalog/sei-cf_cfm.pdf | Resistor
R2, R4, R6 | 3 | 4K7 | CF18JT4K70CT-ND | https://www.seielect.com/catalog/sei-cf_cfm.pdf | Resistor
R7, R10, R13, R14 | 4 | 10K | CF18JT10K0CT-ND | https://www.seielect.com/catalog/sei-cf_cfm.pdf | Resistor
R8, R9 | 2 | 680 | CF18JT680RCT-ND‎ | https://www.seielect.com/catalog/sei-cf_cfm.pdf | Resistor
R11, R12 | 2 | 1K | CF18JT1K00CT-ND‎ | https://www.seielect.com/catalog/sei-cf_cfm.pdf | Resistor
R15, R16 | 2 | 120 | CF18JT120RCT-ND | https://www.seielect.com/catalog/sei-cf_cfm.pdf | Resistor
RN1, RN2, RN3, RN4, RN5 | 5 | 10K | 4609X-101-103LF-ND‎ | https://www.bourns.com/docs/Product-Datasheets/4600x.pdf | 8 resistor network, star topology, bussed resistors, small symbol
S1 | 1 | 1825910-6 | 450-1650-ND | https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1825910&DocType=Customer+Drawing&DocLang=English | SWITCH TACTILE SPST-NO 0.05A 24V
U1 | 1 | Z80-CPU | 269-3898-ND | https://www.zilog.com/manage_directlink.php?filepath=docs/z80/um0080 | 8-bit General Purpose Microprocessor, DIP-40
U2 | 1 | AS6C4008-55PCN | 1450-1178-5-ND‎ | https://www.alliancememory.com/wp-content/uploads/pdf/AS6C4008.pdf | 512K x 8 Low Power CMOS RAM, DIP-32
U3 | 1 | SST39SF010 | SST39SF010A-70-4C-PHE-ND‎ | https://ww1.microchip.com/downloads/en/DeviceDoc/20005022C.pdf | Silicon Storage Technology (SSF) 128k x 8 Flash ROM
U4 | 1 | Z80-CTC | 269-3914-ND | http://www.zilog.com/docs/z80/ps0181.pdf | Z80 CTC DIP-28
U5 | 1 | Z80-SIO-0 | 269-5062-ND‎ | http://www.zilog.com/docs/z80/ps0183.pdf | SCC Serial Communication Controller, DIP-40
U6, U7 | 2 | 74HC374 | 296-12806-5-ND | https://www.ti.com/lit/ds/symlink/cd74hct374.pdf | 8-bit Register, 3-state outputs
U8 | 1 | 74LS244 | 296-36148-5-ND | https://www.ti.com/lit/ds/symlink/sn74ls241.pdf | 8-bit Bus Buffer 3-State outputs
U9 | 1 | 74HC138 | 296-SN74HC138AN-ND | https://www.ti.com/lit/ds/symlink/sn54hc138.pdf | Decoder 3 to 8 active low outputs
U10, U13 | 2 | 74HC32 | 296-12803-5-ND | https://www.ti.com/lit/ds/symlink/cd74hc32.pdf | Quad 2-input OR
U11 | 1 | 74HCT132 | 296-2090-5-ND | https://www.ti.com/lit/ds/symlink/cd74hc132.pdf | Quad 2-input NAND Schmitt trigger
U12 | 1 | ICL3232CPZ | ICL3232CPZ-ND‎ | https://www.renesas.com/us/en/document/dst/icl3221-icl3222-icl3223-icl3232-icl3241-icl3243-datasheet | 3.0V to 5.5V, Low-Power, up to 1Mbps, True RS-232 Transceivers Using Four 0.1μF External Capacitors
U20 | 1 | LM1117-3.3 | NCP1117ST33T3GOSCT-ND | https://www.onsemi.com/pdf/datasheet/ncp1117-d.pdf | 800mA Low-Dropout Linear Regulator, 1.8V fixed output, TO-220/TO-252/TO-263/SOT-223
X1 | 1 | ACH-10.000MHZ-EK | 535-9167-5-ND | https://abracon.com/Oscillators/ACH.pdf | Crystal Clock Oscillator, DIP8-style metal package
X2 | 1 | ECS-2100A-018 | XC231-ND‎ | https://ecsxtal.com/store/pdf/ecs_2100.pdf | Crystal Clock Oscillator, DIP8-style metal package

    
