
	SUBTTL	Accumuator Definitions

FLGS=0					;flag word for bit testing

P=1					;PDL pointer
MBP=2					;PDL pointer for display buffer being filled

IDX1=3					;index of objects currently being processed
IDX2=4

A=5					;temporaries -- other names defined below
B=6
C=7
D=10
T1=11
T2=12
T3=13
T4=14
T5=15

DCP=16					;display chain pointer (wired)
DLP=17					;BLKO pointer of list being output (wired)


; Other names used for the AC's

TYP1==C					;types of objects in IDX1 and IDX2
TYP2==D

X==T1					;X/Y coordinates built by DISPNT macro
Y==T2
PTCMND==T4				;point command placed here by DISPNT

SDLP==T3				;PDL pointer for building sun display

.XCREF FLGS,P,MBP,IDX1,IDX2,A,B,C,D,T1,T2,T3,T4,T5,DCP,DLP
.XREF X,Y,PTCMND,SDLP


; Accumulator names used in older code (CREF'ed to find and eliminate)

F==FLGS
T==T1
TT==T2
MP1==IDX1
MP2==IDX2
R==T3
XFLAG==T4
S==T5
