	SUBTTL	340 Display Definitions

;Command Operation Codes

;----- Valid in Any Mode
GTOPRM==BIT2.9				;this command is guarenteed to place the display
					;into parameter mode regardless of the current mode

;----- Valid in Parameter and Point Commands
PARM==  0				;next command is parameter mode
POINT== BIT2.5				; "      "    "  point      "
VECT==  BIT2.7				; "      "    "  vector     "
VECTC== BIT2.7+BIT2.5			; "      "    "  vector-continue mode
CHAR==  BIT2.6+BIT2.5			; "      "    "  character mode
INCR==  BIT2.7+BIT2.6			; "      "    "  increment  "

;----- Valid in Vector, Vector-Continue, and Increment Modes
ESCAPE==BIT2.9				;return display to parameter mode


;Specific Bits/Values for Different Command Types

;----- Parameter Mode
DISHLT==<GTOPRM,,BIT2.2+BIT2.1>		;stop this display list

;----- Point Mode
DISPNT==BIT2.2				;intensify the current point

;----- Vector and Vector-Continue Modes
DISVCT==BIT2.8				;make this vector visible
NEGX==  BIT1.8				;if on, X shift is negative
NEGY==  BIT2.7				;if on, Y shift is negative

;----- Character Mode (Any Case)
CHRESC==37				;escape from character mode
CHRUC== 35				;shift to upper-case
CHRLC== 36				; "    "  lower-case
CHRLF== 33				;line-feed
CHRCR== 34				;carriage-return
CHRSP== 40				;space

;Macros to Generate Display Commands

;SCALE(VALUE)
;   Function:
;	Generates a parameter mode command to set the display scaling factor.
;   Inputs:
;	VALUE:	The scaling factor as a value from 0 to 3.

DEFINE SCALE (VALUE
<BIT1.7+<VALUE&3>_4>TERMIN


;INTSTY(VALUE)
;   Function:
;	Generates a parameter mode display command to set the display intesity.
;   Inputs:
;	VALUE:	The intensity as a value from 0 through 7.

DEFINE INTSTY (VALUE
<BIT1.4+<VALUE&7>>TERMIN


;SETY(VALUE)
;   Function:
;	Generates a point mode command to set the Y ordinate.
;   Inputs:
;	VALUE:	The Y ordinate as a value from 0 through 1777(8).

DEFINE SETY (VALUE
<BIT2.8+<VALUE&1777'>>TERMIN


;SETX(VALUE)
;   Function:
;	Generates a point mode command to set the X ordinate.
;   Inputs:
;	VALUE:	The X ordinate as a value from 0 through 1777(8).

DEFINE SETX (VALUE
<VALUE&1777'>TERMIN


;VECTOR(XVALUE,YVALUE)
;   Function:
;	Generates a vector or vector-continue command to create a vector.
;   Inputs:
;	XVALUE:	The magnitude (positive) of the X shift.  It is in the range 0
;		through 177(8).
;	YVALUE:	The magnitude of the Y shift.  It is treated identically to XVALUE.

DEFINE VECTOR (XVALUE,YVALUE
<<XVALUE&177'>+<<YVALUE&177'>_8.>>TERMIN

