# cpct_mode_rom_status

> _cpct_mode_rom_status:: .db #0x9D

8-bit space for storing the latest selection of MODE, INT.GENERATOR and ROM status. This lets us know if Lower / Upper ROM are enabled or disabled, if interrupts are enabled or not, and which Video Mode is actually set.

#### Description of the bits

>     [ GGGIRRnn ]

GGG | Command for video mode and ROM selection (100)
I | Interrupt Generation Enabled (1)
RR | Reading from Lower and Upper ROM Disabled (11) (a 0 value means ROM enabled)
nn | Video Mode 1 (01)

Default value: 0x9C = (10011100)

Close