# Firmware&ROM constants

Summary

Firmware&ROM constants |
Constants |
Firmware useful constants | Constants used by firmware routines.

### Constants

### Firmware useful constants

Constants used by firmware routines.

firmware_RST_jp | Memory address that stores a pointer to the start of firmware code, executed on every interruption.
GA_port_byte | Output port where Gate Array (GA) listens.

Close