; This program simply reads which button is pressed on the keyboard,
; and shows the appropriate number in the LEDs

LOOP:
	CALL KIND ; Hangs until a button is pressed
	
	CMA
	
	OUT 30H ; Output it to LEDS
	
	JMP LOOP ; Loop forever