$Id$

Starting from Bochs 2.3 the parameters are organized in a tree structure
instead of a huge flat list. The parameter tree was required for implementing
the save/restore feature, and it gives access to the device state from within
the debugger.
-Volker

Current organization of parameters in the tree

general
  config_interface
  start_mode
  benchmark
  dumpstats
  restore
  restore_path
  debug_running

cpu
  n_processors
  n_cores
  n_threads
  model
  ips
  quantum
  reset_on_triple_fault
  msrs
  cpuid_limit_winnt
  mwait_is_nop

cpuid
  level
  family
  model
  stepping
  vendor_string
  brand_string
  mmx
  sep
  simd
  sse4a
  misaligned_sse
  avx_f16c
  avx_fma
  aes
  sha
  movbe
  adx
  xsave
  xsaveopt
  svm
  vmx
  bmi
  xop
  fma4
  tbm
  apic
  x86_64
  1g_pages
  pcid
  fsgsbase
  smep
  smap
  mwait

memory
  standard
    ram
      guest
      host
      block_size
    rom
      path
      address
      options
    vgarom
      path
  optrom
    0
      path
      addr
    1
      path
      addr
    2
      path
      addr
    3
      path
      addr
  optram
    0
      path
      addr
    1
      path
      addr
    2
      path
      addr
    3
      path
      addr

clock_cmos
  clock_sync
  time0
  cmosimage
    enabled
    path
    rtc_init

pci
  enabled
  chipset
  slot
    1
    2
    3
    4
    5
  advopts
  pcidev
    vendor
    device

display
  display_library
  displaylib_options
  private_colormap
  fullscreen
  screenmode
  vga_extension
  vga_update_interval
  voodoo
    enabled
    model

keyboard_mouse
  keyboard
    type
    serial_delay
    paste_delay
    use_mapping
    keymap
    user_shortcut
  mouse
    type
    enabled

boot_params
  boot_drive1
  boot_drive2
  boot_drive3
  floppy_sig_check

floppy
  0
    devtype
    path
    type
    readonly
    status
  1
    devtype
    path
    type
    readonly
    status

ata
  0
    resources
      enabled
      ioaddr1
      ioaddr2
      irq
    master
      type
      path
      mode
      journal
      cylinders
      heads
      spt
      sect_size
      status
      model
      biosdetect
      translation
    slave
      (same options as master)
  1
    (same options as ata.0)
  2
    (same options as ata.0)
  3
    (same options as ata.0)

ports
  serial
    1
      enabled
      mode
      dev
    2
      (same options as ports.serial.1)
    3
      (same options as ports.serial.1)
    4
      (same options as ports.serial.1)
  parallel
    1
      enabled
      outfile
    2
      (same options as ports.parallel.1)
  usb
    uhci
      enabled
      port1
        device
        options
      port2
        device
        options
    ohci
      (same options as ports.usb.uhci)
    ehci
      (same options as ports.usb.uhci)
      companion
    xhci
      (same options as ports.usb.uhci)
      model
      n_ports
  usb_debug
    type
    reset
    enable
    start_frame
    non_exist

network
  ne2k
    enabled
    ioaddr
    irq
    macaddr
    ethmod
    ethdev
    script
    bootrom
  pnic
    enabled
    macaddr
    ethmod
    ethdev
    script
    bootrom

  e1000
    enabled
    macaddr
    ethmod
    ethdev
    script
    bootrom

sound
  lowlevel
    waveoutdrv
    waveout
    waveindrv
    wavein
    midioutdrv
    midiout
  speaker
    enabled
    mode
  sb16
    enabled
    midimode
    midifile
    wavemode
    wavefile
    log
    loglevel
    dmatimer
  es1370
    enabled
    midimode
    midifile
    wavemode
    wavefile

misc
  port_e9_hack
    enabled
    all_rings
  iodebug_all_rings
  gdbstub
    port
    text_base
    data_base
    bss_base

log
  filename
  prefix
  debugger_filename

menu
  disk
  disk_win32
  memory
  runtime
    cdrom
    usb
    misc

bochs
  (subtree containing Bochs state)

user
  (subtree for user-defined options)
