| MD_SN76489 Library 0.1 Library for SN76489 sound generator

MD_SN74689 Member List

This is the complete list of members for MD_SN74689, including all inherited members.

begin(void) | MD_SN74689 |
isIdle(uint8_t chan) | MD_SN74689 |
MAX_CHANNELS | MD_SN74689 | static
MD_SN74689(const uint8_t *D, uint8_t WE, bool clock) | MD_SN74689 |
noise(noiseType_t noise, uint8_t shiftRate) | MD_SN74689 |
NOISE_CHANNEL | MD_SN74689 | static
NOISE_OFF | MD_SN74689 | static
noiseType_t enum name | MD_SN74689 |
note(uint8_t chan, uint32_t freq) | MD_SN74689 |
PERIODIC_0 enum value | MD_SN74689 |
PERIODIC_1 enum value | MD_SN74689 |
PERIODIC_2 enum value | MD_SN74689 |
PERIODIC_3 enum value | MD_SN74689 |
play(void) | MD_SN74689 |
setADSR(uint8_t chan, adsrEnvelope_t *padsr) | MD_SN74689 |
setADSR(adsrEnvelope_t *padsr) | MD_SN74689 |
setFrequency(uint8_t chan, uint32_t freq) | MD_SN74689 |
setNoise(noiseType_t noise, uint8_t shiftRate) | MD_SN74689 |
setVolume(uint8_t chan, uint8_t v) | MD_SN74689 |
setVolume(uint8_t v) | MD_SN74689 |
tone(uint8_t chan, uint32_t freq, uint8_t volume=VOL_MAX) | MD_SN74689 |
VOL_MAX | MD_SN74689 | static
VOL_OFF | MD_SN74689 | static
WHITE_0 enum value | MD_SN74689 |
WHITE_1 enum value | MD_SN74689 |
WHITE_2 enum value | MD_SN74689 |
WHITE_3 enum value | MD_SN74689 |
~MD_SN74689(void) | MD_SN74689 |