| MD_YM2413 Library 1.0 Library for Yahama YM2413 sound synthesizer

Loading...
Searching...
No Matches
MD_YM2413 Member List

This is the complete list of members for MD_YM2413, including all inherited members.

begin(void) | MD_YM2413 |
CH_BD | MD_YM2413 | static
CH_HH | MD_YM2413 | static
CH_SD | MD_YM2413 | static
CH_TCY | MD_YM2413 | static
CH_TOM | MD_YM2413 | static
CH_UNDEFINED | MD_YM2413 | static
countChannels(void) | MD_YM2413 |
getInstrument(uint8_t chan) | MD_YM2413 |
getVolume(uint8_t chan) | MD_YM2413 |
I_ACOUSTIC_BASS enum value (defined in MD_YM2413) | MD_YM2413 |
I_CLARINET enum value (defined in MD_YM2413) | MD_YM2413 |
I_CUSTOM enum value (defined in MD_YM2413) | MD_YM2413 |
I_EGUITAR enum value (defined in MD_YM2413) | MD_YM2413 |
I_FLUTE enum value (defined in MD_YM2413) | MD_YM2413 |
I_GUITAR enum value (defined in MD_YM2413) | MD_YM2413 |
I_HARPSICHORD enum value (defined in MD_YM2413) | MD_YM2413 |
I_HORN enum value (defined in MD_YM2413) | MD_YM2413 |
I_OBOE enum value (defined in MD_YM2413) | MD_YM2413 |
I_ORGAN enum value (defined in MD_YM2413) | MD_YM2413 |
I_PIANO enum value (defined in MD_YM2413) | MD_YM2413 |
I_SYNTH enum value (defined in MD_YM2413) | MD_YM2413 |
I_SYNTH_BASS enum value (defined in MD_YM2413) | MD_YM2413 |
I_TRUMPET enum value (defined in MD_YM2413) | MD_YM2413 |
I_UNDEFINED enum value (defined in MD_YM2413) | MD_YM2413 |
I_VIBRAPHONE enum value (defined in MD_YM2413) | MD_YM2413 |
I_VIOLIN enum value (defined in MD_YM2413) | MD_YM2413 |
instrument_t enum name | MD_YM2413 |
isIdle(uint8_t chan) | MD_YM2413 |
isPercussion(void) | MD_YM2413 |
isPercussion(uint8_t chan) | MD_YM2413 |
loadInstrument(const uint8_t *data) | MD_YM2413 |
loadInstrumentOPL2(const uint8_t *ins, bool fromPROGMEM=true) | MD_YM2413 |
MAX_OCTAVE | MD_YM2413 | static
MD_YM2413(const uint8_t *D, uint8_t we, uint8_t a0) | MD_YM2413 |
MIN_OCTAVE | MD_YM2413 | static
noteOff(uint8_t chan) | MD_YM2413 |
noteOn(uint8_t chan, uint16_t freq, uint8_t vol, uint16_t duration=0) | MD_YM2413 |
noteOn(uint8_t chan, uint8_t octave, uint8_t note, uint8_t vol, uint16_t duration=0) | MD_YM2413 |
OPL2_DATA_SIZE | MD_YM2413 | static
P_BASS_DRUM enum value (defined in MD_YM2413) | MD_YM2413 |
P_HI_HAT enum value (defined in MD_YM2413) | MD_YM2413 |
P_SNARE_DRUM enum value (defined in MD_YM2413) | MD_YM2413 |
P_TOM_TOM enum value (defined in MD_YM2413) | MD_YM2413 |
P_TOP_CYMBAL enum value (defined in MD_YM2413) | MD_YM2413 |
PERC_CHAN_BASE | MD_YM2413 | static
run(void) | MD_YM2413 |
setInstrument(uint8_t chan, instrument_t instr, uint8_t vol=VOL_MAX) | MD_YM2413 |
setPercussion(bool bEnable) | MD_YM2413 |
setSustain(uint8_t chan, bool sustain) | MD_YM2413 |
setVolume(uint8_t chan, uint8_t v) | MD_YM2413 |
setVolume(uint8_t v) | MD_YM2413 |
VOL_MAX | MD_YM2413 | static
VOL_OFF | MD_YM2413 | static
write(uint8_t addr, uint8_t data) | MD_YM2413 |
~MD_YM2413(void) | MD_YM2413 |