| MD_SN76489 Library 1.0 Library for SN76489 sound generator

MD_SN76489 Member List

This is the complete list of members for MD_SN76489, including all inherited members.

begin(void) | MD_SN76489 | virtual
DATA_BITS | MD_SN76489 | protected
isIdle(uint8_t chan) | MD_SN76489 |
MAX_CHANNELS | MD_SN76489 | static
MD_SN76489(bool clock) | MD_SN76489 |
noise(noiseType_t noise, uint8_t volume, uint16_t duration=0) | MD_SN76489 |
NOISE_CHANNEL | MD_SN76489 | static
NOISE_OFF enum value | MD_SN76489 |
noiseType_t enum name | MD_SN76489 |
note(uint8_t chan, uint16_t freq, uint8_t volume, uint16_t duration=0) | MD_SN76489 |
PERIODIC_0 enum value | MD_SN76489 |
PERIODIC_1 enum value | MD_SN76489 |
PERIODIC_2 enum value | MD_SN76489 |
PERIODIC_3 enum value | MD_SN76489 |
play(void) | MD_SN76489 |
send(uint8_t data) | MD_SN76489 | protected virtual
setADSR(uint8_t chan, adsrEnvelope_t *padsr) | MD_SN76489 |
setADSR(adsrEnvelope_t *padsr) | MD_SN76489 |
setFrequency(uint8_t chan, uint16_t freq) | MD_SN76489 |
setNoise(noiseType_t noise) | MD_SN76489 |
setVolume(uint8_t chan, uint8_t v) | MD_SN76489 |
setVolume(uint8_t v) | MD_SN76489 |
tone(uint8_t chan, uint16_t freq, uint8_t volume, uint16_t duration=0) | MD_SN76489 |
VOL_MAX | MD_SN76489 | static
VOL_OFF | MD_SN76489 | static
WHITE_0 enum value | MD_SN76489 |
WHITE_1 enum value | MD_SN76489 |
WHITE_2 enum value | MD_SN76489 |
WHITE_3 enum value | MD_SN76489 |
~MD_SN76489(void) | MD_SN76489 |