NS_AS(6)

NAME
ns_as - National Semiconductor 16032 assembler

SYNOPSIS
~em/lib.bin/ns/as [options] argument ...

DESCRIPTION
The assembler for the National Semiconductor 16032 is based on the universal assembler uni_ass(6). It is an assembler generating relocatable object code in ack.out(5) format. The mnemonics for the instructions are taken from the NS-16000 Programmers Reference Manual. The syntax of the instruction operands is similar to the syntax used in that manual, although the meaning is sometimes quite different. The cross assembler issued by National Semiconductor associates a type (sb,..) with each symbol and automatically generates sb offset mode for symbols of type sb. This assembler does not record the types, each symbol simply produces an untyped value.

The possible operands are:

general registers
    These are called r0, r1, r2, r3, r4, r5, r6 and r7. The symbol REG is used to indicate use of any of these 8 registers in other operands.

floating point registers
    These are called f0, f1, f2, f3, f4, f5, f6 and f7.

dedicated registers
    All types of dedicated registers can be used with the appropriate instructions. Examples: sb, fp, intbase, ptb1.

expr(REG)
    register relative

expr(fp)
    frame pointer relative

expr(sb)
    static base relative

expr(sp)
    stack pointer relative

expr(pc)
    program counter relative, the expression indicates a location in memory from which the current value of '.' is subtracted by the assembler. E.g. "movw label(pc),r0; label: .word ..." moves the contents of the word at label to r0.

expr(expr(fb))

expr(expr(sb))

expr(expr(sp))
    memory relative

@expr
    absolute

external(expr)+expr
    external

tos top of stack.

Usage of the scaled index operands is allowed.
The convention used to indicate offset length by appending :B, :W or :D to offsets is not implemented. The assembler tries to find out the minimal size needed for any constant in an operand of the instruction placed in the text segment. Offsets in instructions outside .text are always four bytes.
All special operands, e.g. register list, configuration list, have the same format as in the Programmers Reference Manual.
Whenever possible the assembler automatically uses the short(quick) opcodes for jsr(jsb), jump(br), add(addq), cmp(cmpq) and mov(movq).

BUGS
The data types floating and packed-decimal are not supported.
Initialization of floating-point numbers is not possible.
The mnemonics of the slave processor instructions are poorly documented, the format of the NS-16032S-6 data sheet is used.
The documentation gave contradictory information on the format of a few instructions.
-   Three different schemes are presented for the encoding of the last operand of the block instructions.
-   Two different values are specified for the encoding of the msr register in smr and lmr instructions.
-   Two different possibilities are given for the encoding of the instructions movsu and movus.

SEE ALSO
uni_ass(6) ack(1), ack.out(5),
NS 16000 Programmers Reference Manual. Publ. no. 420306565-001PB
NS16032S-6, NS16032S-4 High Performance Microprocessors, november 1982
publ. no. 420306619-002A.

AUTHOR
Ed Keizer, Vrije Universiteit