This is ../../gcc-3.4/gcc/doc/gccint.info, produced by makeinfo version
4.2 from ../../gcc-3.4/gcc/doc/gccint.texi.

Copyright (C) 1988, 1989, 1992, 1993, 1994, 1995, 1996, 1997, 1998,
1999, 2000, 2001, 2002, 2003 Free Software Foundation, Inc.

   Permission is granted to copy, distribute and/or modify this document
under the terms of the GNU Free Documentation License, Version 1.2 or
any later version published by the Free Software Foundation; with the
Invariant Sections being "GNU General Public License" and "Funding Free
Software", the Front-Cover texts being (a) (see below), and with the
Back-Cover Texts being (b) (see below).  A copy of the license is
included in the section entitled "GNU Free Documentation License".

   (a) The FSF's Front-Cover Text is:

   A GNU Manual

   (b) The FSF's Back-Cover Text is:

   You have freedom to copy and modify this GNU Manual, like GNU
software.  Copies published by the Free Software Foundation raise
funds for GNU development.
INFO-DIR-SECTION Programming
START-INFO-DIR-ENTRY
* gccint: (gccint).            Internals of the GNU Compiler Collection.
END-INFO-DIR-ENTRY
   This file documents the internals of the GNU compilers.

   Published by the Free Software Foundation
59 Temple Place - Suite 330
Boston, MA 02111-1307 USA

File: gccint.info,  Node: RTL Template,  Next: Output Template,  Prev: Example,  Up: Machine Desc

RTL Template
============

   The RTL template is used to define which insns match the particular
pattern and how to find their operands.  For named patterns, the RTL
template also says how to construct an insn from specified operands.

   Construction involves substituting specified operands into a copy of
the template.  Matching involves determining the values that serve as
the operands in the insn being matched.  Both of these activities are
controlled by special expression types that direct matching and
substitution of the operands.

`(match_operand:M N PREDICATE CONSTRAINT)'
     This expression is a placeholder for operand number N of the insn.
     When constructing an insn, operand number N will be substituted
     at this point.  When matching an insn, whatever appears at this
     position in the insn will be taken as operand number N; but it
     must satisfy PREDICATE or this instruction pattern will not match
     at all.

     Operand numbers must be chosen consecutively counting from zero in
     each instruction pattern.  There may be only one `match_operand'
     expression in the pattern for each operand number.  Usually
     operands are numbered in the order of appearance in `match_operand'
     expressions.  In the case of a `define_expand', any operand numbers
     used only in `match_dup' expressions have higher values than all
     other operand numbers.

     PREDICATE is a string that is the name of a C function that
     accepts two arguments, an expression and a machine mode.  During
     matching, the function will be called with the putative operand as
     the expression and M as the mode argument (if M is not specified,
     `VOIDmode' will be used, which normally causes PREDICATE to accept
     any mode).  If it returns zero, this instruction pattern fails to
     match.  PREDICATE may be an empty string; then it means no test is
     to be done on the operand, so anything which occurs in this
     position is valid.

     Most of the time, PREDICATE will reject modes other than M--but
     not always.  For example, the predicate `address_operand' uses M
     as the mode of memory ref that the address should be valid for.
     Many predicates accept `const_int' nodes even though their mode is
     `VOIDmode'.

     CONSTRAINT controls reloading and the choice of the best register
     class to use for a value, as explained later (*note Constraints::).

     People are often unclear on the difference between the constraint
     and the predicate.  The predicate helps decide whether a given
     insn matches the pattern.  The constraint plays no role in this
     decision; instead, it controls various decisions in the case of an
     insn which does match.

     On CISC machines, the most common PREDICATE is
     `"general_operand"'.  This function checks that the putative
     operand is either a constant, a register or a memory reference,
     and that it is valid for mode M.

     For an operand that must be a register, PREDICATE should be
     `"register_operand"'.  Using `"general_operand"' would be valid,
     since the reload pass would copy any non-register operands through
     registers, but this would make GCC do extra work, it would prevent
     invariant operands (such as constant) from being removed from
     loops, and it would prevent the register allocator from doing the
     best possible job.  On RISC machines, it is usually most efficient
     to allow PREDICATE to accept only objects that the constraints
     allow.

     For an operand that must be a constant, you must be sure to either
     use `"immediate_operand"' for PREDICATE, or make the instruction
     pattern's extra condition require a constant, or both.  You cannot
     expect the constraints to do this work!  If the constraints allow
     only constants, but the predicate allows something else, the
     compiler will crash when that case arises.

`(match_scratch:M N CONSTRAINT)'
     This expression is also a placeholder for operand number N and
     indicates that operand must be a `scratch' or `reg' expression.

     When matching patterns, this is equivalent to

          (match_operand:M N "scratch_operand" PRED)

     but, when generating RTL, it produces a (`scratch':M) expression.

     If the last few expressions in a `parallel' are `clobber'
     expressions whose operands are either a hard register or
     `match_scratch', the combiner can add or delete them when
     necessary.  *Note Side Effects::.

`(match_dup N)'
     This expression is also a placeholder for operand number N.  It is
     used when the operand needs to appear more than once in the insn.

     In construction, `match_dup' acts just like `match_operand': the
     operand is substituted into the insn being constructed.  But in
     matching, `match_dup' behaves differently.  It assumes that operand
     number N has already been determined by a `match_operand'
     appearing earlier in the recognition template, and it matches only
     an identical-looking expression.

     Note that `match_dup' should not be used to tell the compiler that
     a particular register is being used for two operands (example:
     `add' that adds one register to another; the second register is
     both an input operand and the output operand).  Use a matching
     constraint (*note Simple Constraints::) for those.  `match_dup' is
     for the cases where one operand is used in two places in the
     template, such as an instruction that computes both a quotient and
     a remainder, where the opcode takes two input operands but the RTL
     template has to refer to each of those twice; once for the
     quotient pattern and once for the remainder pattern.

`(match_operator:M N PREDICATE [OPERANDS...])'
     This pattern is a kind of placeholder for a variable RTL expression
     code.

     When constructing an insn, it stands for an RTL expression whose
     expression code is taken from that of operand N, and whose
     operands are constructed from the patterns OPERANDS.

     When matching an expression, it matches an expression if the
     function PREDICATE returns nonzero on that expression _and_ the
     patterns OPERANDS match the operands of the expression.

     Suppose that the function `commutative_operator' is defined as
     follows, to match any expression whose operator is one of the
     commutative arithmetic operators of RTL and whose mode is MODE:

          int
          commutative_operator (x, mode)
               rtx x;
               enum machine_mode mode;
          {
            enum rtx_code code = GET_CODE (x);
            if (GET_MODE (x) != mode)
              return 0;
            return (GET_RTX_CLASS (code) == 'c'
                    || code == EQ || code == NE);
          }

     Then the following pattern will match any RTL expression consisting
     of a commutative operator applied to two general operands:

          (match_operator:SI 3 "commutative_operator"
            [(match_operand:SI 1 "general_operand" "g")
             (match_operand:SI 2 "general_operand" "g")])

     Here the vector `[OPERANDS...]' contains two patterns because the
     expressions to be matched all contain two operands.

     When this pattern does match, the two operands of the commutative
     operator are recorded as operands 1 and 2 of the insn.  (This is
     done by the two instances of `match_operand'.)  Operand 3 of the
     insn will be the entire commutative expression: use `GET_CODE
     (operands[3])' to see which commutative operator was used.

     The machine mode M of `match_operator' works like that of
     `match_operand': it is passed as the second argument to the
     predicate function, and that function is solely responsible for
     deciding whether the expression to be matched "has" that mode.

     When constructing an insn, argument 3 of the gen-function will
     specify the operation (i.e. the expression code) for the
     expression to be made.  It should be an RTL expression, whose
     expression code is copied into a new expression whose operands are
     arguments 1 and 2 of the gen-function.  The subexpressions of
     argument 3 are not used; only its expression code matters.

     When `match_operator' is used in a pattern for matching an insn,
     it usually best if the operand number of the `match_operator' is
     higher than that of the actual operands of the insn.  This improves
     register allocation because the register allocator often looks at
     operands 1 and 2 of insns to see if it can do register tying.

     There is no way to specify constraints in `match_operator'.  The
     operand of the insn which corresponds to the `match_operator'
     never has any constraints because it is never reloaded as a whole.
     However, if parts of its OPERANDS are matched by `match_operand'
     patterns, those parts may have constraints of their own.

`(match_op_dup:M N[OPERANDS...])'
     Like `match_dup', except that it applies to operators instead of
     operands.  When constructing an insn, operand number N will be
     substituted at this point.  But in matching, `match_op_dup' behaves
     differently.  It assumes that operand number N has already been
     determined by a `match_operator' appearing earlier in the
     recognition template, and it matches only an identical-looking
     expression.

`(match_parallel N PREDICATE [SUBPAT...])'
     This pattern is a placeholder for an insn that consists of a
     `parallel' expression with a variable number of elements.  This
     expression should only appear at the top level of an insn pattern.

     When constructing an insn, operand number N will be substituted at
     this point.  When matching an insn, it matches if the body of the
     insn is a `parallel' expression with at least as many elements as
     the vector of SUBPAT expressions in the `match_parallel', if each
     SUBPAT matches the corresponding element of the `parallel', _and_
     the function PREDICATE returns nonzero on the `parallel' that is
     the body of the insn.  It is the responsibility of the predicate
     to validate elements of the `parallel' beyond those listed in the
     `match_parallel'.

     A typical use of `match_parallel' is to match load and store
     multiple expressions, which can contain a variable number of
     elements in a `parallel'.  For example,

          (define_insn ""
            [(match_parallel 0 "load_multiple_operation"
               [(set (match_operand:SI 1 "gpc_reg_operand" "=r")
                     (match_operand:SI 2 "memory_operand" "m"))
                (use (reg:SI 179))
                (clobber (reg:SI 179))])]
            ""
            "loadm 0,0,%1,%2")

     This example comes from `a29k.md'.  The function
     `load_multiple_operation' is defined in `a29k.c' and checks that
     subsequent elements in the `parallel' are the same as the `set' in
     the pattern, except that they are referencing subsequent registers
     and memory locations.

     An insn that matches this pattern might look like:

          (parallel
           [(set (reg:SI 20) (mem:SI (reg:SI 100)))
            (use (reg:SI 179))
            (clobber (reg:SI 179))
            (set (reg:SI 21)
                 (mem:SI (plus:SI (reg:SI 100)
                                  (const_int 4))))
            (set (reg:SI 22)
                 (mem:SI (plus:SI (reg:SI 100)
                                  (const_int 8))))])

`(match_par_dup N [SUBPAT...])'
     Like `match_op_dup', but for `match_parallel' instead of
     `match_operator'.

`(match_insn PREDICATE)'
     Match a complete insn.  Unlike the other `match_*' recognizers,
     `match_insn' does not take an operand number.

     The machine mode M of `match_insn' works like that of
     `match_operand': it is passed as the second argument to the
     predicate function, and that function is solely responsible for
     deciding whether the expression to be matched "has" that mode.

`(match_insn2 N PREDICATE)'
     Match a complete insn.

     The machine mode M of `match_insn2' works like that of
     `match_operand': it is passed as the second argument to the
     predicate function, and that function is solely responsible for
     deciding whether the expression to be matched "has" that mode.


File: gccint.info,  Node: Output Template,  Next: Output Statement,  Prev: RTL Template,  Up: Machine Desc

Output Templates and Operand Substitution
=========================================

   The "output template" is a string which specifies how to output the
assembler code for an instruction pattern.  Most of the template is a
fixed string which is output literally.  The character `%' is used to
specify where to substitute an operand; it can also be used to identify
places where different variants of the assembler require different
syntax.

   In the simplest case, a `%' followed by a digit N says to output
operand N at that point in the string.

   `%' followed by a letter and a digit says to output an operand in an
alternate fashion.  Four letters have standard, built-in meanings
described below.  The machine description macro `PRINT_OPERAND' can
define additional letters with nonstandard meanings.

   `%cDIGIT' can be used to substitute an operand that is a constant
value without the syntax that normally indicates an immediate operand.

   `%nDIGIT' is like `%cDIGIT' except that the value of the constant is
negated before printing.

   `%aDIGIT' can be used to substitute an operand as if it were a
memory reference, with the actual operand treated as the address.  This
may be useful when outputting a "load address" instruction, because
often the assembler syntax for such an instruction requires you to
write the operand as if it were a memory reference.

   `%lDIGIT' is used to substitute a `label_ref' into a jump
instruction.

   `%=' outputs a number which is unique to each instruction in the
entire compilation.  This is useful for making local labels to be
referred to more than once in a single template that generates multiple
assembler instructions.

   `%' followed by a punctuation character specifies a substitution that
does not use an operand.  Only one case is standard: `%%' outputs a `%'
into the assembler code.  Other nonstandard cases can be defined in the
`PRINT_OPERAND' macro.  You must also define which punctuation
characters are valid with the `PRINT_OPERAND_PUNCT_VALID_P' macro.

   The template may generate multiple assembler instructions.  Write
the text for the instructions, with `\;' between them.

   When the RTL contains two operands which are required by constraint
to match each other, the output template must refer only to the
lower-numbered operand.  Matching operands are not always identical,
and the rest of the compiler arranges to put the proper RTL expression
for printing into the lower-numbered operand.

   One use of nonstandard letters or punctuation following `%' is to
distinguish between different assembler languages for the same machine;
for example, Motorola syntax versus MIT syntax for the 68000.  Motorola
syntax requires periods in most opcode names, while MIT syntax does
not.  For example, the opcode `movel' in MIT syntax is `move.l' in
Motorola syntax.  The same file of patterns is used for both kinds of
output syntax, but the character sequence `%.' is used in each place
where Motorola syntax wants a period.  The `PRINT_OPERAND' macro for
Motorola syntax defines the sequence to output a period; the macro for
MIT syntax defines it to do nothing.

   As a special case, a template consisting of the single character `#'
instructs the compiler to first split the insn, and then output the
resulting instructions separately.  This helps eliminate redundancy in
the output templates.   If you have a `define_insn' that needs to emit
multiple assembler instructions, and there is an matching `define_split'
already defined, then you can simply use `#' as the output template
instead of writing an output template that emits the multiple assembler
instructions.

   If the macro `ASSEMBLER_DIALECT' is defined, you can use construct
of the form `{option0|option1|option2}' in the templates.  These
describe multiple variants of assembler language syntax.  *Note
Instruction Output::.


File: gccint.info,  Node: Output Statement,  Next: Constraints,  Prev: Output Template,  Up: Machine Desc

C Statements for Assembler Output
=================================

   Often a single fixed template string cannot produce correct and
efficient assembler code for all the cases that are recognized by a
single instruction pattern.  For example, the opcodes may depend on the
kinds of operands; or some unfortunate combinations of operands may
require extra machine instructions.

   If the output control string starts with a `@', then it is actually
a series of templates, each on a separate line.  (Blank lines and
leading spaces and tabs are ignored.)  The templates correspond to the
pattern's constraint alternatives (*note Multi-Alternative::).  For
example, if a target machine has a two-address add instruction `addr'
to add into a register and another `addm' to add a register to memory,
you might write this pattern:

     (define_insn "addsi3"
       [(set (match_operand:SI 0 "general_operand" "=r,m")
             (plus:SI (match_operand:SI 1 "general_operand" "0,0")
                      (match_operand:SI 2 "general_operand" "g,r")))]
       ""
       "@
        addr %2,%0
        addm %2,%0")

   If the output control string starts with a `*', then it is not an
output template but rather a piece of C program that should compute a
template.  It should execute a `return' statement to return the
template-string you want.  Most such templates use C string literals,
which require doublequote characters to delimit them.  To include these
doublequote characters in the string, prefix each one with `\'.

   If the output control string is written as a brace block instead of a
double-quoted string, it is automatically assumed to be C code.  In that
case, it is not necessary to put in a leading asterisk, or to escape the
doublequotes surrounding C string literals.

   The operands may be found in the array `operands', whose C data type
is `rtx []'.

   It is very common to select different ways of generating assembler
code based on whether an immediate operand is within a certain range.
Be careful when doing this, because the result of `INTVAL' is an
integer on the host machine.  If the host machine has more bits in an
`int' than the target machine has in the mode in which the constant
will be used, then some of the bits you get from `INTVAL' will be
superfluous.  For proper results, you must carefully disregard the
values of those bits.

   It is possible to output an assembler instruction and then go on to
output or compute more of them, using the subroutine `output_asm_insn'.
This receives two arguments: a template-string and a vector of
operands.  The vector may be `operands', or it may be another array of
`rtx' that you declare locally and initialize yourself.

   When an insn pattern has multiple alternatives in its constraints,
often the appearance of the assembler code is determined mostly by
which alternative was matched.  When this is so, the C code can test
the variable `which_alternative', which is the ordinal number of the
alternative that was actually satisfied (0 for the first, 1 for the
second alternative, etc.).

   For example, suppose there are two opcodes for storing zero, `clrreg'
for registers and `clrmem' for memory locations.  Here is how a pattern
could use `which_alternative' to choose between them:

     (define_insn ""
       [(set (match_operand:SI 0 "general_operand" "=r,m")
             (const_int 0))]
       ""
       {
       return (which_alternative == 0
               ? "clrreg %0" : "clrmem %0");
       })

   The example above, where the assembler code to generate was _solely_
determined by the alternative, could also have been specified as
follows, having the output control string start with a `@':

     (define_insn ""
       [(set (match_operand:SI 0 "general_operand" "=r,m")
             (const_int 0))]
       ""
       "@
        clrreg %0
        clrmem %0")


File: gccint.info,  Node: Constraints,  Next: Standard Names,  Prev: Output Statement,  Up: Machine Desc

Operand Constraints
===================

   Each `match_operand' in an instruction pattern can specify a
constraint for the type of operands allowed.  Constraints can say
whether an operand may be in a register, and which kinds of register;
whether the operand can be a memory reference, and which kinds of
address; whether the operand may be an immediate constant, and which
possible values it may have.  Constraints can also require two operands
to match.

* Menu:

* Simple Constraints::  Basic use of constraints.
* Multi-Alternative::   When an insn has two alternative constraint-patterns.
* Class Preferences::   Constraints guide which hard register to put things in.
* Modifiers::           More precise control over effects of constraints.
* Machine Constraints:: Existing constraints for some particular machines.


File: gccint.info,  Node: Simple Constraints,  Next: Multi-Alternative,  Up: Constraints

Simple Constraints
------------------

   The simplest kind of constraint is a string full of letters, each of
which describes one kind of operand that is permitted.  Here are the
letters that are allowed:

whitespace
     Whitespace characters are ignored and can be inserted at any
     position except the first.  This enables each alternative for
     different operands to be visually aligned in the machine
     description even if they have different number of constraints and
     modifiers.

`m'
     A memory operand is allowed, with any kind of address that the
     machine supports in general.

`o'
     A memory operand is allowed, but only if the address is
     "offsettable".  This means that adding a small integer (actually,
     the width in bytes of the operand, as determined by its machine
     mode) may be added to the address and the result is also a valid
     memory address.

     For example, an address which is constant is offsettable; so is an
     address that is the sum of a register and a constant (as long as a
     slightly larger constant is also within the range of
     address-offsets supported by the machine); but an autoincrement or
     autodecrement address is not offsettable.  More complicated
     indirect/indexed addresses may or may not be offsettable depending
     on the other addressing modes that the machine supports.

     Note that in an output operand which can be matched by another
     operand, the constraint letter `o' is valid only when accompanied
     by both `<' (if the target machine has predecrement addressing)
     and `>' (if the target machine has preincrement addressing).

`V'
     A memory operand that is not offsettable.  In other words,
     anything that would fit the `m' constraint but not the `o'
     constraint.

`<'
     A memory operand with autodecrement addressing (either
     predecrement or postdecrement) is allowed.

`>'
     A memory operand with autoincrement addressing (either
     preincrement or postincrement) is allowed.

`r'
     A register operand is allowed provided that it is in a general
     register.

`i'
     An immediate integer operand (one with constant value) is allowed.
     This includes symbolic constants whose values will be known only at
     assembly time.

`n'
     An immediate integer operand with a known numeric value is allowed.
     Many systems cannot support assembly-time constants for operands
     less than a word wide.  Constraints for these operands should use
     `n' rather than `i'.

`I', `J', `K', ... `P'
     Other letters in the range `I' through `P' may be defined in a
     machine-dependent fashion to permit immediate integer operands with
     explicit integer values in specified ranges.  For example, on the
     68000, `I' is defined to stand for the range of values 1 to 8.
     This is the range permitted as a shift count in the shift
     instructions.

`E'
     An immediate floating operand (expression code `const_double') is
     allowed, but only if the target floating point format is the same
     as that of the host machine (on which the compiler is running).

`F'
     An immediate floating operand (expression code `const_double' or
     `const_vector') is allowed.

`G', `H'
     `G' and `H' may be defined in a machine-dependent fashion to
     permit immediate floating operands in particular ranges of values.

`s'
     An immediate integer operand whose value is not an explicit
     integer is allowed.

     This might appear strange; if an insn allows a constant operand
     with a value not known at compile time, it certainly must allow
     any known value.  So why use `s' instead of `i'?  Sometimes it
     allows better code to be generated.

     For example, on the 68000 in a fullword instruction it is possible
     to use an immediate operand; but if the immediate value is between
     -128 and 127, better code results from loading the value into a
     register and using the register.  This is because the load into
     the register can be done with a `moveq' instruction.  We arrange
     for this to happen by defining the letter `K' to mean "any integer
     outside the range -128 to 127", and then specifying `Ks' in the
     operand constraints.

`g'
     Any register, memory or immediate integer operand is allowed,
     except for registers that are not general registers.

`X'
     Any operand whatsoever is allowed, even if it does not satisfy
     `general_operand'.  This is normally used in the constraint of a
     `match_scratch' when certain alternatives will not actually
     require a scratch register.

`0', `1', `2', ... `9'
     An operand that matches the specified operand number is allowed.
     If a digit is used together with letters within the same
     alternative, the digit should come last.

     This number is allowed to be more than a single digit.  If multiple
     digits are encountered consecutively, they are interpreted as a
     single decimal integer.  There is scant chance for ambiguity,
     since to-date it has never been desirable that `10' be interpreted
     as matching either operand 1 _or_ operand 0.  Should this be
     desired, one can use multiple alternatives instead.

     This is called a "matching constraint" and what it really means is
     that the assembler has only a single operand that fills two roles
     considered separate in the RTL insn.  For example, an add insn has
     two input operands and one output operand in the RTL, but on most
     CISC machines an add instruction really has only two operands, one
     of them an input-output operand:

          addl #35,r12

     Matching constraints are used in these circumstances.  More
     precisely, the two operands that match must include one input-only
     operand and one output-only operand.  Moreover, the digit must be a
     smaller number than the number of the operand that uses it in the
     constraint.

     For operands to match in a particular case usually means that they
     are identical-looking RTL expressions.  But in a few special cases
     specific kinds of dissimilarity are allowed.  For example, `*x' as
     an input operand will match `*x++' as an output operand.  For
     proper results in such cases, the output template should always
     use the output-operand's number when printing the operand.

`p'
     An operand that is a valid memory address is allowed.  This is for
     "load address" and "push address" instructions.

     `p' in the constraint must be accompanied by `address_operand' as
     the predicate in the `match_operand'.  This predicate interprets
     the mode specified in the `match_operand' as the mode of the memory
     reference for which the address would be valid.

OTHER-LETTERS
     Other letters can be defined in machine-dependent fashion to stand
     for particular classes of registers or other arbitrary operand
     types.  `d', `a' and `f' are defined on the 68000/68020 to stand
     for data, address and floating point registers.

     The machine description macro `REG_CLASS_FROM_LETTER' has first
     cut at the otherwise unused letters.  If it evaluates to `NO_REGS',
     then `EXTRA_CONSTRAINT' is evaluated.

     A typical use for `EXTRA_CONSTRAINT' would be to distinguish
     certain types of memory references that affect other insn operands.

   In order to have valid assembler code, each operand must satisfy its
constraint.  But a failure to do so does not prevent the pattern from
applying to an insn.  Instead, it directs the compiler to modify the
code so that the constraint will be satisfied.  Usually this is done by
copying an operand into a register.

   Contrast, therefore, the two instruction patterns that follow:

     (define_insn ""
       [(set (match_operand:SI 0 "general_operand" "=r")
             (plus:SI (match_dup 0)
                      (match_operand:SI 1 "general_operand" "r")))]
       ""
       "...")

which has two operands, one of which must appear in two places, and

     (define_insn ""
       [(set (match_operand:SI 0 "general_operand" "=r")
             (plus:SI (match_operand:SI 1 "general_operand" "0")
                      (match_operand:SI 2 "general_operand" "r")))]
       ""
       "...")

which has three operands, two of which are required by a constraint to
be identical.  If we are considering an insn of the form

     (insn N PREV NEXT
       (set (reg:SI 3)
            (plus:SI (reg:SI 6) (reg:SI 109)))
       ...)

the first pattern would not apply at all, because this insn does not
contain two identical subexpressions in the right place.  The pattern
would say, "That does not look like an add instruction; try other
patterns."  The second pattern would say, "Yes, that's an add
instruction, but there is something wrong with it."  It would direct
the reload pass of the compiler to generate additional insns to make
the constraint true.  The results might look like this:

     (insn N2 PREV N
       (set (reg:SI 3) (reg:SI 6))
       ...)
     
     (insn N N2 NEXT
       (set (reg:SI 3)
            (plus:SI (reg:SI 3) (reg:SI 109)))
       ...)

   It is up to you to make sure that each operand, in each pattern, has
constraints that can handle any RTL expression that could be present for
that operand.  (When multiple alternatives are in use, each pattern
must, for each possible combination of operand expressions, have at
least one alternative which can handle that combination of operands.)
The constraints don't need to _allow_ any possible operand--when this is
the case, they do not constrain--but they must at least point the way to
reloading any possible operand so that it will fit.

   * If the constraint accepts whatever operands the predicate permits,
     there is no problem: reloading is never necessary for this operand.

     For example, an operand whose constraints permit everything except
     registers is safe provided its predicate rejects registers.

     An operand whose predicate accepts only constant values is safe
     provided its constraints include the letter `i'.  If any possible
     constant value is accepted, then nothing less than `i' will do; if
     the predicate is more selective, then the constraints may also be
     more selective.

   * Any operand expression can be reloaded by copying it into a
     register.  So if an operand's constraints allow some kind of
     register, it is certain to be safe.  It need not permit all
     classes of registers; the compiler knows how to copy a register
     into another register of the proper class in order to make an
     instruction valid.

   * A nonoffsettable memory reference can be reloaded by copying the
     address into a register.  So if the constraint uses the letter
     `o', all memory references are taken care of.

   * A constant operand can be reloaded by allocating space in memory to
     hold it as preinitialized data.  Then the memory reference can be
     used in place of the constant.  So if the constraint uses the
     letters `o' or `m', constant operands are not a problem.

   * If the constraint permits a constant and a pseudo register used in
     an insn was not allocated to a hard register and is equivalent to
     a constant, the register will be replaced with the constant.  If
     the predicate does not permit a constant and the insn is
     re-recognized for some reason, the compiler will crash.  Thus the
     predicate must always recognize any objects allowed by the
     constraint.

   If the operand's predicate can recognize registers, but the
constraint does not permit them, it can make the compiler crash.  When
this operand happens to be a register, the reload pass will be stymied,
because it does not know how to copy a register temporarily into memory.

   If the predicate accepts a unary operator, the constraint applies to
the operand.  For example, the MIPS processor at ISA level 3 supports an
instruction which adds two registers in `SImode' to produce a `DImode'
result, but only if the registers are correctly sign extended.  This
predicate for the input operands accepts a `sign_extend' of an `SImode'
register.  Write the constraint to indicate the type of register that
is required for the operand of the `sign_extend'.


File: gccint.info,  Node: Multi-Alternative,  Next: Class Preferences,  Prev: Simple Constraints,  Up: Constraints

Multiple Alternative Constraints
--------------------------------

   Sometimes a single instruction has multiple alternative sets of
possible operands.  For example, on the 68000, a logical-or instruction
can combine register or an immediate value into memory, or it can
combine any kind of operand into a register; but it cannot combine one
memory location into another.

   These constraints are represented as multiple alternatives.  An
alternative can be described by a series of letters for each operand.
The overall constraint for an operand is made from the letters for this
operand from the first alternative, a comma, the letters for this
operand from the second alternative, a comma, and so on until the last
alternative.  Here is how it is done for fullword logical-or on the
68000:

     (define_insn "iorsi3"
       [(set (match_operand:SI 0 "general_operand" "=m,d")
             (ior:SI (match_operand:SI 1 "general_operand" "%0,0")
                     (match_operand:SI 2 "general_operand" "dKs,dmKs")))]
       ...)

   The first alternative has `m' (memory) for operand 0, `0' for
operand 1 (meaning it must match operand 0), and `dKs' for operand 2.
The second alternative has `d' (data register) for operand 0, `0' for
operand 1, and `dmKs' for operand 2.  The `=' and `%' in the
constraints apply to all the alternatives; their meaning is explained
in the next section (*note Class Preferences::).

   If all the operands fit any one alternative, the instruction is
valid.  Otherwise, for each alternative, the compiler counts how many
instructions must be added to copy the operands so that that
alternative applies.  The alternative requiring the least copying is
chosen.  If two alternatives need the same amount of copying, the one
that comes first is chosen.  These choices can be altered with the `?'
and `!' characters:

`?'
     Disparage slightly the alternative that the `?' appears in, as a
     choice when no alternative applies exactly.  The compiler regards
     this alternative as one unit more costly for each `?' that appears
     in it.

`!'
     Disparage severely the alternative that the `!' appears in.  This
     alternative can still be used if it fits without reloading, but if
     reloading is needed, some other alternative will be used.

   When an insn pattern has multiple alternatives in its constraints,
often the appearance of the assembler code is determined mostly by which
alternative was matched.  When this is so, the C code for writing the
assembler code can use the variable `which_alternative', which is the
ordinal number of the alternative that was actually satisfied (0 for
the first, 1 for the second alternative, etc.).  *Note Output
Statement::.


File: gccint.info,  Node: Class Preferences,  Next: Modifiers,  Prev: Multi-Alternative,  Up: Constraints

Register Class Preferences
--------------------------

   The operand constraints have another function: they enable the
compiler to decide which kind of hardware register a pseudo register is
best allocated to.  The compiler examines the constraints that apply to
the insns that use the pseudo register, looking for the
machine-dependent letters such as `d' and `a' that specify classes of
registers.  The pseudo register is put in whichever class gets the most
"votes".  The constraint letters `g' and `r' also vote: they vote in
favor of a general register.  The machine description says which
registers are considered general.

   Of course, on some machines all registers are equivalent, and no
register classes are defined.  Then none of this complexity is relevant.


File: gccint.info,  Node: Modifiers,  Next: Machine Constraints,  Prev: Class Preferences,  Up: Constraints

Constraint Modifier Characters
------------------------------

   Here are constraint modifier characters.

`='
     Means that this operand is write-only for this instruction: the
     previous value is discarded and replaced by output data.

`+'
     Means that this operand is both read and written by the
     instruction.

     When the compiler fixes up the operands to satisfy the constraints,
     it needs to know which operands are inputs to the instruction and
     which are outputs from it.  `=' identifies an output; `+'
     identifies an operand that is both input and output; all other
     operands are assumed to be input only.

     If you specify `=' or `+' in a constraint, you put it in the first
     character of the constraint string.

`&'
     Means (in a particular alternative) that this operand is an
     "earlyclobber" operand, which is modified before the instruction is
     finished using the input operands.  Therefore, this operand may
     not lie in a register that is used as an input operand or as part
     of any memory address.

     `&' applies only to the alternative in which it is written.  In
     constraints with multiple alternatives, sometimes one alternative
     requires `&' while others do not.  See, for example, the `movdf'
     insn of the 68000.

     An input operand can be tied to an earlyclobber operand if its only
     use as an input occurs before the early result is written.  Adding
     alternatives of this form often allows GCC to produce better code
     when only some of the inputs can be affected by the earlyclobber.
     See, for example, the `mulsi3' insn of the ARM.

     `&' does not obviate the need to write `='.

`%'
     Declares the instruction to be commutative for this operand and the
     following operand.  This means that the compiler may interchange
     the two operands if that is the cheapest way to make all operands
     fit the constraints.  This is often used in patterns for addition
     instructions that really have only two operands: the result must
     go in one of the arguments.  Here for example, is how the 68000
     halfword-add instruction is defined:

          (define_insn "addhi3"
            [(set (match_operand:HI 0 "general_operand" "=m,r")
               (plus:HI (match_operand:HI 1 "general_operand" "%0,0")
                        (match_operand:HI 2 "general_operand" "di,g")))]
            ...)
     GCC can only handle one commutative pair in an asm; if you use
     more, the compiler may fail.

`#'
     Says that all following characters, up to the next comma, are to be
     ignored as a constraint.  They are significant only for choosing
     register preferences.

`*'
     Says that the following character should be ignored when choosing
     register preferences.  `*' has no effect on the meaning of the
     constraint as a constraint, and no effect on reloading.

     Here is an example: the 68000 has an instruction to sign-extend a
     halfword in a data register, and can also sign-extend a value by
     copying it into an address register.  While either kind of
     register is acceptable, the constraints on an address-register
     destination are less strict, so it is best if register allocation
     makes an address register its goal.  Therefore, `*' is used so
     that the `d' constraint letter (for data register) is ignored when
     computing register preferences.

          (define_insn "extendhisi2"
            [(set (match_operand:SI 0 "general_operand" "=*d,a")
                  (sign_extend:SI
                   (match_operand:HI 1 "general_operand" "0,g")))]
            ...)

