;; Frv Machine Description
;; Copyright (C) 1999, 2000, 2001 Free Software Foundation, Inc.
;; Contributed by Red Hat, Inc.

;; This file is part of GNU CC.

;; GNU CC is free software; you can redistribute it and/or modify
;; it under the terms of the GNU General Public License as published by
;; the Free Software Foundation; either version 2, or (at your option)
;; any later version.

;; GNU CC is distributed in the hope that it will be useful,
;; but WITHOUT ANY WARRANTY; without even the implied warranty of
;; MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
;; GNU General Public License for more details.

;; You should have received a copy of the GNU General Public License
;; along with GNU CC; see the file COPYING.  If not, write to
;; the Free Software Foundation, 59 Temple Place - Suite 330,
;; Boston, MA 02111-1307, USA.

;;- See file "rtl.def" for documentation on define_insn, match_*, et. al.


;; ::::::::::::::::::::
;; ::
;; :: Unspec's used
;; ::
;; ::::::::::::::::::::

(define_constants
  [(UNSPEC_BLOCKAGE		0)
   (UNSPEC_CC_TO_GPR		1)
   (UNSPEC_GPR_TO_CC		2)
   (UNSPEC_PIC_PROLOGUE		3)
   (UNSPEC_CR_LOGIC		4)
   (UNSPEC_STACK_ADJUST		5)
   (UNSPEC_EH_RETURN_EPILOGUE	6)])



;; ::::::::::::::::::::
;; ::
;; :: Constraints
;; ::
;; ::::::::::::::::::::

;; Standard Constraints
;;
;; `m' A memory operand is allowed, with any kind of address that the
;;     machine supports in general.
;;
;; `o' A memory operand is allowed, but only if the address is
;;     "offsettable".  This means that adding a small integer (actually, the
;;     width in bytes of the operand, as determined by its machine mode) may be
;;     added to the address and the result is also a valid memory address.
;;
;; `V' A memory operand that is not offsettable.  In other words,
;;     anything that would fit the `m' constraint but not the `o' constraint.
;;
;; `<' A memory operand with autodecrement addressing (either
;;     predecrement or postdecrement) is allowed.
;;
;; `>' A memory operand with autoincrement addressing (either
;;     preincrement or postincrement) is allowed.
;;
;; `r' A register operand is allowed provided that it is in a general
;;     register.
;;
;; `d', `a', `f', ...
;;     Other letters can be defined in machine-dependent fashion to stand for
;;     particular classes of registers.  `d', `a' and `f' are defined on the
;;     68000/68020 to stand for data, address and floating point registers.
;;
;; `i' An immediate integer operand (one with constant value) is allowed.
;;     This includes symbolic constants whose values will be known only at
;;     assembly time.
;;
;; `n' An immediate integer operand with a known numeric value is allowed.
;;     Many systems cannot support assembly-time constants for operands less
;;     than a word wide.  Constraints for these operands should use `n' rather
;;     than `i'.
;;
;; 'I' First machine-dependent integer constant (6 bit signed ints).
;; 'J' Second machine-dependent integer constant (10 bit signed ints).
;; 'K' Third machine-dependent integer constant (-2048).
;; 'L' Fourth machine-dependent integer constant (16 bit signed ints).
;; 'M' Fifth machine-dependent integer constant (16 bit unsigned ints).
;; 'N' Sixth machine-dependent integer constant (-2047..-1).
;; 'O' Seventh machine-dependent integer constant (zero).
;; 'P' Eighth machine-dependent integer constant (1..2047).
;;
;;     Other letters in the range `I' through `P' may be defined in a
;;     machine-dependent fashion to permit immediate integer operands with
;;     explicit integer values in specified ranges.  For example, on the 68000,
;;     `I' is defined to stand for the range of values 1 to 8.  This is the
;;     range permitted as a shift count in the shift instructions.
;;
;; `E' An immediate floating operand (expression code `const_double') is
;;     allowed, but only if the target floating point format is the same as
;;     that of the host machine (on which the compiler is running).
;;
;; `F' An immediate floating operand (expression code `const_double') is
;;     allowed.
;;
;; 'G' First machine-dependent const_double.
;; 'H' Second machine-dependent const_double.
;;
;; `s' An immediate integer operand whose value is not an explicit
;;     integer is allowed.
;;
;;     This might appear strange; if an insn allows a constant operand with a
;;     value not known at compile time, it certainly must allow any known
;;     value.  So why use `s' instead of `i'?  Sometimes it allows better code
;;     to be generated.
;;
;;     For example, on the 68000 in a fullword instruction it is possible to
;;     use an immediate operand; but if the immediate value is between -128 and
;;     127, better code results from loading the value into a register and
;;     using the register.  This is because the load into the register can be
;;     done with a `moveq' instruction.  We arrange for this to happen by
;;     defining the letter `K' to mean "any integer outside the range -128 to
;;     127", and then specifying `Ks' in the operand constraints.
;;
;; `g' Any register, memory or immediate integer operand is allowed,
;;     except for registers that are not general registers.
;;
;; `X' Any operand whatsoever is allowed, even if it does not satisfy
;;     `general_operand'.  This is normally used in the constraint of a
;;     `match_scratch' when certain alternatives will not actually require a
;;     scratch register.
;;
;; `0' Match operand 0.
;; `1' Match operand 1.
;; `2' Match operand 2.
;; `3' Match operand 3.
;; `4' Match operand 4.
;; `5' Match operand 5.
;; `6' Match operand 6.
;; `7' Match operand 7.
;; `8' Match operand 8.
;; `9' Match operand 9.
;;
;;     An operand that matches the specified operand number is allowed.  If a
;;     digit is used together with letters within the same alternative, the
;;     digit should come last.
;;
;;     This is called a "matching constraint" and what it really means is that
;;     the assembler has only a single operand that fills two roles considered
;;     separate in the RTL insn.  For example, an add insn has two input
;;     operands and one output operand in the RTL, but on most CISC machines an
;;     add instruction really has only two operands, one of them an
;;     input-output operand:
;;
;;          addl #35,r12
;;
;;     Matching constraints are used in these circumstances.  More precisely,
;;     the two operands that match must include one input-only operand and one
;;     output-only operand.  Moreover, the digit must be a smaller number than
;;     the number of the operand that uses it in the constraint.
;;
;;     For operands to match in a particular case usually means that they are
;;     identical-looking RTL expressions.  But in a few special cases specific
;;     kinds of dissimilarity are allowed.  For example, `*x' as an input
;;     operand will match `*x++' as an output operand.  For proper results in
;;     such cases, the output template should always use the output-operand's
;;     number when printing the operand.
;;
;; `p' An operand that is a valid memory address is allowed.  This is for
;;     "load address" and "push address" instructions.
;;
;;     `p' in the constraint must be accompanied by `address_operand' as the
;;     predicate in the `match_operand'.  This predicate interprets the mode
;;     specified in the `match_operand' as the mode of the memory reference for
;;     which the address would be valid.
;;
;; `Q` First non constant, non register machine-dependent insns
;; `R` Second non constant, non register machine-dependent insns
;; `S` Third non constant, non register machine-dependent insns
;; `T` Fourth non constant, non register machine-dependent insns
;; `U` Fifth non constant, non register machine-dependent insns
;;
;;     Letters in the range `Q' through `U' may be defined in a
;;     machine-dependent fashion to stand for arbitrary operand types.  The
;;     machine description macro `EXTRA_CONSTRAINT' is passed the operand as
;;     its first argument and the constraint letter as its second operand.
;;
;;     A typical use for this would be to distinguish certain types of memory
;;     references that affect other insn operands.
;;
;;     Do not define these constraint letters to accept register references
;;     (`reg'); the reload pass does not expect this and would not handle it
;;     properly.

;; Multiple Alternative Constraints
;; `?' Disparage slightly the alternative that the `?' appears in, as a
;;     choice when no alternative applies exactly.  The compiler regards this
;;     alternative as one unit more costly for each `?' that appears in it.
;;
;; `!' Disparage severely the alternative that the `!' appears in.  This
;;     alternative can still be used if it fits without reloading, but if
;;     reloading is needed, some other alternative will be used.

;; Constraint modifiers
;; `=' Means that this operand is write-only for this instruction: the
;;     previous value is discarded and replaced by output data.
;;
;; `+' Means that this operand is both read and written by the
;;     instruction.
;;
;;     When the compiler fixes up the operands to satisfy the constraints, it
;;     needs to know which operands are inputs to the instruction and which are
;;     outputs from it.  `=' identifies an output; `+' identifies an operand
;;     that is both input and output; all other operands are assumed to be
;;     input only.
;;
;; `&' Means (in a particular alternative) that this operand is written
;;     before the instruction is finished using the input operands.  Therefore,
;;     this operand may not lie in a register that is used as an input operand
;;     or as part of any memory address.
;;
;;     `&' applies only to the alternative in which it is written.  In
;;     constraints with multiple alternatives, sometimes one alternative
;;     requires `&' while others do not.
;;
;;     `&' does not obviate the need to write `='.
;;
;; `%' Declares the instruction to be commutative for this operand and the
;;     following operand.  This means that the compiler may interchange the two
;;     operands if that is the cheapest way to make all operands fit the
;;     constraints.  This is often used in patterns for addition instructions
;;     that really have only two operands: the result must go in one of the
;;     arguments.
;;
;; `#' Says that all following characters, up to the next comma, are to be
;;     ignored as a constraint.  They are significant only for choosing
;;     register preferences.
;;
;; `*' Says that the following character should be ignored when choosing
;;     register preferences.  `*' has no effect on the meaning of the
;;     constraint as a constraint, and no effect on reloading.


;; ::::::::::::::::::::
;; ::
;; :: Attributes
;; ::
;; ::::::::::::::::::::

;; The `define_attr' expression is used to define each attribute required by
;; the target machine.  It looks like:
;;
;; (define_attr NAME LIST-OF-VALUES DEFAULT)

;; NAME is a string specifying the name of the attribute being defined.

;; LIST-OF-VALUES is either a string that specifies a comma-separated list of
;; values that can be assigned to the attribute, or a null string to indicate
;; that the attribute takes numeric values.

;; DEFAULT is an attribute expression that gives the value of this attribute
;; for insns that match patterns whose definition does not include an explicit
;; value for this attribute.

;; For each defined attribute, a number of definitions are written to the
;; `insn-attr.h' file.  For cases where an explicit set of values is specified
;; for an attribute, the following are defined:

;; * A `#define' is written for the symbol `HAVE_ATTR_NAME'.
;;
;; * An enumeral class is defined for `attr_NAME' with elements of the
;;   form `UPPER-NAME_UPPER-VALUE' where the attribute name and value are first
;;   converted to upper case.
;;
;; * A function `get_attr_NAME' is defined that is passed an insn and
;;   returns the attribute value for that insn.

;; For example, if the following is present in the `md' file:
;;
;; (define_attr "type" "branch,fp,load,store,arith" ...)
;;
;; the following lines will be written to the file `insn-attr.h'.
;;
;; #define HAVE_ATTR_type
;; enum attr_type {TYPE_BRANCH, TYPE_FP, TYPE_LOAD, TYPE_STORE, TYPE_ARITH};
;; extern enum attr_type get_attr_type ();

;; If the attribute takes numeric values, no `enum' type will be defined and
;; the function to obtain the attribute's value will return `int'.

(define_attr "length" "" (const_int 4))

;; Processor type -- this attribute must exactly match the processor_type
;; enumeration in frv-protos.h.

(define_attr "cpu" "generic,fr500,fr400,fr300,simple,tomcat"
  (const (symbol_ref "frv_cpu_type")))

;; Attribute is "yes" for branches and jumps that span too great a distance
;; to be implemented in the most natural way.  Such instructions will use
;; a call instruction in some way.

(define_attr "far_jump" "yes,no" (const_string "no"))

;; Instruction type

;; The table below summarises the types of media instruction and their
;; scheduling classification.  Headings are:

;; Type:	the name of the define_attr type
;; Conditions:	"yes" if conditional variants are available
;; FR500:	Fujitsu's categorisation for the FR500
;; FR400:	Fujitsu's categorisation for the FR400 (but see below).

;; On the FR400, media instructions are divided into 2 broad categories.
;; Category 1 instructions can execute in either the M0 or M1 unit and can
;; execute in parallel with other category 1 instructions.  Category 2
;; instructions must use the M0 unit, and therefore cannot run in parallel
;; with other media instructions.

;; The FR400 documentation also divides media instructions into one of seven
;; categories (m1 to m7).  m1 to m4 contain both Category 1 and Category 2
;; instructions, so we use a combination of the categories here.

;; Type		Conditional	FR500	FR400
;; ----		----------	-----	-----
;; mlogic	yes		m1	m1:1
;; mrdacc	no		m2	m4:1
;; mwtacc	no		m3	m5:1
;; maveh	no		m1	m1:1
;; msath	no		m1	m1:1
;; maddh	yes		m1	m1:1
;; mqaddh	yes		m1	m1:2
;; mpackh	no		m2	m3:1
;; munpackh	no		m2	m3:2
;; mdpackh	no		m5	m3:2
;; mbhconv	yes		m2	m3:2
;; mrot		no		m2	m3:1
;; mshift	no		m2	m3:1
;; mexpdhw	yes		m2	m3:1
;; mexpdhd	yes		m2	m3:2
;; mwcut	no		m2	m3:2
;; mmulh	yes		m4	m2:1
;; mmulxh	no		m4	m2:1
;; mmach	yes		m4	m2:1
;; mmrdh	no		m4	m2:1
;; mqmulh	yes		m4	m2:2
;; mqmulxh	no		m4	m2:2
;; mqmach	yes		m4	m2:2
;; mcpx		yes		m4	m2:1
;; mqcpx	yes		m4	m2:2
;; mcut		no		m2	m4:1
;; mclracc	no		m3	m4:1
;; mclracca	no		m6	m4:2
;; mdunpackh	no		m2	n/a
;; mbhconve	no		m2	n/a
;; maddacc	no		n/a	m2:1
;; mdaddacc	no		n/a	m2:2
;; mabsh	no		n/a	m1:1
;; mdrot	no		n/a	m3:2
;; mcpl		no		n/a	m3:2
;; mdcut	no		n/a	m4:2
;; mqsath	no		n/a	m1:2
;; mset		no		n/a	m1:1

(define_attr "type"
  "int,sethi,setlo,mul,div,gload,gstore,fload,fstore,movfg,movgf,branch,jump,jumpl,call,spr,trap,fsconv,fsadd,fsmul,fmas,fsdiv,sqrt_single,fdconv,fdadd,fdmul,fddiv,sqrt_double,mlogic,maveh,msath,maddh,mqaddh,mpackh,munpackh,mdpackh,mbhconv,mrot,mshift,mexpdhw,mexpdhd,mwcut,mmulh,mmulxh,mmach,mmrdh,mqmulh,mqmulxh,mqmach,mcpx,mqcpx,mcut,mclracc,mclracca,mdunpackh,mbhconve,mrdacc,mwtacc,maddacc,mdaddacc,mabsh,mdrot,mcpl,mdcut,mqsath,mset,m7,ccr,multi,unknown"
  (const_string "unknown"))



/* This is description of pipeline hazards based on DFA.  The
   following constructions can be used for this:

   o define_cpu_unit string [string]) describes a cpu functional unit
     (separated by comma).

     1st operand: Names of cpu function units.
     2nd operand: Name of automaton (see comments for
     DEFINE_AUTOMATON).

     All define_reservations and define_cpu_units should have unique
     names which can not be "nothing".

   o (exclusion_set string string) means that each CPU function unit
     in the first string can not be reserved simultaneously with each
     unit whose name is in the second string and vise versa.  CPU
     units in the string are separated by commas. For example, it is
     useful for description CPU with fully pipelined floating point
     functional unit which can execute simultaneously only single
     floating point insns or only double floating point insns.

   o (presence_set string string) means that each CPU function unit in
     the first string can not be reserved unless at least one of units
     whose names are in the second string is reserved.  This is an
     asymmetric relation.  CPU units in the string are separated by
     commas.  For example, it is useful for description that slot1 is
     reserved after slot0 reservation for a VLIW processor.

   o (absence_set string string) means that each CPU function unit in
     the first string can not be reserved only if each unit whose name
     is in the second string is not reserved.  This is an asymmetric
     relation (actually exclusion set is analogous to this one but it
     is symmetric).  CPU units in the string are separated by commas.
     For example, it is useful for description that slot0 can not be
     reserved after slot1 or slot2 reservation for a VLIW processor.

   o (define_bypass number out_insn_names in_insn_names) names bypass with
     given latency (the first number) from insns given by the first
     string (see define_insn_reservation) into insns given by the
     second string.  Insn names in the strings are separated by
     commas.

   o (define_automaton string) describes names of an automaton
     generated and used for pipeline hazards recognition.  The names
     are separated by comma.  Actually it is possibly to generate the
     single automaton but unfortunately it can be very large.  If we
     use more one automata, the summary size of the automata usually
     is less than the single one.  The automaton name is used in
     define_cpu_unit.  All automata should have unique names.

   o (define_reservation string string) names reservation (the first
     string) of cpu functional units (the 2nd string).  Sometimes unit
     reservations for different insns contain common parts.  In such
     case, you describe common part and use one its name (the 1st
     parameter) in regular expression in define_insn_reservation.  All
     define_reservations, define results and define_cpu_units should
     have unique names which can not be "nothing".

   o (define_insn_reservation name default_latency condition regexpr)
     describes reservation of cpu functional units (the 3nd operand)
     for instruction which is selected by the condition (the 2nd
     parameter).  The first parameter is used for output of debugging
     information.  The reservations are described by a regular
     expression according the following syntax:

       regexp = regexp "," oneof
              | oneof

       oneof = oneof "|" allof
             | allof

       allof = allof "+" repeat
             | repeat

       repeat = element "*" number
              | element

       element = cpu_function_name
               | reservation_name
               | result_name
               | "nothing"
               | "(" regexp ")"

       1. "," is used for describing start of the next cycle in
          reservation.

       2. "|" is used for describing the reservation described by the
          first regular expression *or* the reservation described by
          the second regular expression *or* etc.

       3. "+" is used for describing the reservation described by the
          first regular expression *and* the reservation described by
          the second regular expression *and* etc.

       4. "*" is used for convinience and simply means sequence in
          which the regular expression are repeated NUMBER times with
          cycle advancing (see ",").

       5. cpu function unit name which means reservation.

       6. reservation name -- see define_reservation.

       7. string "nothing" means no units reservation.

*/

(define_automaton "nodiv, idiv, div")

;; An FR500 packet can contain a single control instruction or a sequence
;; of up to four operations matching the regular expression:

;;	(I FM? I? FM? | FM? FM?) B? B?

;; where I denotes an integer operation, FM a floating-point or media
;; operation, and B a branch operation.  There are two units for each type
;; of instruction: I0 and I1, FM0 and FM1, and B0 and B1.  Units are
;; allocated left-to-right: the first integer instruction uses I0, the
;; second uses I1, and so on.

;; The FR400 is similar to the FR500 except that it allows only 2 operations
;; per packet and has only one branch unit.  We can use the FR500 conflict
;; description for the FR400, but need to define different cpu_units
;; later.

;; Slot/unit combinations available on the FR400 and above:
(define_cpu_unit "sl0_i0, sl0_fm0, sl0_b0, sl0_c" "nodiv")
(define_cpu_unit "sl1_fm0, sl1_i1, sl1_fm1, sl1_b0" "nodiv")

;; These are available on the FR500 and above:
(define_cpu_unit "sl1_b1" "nodiv")
(define_cpu_unit "sl2_i1, sl2_fm1, sl2_b0, sl2_b1" "nodiv")
(define_cpu_unit "sl3_fm1, sl3_b0, sl3_b1"  "nodiv")

;; The following describes conlicts by slots
;; slot0
(exclusion_set "sl0_i0"  "sl0_fm0,sl0_b0,sl0_c")
(exclusion_set "sl0_fm0" "sl0_b0,sl0_c")
(exclusion_set "sl0_b0"  "sl0_c")

;; slot1
(exclusion_set "sl1_fm0" "sl1_i1,sl1_fm1,sl1_b0,sl1_b1")
(exclusion_set "sl1_i1"  "sl1_fm1,sl1_b0,sl1_b1")
(exclusion_set "sl1_fm1" "sl1_b0,sl1_b1")
(exclusion_set "sl1_b0"  "sl1_b1")

;; slot2
(exclusion_set "sl2_i1"  "sl2_fm1,sl2_b0,sl2_b1")
(exclusion_set "sl2_fm1" "sl2_b0,sl2_b1")
(exclusion_set "sl2_b0"  "sl2_b1")

;; slot3
(exclusion_set "sl3_fm1" "sl3_b0,sl3_b1")
(exclusion_set "sl3_b0"  "sl3_b1")

;; The following describes conlicts by units
;; fm0
(exclusion_set "sl0_fm0" "sl1_fm0")

;; b0
(exclusion_set "sl0_b0"  "sl1_b0,sl2_b0,sl3_b0")
(exclusion_set "sl1_b0"  "sl2_b0,sl3_b0")
(exclusion_set "sl2_b0"  "sl3_b0")

;; i1
(exclusion_set "sl1_i1"  "sl2_i1")

;; fm1
(exclusion_set "sl1_fm1" "sl2_fm1,sl3_fm1")
(exclusion_set "sl2_fm1" "sl3_fm1")

;; b1
(exclusion_set "sl1_b1"  "sl2_b1,sl3_b1")
(exclusion_set "sl2_b1"  "sl3_b1")

;; The following describes remaining combinations of conflicts
;; slot0
(exclusion_set "sl0_i0"  "sl1_fm1,sl1_b1")
(exclusion_set "sl0_fm0" "sl1_i1,sl1_b1,sl2_i1,sl2_fm1,sl3_fm1,sl3_b0")
(exclusion_set "sl0_b0"  "sl1_fm0,sl1_i1,sl1_fm1,sl2_i1,sl2_fm1,sl2_b1,\
                          sl3_fm1,sl3_b1")
(exclusion_set "sl0_c"   "sl1_fm0,sl1_i1,sl1_fm1,sl1_b0,sl1_b1,sl2_i1,sl2_fm1,\
                          sl2_b0,sl2_b1,sl3_fm1,sl3_b0,sl3_b1")


;; slot1
(exclusion_set "sl1_fm0" "sl2_b1")
(exclusion_set "sl1_i1"  "sl2_fm1,sl2_b1,sl3_fm1,sl3_b0")
(exclusion_set "sl1_fm1" "sl2_i1,sl2_b1,sl3_b0")
(exclusion_set "sl1_b0"  "sl2_i1,sl2_fm1,sl3_fm1,sl3_b1")
(exclusion_set "sl1_b1"  "sl2_i1,sl2_fm1,sl2_b0,sl3_fm1,sl3_b0")

;; slot2
(exclusion_set "sl2_i1"  "sl3_b1")
(exclusion_set "sl2_fm1" "sl3_b1")
(exclusion_set "sl2_b0"  "sl3_fm1")
(exclusion_set "sl2_b1"  "sl3_fm1,sl3_b0")

;; slot3
(exclusion_set "sl1_fm0" "sl2_i1,sl2_fm1,sl2_b0,sl2_b1,sl3_fm1,sl3_b0,sl3_b1")
(exclusion_set "sl3_fm1" "sl2_i1,sl2_fm1,sl2_b0,sl2_b1,sl3_b0,sl3_b1")

;; ::::::::::::::::::::
;; ::
;; :: Generic/FR500 scheduler description
;; ::
;; ::::::::::::::::::::

;; Define reservation in order to describe only in terms of units.

(define_reservation "i0" "sl0_i0")
(define_reservation "f0" "sl0_fm0|sl1_fm0")
(define_reservation "m0" "f0")
(define_reservation "b0" "sl0_b0|sl1_b0|sl2_b0|sl3_b0")
(define_reservation "c"  "sl0_c")
(define_reservation "i1" "sl1_i1|sl2_i1")
(define_reservation "f1" "sl1_fm1|sl2_fm1|sl3_fm1")
(define_reservation "m1" "f1")
(define_reservation "b1" "sl1_b1|sl2_b1|sl3_b1")

;; Integer insns
;; It is not possibly to issue load & store in one VLIW insn.
(define_cpu_unit "idiv1" "idiv")
(define_cpu_unit "idiv2" "idiv")
(define_cpu_unit "l0"    "nodiv")
(define_cpu_unit "l1"    "nodiv")
(define_cpu_unit "s0"    "nodiv")

(exclusion_set "l1,l0" "s0")

;; We set the default_latency of sethi to be 0 to allow sethi and setlo to be
;; combined in the same VLIW instruction as allowed by the architecture.  This
;; assumes the only use of sethi is always followed by a setlo of the same
;; register.
(define_insn_reservation "i1_sethi" 0
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "sethi"))
  "i0|i1")

(define_insn_reservation "i1_setlo" 1
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "setlo"))
  "i0|i1")

(define_insn_reservation "i1_int" 1
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "int"))
  "i0|i1")

(define_insn_reservation "i1_mul" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "mul"))
  "i0|i1")

(define_insn_reservation "i1_div" 19
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "div"))
  "(i0|i1),(idiv1*18|idiv2*18)")

(define_insn_reservation "i2_gload" 4
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "gload"))
  "(i0|i1)+(l0|l1)")

(define_insn_reservation "i2_fload" 4
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "fload"))
  "(i0|i1)+(l0|l1)")

(define_insn_reservation "i3_gstore" 0
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "gstore"))
  "i0+s0")

(define_insn_reservation "i3_fstore" 0
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "fstore"))
  "i0+s0")

(define_insn_reservation "i4_move_gf" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "movgf"))
  "i0")

(define_insn_reservation "i4_move_fg" 3 
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "movfg"))
  "i0")

(define_insn_reservation "i5" 0
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "jumpl"))
  "i0")

;; Clear/commit is not generated now:
(define_insn_reservation "i6" 0 (const_int 0) "i0|i1")

;;
;; Branch-instructions
;;
(define_insn_reservation "b1/b3" 0
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "jump,branch,ccr"))
  "b0|b1")

;; The following insn is not generated now.

(define_insn_reservation "b2" 0 (const_int 0) "b0")

(define_insn_reservation "b4" 0
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "call"))
  "b0")

;; The following insns are not generated now.
(define_insn_reservation "b5" 0 (const_int 0) "b0|b1")
(define_insn_reservation "b6" 0 (const_int 0) "b0|b1")

;; Control insns
(define_insn_reservation "trap" 0
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "trap"))
  "c")

(define_insn_reservation "control" 0
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "spr"))
  "c")

;; Floating point insns
(define_cpu_unit "add0" "nodiv")
(define_cpu_unit "add1" "nodiv")
(define_cpu_unit "mul0" "nodiv")
(define_cpu_unit "mul1" "nodiv")
(define_cpu_unit "div1" "div")
(define_cpu_unit "div2" "div")
(define_cpu_unit "root" "div")

(define_bypass 4 "f1" "m1,m2,m3,m4,m5,m6,m7")
(define_insn_reservation "f1" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "fsconv,fdconv"))
  "(f0|f1)")

(define_bypass 4 "f2" "m1,m2,m3,m4,m5,m6,m7")
(define_insn_reservation "f2" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "fsadd,fdadd"))
  "(f0|f1)+(add0|add1)")

(define_bypass 4 "f3" "m1,m2,m3,m4,m5,m6,m7")
(define_insn_reservation "f3" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "fsmul,fdmul"))
  "(f0|f1)+(mul0|mul1)")

(define_bypass 11 "f4_div" "m1,m2,m3,m4,m5,m6,m7")
(define_insn_reservation "f4_div" 10
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "fsdiv,fddiv"))
  "(f0|f1),(div1*9|div2*9)")

(define_bypass 16 "f4_root" "m1,m2,m3,m4,m5,m6,m7")
(define_insn_reservation "f4_root" 15
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "sqrt_single,sqrt_double"))
  "(f0|f1)+root*15")

(define_bypass 4 "f5" "m1,m2,m3,m4,m5,m6,m7")
(define_insn_reservation "f5" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "fmas"))
  "(f0|f1)+(add0|add1)+(mul0|mul1)")

;; The following insns are not generated by gcc now:
(define_insn_reservation "f6" 0 (const_int 0) "(f0|f1)+add0+add1")
(define_insn_reservation "f7" 0 (const_int 0) "(f0|f1)+mul0+mul1")

;; Media insns.  Now they are all not generated now.
(define_cpu_unit "m1_0" "nodiv")
(define_cpu_unit "m1_1" "nodiv")
(define_cpu_unit "m2_0" "nodiv")
(define_cpu_unit "m2_1" "nodiv")
(define_cpu_unit "m3_0" "nodiv")
(define_cpu_unit "m3_1" "nodiv")
(define_cpu_unit "m4_0" "nodiv")
(define_cpu_unit "m4_1" "nodiv")
(define_cpu_unit "m5"   "nodiv")
(define_cpu_unit "m6"   "nodiv")
(define_cpu_unit "m7"   "nodiv")

(exclusion_set "m5,m6,m7" "m2_0,m2_1,m3_0,m3_1")
(exclusion_set "m5"       "m6,m7")
(exclusion_set "m6"       "m4_0,m4_1,m7")
(exclusion_set "m7"       "m1_0,m1_1,add0,add1,mul0,mul1")

(define_bypass 2 "m1" "m1,m2,m3,m4,m5,m6,m7")
(define_bypass 4 "m1" "f1,f2,f3,f4_div,f4_root,f5,f6,f7")
(define_insn_reservation "m1" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "mlogic,maveh,msath,maddh,mqaddh"))
  "(m0|m1)+(m1_0|m1_1)")

(define_bypass 2 "m2" "m1,m2,m3,m4,m5,m6,m7")
(define_bypass 4 "m2" "f1,f2,f3,f4_div,f4_root,f5,f6,f7")
(define_insn_reservation "m2" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "mrdacc,mpackh,munpackh,mbhconv,mrot,mshift,mexpdhw,mexpdhd,mwcut,mcut,mdunpackh,mbhconve"))
  "(m0|m1)+(m2_0|m2_1)")

(define_bypass 1 "m3" "m4")
(define_insn_reservation "m3" 2
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "mclracc,mwtacc"))
  "(m0|m1)+(m3_0|m3_1)")

(define_bypass 1 "m4" "m4")
(define_insn_reservation "m4" 2
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "mmulh,mmulxh,mmach,mmrdh,mqmulh,mqmulxh,mqmach,mcpx,mqcpx"))
  "(m0|m1)+(m4_0|m4_1)")

(define_bypass 2 "m5" "m1,m2,m3,m4,m5,m6,m7")
(define_bypass 4 "m5" "f1,f2,f3,f4_div,f4_root,f5,f6,f7")
(define_insn_reservation "m5" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "mdpackh"))
  "(m0|m1)+m5")

(define_bypass 1 "m6" "m4")
(define_insn_reservation "m6" 2
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "mclracca"))
  "(m0|m1)+m6")

(define_bypass 2 "m7" "m1,m2,m3,m4,m5,m6,m7")
(define_bypass 4 "m7" "f1,f2,f3,f4_div,f4_root,f5,f6,f7")

(define_insn_reservation "m7" 3
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "m7"))
  "(m0|m1)+m7")

;; Unknown & multi insns starts on new cycle and the next insn starts
;; on new cycle.  To describe this we consider as a control insn.
(define_insn_reservation "unknown" 1
  (and (eq_attr "cpu" "generic,fr500,tomcat")
       (eq_attr "type" "unknown,multi"))
  "c")

;; ::::::::::::::::::::
;; ::
;; :: FR400 scheduler description
;; ::
;; ::::::::::::::::::::

;; Category 2 media instructions use both media units, but can be packed
;; with non-media instructions.  Use fr400_m1unit to claim the M1 unit
;; without claiming a slot.

(define_cpu_unit "fr400_m1unit" "nodiv")

(define_reservation "fr400_i0"      "sl0_i0")
(define_reservation "fr400_i1"      "sl1_i1")
(define_reservation "fr400_m0"      "sl0_fm0|sl1_fm0")
(define_reservation "fr400_m1"      "sl1_fm1")
(define_reservation "fr400_meither" "fr400_m0|(fr400_m1+fr400_m1unit)")
(define_reservation "fr400_mboth"   "fr400_m0+fr400_m1unit")
(define_reservation "fr400_b"       "sl0_b0|sl1_b0")
(define_reservation "fr400_c"       "sl0_c")

;; Name		Class	Units	Latency
;; ====	        =====	=====	=======
;; int		I1	I0/I1	1
;; sethi	I1	I0/I1	0       -- does not interfere with setlo
;; setlo	I1	I0/I1	1
;; mul		I1	I0	3  (*)
;; div		I1	I0	20 (*)
;; gload	I2	I0	4  (*)
;; fload	I2	I0	4       -- only 3 if read by a media insn
;; gstore	I3	I0	0       -- provides no result
;; fstore	I3	I0	0       -- provides no result
;; movfg	I4	I0	3  (*)
;; movgf	I4	I0	3  (*)
;; jumpl	I5	I0	0       -- provides no result
;;
;; (*) The results of these instructions can be read one cycle earlier
;; than indicated.  The penalty given is for instructions with write-after-
;; write dependencies.

;; The FR400 can only do loads and stores in I0, so we there's no danger
;; of memory unit collision in the same packet.  There's only one divide
;; unit too.

(define_insn_reservation "fr400_i1_int" 1
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "int"))
  "fr400_i0|fr400_i1")

(define_insn_reservation "fr400_i1_sethi" 0
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "sethi"))
  "fr400_i0|fr400_i1")

(define_insn_reservation "fr400_i1_setlo" 1
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "setlo"))
  "fr400_i0|fr400_i1")

(define_insn_reservation "fr400_i1_mul" 3
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "mul"))
  "fr400_i0")

(define_insn_reservation "fr400_i1_div" 20
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "div"))
  "fr400_i0+idiv1*19")

(define_insn_reservation "fr400_i2_gload" 4
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "gload"))
  "fr400_i0")

(define_insn_reservation "fr400_i2_fload" 4
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "fload"))
  "fr400_i0")

(define_insn_reservation "fr400_i3_gstore" 0
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "gstore"))
  "fr400_i0")

(define_insn_reservation "fr400_i3_fstore" 0
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "fstore"))
  "fr400_i0")

(define_insn_reservation "fr400_i4_movfg" 3
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "movfg"))
  "fr400_i0")

(define_insn_reservation "fr400_i4_movgf" 3
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "movgf"))
  "fr400_i0")

(define_insn_reservation "fr400_i5_jumpl" 0
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "jumpl"))
  "fr400_i0")

;; The bypass between FPR loads and media instructions, described above.

(define_bypass 3
  "fr400_i2_fload"
  "fr400_m1_1,fr400_m1_2,\
   fr400_m2_1,fr400_m2_2,\
   fr400_m3_1,fr400_m3_2,\
   fr400_m4_1,fr400_m4_2,\
   fr400_m5")

;; The branch instructions all use the B unit and produce no result.

(define_insn_reservation "fr400_b" 0
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "jump,branch,ccr,call"))
  "fr400_b")

;; Control instructions use the C unit, which excludes all the others.

(define_insn_reservation "fr400_c" 0
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "spr,trap"))
  "fr400_c")

;; Unknown instructions use the C unit, since it requires single-operation
;; packets.

(define_insn_reservation "fr400_unknown" 1
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "unknown,multi"))
  "fr400_c")

;; FP->FP moves are marked as "fsconv" instructions in the define_insns
;; below, but are implemented on the FR400 using "mlogic" instructions.
;; It's easier to class "fsconv" as a "m1:1" instruction than provide
;; separate define_insns for the FR400.

;; M1 instructions store their results in FPRs.  Any instruction can read
;; the result in the following cycle, so no penalty occurs.

(define_insn_reservation "fr400_m1_1" 1
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "fsconv,mlogic,maveh,msath,maddh,mabsh,mset"))
  "fr400_meither")

(define_insn_reservation "fr400_m1_2" 1
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "mqaddh,mqsath"))
  "fr400_mboth")

;; M2 instructions store their results in accumulators, which are read
;; by M2 or M4 media commands.  M2 instructions can read the results in
;; the following cycle, but M4 instructions must wait a cycle more.

(define_bypass 1
  "fr400_m2_1,fr400_m2_2"
  "fr400_m2_1,fr400_m2_2")

(define_insn_reservation "fr400_m2_1" 2
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "mmulh,mmulxh,mmach,mmrdh,mcpx,maddacc"))
  "fr400_meither")

(define_insn_reservation "fr400_m2_2" 2
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "mqmulh,mqmulxh,mqmach,mqcpx,mdaddacc"))
  "fr400_mboth")

;; For our purposes, there seems to be little real difference between
;; M1 and M3 instructions.  Keep them separate anyway in case the distinction
;; is needed later.

(define_insn_reservation "fr400_m3_1" 1
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "mpackh,mrot,mshift,mexpdhw"))
  "fr400_meither")

(define_insn_reservation "fr400_m3_2" 1
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "munpackh,mdpackh,mbhconv,mexpdhd,mwcut,mdrot,mcpl"))
  "fr400_mboth")

;; M4 instructions write to accumulators or FPRs.  MOVFG and STF
;; instructions can read an FPR result in the following cycle, but
;; M-unit instructions must wait a cycle more for either kind of result.

(define_bypass 1
  "fr400_m4_1,fr400_m4_2"
  "fr400_i3_fstore,fr400_i4_movfg")

(define_insn_reservation "fr400_m4_1" 2
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "mrdacc,mcut,mclracc"))
  "fr400_meither")

(define_insn_reservation "fr400_m4_2" 2
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "mclracca,mdcut"))
  "fr400_mboth")

;; M5 instructions always incur a 1-cycle penalty.

(define_insn_reservation "fr400_m5" 2
  (and (eq_attr "cpu" "fr400")
       (eq_attr "type" "mwtacc"))
  "fr400_mboth")

;; ::::::::::::::::::::
;; ::
;; :: Simple/FR300 scheduler description
;; ::
;; ::::::::::::::::::::

;; Fr300 or simple processor.  To describe it as 1 insn issue
;; processor, we use control unit.

(define_insn_reservation "fr300_lat1" 1
  (and (eq_attr "cpu" "fr300,simple")
       (eq_attr "type" "!gload,fload,movfg,movgf"))
  "c")

(define_insn_reservation "fr300_lat2" 2
  (and (eq_attr "cpu" "fr300,simple")
       (eq_attr "type" "gload,fload,movfg,movgf"))
  "c")


;; ::::::::::::::::::::
;; ::
;; :: Delay Slots
;; ::
;; ::::::::::::::::::::

;; The insn attribute mechanism can be used to specify the requirements for
;; delay slots, if any, on a target machine.  An instruction is said to require
;; a "delay slot" if some instructions that are physically after the
;; instruction are executed as if they were located before it.  Classic
;; examples are branch and call instructions, which often execute the following
;; instruction before the branch or call is performed.

;; On some machines, conditional branch instructions can optionally "annul"
;; instructions in the delay slot.  This means that the instruction will not be
;; executed for certain branch outcomes.  Both instructions that annul if the
;; branch is true and instructions that annul if the branch is false are
;; supported.

;; Delay slot scheduling differs from instruction scheduling in that
;; determining whether an instruction needs a delay slot is dependent only
;; on the type of instruction being generated, not on data flow between the
;; instructions.  See the next section for a discussion of data-dependent
;; instruction scheduling.

;; The requirement of an insn needing one or more delay slots is indicated via
;; the `define_delay' expression.  It has the following form:
;;
;; (define_delay TEST
;;   [DELAY-1 ANNUL-TRUE-1 ANNUL-FALSE-1
;;    DELAY-2 ANNUL-TRUE-2 ANNUL-FALSE-2
;;    ...])

;; TEST is an attribute test that indicates whether this `define_delay' applies
;; to a particular insn.  If so, the number of required delay slots is
;; determined by the length of the vector specified as the second argument.  An
;; insn placed in delay slot N must satisfy attribute test DELAY-N.
;; ANNUL-TRUE-N is an attribute test that specifies which insns may be annulled
;; if the branch is true.  Similarly, ANNUL-FALSE-N specifies which insns in
;; the delay slot may be annulled if the branch is false.  If annulling is not
;; supported for that delay slot, `(nil)' should be coded.

;; For example, in the common case where branch and call insns require a single
;; delay slot, which may contain any insn other than a branch or call, the
;; following would be placed in the `md' file:

;; (define_delay (eq_attr "type" "branch,call")
;;		 [(eq_attr "type" "!branch,call") (nil) (nil)])

;; Multiple `define_delay' expressions may be specified.  In this case, each
;; such expression specifies different delay slot requirements and there must
;; be no insn for which tests in two `define_delay' expressions are both true.

;; For example, if we have a machine that requires one delay slot for branches
;; but two for calls, no delay slot can contain a branch or call insn, and any
;; valid insn in the delay slot for the branch can be annulled if the branch is
;; true, we might represent this as follows:

;; (define_delay (eq_attr "type" "branch")
;;   [(eq_attr "type" "!branch,call")
;;    (eq_attr "type" "!branch,call")
;;    (nil)])
;;
;; (define_delay (eq_attr "type" "call")
;;   [(eq_attr "type" "!branch,call") (nil) (nil)
;;    (eq_attr "type" "!branch,call") (nil) (nil)])

;; Note - it is the backend's responsibility to fill any unfilled delay slots
;; at assembler generation time.  This is usually done by adding a special print
;; operand to the delayed insrtuction, and then in the PRINT_OPERAND function
;; calling dbr_sequence_length() to determine how many delay slots were filled.
;; For example:
;;
;; --------------<machine>.md-----------------
;; (define_insn "call"
;;  [(call (match_operand 0 "memory_operand" "m")
;;         (match_operand 1 "" ""))]
;;   ""
;;   "call_delayed %0,%1,%2%#"
;;  [(set_attr "length" "4")
;;   (set_attr "type" "call")])
;;
;; -------------<machine>.h-------------------
;; #define PRINT_OPERAND_PUNCT_VALID_P(CODE) (CODE == '#')
;;
;;  ------------<machine>.c------------------
;; void
;; machine_print_operand (file, x, code)
;;     FILE * file;
;;     rtx    x;
;;     int    code;
;; {
;;   switch (code)
;;   {
;;   case '#':
;;     if (dbr_sequence_length () == 0)
;;       fputs ("\n\tnop", file);
;;     return;

;; ::::::::::::::::::::
;; ::
;; :: Notes on Patterns
;; ::
;; ::::::::::::::::::::

;; If you need to construct a sequence of assembler instructions in order
;; to implement a pattern be sure to escape any backslashes and double quotes
;; that you use, eg:
;;
;; (define_insn "an example"
;;   [(some rtl)]
;;   ""
;;   "*
;;    { static char buffer [100];
;;      sprintf (buffer, \"insn \\t %d\", REGNO (operands[1]));
;;      return buffer;
;;    }"
;; )
;;
;; Also if there is more than one instruction, they can be separated by \\;
;; which is a space saving synonym for \\n\\t:
;;
;; (define_insn "another example"
;;   [(some rtl)]
;;   ""
;;   "*
;;    { static char buffer [100];
;;      sprintf (buffer, \"insn1 \\t %d\\;insn2 \\t %%1\",
;;        REGNO (operands[1]));
;;      return buffer;
;;    }"
;; )
;;


;; ::::::::::::::::::::
;; ::
;; :: Moves
;; ::
;; ::::::::::::::::::::

;; Wrap moves in define_expand to prevent memory->memory moves from being
;; generated at the RTL level, which generates better code for most machines
;; which can't do mem->mem moves.

;; If operand 0 is a `subreg' with mode M of a register whose own mode is wider
;; than M, the effect of this instruction is to store the specified value in
;; the part of the register that corresponds to mode M.  The effect on the rest
;; of the register is undefined.

;; This class of patterns is special in several ways.  First of all, each of
;; these names *must* be defined, because there is no other way to copy a datum
;; from one place to another.

;; Second, these patterns are not used solely in the RTL generation pass.  Even
;; the reload pass can generate move insns to copy values from stack slots into
;; temporary registers.  When it does so, one of the operands is a hard
;; register and the other is an operand that can need to be reloaded into a
;; register.

;; Therefore, when given such a pair of operands, the pattern must
;; generate RTL which needs no reloading and needs no temporary
;; registers--no registers other than the operands.  For example, if
;; you support the pattern with a `define_expand', then in such a
;; case the `define_expand' mustn't call `force_reg' or any other such
;; function which might generate new pseudo registers.

;; This requirement exists even for subword modes on a RISC machine
;; where fetching those modes from memory normally requires several
;; insns and some temporary registers.  Look in `spur.md' to see how
;; the requirement can be satisfied.

;; During reload a memory reference with an invalid address may be passed as an
;; operand.  Such an address will be replaced with a valid address later in the
;; reload pass.  In this case, nothing may be done with the address except to
;; use it as it stands.  If it is copied, it will not be replaced with a valid
;; address.  No attempt should be made to make such an address into a valid
;; address and no routine (such as `change_address') that will do so may be
;; called.  Note that `general_operand' will fail when applied to such an
;; address.
;;
;; The global variable `reload_in_progress' (which must be explicitly declared
;; if required) can be used to determine whether such special handling is
;; required.
;;
;; The variety of operands that have reloads depends on the rest of
;; the machine description, but typically on a RISC machine these can
;; only be pseudo registers that did not get hard registers, while on
;; other machines explicit memory references will get optional
;; reloads.
;;
;; If a scratch register is required to move an object to or from memory, it
;; can be allocated using `gen_reg_rtx' prior to reload.  But this is
;; impossible during and after reload.  If there are cases needing scratch
;; registers after reload, you must define `SECONDARY_INPUT_RELOAD_CLASS' and
;; perhaps also `SECONDARY_OUTPUT_RELOAD_CLASS' to detect them, and provide
;; patterns `reload_inM' or `reload_outM' to handle them.

;; The constraints on a `moveM' must permit moving any hard register to any
;; other hard register provided that `HARD_REGNO_MODE_OK' permits mode M in
;; both registers and `REGISTER_MOVE_COST' applied to their classes returns a
;; value of 2.

;; It is obligatory to support floating point `moveM' instructions
;; into and out of any registers that can hold fixed point values,
;; because unions and structures (which have modes `SImode' or
;; `DImode') can be in those registers and they may have floating
;; point members.

;; There may also be a need to support fixed point `moveM' instructions in and
;; out of floating point registers.  Unfortunately, I have forgotten why this
;; was so, and I don't know whether it is still true.  If `HARD_REGNO_MODE_OK'
;; rejects fixed point values in floating point registers, then the constraints
;; of the fixed point `moveM' instructions must be designed to avoid ever
;; trying to reload into a floating point register.

(define_expand "movqi"
  [(set (match_operand:QI 0 "general_operand" "")
	(match_operand:QI 1 "general_operand" ""))]
  ""
  "
{
  if (!reload_in_progress
      && !reload_completed
      && !register_operand (operands[0], QImode)
      && !reg_or_0_operand (operands[1], QImode))
    operands[1] = copy_to_mode_reg (QImode, operands[1]);
}")

(define_insn "*movqi_load"
  [(set (match_operand:QI 0 "register_operand" "=d,f")
	(match_operand:QI 1 "frv_load_operand" "m,m"))]
  ""
  "* return output_move_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "gload,fload")])

(define_insn "*movqi_internal"
  [(set (match_operand:QI 0 "move_destination_operand" "=d,d,m,m,?f,?f,?d,?m,f")
	(match_operand:QI 1 "move_source_operand"       "L,d,d,O, d, f, f, f,GO"))]
  "register_operand(operands[0], QImode) || reg_or_0_operand (operands[1], QImode)"
  "* return output_move_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "int,int,gstore,gstore,movgf,fsconv,movfg,fstore,movgf")])

(define_expand "movhi"
  [(set (match_operand:HI 0 "general_operand" "")
	(match_operand:HI 1 "general_operand" ""))]
  ""
  "
{
  if (!reload_in_progress
      && !reload_completed
      && !register_operand (operands[0], HImode)
      && !reg_or_0_operand (operands[1], HImode))
    operands[1] = copy_to_mode_reg (HImode, operands[1]);
}")

(define_insn "*movhi_load"
  [(set (match_operand:HI 0 "register_operand" "=d,f")
	(match_operand:HI 1 "frv_load_operand" "m,m"))]
  ""
  "* return output_move_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "gload,fload")])

(define_insn "*movhi_internal"
  [(set (match_operand:HI 0 "move_destination_operand" "=d,d,d,m,m,?f,?f,?d,?m,f")
	(match_operand:HI 1 "move_source_operand"       "L,i,d,d,O, d, f, f, f,GO"))]
  "register_operand(operands[0], HImode) || reg_or_0_operand (operands[1], HImode)"
  "* return output_move_single (operands, insn);"
  [(set_attr "length" "4,8,4,4,4,4,4,4,4,4")
   (set_attr "type" "int,multi,int,gstore,gstore,movgf,fsconv,movfg,fstore,movgf")])

;; Split 2 word load of constants into sethi/setlo instructions
(define_split
  [(set (match_operand:HI 0 "integer_register_operand" "")
	(match_operand:HI 1 "int_2word_operand" ""))]
  "reload_completed"
  [(set (match_dup 0)
	(high:HI (match_dup 1)))
   (set (match_dup 0)
	(lo_sum:HI (match_dup 0)
		(match_dup 1)))]
  "")

(define_insn "movhi_high"
  [(set (match_operand:HI 0 "integer_register_operand" "=d")
	(high:HI (match_operand:HI 1 "int_2word_operand" "i")))]
  ""
  "sethi #hi(%1), %0"
  [(set_attr "type" "sethi")
   (set_attr "length" "4")])

(define_insn "movhi_lo_sum"
  [(set (match_operand:HI 0 "integer_register_operand" "+d")
	(lo_sum:HI (match_dup 0)
		   (match_operand:HI 1 "int_2word_operand" "i")))]
  ""
  "setlo #lo(%1), %0"
  [(set_attr "type" "setlo")
   (set_attr "length" "4")])

(define_expand "movsi"
  [(set (match_operand:SI 0 "move_destination_operand" "")
	(match_operand:SI 1 "move_source_operand" ""))]
  ""
  "
{
  if (frv_emit_movsi (operands[0], operands[1]))
    DONE;
}")

;; Note - it is best to only have one movsi pattern and to handle
;; all the various contingencies by the use of alternatives.  This
;; allows reload the greatest amount of flexability (since reload will
;; only choose amoungst alternatives for a selected insn, it will not
;; replace the insn with another one).

;; Unfortunately, we do have to separate out load-type moves from the rest,
;; and only allow memory source operands in the former.  If we do memory and
;; constant loads in a single pattern, reload will be tempted to force
;; constants into memory when the destination is a floating-point register.
;; That may make a function use a PIC pointer when it didn't before, and we
;; cannot change PIC usage (and hence stack layout) so late in the game.
;; The resulting sequences for loading cosntants into FPRs are preferable
;; even when we're not generating PIC code.

(define_insn "*movsi_load"
  [(set (match_operand:SI 0 "register_operand" "=d,f")
	(match_operand:SI 1 "frv_load_operand" "m,m"))]
  ""
  "* return output_move_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "gload,fload")])

(define_insn "*movsi_internal"
  [(set (match_operand:SI 0 "move_destination_operand" "=d,d,d,m,m,z,d,d,f,f,m,?f,?z")
	(match_operand:SI 1 "move_source_operand"      "LQ,i,d,d,O,d,z,f,d,f,f,GO,GO"))]
  "register_operand (operands[0], SImode) || reg_or_0_operand (operands[1], SImode)"
  "* return output_move_single (operands, insn);"
  [(set_attr "length" "4,8,4,4,4,4,4,4,4,4,4,4,4")
   (set_attr "type" "int,multi,int,gstore,gstore,spr,spr,movfg,movgf,fsconv,fstore,movgf,spr")])

(define_insn "*movsi_lda_sdata"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(plus:SI (match_operand:SI 1 "small_data_register_operand" "d")
		 (match_operand:SI 2 "small_data_symbolic_operand" "Q")))]
  ""
  "addi %1, #gprel12(%2), %0"
  [(set_attr "type" "int")
   (set_attr "length" "4")])

;; Split 2 word load of constants into sethi/setlo instructions
(define_split
  [(set (match_operand:SI 0 "integer_register_operand" "")
	(match_operand:SI 1 "int_2word_operand" ""))]
  "reload_completed"
  [(set (match_dup 0)
	(high:SI (match_dup 1)))
   (set (match_dup 0)
	(lo_sum:SI (match_dup 0)
		(match_dup 1)))]
  "")

(define_insn "movsi_high"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(high:SI (match_operand:SI 1 "int_2word_operand" "i")))]
  ""
  "sethi #hi(%1), %0"
  [(set_attr "type" "sethi")
   (set_attr "length" "4")])

(define_insn "movsi_lo_sum"
  [(set (match_operand:SI 0 "integer_register_operand" "+d")
	(lo_sum:SI (match_dup 0)
		   (match_operand:SI 1 "int_2word_operand" "i")))]
  ""
  "setlo #lo(%1), %0"
  [(set_attr "type" "setlo")
   (set_attr "length" "4")])

;; Split loads of addresses with PIC specified into 3 separate instructions
(define_insn_and_split "*movsi_pic"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(plus:SI (match_operand:SI 1 "pic_register_operand" "d")
		 (match_operand:SI 2 "pic_symbolic_operand" "")))]
  ""
  "#"
  "reload_completed"
  [(set (match_dup 0)
	(high:SI (match_dup 2)))
   (set (match_dup 0)
	(lo_sum:SI (match_dup 0)
		   (match_dup 2)))
   (set (match_dup 0)
	(plus:SI (match_dup 0) (match_dup 1)))]

  ""
  [(set_attr "type" "multi")
   (set_attr "length" "12")])

(define_insn "movsi_high_pic"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(high:SI (match_operand:SI 1 "pic_symbolic_operand" "")))]
  ""
  "sethi #gprelhi(%1), %0"
  [(set_attr "type" "sethi")
   (set_attr "length" "4")])

(define_insn "movsi_lo_sum_pic"
  [(set (match_operand:SI 0 "integer_register_operand" "+d")
	(lo_sum:SI (match_dup 0)
		   (match_operand:SI 1 "pic_symbolic_operand" "")))]
  ""
  "setlo #gprello(%1), %0"
  [(set_attr "type" "setlo")
   (set_attr "length" "4")])

(define_expand "movdi"
  [(set (match_operand:DI 0 "nonimmediate_operand" "")
	(match_operand:DI 1 "general_operand" ""))]
  ""
  "
{
  if (!reload_in_progress
      && !reload_completed
      && !register_operand (operands[0], DImode)
      && !reg_or_0_operand (operands[1], DImode))
    operands[1] = copy_to_mode_reg (DImode, operands[1]);
}")

(define_insn "*movdi_double"
  [(set (match_operand:DI 0 "move_destination_operand" "=e,?h,??d,??f,R,?R,??m,??m,e,?h,??d,??f,?e,??d,?h,??f,R,m,e,??d,e,??d,?h,??f")
	(match_operand:DI 1 "move_source_operand"      " e,h,d,f,e,h,d,f,R,R,m,m,h,f,e,d,GO,GO,GO,GO,nF,nF,GO,GO"))]
  "TARGET_DOUBLE
   && (register_operand (operands[0], DImode)
       || reg_or_0_operand (operands[1], DImode))"
  "* return output_move_double (operands, insn);"
  [(set_attr "length" "8,4,8,8,4,4,8,8,4,4,8,8,4,8,4,8,4,8,8,8,16,16,8,8")
   (set_attr "type" "multi,fdconv,multi,multi,gstore,fstore,gstore,fstore,gload,fload,gload,fload,movfg,movfg,movgf,movgf,gstore,gstore,multi,multi,multi,multi,movgf,movgf")])

(define_insn "*movdi_nodouble"
  [(set (match_operand:DI 0 "move_destination_operand" "=e,?h,??d,??f,R,?R,??m,??m,e,?h,??d,??f,?e,??d,?h,??f,R,m,e,??d,e,??d,?h,??f")
	(match_operand:DI 1 "move_source_operand"      " e,h,d,f,e,h,d,f,R,R,m,m,h,f,e,d,GO,GO,GO,GO,nF,nF,GO,GO"))]
  "!TARGET_DOUBLE
   && (register_operand (operands[0], DImode)
       || reg_or_0_operand (operands[1], DImode))"
  "* return output_move_double (operands, insn);"
  [(set_attr "length" "8,8,8,8,4,4,8,8,4,4,8,8,8,8,8,8,4,8,8,8,16,16,8,8")
   (set_attr "type" "multi,multi,multi,multi,gstore,fstore,gstore,fstore,gload,fload,gload,fload,movfg,movfg,movgf,movgf,gstore,gstore,multi,multi,multi,multi,movgf,movgf")])

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(match_operand:DI 1 "dbl_memory_two_insn_operand" ""))]
  "reload_completed"
  [(const_int 0)]
  "frv_split_double_load (operands[0], operands[1]);")

(define_split
  [(set (match_operand:DI 0 "odd_reg_operand" "")
	(match_operand:DI 1 "memory_operand" ""))]
  "reload_completed"
  [(const_int 0)]
  "frv_split_double_load (operands[0], operands[1]);")

(define_split
  [(set (match_operand:DI 0 "dbl_memory_two_insn_operand" "")
	(match_operand:DI 1 "reg_or_0_operand" ""))]
  "reload_completed"
  [(const_int 0)]
  "frv_split_double_store (operands[0], operands[1]);")

(define_split
  [(set (match_operand:DI 0 "memory_operand" "")
	(match_operand:DI 1 "odd_reg_operand" ""))]
  "reload_completed"
  [(const_int 0)]
  "frv_split_double_store (operands[0], operands[1]);")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(match_operand:DI 1 "register_operand" ""))]
  "reload_completed
   && (odd_reg_operand (operands[0], DImode)
       || odd_reg_operand (operands[1], DImode)
       || (integer_register_operand (operands[0], DImode)
	   && integer_register_operand (operands[1], DImode))
       || (!TARGET_DOUBLE
	   && fpr_operand (operands[0], DImode)
	   && fpr_operand (operands[1], DImode)))"
  [(set (match_dup 2) (match_dup 4))
   (set (match_dup 3) (match_dup 5))]
  "
{
  rtx op0      = operands[0];
  rtx op0_low  = gen_lowpart (SImode, op0);
  rtx op0_high = gen_highpart (SImode, op0);
  rtx op1      = operands[1];
  rtx op1_low  = gen_lowpart (SImode, op1);
  rtx op1_high = gen_highpart (SImode, op1);

  /* We normally copy the low-numbered register first.  However, if the first
     register operand 0 is the same as the second register of operand 1, we
     must copy in the opposite order.  */

  if (REGNO (op0_high) == REGNO (op1_low))
    {
      operands[2] = op0_low;
      operands[3] = op0_high;
      operands[4] = op1_low;
      operands[5] = op1_high;
    }
  else
    {
      operands[2] = op0_high;
      operands[3] = op0_low;
      operands[4] = op1_high;
      operands[5] = op1_low;
    }
}")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(match_operand:DI 1 "const_int_operand" ""))]
  "reload_completed"
  [(set (match_dup 2) (match_dup 4))
   (set (match_dup 3) (match_dup 1))]
  "
{
  rtx op0 = operands[0];
  rtx op1 = operands[1];

  operands[2] = gen_highpart (SImode, op0);
  operands[3] = gen_lowpart (SImode, op0);
  operands[4] = GEN_INT ((INTVAL (op1) < 0) ? -1 : 0);
}")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(match_operand:DI 1 "const_double_operand" ""))]
  "reload_completed"
  [(set (match_dup 2) (match_dup 4))
   (set (match_dup 3) (match_dup 5))]
  "
{
  rtx op0 = operands[0];
  rtx op1 = operands[1];

  operands[2] = gen_highpart (SImode, op0);
  operands[3] = gen_lowpart (SImode, op0);
  operands[4] = GEN_INT (CONST_DOUBLE_HIGH (op1));
  operands[5] = GEN_INT (CONST_DOUBLE_LOW (op1));
}")

;; Floating Point Moves
;;
;; Note - Patterns for SF mode moves are compulsory, but
;; patterns for DF are optional, as GCC can synthesize them.

(define_expand "movsf"
  [(set (match_operand:SF 0 "general_operand" "")
	(match_operand:SF 1 "general_operand" ""))]
  ""
  "
{
  if (!reload_in_progress
      && !reload_completed
      && !register_operand (operands[0], SFmode)
      && !reg_or_0_operand (operands[1], SFmode))
    operands[1] = copy_to_mode_reg (SFmode, operands[1]);
}")

(define_split
  [(set (match_operand:SF 0 "integer_register_operand" "")
	(match_operand:SF 1 "int_2word_operand" ""))]
  "reload_completed"
  [(set (match_dup 0)
	(high:SF (match_dup 1)))
   (set (match_dup 0)
	(lo_sum:SF (match_dup 0)
		(match_dup 1)))]
  "")

(define_insn "*movsf_load_has_fprs"
  [(set (match_operand:SF 0 "register_operand" "=f,d")
	(match_operand:SF 1 "frv_load_operand" "m,m"))]
  "TARGET_HAS_FPRS"
  "* return output_move_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "fload,gload")])

(define_insn "*movsf_internal_has_fprs"
  [(set (match_operand:SF 0 "move_destination_operand" "=f,f,m,m,?f,?d,?d,m,?d")
	(match_operand:SF 1 "move_source_operand" "f,OG,f,OG,d,f,d,d,F"))]
  "TARGET_HAS_FPRS
   && (register_operand (operands[0], SFmode) || reg_or_0_operand (operands[1], SFmode))"
  "* return output_move_single (operands, insn);"
  [(set_attr "length" "4,4,4,4,4,4,4,4,8")
   (set_attr "type" "fsconv,movgf,fstore,gstore,movgf,movfg,int,gstore,multi")])

;; If we don't support the double instructions, prefer gprs over fprs, since it
;; will all be emulated
(define_insn "*movsf_internal_no_fprs"
  [(set (match_operand:SF 0 "move_destination_operand" "=d,d,m,d,d")
	(match_operand:SF 1 "move_source_operand"      " d,OG,dOG,m,F"))]
  "!TARGET_HAS_FPRS
   && (register_operand (operands[0], SFmode) || reg_or_0_operand (operands[1], SFmode))"
  "* return output_move_single (operands, insn);"
  [(set_attr "length" "4,4,4,4,8")
   (set_attr "type" "int,int,gstore,gload,multi")])

(define_insn "movsf_high"
  [(set (match_operand:SF 0 "integer_register_operand" "=d")
	(high:SF (match_operand:SF 1 "int_2word_operand" "i")))]
  ""
  "sethi #hi(%1), %0"
  [(set_attr "type" "sethi")
   (set_attr "length" "4")])

(define_insn "movsf_lo_sum"
  [(set (match_operand:SF 0 "integer_register_operand" "+d")
	(lo_sum:SF (match_dup 0)
		   (match_operand:SF 1 "int_2word_operand" "i")))]
  ""
  "setlo #lo(%1), %0"
  [(set_attr "type" "setlo")
   (set_attr "length" "4")])

(define_expand "movdf"
  [(set (match_operand:DF 0 "nonimmediate_operand" "")
	(match_operand:DF 1 "general_operand" ""))]
  ""
  "
{
  if (!reload_in_progress
      && !reload_completed
      && !register_operand (operands[0], DFmode)
      && !reg_or_0_operand (operands[1], DFmode))
    operands[1] = copy_to_mode_reg (DFmode, operands[1]);
}")

(define_insn "*movdf_double"
  [(set (match_operand:DF 0 "move_destination_operand" "=h,?e,??f,??d,R,?R,??m,??m,h,?e,??f,??d,?h,??f,?e,??d,R,m,h,??f,e,??d")
	(match_operand:DF 1 "move_source_operand"      " h,e,f,d,h,e,f,d,R,R,m,m,e,d,h,f,GO,GO,GO,GO,GO,GO"))]
  "TARGET_DOUBLE
   && (register_operand (operands[0], DFmode)
       || reg_or_0_operand (operands[1], DFmode))"
  "* return output_move_double (operands, insn);"
  [(set_attr "length" "4,8,8,8,4,4,8,8,4,4,8,8,4,8,4,8,4,8,8,8,8,8")
   (set_attr "type" "fdconv,multi,multi,multi,fstore,gstore,fstore,gstore,fload,gload,fload,gload,movgf,movgf,movfg,movfg,gstore,gstore,movgf,movgf,multi,multi")])

;; If we don't support the double instructions, prefer gprs over fprs, since it
;; will all be emulated
(define_insn "*movdf_nodouble"
  [(set (match_operand:DF 0 "move_destination_operand" "=e,?h,??d,??f,R,?R,??m,??m,e,?h,??d,??f,?e,??d,?h,??f,R,m,e,??d,e,??d,?h,??f")
	(match_operand:DF 1 "move_source_operand"      " e,h,d,f,e,h,d,f,R,R,m,m,h,f,e,d,GO,GO,GO,GO,nF,nF,GO,GO"))]
  "!TARGET_DOUBLE
   && (register_operand (operands[0], DFmode)
       || reg_or_0_operand (operands[1], DFmode))"
  "* return output_move_double (operands, insn);"
  [(set_attr "length" "8,8,8,8,4,4,8,8,4,4,8,8,8,8,8,8,4,8,8,8,16,16,8,8")
   (set_attr "type" "multi,multi,multi,multi,gstore,fstore,gstore,fstore,gload,fload,gload,fload,movfg,movfg,movgf,movgf,gstore,gstore,multi,multi,multi,multi,movgf,movgf")])

(define_split
  [(set (match_operand:DF 0 "register_operand" "")
	(match_operand:DF 1 "dbl_memory_two_insn_operand" ""))]
  "reload_completed"
  [(const_int 0)]
  "frv_split_double_load (operands[0], operands[1]);")

(define_split
  [(set (match_operand:DF 0 "odd_reg_operand" "")
	(match_operand:DF 1 "memory_operand" ""))]
  "reload_completed"
  [(const_int 0)]
  "frv_split_double_load (operands[0], operands[1]);")

(define_split
  [(set (match_operand:DF 0 "dbl_memory_two_insn_operand" "")
	(match_operand:DF 1 "reg_or_0_operand" ""))]
  "reload_completed"
  [(const_int 0)]
  "frv_split_double_store (operands[0], operands[1]);")

(define_split
  [(set (match_operand:DF 0 "memory_operand" "")
	(match_operand:DF 1 "odd_reg_operand" ""))]
  "reload_completed"
  [(const_int 0)]
  "frv_split_double_store (operands[0], operands[1]);")

(define_split
  [(set (match_operand:DF 0 "register_operand" "")
	(match_operand:DF 1 "register_operand" ""))]
  "reload_completed
   && (odd_reg_operand (operands[0], DFmode)
       || odd_reg_operand (operands[1], DFmode)
       || (integer_register_operand (operands[0], DFmode)
	   && integer_register_operand (operands[1], DFmode))
       || (!TARGET_DOUBLE
	   && fpr_operand (operands[0], DFmode)
	   && fpr_operand (operands[1], DFmode)))"
  [(set (match_dup 2) (match_dup 4))
   (set (match_dup 3) (match_dup 5))]
  "
{
  rtx op0      = operands[0];
  rtx op0_low  = gen_lowpart (SImode, op0);
  rtx op0_high = gen_highpart (SImode, op0);
  rtx op1      = operands[1];
  rtx op1_low  = gen_lowpart (SImode, op1);
  rtx op1_high = gen_highpart (SImode, op1);

  /* We normally copy the low-numbered register first.  However, if the first
     register operand 0 is the same as the second register of operand 1, we
     must copy in the opposite order.  */

  if (REGNO (op0_high) == REGNO (op1_low))
    {
      operands[2] = op0_low;
      operands[3] = op0_high;
      operands[4] = op1_low;
      operands[5] = op1_high;
    }
  else
    {
      operands[2] = op0_high;
      operands[3] = op0_low;
      operands[4] = op1_high;
      operands[5] = op1_low;
    }
}")

(define_split
  [(set (match_operand:DF 0 "register_operand" "")
	(match_operand:DF 1 "const_int_operand" ""))]
  "reload_completed"
  [(set (match_dup 2) (match_dup 4))
   (set (match_dup 3) (match_dup 1))]
  "
{
  rtx op0 = operands[0];
  rtx op1 = operands[1];

  operands[2] = gen_highpart (SImode, op0);
  operands[3] = gen_lowpart (SImode, op0);
  operands[4] = GEN_INT ((INTVAL (op1) < 0) ? -1 : 0);
}")

(define_split
  [(set (match_operand:DF 0 "register_operand" "")
	(match_operand:DF 1 "const_double_operand" ""))]
  "reload_completed"
  [(set (match_dup 2) (match_dup 4))
   (set (match_dup 3) (match_dup 5))]
  "
{
  rtx op0 = operands[0];
  rtx op1 = operands[1];
  REAL_VALUE_TYPE rv;
  long l[2];

  REAL_VALUE_FROM_CONST_DOUBLE (rv, op1);
  REAL_VALUE_TO_TARGET_DOUBLE (rv, l);

  operands[2] = gen_highpart (SImode, op0);
  operands[3] = gen_lowpart (SImode, op0);
  operands[4] = GEN_INT (l[0]);
  operands[5] = GEN_INT (l[1]);
}")

;; String/block move insn.
;; Argument 0 is the destination
;; Argument 1 is the source
;; Argument 2 is the length
;; Argument 3 is the alignment

(define_expand "movstrsi"
  [(parallel [(set (match_operand:BLK 0 "" "")
		   (match_operand:BLK 1 "" ""))
	      (use (match_operand:SI 2 "" ""))
	      (use (match_operand:SI 3 "" ""))])]
  ""
  "
{
  if (frv_expand_block_move (operands))
    DONE;
  else
    FAIL;
}")

;; String/block clear insn.
;; Argument 0 is the destination
;; Argument 1 is the length
;; Argument 2 is the alignment

(define_expand "clrstrsi"
  [(parallel [(set (match_operand:BLK 0 "" "")
		   (const_int 0))
	      (use (match_operand:SI 1 "" ""))
	      (use (match_operand:SI 2 "" ""))])]
  ""
  "
{
  if (frv_expand_block_clear (operands))
    DONE;
  else
    FAIL;
}")


;; ::::::::::::::::::::
;; ::
;; :: Reload CC registers
;; ::
;; ::::::::::::::::::::

;; Use as a define_expand so that cse/gcse/combine can't accidentally
;; create movcc insns.

(define_expand "movcc"
  [(parallel [(set (match_operand:CC 0 "move_destination_operand" "")
		   (match_operand:CC 1 "move_source_operand" ""))
	      (clobber (match_dup 2))])]
  ""
  "
{
 if (! reload_in_progress && ! reload_completed)
    FAIL;

 operands[2] = gen_rtx_REG (CC_CCRmode, ICR_TEMP);
}")

(define_insn "*internal_movcc"
  [(set (match_operand:CC 0 "move_destination_operand" "=t,d,d,m,d")
	(match_operand:CC 1 "move_source_operand" "d,d,m,d,t"))
   (clobber (match_scratch:CC_CCR 2 "=X,X,X,X,&v"))]
  "reload_in_progress || reload_completed"
  "@
   cmpi %1, #0, %0
   mov %1, %0
   ld%I1%U1 %M1, %0
   st%I0%U0 %1, %M0
   #"
  [(set_attr "length" "4,4,4,4,20")
   (set_attr "type" "int,int,gload,gstore,multi")])

;; To move an ICC value to a GPR for a signed comparison, we create a value
;; that when compared to 0, sets the N and Z flags appropriately (we don't care
;; about the V and C flags, since these comparisons are signed).

(define_split
  [(set (match_operand:CC 0 "integer_register_operand" "")
	(match_operand:CC 1 "icc_operand" ""))
   (clobber (match_operand:CC_CCR 2 "icr_operand" ""))]
  "reload_in_progress || reload_completed"
  [(match_dup 3)]
  "
{
  rtx dest = simplify_gen_subreg (SImode, operands[0], CCmode, 0);
  rtx icc  = operands[1];
  rtx icr  = operands[2];

  start_sequence ();

  emit_insn (gen_rtx_SET (VOIDmode, icr,
			  gen_rtx_LT (CC_CCRmode, icc, const0_rtx)));

  emit_insn (gen_movsi (dest, const1_rtx));

  emit_insn (gen_rtx_COND_EXEC (VOIDmode,
				gen_rtx_NE (CC_CCRmode, icr, const0_rtx),
				gen_rtx_SET (VOIDmode, dest,
					     gen_rtx_NEG (SImode, dest))));

  emit_insn (gen_rtx_SET (VOIDmode, icr,
			  gen_rtx_EQ (CC_CCRmode, icc, const0_rtx)));

  emit_insn (gen_rtx_COND_EXEC (VOIDmode,
				gen_rtx_NE (CC_CCRmode, icr, const0_rtx),
				gen_rtx_SET (VOIDmode, dest, const0_rtx)));

  operands[3] = get_insns ();
  end_sequence ();
}")

(define_expand "reload_incc"
  [(parallel [(set (match_operand:CC 2 "integer_register_operand" "=&d")
		   (match_operand:CC 1 "memory_operand" "m"))
	      (clobber (match_scratch:CC_CCR 3 ""))])
   (parallel [(set (match_operand:CC 0 "icc_operand" "=t")
		   (match_dup 2))
	      (clobber (match_scratch:CC_CCR 4 ""))])]
  ""
  "")

(define_expand "reload_outcc"
  [(parallel [(set (match_operand:CC 2 "integer_register_operand" "=&d")
		   (match_operand:CC 1 "icc_operand" "t"))
	      (clobber (match_dup 3))])
   (parallel [(set (match_operand:CC 0 "memory_operand" "=m")
		   (match_dup 2))
	      (clobber (match_scratch:CC_CCR 4 ""))])]
  ""
  "operands[3] = gen_rtx_REG (CC_CCRmode, ICR_TEMP);")

;; Reload CC_UNSmode for unsigned integer comparisons
;; Use define_expand so that cse/gcse/combine can't create movcc_uns insns

(define_expand "movcc_uns"
  [(parallel [(set (match_operand:CC_UNS 0 "move_destination_operand" "")
		   (match_operand:CC_UNS 1 "move_source_operand" ""))
	      (clobber (match_dup 2))])]
  ""
  "
{
 if (! reload_in_progress && ! reload_completed)
    FAIL;
 operands[2] = gen_rtx_REG (CC_CCRmode, ICR_TEMP);
}")

(define_insn "*internal_movcc_uns"
  [(set (match_operand:CC_UNS 0 "move_destination_operand" "=t,d,d,m,d")
	(match_operand:CC_UNS 1 "move_source_operand" "d,d,m,d,t"))
   (clobber (match_scratch:CC_CCR 2 "=X,X,X,X,&v"))]
  "reload_in_progress || reload_completed"
  "@
   cmpi %1, #1, %0
   mov %1, %0
   ld%I1%U1 %M1, %0
   st%I0%U0 %1, %M0
   #"
  [(set_attr "length" "4,4,4,4,20")
   (set_attr "type" "int,int,gload,gstore,multi")])

;; To move an ICC value to a GPR for an unsigned comparison, we create a value
;; that when compared to 1, sets the Z, V, and C flags appropriately (we don't
;; care about the N flag, since these comparisons are unsigned).

(define_split
  [(set (match_operand:CC_UNS 0 "integer_register_operand" "")
	(match_operand:CC_UNS 1 "icc_operand" ""))
   (clobber (match_operand:CC_CCR 2 "icr_operand" ""))]
  "reload_in_progress || reload_completed"
  [(match_dup 3)]
  "
{
  rtx dest = simplify_gen_subreg (SImode, operands[0], CC_UNSmode, 0);
  rtx icc  = operands[1];
  rtx icr  = operands[2];

  start_sequence ();

  emit_insn (gen_rtx_SET (VOIDmode, icr,
			  gen_rtx_GTU (CC_CCRmode, icc, const0_rtx)));

  emit_insn (gen_movsi (dest, const1_rtx));

  emit_insn (gen_rtx_COND_EXEC (VOIDmode,
				gen_rtx_NE (CC_CCRmode, icr, const0_rtx),
				gen_addsi3 (dest, dest, dest)));

  emit_insn (gen_rtx_SET (VOIDmode, icr,
			  gen_rtx_LTU (CC_CCRmode, icc, const0_rtx)));

  emit_insn (gen_rtx_COND_EXEC (VOIDmode,
				gen_rtx_NE (CC_CCRmode, icr, const0_rtx),
				gen_rtx_SET (VOIDmode, dest, const0_rtx)));

  operands[3] = get_insns ();
  end_sequence ();
}")

(define_expand "reload_incc_uns"
  [(parallel [(set (match_operand:CC_UNS 2 "integer_register_operand" "=&d")
		   (match_operand:CC_UNS 1 "memory_operand" "m"))
	      (clobber (match_scratch:CC_CCR 3 ""))])
   (parallel [(set (match_operand:CC_UNS 0 "icc_operand" "=t")
		   (match_dup 2))
	      (clobber (match_scratch:CC_CCR 4 ""))])]
  ""
  "")

(define_expand "reload_outcc_uns"
  [(parallel [(set (match_operand:CC_UNS 2 "integer_register_operand" "=&d")
		   (match_operand:CC_UNS 1 "icc_operand" "t"))
	      (clobber (match_dup 3))])
   (parallel [(set (match_operand:CC_UNS 0 "memory_operand" "=m")
		   (match_dup 2))
	      (clobber (match_scratch:CC_CCR 4 ""))])]
  ""
  "operands[3] = gen_rtx_REG (CC_CCRmode, ICR_TEMP);")

;; Reload CC_FPmode for floating point comparisons
;; We use a define_expand here so that cse/gcse/combine can't accidentally
;; create movcc insns.  If this was a named define_insn, we would not be able
;; to make it conditional on reload.

(define_expand "movcc_fp"
  [(set (match_operand:CC_FP 0 "move_destination_operand" "")
	(match_operand:CC_FP 1 "move_source_operand" ""))]
  "TARGET_HAS_FPRS"
  "
{
 if (! reload_in_progress && ! reload_completed)
    FAIL;
}")

(define_insn "*movcc_fp_internal"
  [(set (match_operand:CC_FP 0 "move_destination_operand" "=d,d,d,m")
	(match_operand:CC_FP 1 "move_source_operand" "u,d,m,d"))]
  "TARGET_HAS_FPRS && (reload_in_progress || reload_completed)"
  "@
   #
   mov %1, %0
   ld%I1%U1 %M1, %0
   st%I0%U0 %1, %M0"
  [(set_attr "length" "12,4,4,4")
   (set_attr "type" "multi,int,gload,gstore")])


(define_expand "reload_incc_fp"
  [(match_operand:CC_FP 0 "fcc_operand" "=u")
   (match_operand:CC_FP 1 "memory_operand" "m")
   (match_operand:TI 2 "integer_register_operand" "=&d")]
  "TARGET_HAS_FPRS"
  "
{
  rtx cc_op2 = simplify_gen_subreg (CC_FPmode, operands[2], TImode, 0);
  rtx int_op2 = simplify_gen_subreg (SImode, operands[2], TImode, 0);
  rtx temp1 = simplify_gen_subreg (SImode, operands[2], TImode, 4);
  rtx temp2 = simplify_gen_subreg (SImode, operands[2], TImode, 8);
  int shift = CC_SHIFT_RIGHT (REGNO (operands[0]));
  HOST_WIDE_INT mask;

  emit_insn (gen_movcc_fp (cc_op2, operands[1]));
  if (shift)
    emit_insn (gen_ashlsi3 (int_op2, int_op2, GEN_INT (shift)));

  mask = ~ ((HOST_WIDE_INT)CC_MASK << shift);
  emit_insn (gen_movsi (temp1, GEN_INT (mask)));
  emit_insn (gen_update_fcc (operands[0], int_op2, temp1, temp2));
  DONE;
}")

(define_expand "reload_outcc_fp"
  [(set (match_operand:CC_FP 2 "integer_register_operand" "=&d")
	(match_operand:CC_FP 1 "fcc_operand" "u"))
   (set (match_operand:CC_FP 0 "memory_operand" "=m")
	(match_dup 2))]
  "TARGET_HAS_FPRS"
 "")

;; Convert a FCC value to gpr
(define_insn "read_fcc"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(unspec:SI [(match_operand:CC_FP 1 "fcc_operand" "u")]
		   UNSPEC_CC_TO_GPR))]
  "TARGET_HAS_FPRS"
  "movsg ccr, %0"
  [(set_attr "type" "spr")
   (set_attr "length" "4")])

(define_split
  [(set (match_operand:CC_FP 0 "integer_register_operand" "")
	(match_operand:CC_FP 1 "fcc_operand" ""))]
  "reload_completed && TARGET_HAS_FPRS"
  [(match_dup 2)]
  "
{
  rtx int_op0 = simplify_gen_subreg (SImode, operands[0], CC_FPmode, 0);
  int shift = CC_SHIFT_RIGHT (REGNO (operands[1]));

  start_sequence ();

  emit_insn (gen_read_fcc (int_op0, operands[1]));
  if (shift)
    emit_insn (gen_lshrsi3 (int_op0, int_op0, GEN_INT (shift)));

  emit_insn (gen_andsi3 (int_op0, int_op0, GEN_INT (CC_MASK)));

  operands[2] = get_insns ();
  end_sequence ();
}")

;; Move a gpr value to FCC.
;; Operand0 = FCC
;; Operand1 = reloaded value shifted appropriately
;; Operand2 = mask to eliminate current register
;; Operand3 = temporary to load/store ccr
(define_insn "update_fcc"
  [(set (match_operand:CC_FP 0 "fcc_operand" "=u")
	(unspec:CC_FP [(match_operand:SI 1 "integer_register_operand" "d")
		       (match_operand:SI 2 "integer_register_operand" "d")]
		      UNSPEC_GPR_TO_CC))
   (clobber (match_operand:SI 3 "integer_register_operand" "=&d"))]
  "TARGET_HAS_FPRS"
  "movsg ccr, %3\;and %2, %3, %3\;or %1, %3, %3\;movgs %3, ccr"
  [(set_attr "type" "multi")
   (set_attr "length" "16")])

;; Reload CC_CCRmode for conditional execution registers
(define_insn "movcc_ccr"
  [(set (match_operand:CC_CCR 0 "move_destination_operand" "=d,d,d,m,v,?w,C,d")
	(match_operand:CC_CCR 1 "move_source_operand" "C,d,m,d,n,n,C,L"))]
  ""
  "@
   #
   mov %1, %0
   ld%I1%U1 %M1, %0
   st%I0%U0 %1, %M0
   #
   #
   orcr %1, %1, %0
   setlos #%1, %0"
  [(set_attr "length" "8,4,4,4,8,12,4,4")
   (set_attr "type" "multi,int,gload,gstore,multi,multi,ccr,int")])

(define_expand "reload_incc_ccr"
  [(match_operand:CC_CCR 0 "cr_operand" "=C")
   (match_operand:CC_CCR 1 "memory_operand" "m")
   (match_operand:CC_CCR 2 "integer_register_operand" "=&d")]
  ""
  "
{
  rtx icc = gen_rtx_REG (CCmode, ICC_TEMP);
  rtx int_op2 = simplify_gen_subreg (SImode, operands[2], CC_CCRmode, 0);
  rtx icr = (ICR_P (REGNO (operands[0]))
	     ? operands[0] : gen_rtx_REG (CC_CCRmode, ICR_TEMP));

  emit_insn (gen_movcc_ccr (operands[2], operands[1]));
  emit_insn (gen_cmpsi_cc (icc, int_op2, const0_rtx));
  emit_insn (gen_movcc_ccr (icr, gen_rtx_NE (CC_CCRmode, icc, const0_rtx)));

  if (! ICR_P (REGNO (operands[0])))
    emit_insn (gen_movcc_ccr (operands[0], icr));

  DONE;
}")

(define_expand "reload_outcc_ccr"
  [(set (match_operand:CC_CCR 2 "integer_register_operand" "=&d")
	(match_operand:CC_CCR 1 "cr_operand" "C"))
   (set (match_operand:CC_CCR 0 "memory_operand" "=m")
	(match_dup 2))]
  ""
  "")

(define_split
  [(set (match_operand:CC_CCR 0 "integer_register_operand" "")
	(match_operand:CC_CCR 1 "cr_operand" ""))]
  "reload_completed"
  [(match_dup 2)]
  "
{
  rtx int_op0 = simplify_gen_subreg (SImode, operands[0], CC_CCRmode, 0);

  start_sequence ();
  emit_move_insn (operands[0], const1_rtx);
  emit_insn (gen_rtx_COND_EXEC (VOIDmode,
				gen_rtx_EQ (CC_CCRmode,
					    operands[1],
					    const0_rtx),
				gen_rtx_SET (VOIDmode, int_op0,
					     const0_rtx)));

  operands[2] = get_insns ();
  end_sequence ();
}")

(define_split
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(match_operand:CC_CCR 1 "const_int_operand" ""))]
  "reload_completed"
  [(match_dup 2)]
  "
{
  rtx icc = gen_rtx_REG (CCmode, ICC_TEMP);
  rtx r0  = gen_rtx_REG (SImode, GPR_FIRST);
  rtx icr = (ICR_P (REGNO (operands[0]))
	     ? operands[0] : gen_rtx_REG (CC_CCRmode, ICR_TEMP));

  start_sequence ();

 emit_insn (gen_cmpsi_cc (icc, r0, const0_rtx));

  emit_insn (gen_movcc_ccr (icr,
			    gen_rtx_fmt_ee (((INTVAL (operands[1]) == 0)
					     ? EQ : NE), CC_CCRmode,
					    r0, const0_rtx)));

  if (! ICR_P (REGNO (operands[0])))
    emit_insn (gen_movcc_ccr (operands[0], icr));

  operands[2] = get_insns ();
  end_sequence ();
}")


;; ::::::::::::::::::::
;; ::
;; :: Conversions
;; ::
;; ::::::::::::::::::::

;; Signed conversions from a smaller integer to a larger integer
;;
;; These operations are optional.  If they are not
;; present GCC will synthesize them for itself
;; Even though frv does not provide these instructions, we define them
;; to allow load + sign extend to be collapsed together
(define_insn "extendqihi2"
  [(set (match_operand:HI 0 "integer_register_operand" "=d,d")
	(sign_extend:HI (match_operand:QI 1 "gpr_or_memory_operand" "d,m")))]
  ""
  "@
   #
   ldsb%I1%U1 %M1,%0"
  [(set_attr "length" "8,4")
   (set_attr "type" "multi,gload")])

(define_split
  [(set (match_operand:HI 0 "integer_register_operand" "")
	(sign_extend:HI (match_operand:QI 1 "integer_register_operand" "")))]
  "reload_completed"
  [(match_dup 2)
   (match_dup 3)]
  "
{
  rtx op0   = gen_lowpart (SImode, operands[0]);
  rtx op1   = gen_lowpart (SImode, operands[1]);
  rtx shift = GEN_INT (24);

  operands[2] = gen_ashlsi3 (op0, op1, shift);
  operands[3] = gen_ashrsi3 (op0, op0, shift);
}")

(define_insn "extendqisi2"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d")
	(sign_extend:SI (match_operand:QI 1 "gpr_or_memory_operand" "d,m")))]
  ""
  "@
   #
   ldsb%I1%U1 %M1,%0"
  [(set_attr "length" "8,4")
   (set_attr "type" "multi,gload")])

(define_split
  [(set (match_operand:SI 0 "integer_register_operand" "")
	(sign_extend:SI (match_operand:QI 1 "integer_register_operand" "")))]
  "reload_completed"
  [(match_dup 2)
   (match_dup 3)]
  "
{
  rtx op0   = gen_lowpart (SImode, operands[0]);
  rtx op1   = gen_lowpart (SImode, operands[1]);
  rtx shift = GEN_INT (24);

  operands[2] = gen_ashlsi3 (op0, op1, shift);
  operands[3] = gen_ashrsi3 (op0, op0, shift);
}")

;;(define_insn "extendqidi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(sign_extend:DI (match_operand:QI 1 "general_operand" "g")))]
;;  ""
;;  "extendqihi2 %0,%1"
;;  [(set_attr "length" "4")])

(define_insn "extendhisi2"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d")
	(sign_extend:SI (match_operand:HI 1 "gpr_or_memory_operand" "d,m")))]
  ""
  "@
   #
   ldsh%I1%U1 %M1,%0"
  [(set_attr "length" "8,4")
   (set_attr "type" "multi,gload")])

(define_split
  [(set (match_operand:SI 0 "integer_register_operand" "")
	(sign_extend:SI (match_operand:HI 1 "integer_register_operand" "")))]
  "reload_completed"
  [(match_dup 2)
   (match_dup 3)]
  "
{
  rtx op0   = gen_lowpart (SImode, operands[0]);
  rtx op1   = gen_lowpart (SImode, operands[1]);
  rtx shift = GEN_INT (16);

  operands[2] = gen_ashlsi3 (op0, op1, shift);
  operands[3] = gen_ashrsi3 (op0, op0, shift);
}")

;;(define_insn "extendhidi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(sign_extend:DI (match_operand:HI 1 "general_operand" "g")))]
;;  ""
;;  "extendhihi2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "extendsidi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(sign_extend:DI (match_operand:SI 1 "general_operand" "g")))]
;;  ""
;;  "extendsidi2 %0,%1"
;;  [(set_attr "length" "4")])

;; Unsigned conversions from a smaller integer to a larger integer
(define_insn "zero_extendqihi2"
  [(set (match_operand:HI 0 "integer_register_operand" "=d,d,d")
	(zero_extend:HI
	  (match_operand:QI 1 "gpr_or_memory_operand" "d,L,m")))]
  ""
  "@
   andi %1,#0xff,%0
   setlos %1,%0
   ldub%I1%U1 %M1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int,int,gload")])

(define_insn "zero_extendqisi2"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d,d")
	(zero_extend:SI
	  (match_operand:QI 1 "gpr_or_memory_operand" "d,L,m")))]
  ""
  "@
   andi %1,#0xff,%0
   setlos %1,%0
   ldub%I1%U1 %M1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int,int,gload")])

;;(define_insn "zero_extendqidi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(zero_extend:DI (match_operand:QI 1 "general_operand" "g")))]
;;  ""
;;  "zero_extendqihi2 %0,%1"
;;  [(set_attr "length" "4")])

;; Do not set the type for the sethi to "sethi", since the scheduler will think
;; the sethi takes 0 cycles as part of allowing sethi/setlo to be in the same
;; VLIW instruction.
(define_insn "zero_extendhisi2"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d")
	(zero_extend:SI (match_operand:HI 1 "gpr_or_memory_operand" "0,m")))]
  ""
  "@
    sethi #hi(#0),%0
    lduh%I1%U1 %M1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int,gload")])

;;(define_insn "zero_extendhidi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(zero_extend:DI (match_operand:HI 1 "general_operand" "g")))]
;;  ""
;;  "zero_extendhihi2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "zero_extendsidi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(zero_extend:DI (match_operand:SI 1 "general_operand" "g")))]
;;  ""
;;  "zero_extendsidi2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;;; Convert between floating point types of different sizes.
;;
;;(define_insn "extendsfdf2"
;;  [(set (match_operand:DF 0 "register_operand" "=r")
;;	(float_extend:DF (match_operand:SF 1 "register_operand" "r")))]
;;  ""
;;  "extendsfdf2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "truncdfsf2"
;;  [(set (match_operand:SF 0 "register_operand" "=r")
;;	(float_truncate:SF (match_operand:DF 1 "register_operand" "r")))]
;;  ""
;;  "truncdfsf2 %0,%1"
;;  [(set_attr "length" "4")])

;;;; Convert between signed integer types and floating point.
(define_insn "floatsisf2"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(float:SF (match_operand:SI 1 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fitos %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fsconv")])

(define_insn "floatsidf2"
  [(set (match_operand:DF 0 "fpr_operand" "=h")
	(float:DF (match_operand:SI 1 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "fitod %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fdconv")])

;;(define_insn "floatdisf2"
;;  [(set (match_operand:SF 0 "register_operand" "=r")
;;	(float:SF (match_operand:DI 1 "register_operand" "r")))]
;;  ""
;;  "floatdisf2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "floatdidf2"
;;  [(set (match_operand:DF 0 "register_operand" "=r")
;;	(float:DF (match_operand:DI 1 "register_operand" "r")))]
;;  ""
;;  "floatdidf2 %0,%1"
;;  [(set_attr "length" "4")])

(define_insn "fix_truncsfsi2"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(fix:SI (match_operand:SF 1 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fstoi %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fsconv")])

(define_insn "fix_truncdfsi2"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(fix:SI (match_operand:DF 1 "fpr_operand" "h")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "fdtoi %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fdconv")])

;;(define_insn "fix_truncsfdi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(fix:DI (match_operand:SF 1 "register_operand" "r")))]
;;  ""
;;  "fix_truncsfdi2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "fix_truncdfdi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(fix:DI (match_operand:DF 1 "register_operand" "r")))]
;;  ""
;;  "fix_truncdfdi2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;;; Convert between unsigned integer types and floating point.
;;
;;(define_insn "floatunssisf2"
;;  [(set (match_operand:SF 0 "register_operand" "=r")
;;	(unsigned_float:SF (match_operand:SI 1 "register_operand" "r")))]
;;  ""
;;  "floatunssisf2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "floatunssidf2"
;;  [(set (match_operand:DF 0 "register_operand" "=r")
;;	(unsigned_float:DF (match_operand:SI 1 "register_operand" "r")))]
;;  ""
;;  "floatunssidf2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "floatunsdisf2"
;;  [(set (match_operand:SF 0 "register_operand" "=r")
;;	(unsigned_float:SF (match_operand:DI 1 "register_operand" "r")))]
;;  ""
;;  "floatunsdisf2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "floatunsdidf2"
;;  [(set (match_operand:DF 0 "register_operand" "=r")
;;	(unsigned_float:DF (match_operand:DI 1 "register_operand" "r")))]
;;  ""
;;  "floatunsdidf2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "fixuns_truncsfsi2"
;;  [(set (match_operand:SI 0 "register_operand" "=r")
;;	(unsigned_fix:SI (match_operand:SF 1 "register_operand" "r")))]
;;  ""
;;  "fixuns_truncsfsi2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "fixuns_truncdfsi2"
;;  [(set (match_operand:SI 0 "register_operand" "=r")
;;	(unsigned_fix:SI (match_operand:DF 1 "register_operand" "r")))]
;;  ""
;;  "fixuns_truncdfsi2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "fixuns_truncsfdi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(unsigned_fix:DI (match_operand:SF 1 "register_operand" "r")))]
;;  ""
;;  "fixuns_truncsfdi2 %0,%1"
;;  [(set_attr "length" "4")])
;;
;;(define_insn "fixuns_truncdfdi2"
;;  [(set (match_operand:DI 0 "register_operand" "=r")
;;	(unsigned_fix:DI (match_operand:DF 1 "register_operand" "r")))]
;;  ""
;;  "fixuns_truncdfdi2 %0,%1"
;;  [(set_attr "length" "4")])


;; ::::::::::::::::::::
;; ::
;; :: 32 bit Integer arithmetic
;; ::
;; ::::::::::::::::::::

;; Addition
(define_insn "addsi3"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(plus:SI (match_operand:SI 1 "integer_register_operand" "%d")
		 (match_operand:SI 2 "gpr_or_int12_operand" "dNOP")))]
  ""
  "add%I2 %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

;; Subtraction.  No need to worry about constants, since the compiler
;; canonicalizes them into addsi3's.  We prevent SUBREG's here to work around a
;; combine bug, that combines the 32x32->upper 32 bit multiply that uses a
;; SUBREG with a minus that shows up in modulus by constants.
(define_insn "subsi3"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(minus:SI (match_operand:SI 1 "gpr_no_subreg_operand" "d")
		  (match_operand:SI 2 "gpr_no_subreg_operand" "d")))]
  ""
  "sub %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

;; Signed multiplication producing 64 bit results from 32 bit inputs
;; Note, frv doesn't have a 32x32->32 bit multiply, but the compiler
;; will do the 32x32->64 bit multiply and use the bottom word.
(define_expand "mulsidi3"
  [(set (match_operand:DI 0 "integer_register_operand" "")
	(mult:DI (sign_extend:DI (match_operand:SI 1 "integer_register_operand" ""))
		 (sign_extend:DI (match_operand:SI 2 "gpr_or_int12_operand" ""))))]
  ""
  "
{
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      emit_insn (gen_mulsidi3_const (operands[0], operands[1], operands[2]));
      DONE;
    }
}")

(define_insn "*mulsidi3_reg"
  [(set (match_operand:DI 0 "even_gpr_operand" "=e")
	(mult:DI (sign_extend:DI (match_operand:SI 1 "integer_register_operand" "%d"))
		 (sign_extend:DI (match_operand:SI 2 "integer_register_operand" "d"))))]
  ""
  "smul %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "mul")])

(define_insn "mulsidi3_const"
  [(set (match_operand:DI 0 "even_gpr_operand" "=e")
	(mult:DI (sign_extend:DI (match_operand:SI 1 "integer_register_operand" "d"))
		 (match_operand:SI 2 "int12_operand" "NOP")))]
  ""
  "smuli %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "mul")])

;; Unsigned multiplication producing 64 bit results from 32 bit inputs
(define_expand "umulsidi3"
  [(set (match_operand:DI 0 "even_gpr_operand" "")
	(mult:DI (zero_extend:DI (match_operand:SI 1 "integer_register_operand" ""))
		 (zero_extend:DI (match_operand:SI 2 "gpr_or_int12_operand" ""))))]
  ""
  "
{
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      emit_insn (gen_umulsidi3_const (operands[0], operands[1], operands[2]));
      DONE;
    }
}")

(define_insn "*mulsidi3_reg"
  [(set (match_operand:DI 0 "even_gpr_operand" "=e")
	(mult:DI (zero_extend:DI (match_operand:SI 1 "integer_register_operand" "%d"))
		 (zero_extend:DI (match_operand:SI 2 "integer_register_operand" "d"))))]
  ""
  "umul %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "mul")])

(define_insn "umulsidi3_const"
  [(set (match_operand:DI 0 "even_gpr_operand" "=e")
	(mult:DI (zero_extend:DI (match_operand:SI 1 "integer_register_operand" "d"))
		 (match_operand:SI 2 "int12_operand" "NOP")))]
  ""
  "umuli %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "mul")])

;; Signed Division
(define_insn "divsi3"
  [(set (match_operand:SI 0 "register_operand" "=d,d")
	(div:SI (match_operand:SI 1 "register_operand" "d,d")
		(match_operand:SI 2 "gpr_or_int12_operand" "d,NOP")))]
  ""
  "sdiv%I2 %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "div")])

;; Unsigned Division
(define_insn "udivsi3"
  [(set (match_operand:SI 0 "register_operand" "=d,d")
	(udiv:SI (match_operand:SI 1 "register_operand" "d,d")
		 (match_operand:SI 2 "gpr_or_int12_operand" "d,NOP")))]
  ""
  "udiv%I2 %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "div")])

;; Negation
(define_insn "negsi2"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(neg:SI (match_operand:SI 1 "integer_register_operand" "d")))]
  ""
  "sub %.,%1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

;; Find first one bit
;; (define_insn "ffssi2"
;;   [(set (match_operand:SI 0 "register_operand" "=r")
;; 	(ffs:SI (match_operand:SI 1 "register_operand" "r")))]
;;   ""
;;   "ffssi2 %0,%1"
;;   [(set_attr "length" "4")])


;; ::::::::::::::::::::
;; ::
;; :: 64 bit Integer arithmetic
;; ::
;; ::::::::::::::::::::

;; Addition
(define_expand "adddi3"
  [(parallel [(set (match_operand:DI 0 "integer_register_operand" "")
		   (plus:DI (match_operand:DI 1 "integer_register_operand" "")
			    (match_operand:DI 2 "gpr_or_int10_operand" "")))
	      (clobber (match_scratch:CC 3 ""))])]
  ""
  "
{
  if (GET_CODE (operands[2]) == CONST_INT
      && INTVAL (operands[2]) == -2048
      && !no_new_pseudos)
    operands[2] = force_reg (DImode, operands[2]);
}")

(define_insn_and_split "*adddi3_internal"
  [(set (match_operand:DI 0 "integer_register_operand" "=&e,e,e,&e,e,&e,e")
	(plus:DI (match_operand:DI 1 "integer_register_operand" "%e,0,e,e,0,e,0")
		 (match_operand:DI 2 "gpr_or_int10_operand" "e,e,0,N,N,OP,OP")))
   (clobber (match_scratch:CC 3 "=t,t,t,t,t,t,t"))]
  "GET_CODE (operands[2]) != CONST_INT || INTVAL (operands[2]) != -2048"
  "#"
  "reload_completed"
  [(match_dup 4)
   (match_dup 5)]
  "
{
  rtx op0_high = gen_highpart (SImode, operands[0]);
  rtx op1_high = gen_highpart (SImode, operands[1]);
  rtx op0_low  = gen_lowpart (SImode, operands[0]);
  rtx op1_low  = gen_lowpart (SImode, operands[1]);
  rtx op2 = operands[2];
  rtx op3 = operands[3];

  if (GET_CODE (op2) != CONST_INT)
    {
      rtx op2_high = gen_highpart (SImode, operands[2]);
      rtx op2_low  = gen_lowpart (SImode, operands[2]);
      operands[4] = gen_adddi3_lower (op0_low, op1_low, op2_low, op3);
      operands[5] = gen_adddi3_upper (op0_high, op1_high, op2_high, op3);
    }
  else if (INTVAL (op2) >= 0)
    {
      operands[4] = gen_adddi3_lower (op0_low, op1_low, op2, op3);
      operands[5] = gen_adddi3_upper (op0_high, op1_high, const0_rtx, op3);
    }
  else
    {
      operands[4] = gen_subdi3_lower (op0_low, op1_low,
				      GEN_INT (- INTVAL (op2)), op3);
      operands[5] = gen_subdi3_upper (op0_high, op1_high, const0_rtx, op3);
    }
}"
  [(set_attr "length" "8")
   (set_attr "type" "multi")])

;; Subtraction  No need to worry about constants, since the compiler
;; canonicalizes them into adddi3's.
(define_expand "subdi3"
  [(parallel [(set (match_operand:DI 0 "integer_register_operand" "")
		   (minus:DI (match_operand:DI 1 "integer_register_operand" "")
			     (match_operand:DI 2 "integer_register_operand" "")))
	      (clobber (match_dup 3))])]
  ""
  "
{
  operands[3] = gen_reg_rtx (CCmode);
}")

(define_insn_and_split "*subdi3_internal"
  [(set (match_operand:DI 0 "integer_register_operand" "=&e,e,e")
	(minus:DI (match_operand:DI 1 "integer_register_operand" "e,0,e")
		  (match_operand:DI 2 "integer_register_operand" "e,e,0")))
   (clobber (match_operand:CC 3 "icc_operand" "=t,t,t"))]
  ""
  "#"
  "reload_completed"
  [(match_dup 4)
   (match_dup 5)]
  "
{
  rtx op0_high = gen_highpart (SImode, operands[0]);
  rtx op1_high = gen_highpart (SImode, operands[1]);
  rtx op2_high = gen_highpart (SImode, operands[2]);
  rtx op0_low  = gen_lowpart (SImode, operands[0]);
  rtx op1_low  = gen_lowpart (SImode, operands[1]);
  rtx op2_low  = gen_lowpart (SImode, operands[2]);
  rtx op3 = operands[3];

  operands[4] = gen_subdi3_lower (op0_low, op1_low, op2_low, op3);
  operands[5] = gen_subdi3_upper (op0_high, op1_high, op2_high, op3);
}"
  [(set_attr "length" "8")
   (set_attr "type" "multi")])

;; Patterns for addsi3/subdi3 after spliting
(define_insn "adddi3_lower"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(plus:SI (match_operand:SI 1 "integer_register_operand" "d")
		 (match_operand:SI 2 "gpr_or_int10_operand" "dOP")))
   (set (match_operand:CC 3 "icc_operand" "=t")
	(compare:CC (plus:SI (match_dup 1)
			     (match_dup 2))
		    (const_int 0)))]
  "GET_CODE (operands[2]) != CONST_INT || INTVAL (operands[2]) >= 0"
  "add%I2cc %1,%2,%0,%3"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_insn "adddi3_upper"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d")
	(plus:SI (match_operand:SI 1 "integer_register_operand" "d,d")
		 (plus:SI (match_operand:SI 2 "reg_or_0_operand" "d,O")
			  (match_operand:CC 3 "icc_operand" "t,t"))))]
  ""
  "@
   addx %1,%2,%0,%3
   addx %1,%.,%0,%3"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_insn "subdi3_lower"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(minus:SI (match_operand:SI 1 "integer_register_operand" "d")
		  (match_operand:SI 2 "gpr_or_int10_operand" "dOP")))
   (set (match_operand:CC 3 "icc_operand" "=t")
	(compare:CC (plus:SI (match_dup 1)
			     (match_dup 2))
		    (const_int 0)))]
  "GET_CODE (operands[2]) != CONST_INT || INTVAL (operands[2]) >= 0"
  "sub%I2cc %1,%2,%0,%3"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_insn "subdi3_upper"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d")
	(minus:SI (match_operand:SI 1 "integer_register_operand" "d,d")
		  (minus:SI (match_operand:SI 2 "reg_or_0_operand" "d,O")
			    (match_operand:CC 3 "icc_operand" "t,t"))))]
  ""
  "@
   subx %1,%2,%0,%3
   subx %1,%.,%0,%3"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

;; Multiplication (same size)
;; (define_insn "muldi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(mult:DI (match_operand:DI 1 "register_operand" "%r")
;; 		 (match_operand:DI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "muldi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Signed Division
;; (define_insn "divdi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(div:DI (match_operand:DI 1 "register_operand" "r")
;; 		(match_operand:DI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "divdi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Undsgned Division
;; (define_insn "udivdi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(udiv:DI (match_operand:DI 1 "register_operand" "r")
;; 		 (match_operand:DI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "udivdi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Negation
;; (define_insn "negdi2"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(neg:DI (match_operand:DI 1 "register_operand" "r")))]
;;   ""
;;   "negdi2 %0,%1"
;;   [(set_attr "length" "4")])

;; Find first one bit
;; (define_insn "ffsdi2"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(ffs:DI (match_operand:DI 1 "register_operand" "r")))]
;;   ""
;;   "ffsdi2 %0,%1"
;;   [(set_attr "length" "4")])


;; ::::::::::::::::::::
;; ::
;; :: 32 bit floating point arithmetic
;; ::
;; ::::::::::::::::::::

;; Addition
(define_insn "addsf3"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(plus:SF (match_operand:SF 1 "fpr_operand" "%f")
		 (match_operand:SF 2 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fadds %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fsadd")])

;; Subtraction
(define_insn "subsf3"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(minus:SF (match_operand:SF 1 "fpr_operand" "f")
		  (match_operand:SF 2 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fsubs %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fsadd")])

;; Multiplication
(define_insn "mulsf3"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(mult:SF (match_operand:SF 1 "fpr_operand" "%f")
		 (match_operand:SF 2 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fmuls %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fsmul")])

;; Multiplication with addition/subtraction
(define_insn "*muladdsf4"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(plus:SF (mult:SF (match_operand:SF 1 "fpr_operand" "%f")
			  (match_operand:SF 2 "fpr_operand" "f"))
		 (match_operand:SF 3 "fpr_operand" "0")))]
  "TARGET_HARD_FLOAT && TARGET_MULADD"
  "fmadds %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fmas")])

(define_insn "*mulsubsf4"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(minus:SF (mult:SF (match_operand:SF 1 "fpr_operand" "%f")
			   (match_operand:SF 2 "fpr_operand" "f"))
		  (match_operand:SF 3 "fpr_operand" "0")))]
  "TARGET_HARD_FLOAT && TARGET_MULADD"
  "fmsubs %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fmas")])

;; Division
(define_insn "divsf3"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(div:SF (match_operand:SF 1 "fpr_operand" "f")
		(match_operand:SF 2 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fdivs %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fsdiv")])

;; Negation
(define_insn "negsf2"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(neg:SF (match_operand:SF 1 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fnegs %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fsconv")])

;; Absolute value
(define_insn "abssf2"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(abs:SF (match_operand:SF 1 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fabss %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fsconv")])

;; Square root
(define_insn "sqrtsf2"
  [(set (match_operand:SF 0 "fpr_operand" "=f")
	(sqrt:SF (match_operand:SF 1 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fsqrts %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "sqrt_single")])


;; ::::::::::::::::::::
;; ::
;; :: 64 bit floating point arithmetic
;; ::
;; ::::::::::::::::::::

;; Addition
(define_insn "adddf3"
  [(set (match_operand:DF 0 "even_fpr_operand" "=h")
	(plus:DF (match_operand:DF 1 "fpr_operand" "%h")
		 (match_operand:DF 2 "fpr_operand" "h")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "faddd %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fdadd")])

;; Subtraction
(define_insn "subdf3"
  [(set (match_operand:DF 0 "even_fpr_operand" "=h")
	(minus:DF (match_operand:DF 1 "fpr_operand" "h")
		  (match_operand:DF 2 "fpr_operand" "h")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "fsubd %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fdadd")])

;; Multiplication
(define_insn "muldf3"
  [(set (match_operand:DF 0 "even_fpr_operand" "=h")
	(mult:DF (match_operand:DF 1 "fpr_operand" "%h")
		 (match_operand:DF 2 "fpr_operand" "h")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "fmuld %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fdmul")])

;; Multiplication with addition/subtraction
(define_insn "*muladddf4"
  [(set (match_operand:DF 0 "fpr_operand" "=f")
	(plus:DF (mult:DF (match_operand:DF 1 "fpr_operand" "%f")
			  (match_operand:DF 2 "fpr_operand" "f"))
		 (match_operand:DF 3 "fpr_operand" "0")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE && TARGET_MULADD"
  "fmaddd %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fmas")])

(define_insn "*mulsubdf4"
  [(set (match_operand:DF 0 "fpr_operand" "=f")
	(minus:DF (mult:DF (match_operand:DF 1 "fpr_operand" "%f")
			   (match_operand:DF 2 "fpr_operand" "f"))
		  (match_operand:DF 3 "fpr_operand" "0")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE && TARGET_MULADD"
  "fmsubd %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fmas")])

;; Division
(define_insn "divdf3"
  [(set (match_operand:DF 0 "even_fpr_operand" "=h")
	(div:DF (match_operand:DF 1 "fpr_operand" "h")
		(match_operand:DF 2 "fpr_operand" "h")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "fdivd %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fddiv")])

;; Negation
(define_insn "negdf2"
  [(set (match_operand:DF 0 "even_fpr_operand" "=h")
	(neg:DF (match_operand:DF 1 "fpr_operand" "h")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "fnegd %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fdconv")])

;; Absolute value
(define_insn "absdf2"
  [(set (match_operand:DF 0 "even_fpr_operand" "=h")
	(abs:DF (match_operand:DF 1 "fpr_operand" "h")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "fabsd %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fdconv")])

;; Square root
(define_insn "sqrtdf2"
  [(set (match_operand:DF 0 "even_fpr_operand" "=h")
	(sqrt:DF (match_operand:DF 1 "fpr_operand" "h")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "fsqrtd %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "sqrt_double")])


;; ::::::::::::::::::::
;; ::
;; :: 32 bit Integer Shifts and Rotates
;; ::
;; ::::::::::::::::::::

;; Arithmetic Shift Left
(define_insn "ashlsi3"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d")
	(ashift:SI (match_operand:SI 1 "integer_register_operand" "d,d")
		   (match_operand:SI 2 "gpr_or_int12_operand" "d,NOP")))]
  ""
  "sll%I2 %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

;; Arithmetic Shift Right
(define_insn "ashrsi3"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d")
	(ashiftrt:SI (match_operand:SI 1 "integer_register_operand" "d,d")
		     (match_operand:SI 2 "gpr_or_int12_operand" "d,NOP")))]
  ""
  "sra%I2 %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

;; Logical Shift Right
(define_insn "lshrsi3"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d")
	(lshiftrt:SI (match_operand:SI 1 "integer_register_operand" "d,d")
		     (match_operand:SI 2 "gpr_or_int12_operand" "d,NOP")))]
  ""
  "srl%I2 %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

;; Rotate Left
;; (define_insn "rotlsi3"
;;   [(set (match_operand:SI 0 "register_operand" "=r")
;; 	(rotate:SI (match_operand:SI 1 "register_operand" "r")
;; 		   (match_operand:SI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "rotlsi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Rotate Right
;; (define_insn "rotrsi3"
;;   [(set (match_operand:SI 0 "register_operand" "=r")
;; 	(rotatert:SI (match_operand:SI 1 "register_operand" "r")
;; 		     (match_operand:SI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "rotrsi3 %0,%1,%2"
;;   [(set_attr "length" "4")])


;; ::::::::::::::::::::
;; ::
;; :: 64 bit Integer Shifts and Rotates
;; ::
;; ::::::::::::::::::::

;; Arithmetic Shift Left
;; (define_insn "ashldi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(ashift:DI (match_operand:DI 1 "register_operand" "r")
;; 		   (match_operand:SI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "ashldi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Arithmetic Shift Right
;; (define_insn "ashrdi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(ashiftrt:DI (match_operand:DI 1 "register_operand" "r")
;; 		     (match_operand:SI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "ashrdi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Logical Shift Right
;; (define_insn "lshrdi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(lshiftrt:DI (match_operand:DI 1 "register_operand" "r")
;; 		     (match_operand:SI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "lshrdi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Rotate Left
;; (define_insn "rotldi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(rotate:DI (match_operand:DI 1 "register_operand" "r")
;; 		   (match_operand:SI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "rotldi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Rotate Right
;; (define_insn "rotrdi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(rotatert:DI (match_operand:DI 1 "register_operand" "r")
;; 		     (match_operand:SI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "rotrdi3 %0,%1,%2"
;;   [(set_attr "length" "4")])


;; ::::::::::::::::::::
;; ::
;; :: 32 Bit Integer Logical operations
;; ::
;; ::::::::::::::::::::

;; Logical AND, 32 bit integers
(define_insn "andsi3_media"
  [(set (match_operand:SI 0 "gpr_or_fpr_operand" "=d,f")
	(and:SI (match_operand:SI 1 "gpr_or_fpr_operand" "%d,f")
		(match_operand:SI 2 "gpr_fpr_or_int12_operand" "dNOP,f")))]
  "TARGET_MEDIA"
  "@
   and%I2 %1, %2, %0
   mand %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "int,mlogic")])

(define_insn "andsi3_nomedia"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(and:SI (match_operand:SI 1 "integer_register_operand" "%d")
		(match_operand:SI 2 "gpr_or_int12_operand" "dNOP")))]
  "!TARGET_MEDIA"
  "and%I2 %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_expand "andsi3"
  [(set (match_operand:SI 0 "gpr_or_fpr_operand" "")
	(and:SI (match_operand:SI 1 "gpr_or_fpr_operand" "")
		(match_operand:SI 2 "gpr_fpr_or_int12_operand" "")))]
  ""
  "")

;; Inclusive OR, 32 bit integers
(define_insn "iorsi3_media"
  [(set (match_operand:SI 0 "gpr_or_fpr_operand" "=d,f")
	(ior:SI (match_operand:SI 1 "gpr_or_fpr_operand" "%d,f")
		(match_operand:SI 2 "gpr_fpr_or_int12_operand" "dNOP,f")))]
  "TARGET_MEDIA"
  "@
   or%I2 %1, %2, %0
   mor %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "int,mlogic")])

(define_insn "iorsi3_nomedia"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(ior:SI (match_operand:SI 1 "integer_register_operand" "%d")
		(match_operand:SI 2 "gpr_or_int12_operand" "dNOP")))]
  "!TARGET_MEDIA"
  "or%I2 %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_expand "iorsi3"
  [(set (match_operand:SI 0 "gpr_or_fpr_operand" "")
	(ior:SI (match_operand:SI 1 "gpr_or_fpr_operand" "")
		(match_operand:SI 2 "gpr_fpr_or_int12_operand" "")))]
  ""
  "")

;; Exclusive OR, 32 bit integers
(define_insn "xorsi3_media"
  [(set (match_operand:SI 0 "gpr_or_fpr_operand" "=d,f")
	(xor:SI (match_operand:SI 1 "gpr_or_fpr_operand" "%d,f")
		(match_operand:SI 2 "gpr_fpr_or_int12_operand" "dNOP,f")))]
  "TARGET_MEDIA"
  "@
   xor%I2 %1, %2, %0
   mxor %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "int,mlogic")])

(define_insn "xorsi3_nomedia"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(xor:SI (match_operand:SI 1 "integer_register_operand" "%d")
		(match_operand:SI 2 "gpr_or_int12_operand" "dNOP")))]
  "!TARGET_MEDIA"
  "xor%I2 %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_expand "xorsi3"
  [(set (match_operand:SI 0 "gpr_or_fpr_operand" "")
	(xor:SI (match_operand:SI 1 "gpr_or_fpr_operand" "")
		(match_operand:SI 2 "gpr_fpr_or_int12_operand" "")))]
  ""
  "")

;; One's complement, 32 bit integers
(define_insn "one_cmplsi2_media"
  [(set (match_operand:SI 0 "gpr_or_fpr_operand" "=d,f")
	(not:SI (match_operand:SI 1 "gpr_or_fpr_operand" "d,f")))]
  "TARGET_MEDIA"
  "@
   not %1, %0
   mnot %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "int,mlogic")])

(define_insn "one_cmplsi2_nomedia"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(not:SI (match_operand:SI 1 "integer_register_operand" "d")))]
  "!TARGET_MEDIA"
  "not %1,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_expand "one_cmplsi2"
  [(set (match_operand:SI 0 "gpr_or_fpr_operand" "")
	(not:SI (match_operand:SI 1 "gpr_or_fpr_operand" "")))]
  ""
  "")


;; ::::::::::::::::::::
;; ::
;; :: 64 Bit Integer Logical operations
;; ::
;; ::::::::::::::::::::

;; Logical AND, 64 bit integers
;; (define_insn "anddi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(and:DI (match_operand:DI 1 "register_operand" "%r")
;; 		(match_operand:DI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "anddi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Includive OR, 64 bit integers
;; (define_insn "iordi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(ior:DI (match_operand:DI 1 "register_operand" "%r")
;; 		(match_operand:DI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "iordi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; Excludive OR, 64 bit integers
;; (define_insn "xordi3"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(xor:DI (match_operand:DI 1 "register_operand" "%r")
;; 		(match_operand:DI 2 "nonmemory_operand" "ri")))]
;;   ""
;;   "xordi3 %0,%1,%2"
;;   [(set_attr "length" "4")])

;; One's complement, 64 bit integers
;; (define_insn "one_cmpldi2"
;;   [(set (match_operand:DI 0 "register_operand" "=r")
;; 	(not:DI (match_operand:DI 1 "register_operand" "r")))]
;;   ""
;;   "notdi3 %0,%1"
;;   [(set_attr "length" "4")])


;; ::::::::::::::::::::
;; ::
;; :: Combination of integer operation with comparison
;; ::
;; ::::::::::::::::::::

(define_insn "*combo_intop_compare1"
  [(set (match_operand:CC 0 "icc_operand" "=t")
	(compare:CC (match_operator:SI 1 "intop_compare_operator"
				       [(match_operand:SI 2 "integer_register_operand" "d")
					(match_operand:SI 3 "gpr_or_int10_operand" "dJ")])
		    (const_int 0)))]
  ""
  "%O1%I3cc %2, %3, %., %0"
  [(set_attr "type" "int")
   (set_attr "length" "4")])

(define_insn "*combo_intop_compare2"
  [(set (match_operand:CC_UNS 0 "icc_operand" "=t")
	(compare:CC_UNS (match_operator:SI 1 "intop_compare_operator"
					   [(match_operand:SI 2 "integer_register_operand" "d")
					    (match_operand:SI 3 "gpr_or_int10_operand" "dJ")])
			(const_int 0)))]
  ""
  "%O1%I3cc %2, %3, %., %0"
  [(set_attr "type" "int")
   (set_attr "length" "4")])

(define_insn "*combo_intop_compare3"
  [(set (match_operand:CC 0 "icc_operand" "=t")
	(compare:CC (match_operator:SI 1 "intop_compare_operator"
				       [(match_operand:SI 2 "integer_register_operand" "d")
					(match_operand:SI 3 "gpr_or_int10_operand" "dJ")])
		    (const_int 0)))
   (set (match_operand:SI 4 "integer_register_operand" "=d")
	(match_operator:SI 5 "intop_compare_operator"
			   [(match_dup 2)
			    (match_dup 3)]))]
  "GET_CODE (operands[1]) == GET_CODE (operands[5])"
  "%O1%I3cc %2, %3, %4, %0"
  [(set_attr "type" "int")
   (set_attr "length" "4")])

(define_insn "*combo_intop_compare4"
  [(set (match_operand:CC_UNS 0 "icc_operand" "=t")
	(compare:CC_UNS (match_operator:SI 1 "intop_compare_operator"
					   [(match_operand:SI 2 "integer_register_operand" "d")
					    (match_operand:SI 3 "gpr_or_int10_operand" "dJ")])
		    (const_int 0)))
   (set (match_operand:SI 4 "integer_register_operand" "=d")
	(match_operator:SI 5 "intop_compare_operator"
			   [(match_dup 2)
			    (match_dup 3)]))]
  "GET_CODE (operands[1]) == GET_CODE (operands[5])"
  "%O1%I3cc %2, %3, %4, %0"
  [(set_attr "type" "int")
   (set_attr "length" "4")])


;; ::::::::::::::::::::
;; ::
;; :: Comparisons
;; ::
;; ::::::::::::::::::::

;; Note, we store the operands in the comparison insns, and use them later
;; when generating the branch or scc operation.

;; First the routines called by the machine independent part of the compiler
(define_expand "cmpsi"
  [(set (cc0)
        (compare (match_operand:SI 0 "integer_register_operand" "")
  		 (match_operand:SI 1 "gpr_or_int10_operand" "")))]
  ""
  "
{
  frv_compare_op0 = operands[0];
  frv_compare_op1 = operands[1];
  DONE;
}")

;(define_expand "cmpdi"
;  [(set (cc0)
;        (compare (match_operand:DI 0 "register_operand" "")
;  		 (match_operand:DI 1 "nonmemory_operand" "")))]
;  ""
;  "
;{
;  frv_compare_op0 = operands[0];
;  frv_compare_op1 = operands[1];
;  DONE;
;}")

(define_expand "cmpsf"
 [(set (cc0)
       (compare (match_operand:SF 0 "fpr_operand" "")
 		 (match_operand:SF 1 "fpr_operand" "")))]
 "TARGET_HARD_FLOAT"
 "
{
  frv_compare_op0 = operands[0];
  frv_compare_op1 = operands[1];
  DONE;
}")

(define_expand "cmpdf"
  [(set (cc0)
        (compare (match_operand:DF 0 "fpr_operand" "")
  		 (match_operand:DF 1 "fpr_operand" "")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "
{
  frv_compare_op0 = operands[0];
  frv_compare_op1 = operands[1];
  DONE;
}")

;; Now, the actual comparisons, generated by the branch and/or scc operations

(define_insn "cmpsi_cc"
  [(set (match_operand:CC 0 "icc_operand" "=t,t")
	(compare:CC (match_operand:SI 1 "integer_register_operand" "d,d")
		    (match_operand:SI 2 "gpr_or_int10_operand" "d,J")))]
  ""
  "cmp%I2 %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_insn "*cmpsi_cc_uns"
  [(set (match_operand:CC_UNS 0 "icc_operand" "=t,t")
	(compare:CC_UNS (match_operand:SI 1 "integer_register_operand" "d,d")
			(match_operand:SI 2 "gpr_or_int10_operand" "d,J")))]
  ""
  "cmp%I2 %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_insn "*cmpsf_cc_fp"
  [(set (match_operand:CC_FP 0 "fcc_operand" "=u")
	(compare:CC_FP (match_operand:SF 1 "fpr_operand" "f")
		       (match_operand:SF 2 "fpr_operand" "f")))]
  "TARGET_HARD_FLOAT"
  "fcmps %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fsadd")])

(define_insn "*cmpdf_cc_fp"
  [(set (match_operand:CC_FP 0 "fcc_operand" "=u")
	(compare:CC_FP (match_operand:DF 1 "even_fpr_operand" "h")
		       (match_operand:DF 2 "even_fpr_operand" "h")))]
  "TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "fcmpd %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "fdadd")])


;; ::::::::::::::::::::
;; ::
;; :: Branches
;; ::
;; ::::::::::::::::::::

;; Define_expands called by the machine independent part of the compiler
;; to allocate a new comparison register.  Each of these named patterns
;; must be present, and they cannot be amalgamated into one pattern.
;;
;; If a fixed condition code register is being used, (as opposed to, say,
;; using cc0), then the expands should look like this:
;;
;; (define_expand "<name_of_test>"
;;   [(set (reg:CC <number_of_CC_register>)
;; 	(compare:CC (match_dup 1)
;; 		    (match_dup 2)))
;;    (set (pc)
;; 	(if_then_else (eq:CC (reg:CC <number_of_CC_register>)
;; 			     (const_int 0))
;; 		      (label_ref (match_operand 0 "" ""))
;; 		      (pc)))]
;;   ""
;;   "{
;;     operands[1] = frv_compare_op0;
;;     operands[2] = frv_compare_op1;
;;   }"
;; )

(define_expand "beq"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (EQ, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "bne"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (NE, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "blt"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (LT, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "ble"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (LE, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "bgt"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (GT, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "bge"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (GE, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "bltu"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (LTU, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "bleu"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (LEU, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "bgtu"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (GTU, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "bgeu"
  [(use (match_operand 0 "" ""))]
  ""
  "
{
  if (! frv_emit_cond_branch (GEU, operands[0]))
    FAIL;

  DONE;
}")

;; Actual branches.  We must allow for the (label_ref) and the (pc) to be
;; swapped.  If they are swapped, it reverses the sense of the branch.
;;
;; Note - unlike the define expands above, these patterns can be amalgamated
;; into one pattern for branch-if-true and one for branch-if-false.  This does
;; require an operand operator to select the correct branch mnemonic.
;;
;; If a fixed condition code register is being used, (as opposed to, say,
;; using cc0), then the expands could look like this:
;;
;; (define_insn "*branch_true"
;;   [(set (pc)
;; 	(if_then_else (match_operator:CC 0 "comparison_operator"
;; 					 [(reg:CC <number_of_CC_register>)
;; 					  (const_int 0)])
;; 		      (label_ref (match_operand 1 "" ""))
;; 		      (pc)))]
;;   ""
;;   "b%B0 %1"
;;   [(set_attr "length" "4")]
;; )
;;
;; In the above example the %B is a directive to frv_print_operand()
;; to decode and print the correct branch mnemonic.

(define_insn "*branch_signed_true"
  [(set (pc)
	(if_then_else (match_operator:CC 0 "signed_relational_operator"
					 [(match_operand 1 "icc_operand" "t")
					  (const_int 0)])
		      (label_ref (match_operand 2 "" ""))
		      (pc)))]
  ""
  "*
{
  if (get_attr_length (insn) == 4)
    return \"b%c0 %1,%#,%l2\";
  else
    return \"b%C0 %1,%#,1f\;call %l2\\n1:\";
}"
  [(set (attr "length")
	(if_then_else
	    (and (ge (minus (match_dup 2) (pc)) (const_int -32768))
		 (le (minus (match_dup 2) (pc)) (const_int 32764)))
	    (const_int 4)
	    (const_int 8)))
   (set (attr "far_jump")
        (if_then_else
	    (eq_attr "length" "4")
	    (const_string "no")
	    (const_string "yes")))
   (set (attr "type")
	(if_then_else
	    (eq_attr "length" "4")
	    (const_string "branch")
	    (const_string "multi")))])

(define_insn "*branch_signed_false"
  [(set (pc)
	(if_then_else (match_operator:CC 0 "signed_relational_operator"
					 [(match_operand 1 "icc_operand" "t")
					  (const_int 0)])
		      (pc)
		      (label_ref (match_operand 2 "" ""))))]
  ""
  "*
{
  if (get_attr_length (insn) == 4)
    return \"b%C0 %1,%#,%l2\";
  else
    return \"b%c0 %1,%#,1f\;call %l2\\n1:\";
}"
  [(set (attr "length")
	(if_then_else
	    (and (ge (minus (match_dup 2) (pc)) (const_int -32768))
		 (le (minus (match_dup 2) (pc)) (const_int 32764)))
	    (const_int 4)
	    (const_int 8)))
   (set (attr "far_jump")
        (if_then_else
	    (eq_attr "length" "4")
	    (const_string "no")
	    (const_string "yes")))
   (set (attr "type")
	(if_then_else
	    (eq_attr "length" "4")
	    (const_string "branch")
	    (const_string "multi")))])

(define_insn "*branch_unsigned_true"
  [(set (pc)
	(if_then_else (match_operator:CC_UNS 0 "unsigned_relational_operator"
					     [(match_operand 1 "icc_operand" "t")
					      (const_int 0)])
		      (label_ref (match_operand 2 "" ""))
		      (pc)))]
  ""
  "*
{
  if (get_attr_length (insn) == 4)
    return \"b%c0 %1,%#,%l2\";
  else
    return \"b%C0 %1,%#,1f\;call %l2\\n1:\";
}"
  [(set (attr "length")
	(if_then_else
	    (and (ge (minus (match_dup 2) (pc)) (const_int -32768))
		 (le (minus (match_dup 2) (pc)) (const_int 32764)))
	    (const_int 4)
	    (const_int 8)))
   (set (attr "far_jump")
        (if_then_else
	    (eq_attr "length" "4")
	    (const_string "no")
	    (const_string "yes")))
   (set (attr "type")
	(if_then_else
	    (eq_attr "length" "4")
	    (const_string "branch")
	    (const_string "multi")))])

(define_insn "*branch_unsigned_false"
  [(set (pc)
	(if_then_else (match_operator:CC_UNS 0 "unsigned_relational_operator"
					     [(match_operand 1 "icc_operand" "t")
					      (const_int 0)])
		      (pc)
		      (label_ref (match_operand 2 "" ""))))]
  ""
  "*
{
  if (get_attr_length (insn) == 4)
    return \"b%C0 %1,%#,%l2\";
  else
    return \"b%c0 %1,%#,1f\;call %l2\\n1:\";
}"
  [(set (attr "length")
	(if_then_else
	    (and (ge (minus (match_dup 2) (pc)) (const_int -32768))
		 (le (minus (match_dup 2) (pc)) (const_int 32764)))
	    (const_int 4)
	    (const_int 8)))
   (set (attr "far_jump")
        (if_then_else
	    (eq_attr "length" "4")
	    (const_string "no")
	    (const_string "yes")))
   (set (attr "type")
	(if_then_else
	    (eq_attr "length" "4")
	    (const_string "branch")
	    (const_string "multi")))])

(define_insn "*branch_fp_true"
  [(set (pc)
	(if_then_else (match_operator:CC_FP 0 "float_relational_operator"
					    [(match_operand 1 "fcc_operand" "u")
					     (const_int 0)])
		      (label_ref (match_operand 2 "" ""))
		      (pc)))]
  ""
  "*
{
  if (get_attr_length (insn) == 4)
    return \"fb%f0 %1,%#,%l2\";
  else
    return \"fb%F0 %1,%#,1f\;call %l2\\n1:\";
}"
  [(set (attr "length")
	(if_then_else
	    (and (ge (minus (match_dup 2) (pc)) (const_int -32768))
		 (le (minus (match_dup 2) (pc)) (const_int 32764)))
	    (const_int 4)
	    (const_int 8)))
   (set (attr "far_jump")
        (if_then_else
	    (eq_attr "length" "4")
	    (const_string "no")
	    (const_string "yes")))
   (set (attr "type")
	(if_then_else
	    (eq_attr "length" "4")
	    (const_string "branch")
	    (const_string "multi")))])

(define_insn "*branch_fp_false"
  [(set (pc)
	(if_then_else (match_operator:CC_FP 0 "float_relational_operator"
					    [(match_operand 1 "fcc_operand" "u")
					     (const_int 0)])
		      (pc)
		      (label_ref (match_operand 2 "" ""))))]
  ""
  "*
{
  if (get_attr_length (insn) == 4)
    return \"fb%F0 %1,%#,%l2\";
  else
    return \"fb%f0 %1,%#,1f\;call %l2\\n1:\";
}"
  [(set (attr "length")
	(if_then_else
	    (and (ge (minus (match_dup 2) (pc)) (const_int -32768))
		 (le (minus (match_dup 2) (pc)) (const_int 32764)))
	    (const_int 4)
	    (const_int 8)))
   (set (attr "far_jump")
        (if_then_else
	    (eq_attr "length" "4")
	    (const_string "no")
	    (const_string "yes")))
   (set (attr "type")
	(if_then_else
	    (eq_attr "length" "4")
	    (const_string "branch")
	    (const_string "multi")))])


;; ::::::::::::::::::::
;; ::
;; :: Set flag operations
;; ::
;; ::::::::::::::::::::

;; Define_expands called by the machine independent part of the compiler
;; to allocate a new comparison register

(define_expand "seq"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (EQ, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "sne"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (NE, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "slt"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (LT, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "sle"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (LE, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "sgt"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (GT, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "sge"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (GE, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "sltu"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (LTU, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "sleu"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (LEU, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "sgtu"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (GTU, operands[0]))
    FAIL;

  DONE;
}")

(define_expand "sgeu"
  [(match_operand:SI 0 "integer_register_operand" "")]
  "TARGET_SCC"
  "
{
  if (! frv_emit_scc (GEU, operands[0]))
    FAIL;

  DONE;
}")

(define_insn "*scc_signed"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(match_operator:SI 1 "signed_relational_operator"
			   [(match_operand:CC 2 "icc_operand" "t")
			    (const_int 0)]))
   (clobber (match_operand:CC_CCR 3 "icr_operand" "=v"))]
  ""
  "#"
  [(set_attr "length" "12")
   (set_attr "type" "multi")])

(define_insn "*scc_unsigned"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(match_operator:SI 1 "unsigned_relational_operator"
			   [(match_operand:CC_UNS 2 "icc_operand" "t")
			    (const_int 0)]))
   (clobber (match_operand:CC_CCR 3 "icr_operand" "=v"))]
  ""
  "#"
  [(set_attr "length" "12")
   (set_attr "type" "multi")])

(define_insn "*scc_float"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(match_operator:SI 1 "float_relational_operator"
			   [(match_operand:CC_FP 2 "fcc_operand" "u")
			    (const_int 0)]))
   (clobber (match_operand:CC_CCR 3 "fcr_operand" "=w"))]
  ""
  "#"
  [(set_attr "length" "12")
   (set_attr "type" "multi")])

;; XXX -- add reload_completed to the splits, because register allocation
;; currently isn't ready to see cond_exec packets.
(define_split
  [(set (match_operand:SI 0 "integer_register_operand" "")
	(match_operator:SI 1 "relational_operator"
			   [(match_operand 2 "cc_operand" "")
			    (const_int 0)]))
   (clobber (match_operand 3 "cr_operand" ""))]
  "reload_completed"
  [(match_dup 4)]
  "operands[4] = frv_split_scc (operands[0], operands[1], operands[2],
				operands[3], (HOST_WIDE_INT) 1);")

(define_insn "*scc_neg1_signed"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(neg:SI (match_operator:SI 1 "signed_relational_operator"
				   [(match_operand:CC 2 "icc_operand" "t")
				    (const_int 0)])))
   (clobber (match_operand:CC_CCR 3 "icr_operand" "=v"))]
  ""
  "#"
  [(set_attr "length" "12")
   (set_attr "type" "multi")])

(define_insn "*scc_neg1_unsigned"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(neg:SI (match_operator:SI 1 "unsigned_relational_operator"
				   [(match_operand:CC_UNS 2 "icc_operand" "t")
				    (const_int 0)])))
   (clobber (match_operand:CC_CCR 3 "icr_operand" "=v"))]
  ""
  "#"
  [(set_attr "length" "12")
   (set_attr "type" "multi")])

(define_insn "*scc_neg1_float"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
	(neg:SI (match_operator:SI 1 "float_relational_operator"
				   [(match_operand:CC_FP 2 "fcc_operand" "u")
				    (const_int 0)])))
   (clobber (match_operand:CC_CCR 3 "fcr_operand" "=w"))]
  ""
  "#"
  [(set_attr "length" "12")
   (set_attr "type" "multi")])

(define_split
  [(set (match_operand:SI 0 "integer_register_operand" "")
	(neg:SI (match_operator:SI 1 "relational_operator"
				   [(match_operand 2 "cc_operand" "")
				    (const_int 0)])))
   (clobber (match_operand 3 "cr_operand" ""))]
  "reload_completed"
  [(match_dup 4)]
  "operands[4] = frv_split_scc (operands[0], operands[1], operands[2],
				operands[3], (HOST_WIDE_INT) -1);")


;; ::::::::::::::::::::
;; ::
;; :: Conditionally executed instructions
;; ::
;; ::::::::::::::::::::

;; Convert ICC/FCC comparison into CCR bits so we can do conditional execution
(define_insn "*ck_signed"
  [(set (match_operand:CC_CCR 0 "icr_operand" "=v")
	(match_operator:CC_CCR 1 "signed_relational_operator"
			       [(match_operand:CC 2 "icc_operand" "t")
				(const_int 0)]))]
  ""
  "ck%c1 %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "ccr")])

(define_insn "*ck_unsigned"
  [(set (match_operand:CC_CCR 0 "icr_operand" "=v")
	(match_operator:CC_CCR 1 "unsigned_relational_operator"
			       [(match_operand:CC_UNS 2 "icc_operand" "t")
				(const_int 0)]))]
  ""
  "ck%c1 %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "ccr")])

(define_insn "*fck_float"
  [(set (match_operand:CC_CCR 0 "fcr_operand" "=w")
	(match_operator:CC_CCR 1 "float_relational_operator"
			       [(match_operand:CC_FP 2 "fcc_operand" "u")
				(const_int 0)]))]
  "TARGET_HAS_FPRS"
  "fck%c1 %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "ccr")])

;; Conditionally convert ICC/FCC comparison into CCR bits to provide && and ||
;; tests in conditional execution
(define_insn "cond_exec_ck"
  [(set (match_operand:CC_CCR 0 "cr_operand" "=v,w")
	(if_then_else:CC_CCR (match_operator 1 "ccr_eqne_operator"
					     [(match_operand 2 "cr_operand" "C,C")
					      (const_int 0)])
			     (match_operator 3 "relational_operator"
					     [(match_operand 4 "cc_operand" "t,u")
					      (const_int 0)])
			     (const_int 0)))]
  ""
  "@
   cck%c3 %4, %0, %2, %e1
   cfck%f3 %4, %0, %2, %e1"
  [(set_attr "length" "4")
   (set_attr "type" "ccr")])

;; Conditionally set a register to either 0 or another register
(define_insn "*cond_exec_movqi"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C,C,C,C,C,C")
		     (const_int 0)])
    (set (match_operand:QI 2 "condexec_dest_operand" "=d,d,U,?f,?f,?d")
	 (match_operand:QI 3 "condexec_source_operand" "dO,U,dO,f,d,f")))]
  "register_operand(operands[2], QImode) || reg_or_0_operand (operands[3], QImode)"
  "* return output_condmove_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "int,gload,gstore,fsconv,movgf,movfg")])

(define_insn "*cond_exec_movhi"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C,C,C,C,C,C")
		     (const_int 0)])
    (set (match_operand:HI 2 "condexec_dest_operand" "=d,d,U,?f,?f,?d")
	 (match_operand:HI 3 "condexec_source_operand" "dO,U,dO,f,d,f")))]
  "register_operand(operands[2], HImode) || reg_or_0_operand (operands[3], HImode)"
  "* return output_condmove_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "int,gload,gstore,fsconv,movgf,movfg")])

(define_insn "*cond_exec_movsi"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C,C,C,C,C,C,C,C")
		     (const_int 0)])
    (set (match_operand:SI 2 "condexec_dest_operand" "=d,d,U,?f,?f,?d,?f,?m")
	 (match_operand:SI 3 "condexec_source_operand" "dO,U,dO,f,d,f,m,f")))]
  "register_operand(operands[2], SImode) || reg_or_0_operand (operands[3], SImode)"
  "* return output_condmove_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "int,gload,gstore,fsconv,movgf,movfg,fload,fstore")])


(define_insn "*cond_exec_movsf_has_fprs"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C,C,C,C,C,C,C,C,C,C")
		     (const_int 0)])
    (set (match_operand:SF 2 "condexec_dest_operand" "=f,?d,?d,?f,f,f,?d,U,?U,U")
	 (match_operand:SF 3 "condexec_source_operand" "f,d,f,d,G,U,U,f,d,G")))]
  "TARGET_HAS_FPRS"
  "* return output_condmove_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "fsconv,int,movgf,movfg,movgf,fload,gload,fstore,gstore,gstore")])

(define_insn "*cond_exec_movsf_no_fprs"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C,C,C")
		     (const_int 0)])
    (set (match_operand:SF 2 "condexec_dest_operand" "=d,d,U")
	 (match_operand:SF 3 "condexec_source_operand" "d,U,dG")))]
  "! TARGET_HAS_FPRS"
  "* return output_condmove_single (operands, insn);"
  [(set_attr "length" "4")
   (set_attr "type" "int,gload,gstore")])

(define_insn "*cond_exec_si_binary1"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "integer_register_operand" "=d")
	 (match_operator:SI 3 "condexec_si_binary_operator"
			    [(match_operand:SI 4 "integer_register_operand" "d")
			     (match_operand:SI 5 "integer_register_operand" "d")])))]
  ""
  "*
{
  switch (GET_CODE (operands[3]))
    {
      case PLUS:     return \"cadd %4, %z5, %2, %1, %e0\";
      case MINUS:    return \"csub %4, %z5, %2, %1, %e0\";
      case AND:      return \"cand %4, %z5, %2, %1, %e0\";
      case IOR:      return \"cor %4, %z5, %2, %1, %e0\";
      case XOR:      return \"cxor %4, %z5, %2, %1, %e0\";
      case ASHIFT:   return \"csll %4, %z5, %2, %1, %e0\";
      case ASHIFTRT: return \"csra %4, %z5, %2, %1, %e0\";
      case LSHIFTRT: return \"csrl %4, %z5, %2, %1, %e0\";
      default:       abort ();
    }
}"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_insn "*cond_exec_si_binary2"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "fpr_operand" "=f")
	 (match_operator:SI 3 "condexec_si_media_operator"
			    [(match_operand:SI 4 "fpr_operand" "f")
			     (match_operand:SI 5 "fpr_operand" "f")])))]
  "TARGET_MEDIA"
  "*
{
  switch (GET_CODE (operands[3]))
    {
      case AND: return \"cmand %4, %5, %2, %1, %e0\";
      case IOR: return \"cmor %4, %5, %2, %1, %e0\";
      case XOR: return \"cmxor %4, %5, %2, %1, %e0\";
      default:  abort ();
    }
}"
  [(set_attr "length" "4")
   (set_attr "type" "mlogic")])

;; Note, flow does not (currently) know how to handle an operation that uses
;; only part of the hard registers allocated for a multiregister value, such as
;; DImode in this case if the user is only interested in the lower 32-bits.  So
;; we emit a USE of the entire register after the csmul instruction so it won't
;; get confused.  See frv_ifcvt_modify_insn for more details.

(define_insn "*cond_exec_si_smul"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:DI 2 "even_gpr_operand" "=e")
	 (mult:DI (sign_extend:DI (match_operand:SI 3 "integer_register_operand" "%d"))
		  (sign_extend:DI (match_operand:SI 4 "integer_register_operand" "d")))))]
  ""
  "csmul %3, %4, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "mul")])

(define_insn "*cond_exec_si_divide"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "integer_register_operand" "=d")
	 (match_operator:SI 3 "condexec_si_divide_operator"
			    [(match_operand:SI 4 "integer_register_operand" "d")
			     (match_operand:SI 5 "integer_register_operand" "d")])))]
  ""
  "*
{
  switch (GET_CODE (operands[3]))
    {
      case DIV:  return \"csdiv %4, %z5, %2, %1, %e0\";
      case UDIV: return \"cudiv %4, %z5, %2, %1, %e0\";
      default:   abort ();
    }
}"
  [(set_attr "length" "4")
   (set_attr "type" "div")])

(define_insn "*cond_exec_si_unary1"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "integer_register_operand" "=d")
	 (match_operator:SI 3 "condexec_si_unary_operator"
			    [(match_operand:SI 4 "integer_register_operand" "d")])))]
  ""
  "*
{
  switch (GET_CODE (operands[3]))
    {
      case NOT: return \"cnot %4, %2, %1, %e0\";
      case NEG: return \"csub %., %4, %2, %1, %e0\";
      default:  abort ();
    }
}"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_insn "*cond_exec_si_unary2"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "fpr_operand" "=f")
	 (not:SI (match_operand:SI 3 "fpr_operand" "f"))))]
  "TARGET_MEDIA"
  "cmnot %3, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "mlogic")])

(define_insn "*cond_exec_cmpsi_cc"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:CC 2 "icc_operand" "=t")
	 (compare:CC (match_operand:SI 3 "integer_register_operand" "d")
		     (match_operand:SI 4 "reg_or_0_operand" "dO"))))]
  "reload_completed
   && REGNO (operands[1]) == REGNO (operands[2]) - ICC_FIRST + ICR_FIRST"
  "ccmp %3, %z4, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_insn "*cond_exec_cmpsi_cc_uns"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:CC_UNS 2 "icc_operand" "=t")
	 (compare:CC_UNS (match_operand:SI 3 "integer_register_operand" "d")
			 (match_operand:SI 4 "reg_or_0_operand" "dO"))))]
  "reload_completed
   && REGNO (operands[1]) == REGNO (operands[2]) - ICC_FIRST + ICR_FIRST"
  "ccmp %3, %z4, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

(define_insn "*cond_exec_sf_conv"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SF 2 "fpr_operand" "=f")
	 (match_operator:SF 3 "condexec_sf_conv_operator"
			    [(match_operand:SF 4 "fpr_operand" "f")])))]
  "TARGET_HARD_FLOAT"
  "*
{
  switch (GET_CODE (operands[3]))
    {
      case ABS: return \"cfabss %4, %2, %1, %e0\";
      case NEG: return \"cfnegs %4, %2, %1, %e0\";
      default:  abort ();
    }
}"
  [(set_attr "length" "4")
   (set_attr "type" "fsconv")])

(define_insn "*cond_exec_sf_add"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SF 2 "fpr_operand" "=f")
	 (match_operator:SF 3 "condexec_sf_add_operator"
			    [(match_operand:SF 4 "fpr_operand" "f")
			     (match_operand:SF 5 "fpr_operand" "f")])))]
  "TARGET_HARD_FLOAT"
  "*
{
  switch (GET_CODE (operands[3]))
    {
      case PLUS:  return \"cfadds %4, %5, %2, %1, %e0\";
      case MINUS: return \"cfsubs %4, %5, %2, %1, %e0\";
      default:    abort ();
    }
}"
  [(set_attr "length" "4")
   (set_attr "type" "fsadd")])

(define_insn "*cond_exec_sf_mul"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SF 2 "fpr_operand" "=f")
	 (mult:SF (match_operand:SF 3 "fpr_operand" "f")
		  (match_operand:SF 4 "fpr_operand" "f"))))]
  "TARGET_HARD_FLOAT"
  "cfmuls %3, %4, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "fsmul")])

(define_insn "*cond_exec_sf_div"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SF 2 "fpr_operand" "=f")
	 (div:SF (match_operand:SF 3 "fpr_operand" "f")
		 (match_operand:SF 4 "fpr_operand" "f"))))]
  "TARGET_HARD_FLOAT"
  "cfdivs %3, %4, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "fsdiv")])

(define_insn "*cond_exec_sf_sqrt"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SF 2 "fpr_operand" "=f")
	 (sqrt:SF (match_operand:SF 3 "fpr_operand" "f"))))]
  "TARGET_HARD_FLOAT"
  "cfsqrts %3, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "fsdiv")])

(define_insn "*cond_exec_cmpsi_cc_fp"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:CC_FP 2 "fcc_operand" "=u")
	 (compare:CC_FP (match_operand:SF 3 "fpr_operand" "f")
			(match_operand:SF 4 "fpr_operand" "f"))))]
  "reload_completed && TARGET_HARD_FLOAT
   && REGNO (operands[1]) == REGNO (operands[2]) - FCC_FIRST + FCR_FIRST"
  "cfcmps %3, %4, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "fsconv")])


;; ::::::::::::::::::::
;; ::
;; :: Logical operations on CR registers
;; ::
;; ::::::::::::::::::::

;; We use UNSPEC to encode andcr/iorcr/etc. rather than the normal RTL
;; operations, since the RTL operations only have an idea of TRUE and FALSE,
;; while the CRs have TRUE, FALSE, and UNDEFINED.

(define_expand "andcr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_operand:CC_CCR 2 "cr_operand" "")
			(const_int 0)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_expand "orcr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_operand:CC_CCR 2 "cr_operand" "")
			(const_int 1)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_expand "xorcr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_operand:CC_CCR 2 "cr_operand" "")
			(const_int 2)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_expand "nandcr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_operand:CC_CCR 2 "cr_operand" "")
			(const_int 3)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_expand "norcr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_operand:CC_CCR 2 "cr_operand" "")
			(const_int 4)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_expand "andncr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_operand:CC_CCR 2 "cr_operand" "")
			(const_int 5)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_expand "orncr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_operand:CC_CCR 2 "cr_operand" "")
			(const_int 6)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_expand "nandncr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_operand:CC_CCR 2 "cr_operand" "")
			(const_int 7)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_expand "norncr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_operand:CC_CCR 2 "cr_operand" "")
			(const_int 8)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_expand "notcr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "")
			(match_dup 1)
			(const_int 9)] UNSPEC_CR_LOGIC))]
  ""
  "")

(define_insn "*logical_cr"
  [(set (match_operand:CC_CCR 0 "cr_operand" "=C")
	(unspec:CC_CCR [(match_operand:CC_CCR 1 "cr_operand" "C")
			(match_operand:CC_CCR 2 "cr_operand" "C")
			(match_operand:SI 3 "const_int_operand" "n")]
		       UNSPEC_CR_LOGIC))]
  ""
  "*
{
  switch (INTVAL (operands[3]))
  {
  default: break;
  case 0: return \"andcr %1, %2, %0\";
  case 1: return \"orcr %1, %2, %0\";
  case 2: return \"xorcr %1, %2, %0\";
  case 3: return \"nandcr %1, %2, %0\";
  case 4: return \"norcr %1, %2, %0\";
  case 5: return \"andncr %1, %2, %0\";
  case 6: return \"orncr %1, %2, %0\";
  case 7: return \"nandncr %1, %2, %0\";
  case 8: return \"norncr %1, %2, %0\";
  case 9: return \"notcr %1, %0\";
  }

  fatal_insn (\"logical_cr\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "ccr")])


;; ::::::::::::::::::::
;; ::
;; :: Conditional move instructions
;; ::
;; ::::::::::::::::::::


;; - conditional moves based on floating-point comparisons require
;;   TARGET_HARD_FLOAT, because an FPU is required to do the comparison.

;; - conditional moves between FPRs based on integer comparisons
;;   require TARGET_HAS_FPRS.

(define_expand "movqicc"
  [(set (match_operand:QI 0 "integer_register_operand" "")
	(if_then_else:QI (match_operand 1 "" "")
			 (match_operand:QI 2 "gpr_or_int_operand" "")
			 (match_operand:QI 3 "gpr_or_int_operand" "")))]
  "TARGET_COND_MOVE"
  "
{
  if (!frv_emit_cond_move (operands[0], operands[1], operands[2], operands[3]))
    FAIL;

  DONE;
}")

(define_insn "*movqicc_internal1_signed"
  [(set (match_operand:QI 0 "integer_register_operand" "=d,d,d")
	(if_then_else:QI (match_operator:CC 1 "signed_relational_operator"
			     [(match_operand:CC 2 "icc_operand" "t,t,t")
			      (const_int 0)])
			 (match_operand:QI 3 "reg_or_0_operand" "0,dO,dO")
			 (match_operand:QI 4 "reg_or_0_operand" "dO,0,dO")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  ""
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movqicc_internal1_unsigned"
  [(set (match_operand:QI 0 "integer_register_operand" "=d,d,d")
	(if_then_else:QI (match_operator:CC_UNS 1 "unsigned_relational_operator"
			     [(match_operand:CC_UNS 2 "icc_operand" "t,t,t")
			      (const_int 0)])
			 (match_operand:QI 3 "reg_or_0_operand" "0,dO,dO")
			 (match_operand:QI 4 "reg_or_0_operand" "dO,0,dO")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  ""
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movqicc_internal1_float"
  [(set (match_operand:QI 0 "integer_register_operand" "=d,d,d")
	(if_then_else:QI (match_operator:CC_FP 1 "float_relational_operator"
			     [(match_operand:CC_FP 2 "fcc_operand" "u,u,u")
			      (const_int 0)])
			 (match_operand:QI 3 "reg_or_0_operand" "0,dO,dO")
			 (match_operand:QI 4 "reg_or_0_operand" "dO,0,dO")))
   (clobber (match_operand:CC_CCR 5 "fcr_operand" "=w,w,w"))]
  "TARGET_HARD_FLOAT"
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movqicc_internal2_signed"
  [(set (match_operand:QI 0 "integer_register_operand" "=d,d,d,d,d")
	(if_then_else:QI (match_operator:CC 1 "signed_relational_operator"
			     [(match_operand:CC 2 "icc_operand" "t,t,t,t,t")
			      (const_int 0)])
			 (match_operand:QI 3 "const_int_operand" "O,O,L,n,n")
			 (match_operand:QI 4 "const_int_operand" "L,n,O,O,n")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v,v,v"))]
  "(INTVAL (operands[3]) == 0
    || INTVAL (operands[4]) == 0
    || (IN_RANGE_P (INTVAL (operands[3]), -2048, 2047)
        && IN_RANGE_P (INTVAL (operands[4]) - INTVAL (operands[3]), -2048, 2047)))"
  "#"
  [(set_attr "length" "8,12,8,12,12")
   (set_attr "type" "multi")])

(define_insn "*movqicc_internal2_unsigned"
  [(set (match_operand:QI 0 "integer_register_operand" "=d,d,d,d,d")
	(if_then_else:QI (match_operator:CC_UNS 1 "unsigned_relational_operator"
			     [(match_operand:CC_UNS 2 "icc_operand" "t,t,t,t,t")
			      (const_int 0)])
			 (match_operand:QI 3 "const_int_operand" "O,O,L,n,n")
			 (match_operand:QI 4 "const_int_operand" "L,n,O,O,n")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v,v,v"))]
  "(INTVAL (operands[3]) == 0
    || INTVAL (operands[4]) == 0
    || (IN_RANGE_P (INTVAL (operands[3]), -2048, 2047)
        && IN_RANGE_P (INTVAL (operands[4]) - INTVAL (operands[3]), -2048, 2047)))"
  "#"
  [(set_attr "length" "8,12,8,12,12")
   (set_attr "type" "multi")])

(define_insn "*movqicc_internal2_float"
  [(set (match_operand:QI 0 "integer_register_operand" "=d,d,d,d,d")
	(if_then_else:QI (match_operator:CC_FP 1 "float_relational_operator"
			     [(match_operand:CC_FP 2 "fcc_operand" "u,u,u,u,u")
			      (const_int 0)])
			 (match_operand:QI 3 "const_int_operand" "O,O,L,n,n")
			 (match_operand:QI 4 "const_int_operand" "L,n,O,O,n")))
   (clobber (match_operand:CC_CCR 5 "fcr_operand" "=w,w,w,w,w"))]
  "TARGET_HARD_FLOAT
   && (INTVAL (operands[3]) == 0
       || INTVAL (operands[4]) == 0
       || (IN_RANGE_P (INTVAL (operands[3]), -2048, 2047)
	   && IN_RANGE_P (INTVAL (operands[4]) - INTVAL (operands[3]), -2048, 2047)))"
  "#"
  [(set_attr "length" "8,12,8,12,12")
   (set_attr "type" "multi")])

(define_split
  [(set (match_operand:QI 0 "integer_register_operand" "")
	(if_then_else:QI (match_operator 1 "relational_operator"
			     [(match_operand 2 "cc_operand" "")
			      (const_int 0)])
			 (match_operand:QI 3 "gpr_or_int_operand" "")
			 (match_operand:QI 4 "gpr_or_int_operand" "")))
   (clobber (match_operand:CC_CCR 5 "cr_operand" ""))]
  "reload_completed"
  [(match_dup 6)]
  "operands[6] = frv_split_cond_move (operands);")

(define_expand "movhicc"
  [(set (match_operand:HI 0 "integer_register_operand" "")
	(if_then_else:HI (match_operand 1 "" "")
			 (match_operand:HI 2 "gpr_or_int_operand" "")
			 (match_operand:HI 3 "gpr_or_int_operand" "")))]
  "TARGET_COND_MOVE"
  "
{
  if (!frv_emit_cond_move (operands[0], operands[1], operands[2], operands[3]))
    FAIL;

  DONE;
}")

(define_insn "*movhicc_internal1_signed"
  [(set (match_operand:HI 0 "integer_register_operand" "=d,d,d")
	(if_then_else:HI (match_operator:CC 1 "signed_relational_operator"
			     [(match_operand:CC 2 "icc_operand" "t,t,t")
			      (const_int 0)])
			 (match_operand:HI 3 "reg_or_0_operand" "0,dO,dO")
			 (match_operand:HI 4 "reg_or_0_operand" "dO,0,dO")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  ""
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movhicc_internal1_unsigned"
  [(set (match_operand:HI 0 "integer_register_operand" "=d,d,d")
	(if_then_else:HI (match_operator:CC_UNS 1 "unsigned_relational_operator"
			     [(match_operand:CC_UNS 2 "icc_operand" "t,t,t")
			      (const_int 0)])
			 (match_operand:HI 3 "reg_or_0_operand" "0,dO,dO")
			 (match_operand:HI 4 "reg_or_0_operand" "dO,0,dO")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  ""
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movhicc_internal1_float"
  [(set (match_operand:HI 0 "integer_register_operand" "=d,d,d")
	(if_then_else:HI (match_operator:CC_FP 1 "float_relational_operator"
			     [(match_operand:CC_FP 2 "fcc_operand" "u,u,u")
			      (const_int 0)])
			 (match_operand:HI 3 "reg_or_0_operand" "0,dO,dO")
			 (match_operand:HI 4 "reg_or_0_operand" "dO,0,dO")))
   (clobber (match_operand:CC_CCR 5 "fcr_operand" "=w,w,w"))]
  "TARGET_HARD_FLOAT"
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movhicc_internal2_signed"
  [(set (match_operand:HI 0 "integer_register_operand" "=d,d,d,d,d")
	(if_then_else:HI (match_operator:CC 1 "signed_relational_operator"
			     [(match_operand:CC 2 "icc_operand" "t,t,t,t,t")
			      (const_int 0)])
			 (match_operand:HI 3 "const_int_operand" "O,O,L,n,n")
			 (match_operand:HI 4 "const_int_operand" "L,n,O,O,n")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v,v,v"))]
  "(INTVAL (operands[3]) == 0
    || INTVAL (operands[4]) == 0
    || (IN_RANGE_P (INTVAL (operands[3]), -2048, 2047)
        && IN_RANGE_P (INTVAL (operands[4]) - INTVAL (operands[3]), -2048, 2047)))"
  "#"
  [(set_attr "length" "8,12,8,12,12")
   (set_attr "type" "multi")])

(define_insn "*movhicc_internal2_unsigned"
  [(set (match_operand:HI 0 "integer_register_operand" "=d,d,d,d,d")
	(if_then_else:HI (match_operator:CC_UNS 1 "unsigned_relational_operator"
			     [(match_operand:CC_UNS 2 "icc_operand" "t,t,t,t,t")
			      (const_int 0)])
			 (match_operand:HI 3 "const_int_operand" "O,O,L,n,n")
			 (match_operand:HI 4 "const_int_operand" "L,n,O,O,n")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v,v,v"))]
  "(INTVAL (operands[3]) == 0
    || INTVAL (operands[4]) == 0
    || (IN_RANGE_P (INTVAL (operands[3]), -2048, 2047)
        && IN_RANGE_P (INTVAL (operands[4]) - INTVAL (operands[3]), -2048, 2047)))"
  "#"
  [(set_attr "length" "8,12,8,12,12")
   (set_attr "type" "multi")])

(define_insn "*movhicc_internal2_float"
  [(set (match_operand:HI 0 "integer_register_operand" "=d,d,d,d,d")
	(if_then_else:HI (match_operator:CC_FP 1 "float_relational_operator"
			     [(match_operand:CC_FP 2 "fcc_operand" "u,u,u,u,u")
			      (const_int 0)])
			 (match_operand:HI 3 "const_int_operand" "O,O,L,n,n")
			 (match_operand:HI 4 "const_int_operand" "L,n,O,O,n")))
   (clobber (match_operand:CC_CCR 5 "fcr_operand" "=w,w,w,w,w"))]
  "TARGET_HARD_FLOAT
   && (INTVAL (operands[3]) == 0
       || INTVAL (operands[4]) == 0
       || (IN_RANGE_P (INTVAL (operands[3]), -2048, 2047)
	   && IN_RANGE_P (INTVAL (operands[4]) - INTVAL (operands[3]), -2048, 2047)))"
  "#"
  [(set_attr "length" "8,12,8,12,12")
   (set_attr "type" "multi")])

(define_split
  [(set (match_operand:HI 0 "integer_register_operand" "")
	(if_then_else:HI (match_operator 1 "relational_operator"
			     [(match_operand 2 "cc_operand" "")
			      (const_int 0)])
			 (match_operand:HI 3 "gpr_or_int_operand" "")
			 (match_operand:HI 4 "gpr_or_int_operand" "")))
   (clobber (match_operand:CC_CCR 5 "cr_operand" ""))]
  "reload_completed"
  [(match_dup 6)]
  "operands[6] = frv_split_cond_move (operands);")

(define_expand "movsicc"
  [(set (match_operand:SI 0 "integer_register_operand" "")
	(if_then_else:SI (match_operand 1 "" "")
			 (match_operand:SI 2 "gpr_or_int_operand" "")
			 (match_operand:SI 3 "gpr_or_int_operand" "")))]
  "TARGET_COND_MOVE"
  "
{
  if (!frv_emit_cond_move (operands[0], operands[1], operands[2], operands[3]))
    FAIL;

  DONE;
}")

(define_insn "*movsicc_internal1_signed"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d,d")
	(if_then_else:SI (match_operator:CC 1 "signed_relational_operator"
			     [(match_operand:CC 2 "icc_operand" "t,t,t")
			      (const_int 0)])
			 (match_operand:SI 3 "reg_or_0_operand" "0,dO,dO")
			 (match_operand:SI 4 "reg_or_0_operand" "dO,0,dO")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  ""
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movsicc_internal1_unsigned"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d,d")
	(if_then_else:SI (match_operator:CC_UNS 1 "unsigned_relational_operator"
			     [(match_operand:CC_UNS 2 "icc_operand" "t,t,t")
			      (const_int 0)])
			 (match_operand:SI 3 "reg_or_0_operand" "0,dO,dO")
			 (match_operand:SI 4 "reg_or_0_operand" "dO,0,dO")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  ""
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movsicc_internal1_float"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d,d")
	(if_then_else:SI (match_operator:CC_FP 1 "float_relational_operator"
			     [(match_operand:CC_FP 2 "fcc_operand" "u,u,u")
			      (const_int 0)])
			 (match_operand:SI 3 "reg_or_0_operand" "0,dO,dO")
			 (match_operand:SI 4 "reg_or_0_operand" "dO,0,dO")))
   (clobber (match_operand:CC_CCR 5 "fcr_operand" "=w,w,w"))]
  "TARGET_HARD_FLOAT"
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movsicc_internal2_signed"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d,d,d,d")
	(if_then_else:SI (match_operator:CC 1 "signed_relational_operator"
			     [(match_operand:CC 2 "icc_operand" "t,t,t,t,t")
			      (const_int 0)])
			 (match_operand:SI 3 "const_int_operand" "O,O,L,n,n")
			 (match_operand:SI 4 "const_int_operand" "L,n,O,O,n")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v,v,v"))]
  "(INTVAL (operands[3]) == 0
    || INTVAL (operands[4]) == 0
    || (IN_RANGE_P (INTVAL (operands[3]), -2048, 2047)
        && IN_RANGE_P (INTVAL (operands[4]) - INTVAL (operands[3]), -2048, 2047)))"
  "#"
  [(set_attr "length" "8,12,8,12,12")
   (set_attr "type" "multi")])

(define_insn "*movsicc_internal2_unsigned"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d,d,d,d")
	(if_then_else:SI (match_operator:CC_UNS 1 "unsigned_relational_operator"
			     [(match_operand:CC_UNS 2 "icc_operand" "t,t,t,t,t")
			      (const_int 0)])
			 (match_operand:SI 3 "const_int_operand" "O,O,L,n,n")
			 (match_operand:SI 4 "const_int_operand" "L,n,O,O,n")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v,v,v"))]
  "(INTVAL (operands[3]) == 0
    || INTVAL (operands[4]) == 0
    || (IN_RANGE_P (INTVAL (operands[3]), -2048, 2047)
        && IN_RANGE_P (INTVAL (operands[4]) - INTVAL (operands[3]), -2048, 2047)))"
  "#"
  [(set_attr "length" "8,12,8,12,12")
   (set_attr "type" "multi")])

(define_insn "*movsicc_internal2_float"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d,d,d,d")
	(if_then_else:SI (match_operator:CC_FP 1 "float_relational_operator"
			     [(match_operand:CC_FP 2 "fcc_operand" "u,u,u,u,u")
			      (const_int 0)])
			 (match_operand:SI 3 "const_int_operand" "O,O,L,n,n")
			 (match_operand:SI 4 "const_int_operand" "L,n,O,O,n")))
   (clobber (match_operand:CC_CCR 5 "fcr_operand" "=w,w,w,w,w"))]
  "TARGET_HARD_FLOAT
   && (INTVAL (operands[3]) == 0
       || INTVAL (operands[4]) == 0
       || (IN_RANGE_P (INTVAL (operands[3]), -2048, 2047)
	   && IN_RANGE_P (INTVAL (operands[4]) - INTVAL (operands[3]), -2048, 2047)))"
  "#"
  [(set_attr "length" "8,12,8,12,12")
   (set_attr "type" "multi")])

(define_split
  [(set (match_operand:SI 0 "integer_register_operand" "")
	(if_then_else:SI (match_operator 1 "relational_operator"
			     [(match_operand 2 "cc_operand" "")
			      (const_int 0)])
			 (match_operand:SI 3 "gpr_or_int_operand" "")
			 (match_operand:SI 4 "gpr_or_int_operand" "")))
   (clobber (match_operand:CC_CCR 5 "cr_operand" ""))]
  "reload_completed"
  [(match_dup 6)]
  "operands[6] = frv_split_cond_move (operands);")

(define_expand "movsfcc"
  [(set (match_operand:SF 0 "register_operand" "")
	(if_then_else:SF (match_operand 1 "" "")
			 (match_operand:SF 2 "register_operand" "")
			 (match_operand:SF 3 "register_operand" "")))]
  "TARGET_COND_MOVE"
  "
{
  if (!frv_emit_cond_move (operands[0], operands[1], operands[2], operands[3]))
    FAIL;

  DONE;
}")

(define_insn "*movsfcc_has_fprs_signed"
  [(set (match_operand:SF 0 "register_operand" "=f,f,f,?f,?f,?d")
	(if_then_else:SF (match_operator:CC 1 "signed_relational_operator"
			     [(match_operand:CC 2 "icc_operand" "t,t,t,t,t,t")
			      (const_int 0)])
			 (match_operand:SF 3 "register_operand" "0,f,f,f,d,fd")
			 (match_operand:SF 4 "register_operand" "f,0,f,d,fd,fd")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v,v,v,v"))]
  "TARGET_HAS_FPRS"
  "#"
  [(set_attr "length" "8,8,12,12,12,12")
   (set_attr "type" "multi")])

(define_insn "*movsfcc_has_fprs_unsigned"
  [(set (match_operand:SF 0 "register_operand" "=f,f,f,?f,?f,?d")
	(if_then_else:SF (match_operator:CC_UNS 1 "unsigned_relational_operator"
			     [(match_operand:CC_UNS 2 "icc_operand" "t,t,t,t,t,t")
			      (const_int 0)])
			 (match_operand:SF 3 "register_operand" "0,f,f,f,d,fd")
			 (match_operand:SF 4 "register_operand" "f,0,f,d,fd,fd")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v,v,v,v"))]
  "TARGET_HAS_FPRS"
  "#"
  [(set_attr "length" "8,8,12,12,12,12")
   (set_attr "type" "multi")])

(define_insn "*movsfcc_hardfloat_float"
  [(set (match_operand:SF 0 "register_operand" "=f,f,f,?f,?f,?d")
	(if_then_else:SF (match_operator:CC_FP 1 "float_relational_operator"
			     [(match_operand:CC_FP 2 "fcc_operand" "u,u,u,u,u,u")
			      (const_int 0)])
			 (match_operand:SF 3 "register_operand" "0,f,f,f,d,fd")
			 (match_operand:SF 4 "register_operand" "f,0,f,d,fd,fd")))
   (clobber (match_operand:CC_CCR 5 "fcr_operand" "=w,w,w,w,w,w"))]
  "TARGET_HARD_FLOAT"
  "#"
  [(set_attr "length" "8,8,12,12,12,12")
   (set_attr "type" "multi")])

(define_insn "*movsfcc_no_fprs_signed"
  [(set (match_operand:SF 0 "integer_register_operand" "=d,d,d")
	(if_then_else:SF (match_operator:CC 1 "signed_relational_operator"
			     [(match_operand:CC 2 "icc_operand" "t,t,t")
			      (const_int 0)])
			 (match_operand:SF 3 "integer_register_operand" "0,d,d")
			 (match_operand:SF 4 "integer_register_operand" "d,0,d")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  "! TARGET_HAS_FPRS"
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_insn "*movsfcc_no_fprs_unsigned"
  [(set (match_operand:SF 0 "integer_register_operand" "=d,d,d")
	(if_then_else:SF (match_operator:CC_UNS 1 "unsigned_relational_operator"
			     [(match_operand:CC_UNS 2 "icc_operand" "t,t,t")
			      (const_int 0)])
			 (match_operand:SF 3 "integer_register_operand" "0,d,d")
			 (match_operand:SF 4 "integer_register_operand" "d,0,d")))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  "! TARGET_HAS_FPRS"
  "#"
  [(set_attr "length" "8,8,12")
   (set_attr "type" "multi")])

(define_split
  [(set (match_operand:SF 0 "register_operand" "")
	(if_then_else:SF (match_operator 1 "relational_operator"
			     [(match_operand 2 "cc_operand" "")
			      (const_int 0)])
			 (match_operand:SF 3 "register_operand" "")
			 (match_operand:SF 4 "register_operand" "")))
   (clobber (match_operand:CC_CCR 5 "cr_operand" ""))]
  "reload_completed"
  [(match_dup 6)]
  "operands[6] = frv_split_cond_move (operands);")


;; ::::::::::::::::::::
;; ::
;; :: Minimum, maximum, and integer absolute value
;; ::
;; ::::::::::::::::::::

;; These 'instructions' are provided to give the compiler a slightly better
;; nudge at register allocation, then it would if it constructed the
;; instructions from basic building blocks (since it indicates it prefers one
;; of the operands to be the same as the destination.  It also helps the
;; earlier passes of the compiler, by not breaking things into small basic
;; blocks.

(define_expand "abssi2"
  [(parallel [(set (match_operand:SI 0 "integer_register_operand" "")
		   (abs:SI (match_operand:SI 1 "integer_register_operand" "")))
	      (clobber (match_dup 2))
	      (clobber (match_dup 3))])]
  "TARGET_COND_MOVE"
  "
{
  operands[2] = gen_reg_rtx (CCmode);
  operands[3] = gen_reg_rtx (CC_CCRmode);
}")

(define_insn_and_split "*abssi2_internal"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d")
	(abs:SI (match_operand:SI 1 "integer_register_operand" "0,d")))
   (clobber (match_operand:CC 2 "icc_operand" "=t,t"))
   (clobber (match_operand:CC_CCR 3 "icr_operand" "=v,v"))]
  "TARGET_COND_MOVE"
  "#"
  "reload_completed"
  [(match_dup 4)]
  "operands[4] = frv_split_abs (operands);"
  [(set_attr "length" "12,16")
   (set_attr "type" "multi")])

(define_expand "sminsi3"
  [(parallel [(set (match_operand:SI 0 "integer_register_operand" "")
		   (smin:SI (match_operand:SI 1 "integer_register_operand" "")
			    (match_operand:SI 2 "gpr_or_int10_operand" "")))
	      (clobber (match_dup 3))
	      (clobber (match_dup 4))])]
  "TARGET_COND_MOVE"
  "
{
  operands[3] = gen_reg_rtx (CCmode);
  operands[4] = gen_reg_rtx (CC_CCRmode);
}")

(define_expand "smaxsi3"
  [(parallel [(set (match_operand:SI 0 "integer_register_operand" "")
		   (smax:SI (match_operand:SI 1 "integer_register_operand" "")
			    (match_operand:SI 2 "gpr_or_int10_operand" "")))
	      (clobber (match_dup 3))
	      (clobber (match_dup 4))])]
  "TARGET_COND_MOVE"
  "
{
  operands[3] = gen_reg_rtx (CCmode);
  operands[4] = gen_reg_rtx (CC_CCRmode);
}")

(define_insn_and_split "*minmax_si_signed"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d,&d")
	(match_operator:SI 1 "minmax_operator"
			   [(match_operand:SI 2 "integer_register_operand" "%0,dO,d")
			    (match_operand:SI 3 "gpr_or_int10_operand" "dO,0,dJ")]))
   (clobber (match_operand:CC 4 "icc_operand" "=t,t,t"))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  "TARGET_COND_MOVE"
  "#"
  "reload_completed"
  [(match_dup 6)]
  "operands[6] = frv_split_minmax (operands);"
  [(set_attr "length" "12,12,16")
   (set_attr "type" "multi")])

(define_expand "uminsi3"
  [(parallel [(set (match_operand:SI 0 "integer_register_operand" "")
		   (umin:SI (match_operand:SI 1 "integer_register_operand" "")
			    (match_operand:SI 2 "gpr_or_int10_operand" "")))
	      (clobber (match_dup 3))
	      (clobber (match_dup 4))])]
  "TARGET_COND_MOVE"
  "
{
  operands[3] = gen_reg_rtx (CC_UNSmode);
  operands[4] = gen_reg_rtx (CC_CCRmode);
}")

(define_expand "umaxsi3"
  [(parallel [(set (match_operand:SI 0 "integer_register_operand" "")
		   (umax:SI (match_operand:SI 1 "integer_register_operand" "")
			    (match_operand:SI 2 "gpr_or_int10_operand" "")))
	      (clobber (match_dup 3))
	      (clobber (match_dup 4))])]
  "TARGET_COND_MOVE"
  "
{
  operands[3] = gen_reg_rtx (CC_UNSmode);
  operands[4] = gen_reg_rtx (CC_CCRmode);
}")

(define_insn_and_split "*minmax_si_unsigned"
  [(set (match_operand:SI 0 "integer_register_operand" "=d,d,&d")
	(match_operator:SI 1 "minmax_operator"
			   [(match_operand:SI 2 "integer_register_operand" "%0,dO,d")
			    (match_operand:SI 3 "gpr_or_int10_operand" "dO,0,dJ")]))
   (clobber (match_operand:CC_UNS 4 "icc_operand" "=t,t,t"))
   (clobber (match_operand:CC_CCR 5 "icr_operand" "=v,v,v"))]
  "TARGET_COND_MOVE"
  "#"
  "reload_completed"
  [(match_dup 6)]
  "operands[6] = frv_split_minmax (operands);"
  [(set_attr "length" "12,12,16")
   (set_attr "type" "multi")])

(define_expand "sminsf3"
  [(parallel [(set (match_operand:SF 0 "fpr_operand" "")
		   (smin:SF (match_operand:SF 1 "fpr_operand" "")
			    (match_operand:SF 2 "fpr_operand" "")))
	      (clobber (match_dup 3))
	      (clobber (match_dup 4))])]
  "TARGET_COND_MOVE && TARGET_HARD_FLOAT"
  "
{
  operands[3] = gen_reg_rtx (CC_FPmode);
  operands[4] = gen_reg_rtx (CC_CCRmode);
}")

(define_expand "smaxsf3"
  [(parallel [(set (match_operand:SF 0 "fpr_operand" "")
		   (smax:SF (match_operand:SF 1 "fpr_operand" "")
			    (match_operand:SF 2 "fpr_operand" "")))
	      (clobber (match_dup 3))
	      (clobber (match_dup 4))])]
  "TARGET_COND_MOVE && TARGET_HARD_FLOAT"
  "
{
  operands[3] = gen_reg_rtx (CC_FPmode);
  operands[4] = gen_reg_rtx (CC_CCRmode);
}")

(define_insn_and_split "*minmax_sf"
  [(set (match_operand:SF 0 "fpr_operand" "=f,f,f")
	(match_operator:SF 1 "minmax_operator"
			   [(match_operand:SF 2 "fpr_operand" "%0,f,f")
			    (match_operand:SF 3 "fpr_operand" "f,0,f")]))
   (clobber (match_operand:CC_FP 4 "fcc_operand" "=u,u,u"))
   (clobber (match_operand:CC_CCR 5 "fcr_operand" "=w,w,w"))]
  "TARGET_COND_MOVE && TARGET_HARD_FLOAT"
  "#"
  "reload_completed"
  [(match_dup 6)]
  "operands[6] = frv_split_minmax (operands);"
  [(set_attr "length" "12,12,16")
   (set_attr "type" "multi")])

(define_expand "smindf3"
  [(parallel [(set (match_operand:DF 0 "fpr_operand" "")
		   (smin:DF (match_operand:DF 1 "fpr_operand" "")
			    (match_operand:DF 2 "fpr_operand" "")))
	      (clobber (match_dup 3))
	      (clobber (match_dup 4))])]
  "TARGET_COND_MOVE && TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "
{
  operands[3] = gen_reg_rtx (CC_FPmode);
  operands[4] = gen_reg_rtx (CC_CCRmode);
}")

(define_expand "smaxdf3"
  [(parallel [(set (match_operand:DF 0 "fpr_operand" "")
		   (smax:DF (match_operand:DF 1 "fpr_operand" "")
			    (match_operand:DF 2 "fpr_operand" "")))
	      (clobber (match_dup 3))
	      (clobber (match_dup 4))])]
  "TARGET_COND_MOVE && TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "
{
  operands[3] = gen_reg_rtx (CC_FPmode);
  operands[4] = gen_reg_rtx (CC_CCRmode);
}")

(define_insn_and_split "*minmax_df"
  [(set (match_operand:DF 0 "fpr_operand" "=f,f,f")
	(match_operator:DF 1 "minmax_operator"
			   [(match_operand:DF 2 "fpr_operand" "%0,f,f")
			    (match_operand:DF 3 "fpr_operand" "f,0,f")]))
   (clobber (match_operand:CC_FP 4 "fcc_operand" "=u,u,u"))
   (clobber (match_operand:CC_CCR 5 "fcr_operand" "=w,w,w"))]
  "TARGET_COND_MOVE && TARGET_HARD_FLOAT && TARGET_DOUBLE"
  "#"
  "reload_completed"
  [(match_dup 6)]
  "operands[6] = frv_split_minmax (operands);"
  [(set_attr "length" "12,12,16")
   (set_attr "type" "multi")])


;; ::::::::::::::::::::
;; ::
;; :: Call and branch instructions
;; ::
;; ::::::::::::::::::::

;; Subroutine call instruction returning no value.  Operand 0 is the function
;; to call; operand 1 is the number of bytes of arguments pushed (in mode
;; `SImode', except it is normally a `const_int'); operand 2 is the number of
;; registers used as operands.

;; On most machines, operand 2 is not actually stored into the RTL pattern.  It
;; is supplied for the sake of some RISC machines which need to put this
;; information into the assembler code; they can put it in the RTL instead of
;; operand 1.

(define_expand "call"
  [(use (match_operand:QI 0 "" ""))
   (use (match_operand 1 "" ""))
   (use (match_operand 2 "" ""))
   (use (match_operand 3 "" ""))]
  ""
  "
{
  rtx lr = gen_rtx_REG (Pmode, LR_REGNO);
  rtx addr;

  if (GET_CODE (operands[0]) != MEM)
    abort ();

  addr = XEXP (operands[0], 0);
  if (! call_operand (addr, Pmode))
    addr = force_reg (Pmode, addr);

  if (! operands[2])
    operands[2] = const0_rtx;

  emit_call_insn (gen_call_internal (addr, operands[1], operands[2], lr));
  DONE;
}")

(define_insn "call_internal"
  [(call (mem:QI (match_operand:SI 0 "call_operand" "S,dNOP"))
	 (match_operand 1 "" ""))
   (use (match_operand 2 "" ""))
   (clobber (match_operand:SI 3 "lr_operand" "=l,l"))]
  ""
  "@
   call %0
   call%i0l %M0"
  [(set_attr "length" "4")
   (set_attr "type" "call,jumpl")])

;; Subroutine call instruction returning a value.  Operand 0 is the hard
;; register in which the value is returned.  There are three more operands, the
;; same as the three operands of the `call' instruction (but with numbers
;; increased by one).

;; Subroutines that return `BLKmode' objects use the `call' insn.

(define_expand "call_value"
  [(use (match_operand 0 "" ""))
   (use (match_operand:QI 1 "" ""))
   (use (match_operand 2 "" ""))
   (use (match_operand 3 "" ""))
   (use (match_operand 4 "" ""))]
  ""
  "
{
  rtx lr = gen_rtx_REG (Pmode, LR_REGNO);
  rtx addr;

  if (GET_CODE (operands[1]) != MEM)
    abort ();

  addr = XEXP (operands[1], 0);
  if (! call_operand (addr, Pmode))
    addr = force_reg (Pmode, addr);

  if (! operands[3])
    operands[3] = const0_rtx;

  emit_call_insn (gen_call_value_internal (operands[0], addr, operands[2],
					   operands[3], lr));
  DONE;
}")

(define_insn "call_value_internal"
  [(set (match_operand 0 "register_operand" "=d,d")
	(call (mem:QI (match_operand:SI 1 "call_operand" "S,dNOP"))
		      (match_operand 2 "" "")))
   (use (match_operand 3 "" ""))
   (clobber (match_operand:SI 4 "lr_operand" "=l,l"))]
  ""
  "@
   call %1
   call%i1l %M1"
  [(set_attr "length" "4")
   (set_attr "type" "call,jumpl")])

;; return instruction generated instead of jmp to epilog
(define_expand "return"
  [(parallel [(return)
	      (use (match_dup 0))
	      (use (const_int 1))])]
  "direct_return_p ()"
  "
{
  operands[0] = gen_rtx_REG (Pmode, LR_REGNO);
}")

;; return instruction generated by the epilogue
(define_expand "epilogue_return"
  [(parallel [(return)
	      (use (match_operand:SI 0 "register_operand" ""))
	      (use (const_int 0))])]
  ""
  "")

(define_insn "*return_internal"
  [(return)
   (use (match_operand:SI 0 "register_operand" "l,d"))
   (use (match_operand:SI 1 "immediate_operand" "n,n"))]
  ""
  "@
    ret
    jmpl @(%0,%.)"
  [(set_attr "length" "4")
   (set_attr "type" "jump,jumpl")])

;; A version of addsi3 for deallocating stack space at the end of the
;; epilogue.  The addition is done in parallel with an (unspec_volatile),
;; which represents the clobbering of the deallocated space.
(define_insn "stack_adjust"
  [(set (match_operand:SI 0 "register_operand" "=d")
        (plus:SI (match_operand:SI 1 "register_operand" "d")
		 (match_operand:SI 2 "general_operand" "dNOP")))
   (unspec_volatile [(const_int 0)] UNSPEC_STACK_ADJUST)]
  ""
  "add%I2 %1,%2,%0"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

;; Normal unconditional jump

;; Use the "call" instruction for long branches, but prefer to use "bra" for
;; short ones since it does not force us to save the link register.

;; This define_insn uses the branch-shortening code to decide which
;; instruction it emits.  Since the main branch-shortening interface is
;; through get_attr_length(), the two alternatives must be given different
;; lengths.  Here we pretend that the far jump is 8 rather than 4 bytes
;; long, though both alternatives are really the same size.
(define_insn "jump"
  [(set (pc) (label_ref (match_operand 0 "" "")))]
  ""
  "*
{
  if (get_attr_length (insn) == 4)
    return \"bra %l0\";
  else
    return \"call %l0\";
}"
  [(set (attr "length")
        (if_then_else
	    (and (ge (minus (match_dup 0) (pc)) (const_int -32768))
		 (le (minus (match_dup 0) (pc)) (const_int 32764)))
	    (const_int 4)
	    (const_int 8)))
   (set (attr "far_jump")
        (if_then_else
	    (eq_attr "length" "4")
	    (const_string "no")
	    (const_string "yes")))
   (set (attr "type")
	(if_then_else
	    (eq_attr "length" "4")
	    (const_string "jump")
	    (const_string "call")))])

;; Indirect jump through a register
(define_insn "indirect_jump"
  [(set (pc) (match_operand:SI 0 "register_operand" "d,l"))]
  ""
  "@
   jmpl @(%0,%.)
   bralr"
  [(set_attr "length" "4")
   (set_attr "type" "jumpl,branch")])

;; Instruction to jump to a variable address.  This is a low-level capability
;; which can be used to implement a dispatch table when there is no `casesi'
;; pattern.  Either the 'casesi' pattern or the 'tablejump' pattern, or both,
;; MUST be present in this file.

;; This pattern requires two operands: the address or offset, and a label which
;; should immediately precede the jump table.  If the macro
;; `CASE_VECTOR_PC_RELATIVE' is defined then the first operand is an offset
;; which counts from the address of the table; otherwise, it is an absolute
;; address to jump to.  In either case, the first operand has mode `Pmode'.

;; The `tablejump' insn is always the last insn before the jump table it uses.
;; Its assembler code normally has no need to use the second operand, but you
;; should incorporate it in the RTL pattern so that the jump optimizer will not
;; delete the table as unreachable code.

(define_expand "tablejump"
  [(parallel [(set (pc) (match_operand:SI 0 "address_operand" "p"))
	      (use (label_ref (match_operand 1 "" "")))])]
  "!flag_pic"
  "")

(define_insn "tablejump_insn"
  [(set (pc) (match_operand:SI 0 "address_operand" "p"))
   (use (label_ref (match_operand 1 "" "")))]
  ""
  "jmp%I0l %M0"
  [(set_attr "length" "4")
   (set_attr "type" "jumpl")])

;; Implement switch statements when generating PIC code.  Switches are
;; implemented by `tablejump' when not using -fpic.

;; Emit code here to do the range checking and make the index zero based.
;; operand 0 is the index
;; operand 1 is the lower bound
;; operand 2 is the range of indices (highest - lowest + 1)
;; operand 3 is the label that precedes the table itself
;; operand 4 is the fall through label

(define_expand "casesi"
  [(use (match_operand:SI 0 "integer_register_operand" ""))
   (use (match_operand:SI 1 "const_int_operand" ""))
   (use (match_operand:SI 2 "const_int_operand" ""))
   (use (match_operand 3 "" ""))
   (use (match_operand 4 "" ""))]
  "flag_pic"
  "
{
  rtx indx;
  rtx scale;
  rtx low = operands[1];
  rtx range = operands[2];
  rtx table = operands[3];
  rtx treg;
  rtx fail = operands[4];
  rtx mem;
  rtx reg2;
  rtx reg3;

  if (GET_CODE (operands[1]) != CONST_INT)
    abort ();

  if (GET_CODE (operands[2]) != CONST_INT)
    abort ();

  /* If we can't generate an immediate instruction, promote to register */
  if (! IN_RANGE_P (INTVAL (range), -2048, 2047))
    range = force_reg (SImode, range);

  /* If low bound is 0, we don't have to subtract it.  */
  if (INTVAL (operands[1]) == 0)
    indx = operands[0];
  else
    {
      indx = gen_reg_rtx (SImode);
      if (IN_RANGE_P (INTVAL (low), -2047, 2048))
	emit_insn (gen_addsi3 (indx, operands[0], GEN_INT (- INTVAL (low))));
      else
	emit_insn (gen_subsi3 (indx, operands[0], force_reg (SImode, low)));
    }

  /* Do an unsigned comparison (in the proper mode) between the index
     expression and the value which represents the length of the range.
     Since we just finished subtracting the lower bound of the range
     from the index expression, this comparison allows us to simultaneously
     check that the original index expression value is both greater than
     or equal to the minimum value of the range and less than or equal to
     the maximum value of the range.  */

  emit_cmp_and_jump_insns (indx, range, GTU, NULL_RTX, SImode, 1, fail);

  /* Move the table address to a register */
  treg = gen_reg_rtx (Pmode);
  emit_insn (gen_movsi (treg, gen_rtx_LABEL_REF (VOIDmode, table)));

  /* scale index-low by wordsize */
  scale = gen_reg_rtx (SImode);
  emit_insn (gen_ashlsi3 (scale, indx, GEN_INT (2)));

  /* Load the address, add the start of the table back in,
     and jump to it.  */
  mem = gen_rtx_MEM (SImode, gen_rtx_PLUS (Pmode, scale, treg));
  reg2 = gen_reg_rtx (SImode);
  reg3 = gen_reg_rtx (SImode);
  emit_insn (gen_movsi (reg2, mem));
  emit_insn (gen_addsi3 (reg3, reg2, treg));
  emit_jump_insn (gen_tablejump_insn (reg3, table));
  DONE;
}")


;; ::::::::::::::::::::
;; ::
;; :: Prologue and Epilogue instructions
;; ::
;; ::::::::::::::::::::

;; Called after register allocation to add any instructions needed for the
;; prologue.  Using a prologue insn is favored compared to putting all of the
;; instructions in the FUNCTION_PROLOGUE macro, since it allows the scheduler
;; to intermix instructions with the saves of the caller saved registers.  In
;; some cases, it might be necessary to emit a barrier instruction as the last
;; insn to prevent such scheduling.
(define_expand "prologue"
  [(const_int 1)]
  ""
  "
{
  frv_expand_prologue ();
  DONE;
}")

;; Called after register allocation to add any instructions needed for the
;; epilogue.  Using an epilogue insn is favored compared to putting all of the
;; instructions in the FUNCTION_EPILOGUE macro, since it allows the scheduler
;; to intermix instructions with the restires of the caller saved registers.
;; In some cases, it might be necessary to emit a barrier instruction as the
;; first insn to prevent such scheduling.
(define_expand "epilogue"
  [(const_int 2)]
  ""
  "
{
  frv_expand_epilogue (FALSE);
  DONE;
}")

;; This pattern, if defined, emits RTL for exit from a function without the final
;; branch back to the calling function.  This pattern will be emitted before any
;; sibling call (aka tail call) sites.
;;
;; The sibcall_epilogue pattern must not clobber any arguments used for
;; parameter passing or any stack slots for arguments passed to the current
;; function.
(define_expand "sibcall_epilogue"
  [(const_int 3)]
  ""
  "
{
  frv_expand_epilogue (TRUE);
  DONE;
}")

;; Set up the pic register to hold the address of the pic table
(define_insn "pic_prologue"
  [(set (match_operand:SI 0 "integer_register_operand" "=d")
        (unspec_volatile:SI [(const_int 0)] UNSPEC_PIC_PROLOGUE))
   (clobber (match_operand:SI 1 "lr_operand" "=l"))
   (clobber (match_operand:SI 2 "integer_register_operand" "=d"))]
  ""
  "*
{
  static int frv_pic_labelno = 0;

  operands[3] = GEN_INT (frv_pic_labelno++);
  return \"call %P3\\n%P3:\;movsg %1, %0\;sethi #gprelhi(%P3), %2\;setlo #gprello(%P3), %2\;sub %0,%2,%0\";
}"
  [(set_attr "length" "16")
   (set_attr "type" "multi")])

;; ::::::::::::::::::::
;; ::
;; :: Miscellaneous instructions
;; ::
;; ::::::::::::::::::::

;; No operation, needed in case the user uses -g but not -O.
(define_insn "nop"
  [(const_int 0)]
  ""
  "nop"
  [(set_attr "length" "4")
   (set_attr "type" "int")])

;; Pseudo instruction that prevents the scheduler from moving code above this
;; point.  Note, type unknown is used to make sure the VLIW instructions are
;; not continued past this point.
(define_insn "blockage"
  [(unspec_volatile [(const_int 0)] UNSPEC_BLOCKAGE)]
  ""
  "# blockage"
  [(set_attr "length" "0")
   (set_attr "type" "unknown")])

;; ::::::::::::::::::::
;; ::
;; :: Media instructions
;; ::
;; ::::::::::::::::::::

;; Unimplemented instructions:
;;   - MCMPSH, MCMPUH

(define_constants
  [(UNSPEC_MLOGIC		100)
   (UNSPEC_MNOT			101)
   (UNSPEC_MAVEH		102)
   (UNSPEC_MSATH		103)
   (UNSPEC_MADDH		104)
   (UNSPEC_MQADDH		105)
   (UNSPEC_MPACKH		106)
   (UNSPEC_MUNPACKH		107)
   (UNSPEC_MDPACKH		108)
   (UNSPEC_MBTOH		109)
   (UNSPEC_MHTOB		110)
   (UNSPEC_MROT			111)
   (UNSPEC_MSHIFT		112)
   (UNSPEC_MEXPDHW		113)
   (UNSPEC_MEXPDHD		114)
   (UNSPEC_MWCUT		115)
   (UNSPEC_MMULH		116)
   (UNSPEC_MMULXH		117)
   (UNSPEC_MMACH		118)
   (UNSPEC_MMRDH		119)
   (UNSPEC_MQMULH		120)
   (UNSPEC_MQMULXH		121)
   (UNSPEC_MQMACH		122)
   (UNSPEC_MCPX			123)
   (UNSPEC_MQCPX		124)
   (UNSPEC_MCUT			125)
   (UNSPEC_MRDACC		126)
   (UNSPEC_MRDACCG		127)
   (UNSPEC_MWTACC		128)
   (UNSPEC_MWTACCG		129)
   (UNSPEC_MTRAP		130)
   (UNSPEC_MCLRACC		131)
   (UNSPEC_MCLRACCA		132)
   (UNSPEC_MCOP1		133)
   (UNSPEC_MCOP2		134)
   (UNSPEC_MDUNPACKH		135)
   (UNSPEC_MDUNPACKH_INTERNAL	136)
   (UNSPEC_MBTOHE		137)
   (UNSPEC_MBTOHE_INTERNAL	138)
   (UNSPEC_MBTOHE		137)
   (UNSPEC_MBTOHE_INTERNAL	138)
   (UNSPEC_MQMACH2		139)
   (UNSPEC_MADDACC		140)
   (UNSPEC_MDADDACC		141)
   (UNSPEC_MABSHS		142)
   (UNSPEC_MDROTLI		143)
   (UNSPEC_MCPLHI		144)
   (UNSPEC_MCPLI		145)
   (UNSPEC_MDCUTSSI		146)
   (UNSPEC_MQSATHS		147)
   (UNSPEC_MHSETLOS		148)
   (UNSPEC_MHSETLOH		149)
   (UNSPEC_MHSETHIS		150)
   (UNSPEC_MHSETHIH		151)
   (UNSPEC_MHDSETS		152)
   (UNSPEC_MHDSETH		153)
])

;; Logic operations: type "mlogic"

(define_expand "mand"
  [(set (match_operand:SI 0 "fpr_operand" "")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "")
		    (match_operand:SI 2 "fpr_operand" "")
		    (match_dup 3)]
		   UNSPEC_MLOGIC))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MAND);")

(define_expand "mor"
  [(set (match_operand:SI 0 "fpr_operand" "")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "")
		    (match_operand:SI 2 "fpr_operand" "")
		    (match_dup 3)]
		   UNSPEC_MLOGIC))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MOR);")

(define_expand "mxor"
  [(set (match_operand:SI 0 "fpr_operand" "")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "")
		    (match_operand:SI 2 "fpr_operand" "")
		    (match_dup 3)]
		   UNSPEC_MLOGIC))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MXOR);")

(define_insn "*mlogic"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
		    (match_operand:SI 2 "fpr_operand" "f")
		    (match_operand:SI 3 "const_int_operand" "n")]
		   UNSPEC_MLOGIC))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		 break;
  case FRV_BUILTIN_MAND: return \"mand %1, %2, %0\";
  case FRV_BUILTIN_MOR:  return \"mor %1, %2, %0\";
  case FRV_BUILTIN_MXOR: return \"mxor %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mlogic\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mlogic")])

(define_insn "*cond_exec_mlogic"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "fpr_operand" "=f")
         (unspec:SI [(match_operand:SI 3 "fpr_operand" "f")
		     (match_operand:SI 4 "fpr_operand" "f")
		     (match_operand:SI 5 "const_int_operand" "n")]
		    UNSPEC_MLOGIC)))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[5]))
  {
  default:		    break;
  case FRV_BUILTIN_MAND: return \"cmand %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MOR:  return \"cmor %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MXOR: return \"cmxor %3, %4, %2, %1, %e0\";
  }

  fatal_insn (\"Bad media insn, cond_exec_mlogic\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mlogic")])

;; Logical not: type "mlogic"

(define_insn "mnot"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")] UNSPEC_MNOT))]
  "TARGET_MEDIA"
  "mnot %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mlogic")])

(define_insn "*cond_exec_mnot"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "fpr_operand" "=f")
         (unspec:SI [(match_operand:SI 3 "fpr_operand" "f")] UNSPEC_MNOT)))]
  "TARGET_MEDIA"
  "cmnot %3, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "mlogic")])

;; Dual average (halfword): type "maveh"

(define_insn "maveh"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")]
		   UNSPEC_MAVEH))]
  "TARGET_MEDIA"
  "maveh %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "maveh")])

;; Dual saturation (halfword): type "msath"

(define_expand "msaths"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_dup 3)]
                   UNSPEC_MSATH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MSATHS);")

(define_expand "msathu"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_dup 3)]
                   UNSPEC_MSATH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MSATHU);")

(define_insn "*msath"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_operand:SI 3 "const_int_operand" "n")]
		   UNSPEC_MSATH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		    break;
  case FRV_BUILTIN_MSATHS:  return \"msaths %1, %2, %0\";
  case FRV_BUILTIN_MSATHU:  return \"msathu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, msath\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "msath")])

;; Dual addition/subtraction with saturation (halfword): type "maddh"

(define_expand "maddhss"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_dup 3)]
		   UNSPEC_MADDH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MADDHSS);")

(define_expand "maddhus"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_dup 3)]
                   UNSPEC_MADDH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MADDHUS);")

(define_expand "msubhss"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_dup 3)]
                   UNSPEC_MADDH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MSUBHSS);")

(define_expand "msubhus"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_dup 3)]
                   UNSPEC_MADDH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MSUBHUS);")

(define_insn "*maddh"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_operand:SI 3 "const_int_operand" "n")]
		   UNSPEC_MADDH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		    break;
  case FRV_BUILTIN_MADDHSS: return \"maddhss %1, %2, %0\";
  case FRV_BUILTIN_MADDHUS: return \"maddhus %1, %2, %0\";
  case FRV_BUILTIN_MSUBHSS: return \"msubhss %1, %2, %0\";
  case FRV_BUILTIN_MSUBHUS: return \"msubhus %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, maddh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "maddh")])

(define_insn "*cond_exec_maddh"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "fpr_operand" "=f")
	 (unspec:SI [(match_operand:SI 3 "fpr_operand" "f")
		     (match_operand:SI 4 "fpr_operand" "f")
		     (match_operand:SI 5 "const_int_operand" "n")]
		    UNSPEC_MADDH)))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[5]))
  {
  default:		    break;
  case FRV_BUILTIN_MADDHSS: return \"cmaddhss %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MADDHUS: return \"cmaddhus %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MSUBHSS: return \"cmsubhss %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MSUBHUS: return \"cmsubhus %3, %4, %2, %1, %e0\";
  }

  fatal_insn (\"Bad media insn, cond_exec_maddh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "maddh")])

;; Quad addition/subtraction with saturation (halfword): type "mqaddh"

(define_expand "mqaddhss"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:DI 1 "even_fpr_operand" "h")
                    (match_operand:DI 2 "even_fpr_operand" "h")
		    (match_dup 3)]
		   UNSPEC_MQADDH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MQADDHSS);")

(define_expand "mqaddhus"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:DI 1 "even_fpr_operand" "h")
                    (match_operand:DI 2 "even_fpr_operand" "h")
		    (match_dup 3)]
		   UNSPEC_MQADDH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MQADDHUS);")

(define_expand "mqsubhss"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:DI 1 "even_fpr_operand" "h")
                    (match_operand:DI 2 "even_fpr_operand" "h")
		    (match_dup 3)]
		   UNSPEC_MQADDH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MQSUBHSS);")

(define_expand "mqsubhus"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:DI 1 "even_fpr_operand" "h")
                    (match_operand:DI 2 "even_fpr_operand" "h")
		    (match_dup 3)]
		   UNSPEC_MQADDH))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MQSUBHUS);")

(define_insn "*mqaddh"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:DI 1 "even_fpr_operand" "h")
                    (match_operand:DI 2 "even_fpr_operand" "h")
		    (match_operand:SI 3 "const_int_operand" "n")]
		   UNSPEC_MQADDH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		     break;
  case FRV_BUILTIN_MQADDHSS: return \"mqaddhss %1, %2, %0\";
  case FRV_BUILTIN_MQADDHUS: return \"mqaddhus %1, %2, %0\";
  case FRV_BUILTIN_MQSUBHSS: return \"mqsubhss %1, %2, %0\";
  case FRV_BUILTIN_MQSUBHUS: return \"mqsubhus %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mqaddh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mqaddh")])

(define_insn "*cond_exec_mqaddh"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:DI 2 "even_fpr_operand" "=h")
         (unspec:DI [(match_operand:DI 3 "even_fpr_operand" "h")
                     (match_operand:DI 4 "even_fpr_operand" "h")
		     (match_operand:SI 5 "const_int_operand" "n")]
		    UNSPEC_MQADDH)))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[5]))
  {
  default:		     break;
  case FRV_BUILTIN_MQADDHSS: return \"cmqaddhss %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MQADDHUS: return \"cmqaddhus %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MQSUBHSS: return \"cmqsubhss %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MQSUBHUS: return \"cmqsubhus %3, %4, %2, %1, %e0\";
  }

  fatal_insn (\"Bad media insn, cond_exec_mqaddh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mqaddh")])

;; Pack halfword: type "mpackh"

(define_insn "mpackh"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:HI 1 "fpr_operand" "f")
                    (match_operand:HI 2 "fpr_operand" "f")]
		   UNSPEC_MPACKH))]
  "TARGET_MEDIA"
  "mpackh %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mpackh")])

;; Unpack halfword: type "mpackh"

(define_insn "munpackh"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:SI 1 "fpr_operand" "f")]
		   UNSPEC_MUNPACKH))]
  "TARGET_MEDIA"
  "munpackh %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "munpackh")])

;; Dual pack halfword: type "mdpackh"

(define_insn "mdpackh"
    [(set (match_operand:DI 0 "even_fpr_operand" "=h")
	  (unspec:DI [(match_operand:DI 1 "even_fpr_operand" "h")
		      (match_operand:DI 2 "even_fpr_operand" "h")]
		     UNSPEC_MDPACKH))]
  "TARGET_MEDIA"
  "mdpackh %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mdpackh")])

;; Byte-halfword conversion: type "mbhconv"

(define_insn "mbtoh"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:SI 1 "fpr_operand" "f")]
		   UNSPEC_MBTOH))]
  "TARGET_MEDIA"
  "mbtoh %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mbhconv")])

(define_insn "*cond_exec_mbtoh"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:DI 2 "even_fpr_operand" "=h")
	 (unspec:DI [(match_operand:SI 3 "fpr_operand" "f")]
		    UNSPEC_MBTOH)))]
  "TARGET_MEDIA"
  "cmbtoh %3, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "mbhconv")])

(define_insn "mhtob"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:DI 1 "even_fpr_operand" "h")]
		   UNSPEC_MHTOB))]
  "TARGET_MEDIA"
  "mhtob %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mbhconv")])

(define_insn "*cond_exec_mhtob"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "fpr_operand" "=f")
	 (unspec:SI [(match_operand:DI 3 "even_fpr_operand" "h")]
		    UNSPEC_MHTOB)))]
  "TARGET_MEDIA"
  "cmhtob %3, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "mbhconv")])

;; Rotate: type "mrot"

(define_expand "mrotli"
  [(set (match_operand:SI 0 "fpr_operand" "")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "")
                    (match_operand:SI 2 "uint5_operand" "")
		    (match_dup 3)]
		   UNSPEC_MROT))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MROTLI);")

(define_expand "mrotri"
  [(set (match_operand:SI 0 "fpr_operand" "")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "")
                    (match_operand:SI 2 "uint5_operand" "")
		    (match_dup 3)]
		   UNSPEC_MROT))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MROTRI);")

(define_insn "*mrot"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "uint5_operand" "I")
		    (match_operand:SI 3 "const_int_operand" "n")]
		   UNSPEC_MROT))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		   break;
  case FRV_BUILTIN_MROTLI: return \"mrotli %1, %2, %0\";
  case FRV_BUILTIN_MROTRI: return \"mrotri %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mrot\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mrot")])

;; Dual shift halfword: type "msh"

(define_expand "msllhi"
  [(set (match_operand:SI 0 "fpr_operand" "")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "")
                    (match_operand:SI 2 "uint4_operand" "")
		    (match_dup 3)]
		   UNSPEC_MSHIFT))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MSLLHI);")

(define_expand "msrlhi"
  [(set (match_operand:SI 0 "fpr_operand" "")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "")
                    (match_operand:SI 2 "uint4_operand" "")
		    (match_dup 3)]
		   UNSPEC_MSHIFT))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MSRLHI);")

(define_expand "msrahi"
  [(set (match_operand:SI 0 "fpr_operand" "")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "")
                    (match_operand:SI 2 "uint4_operand" "")
		    (match_dup 3)]
		   UNSPEC_MSHIFT))]
  "TARGET_MEDIA"
  "operands[3] = GEN_INT (FRV_BUILTIN_MSRAHI);")

(define_insn "*mshift"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "uint4_operand" "I")
		    (match_operand:SI 3 "const_int_operand" "n")]
		   UNSPEC_MSHIFT))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		   break;
  case FRV_BUILTIN_MSLLHI: return \"msllhi %1, %2, %0\";
  case FRV_BUILTIN_MSRLHI: return \"msrlhi %1, %2, %0\";
  case FRV_BUILTIN_MSRAHI: return \"msrahi %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mshift\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mshift")])

;; Expand halfword to word: type "mexpdhw"

(define_insn "mexpdhw"
  [(set (match_operand:SI 0 "even_fpr_operand" "=h")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "uint1_operand" "I")]
		   UNSPEC_MEXPDHW))]
  "TARGET_MEDIA"
  "mexpdhw %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mexpdhw")])

(define_insn "*cond_exec_mexpdhw"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:SI 2 "even_fpr_operand" "=h")
	 (unspec:SI [(match_operand:SI 3 "fpr_operand" "f")
		     (match_operand:SI 4 "uint1_operand" "I")]
		    UNSPEC_MEXPDHW)))]
  "TARGET_MEDIA"
  "cmexpdhw %3, %4, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "mexpdhw")])

;; Expand halfword to double: type "mexpdhd"

(define_insn "mexpdhd"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "uint1_operand" "I")]
		   UNSPEC_MEXPDHD))]
  "TARGET_MEDIA"
  "mexpdhd %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mexpdhd")])

(define_insn "*cond_exec_mexpdhd"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (set (match_operand:DI 2 "even_fpr_operand" "=h")
	 (unspec:DI [(match_operand:SI 3 "fpr_operand" "f")
		     (match_operand:SI 4 "uint1_operand" "I")]
		    UNSPEC_MEXPDHD)))]
  "TARGET_MEDIA"
  "cmexpdhd %3, %4, %2, %1, %e0"
  [(set_attr "length" "4")
   (set_attr "type" "mexpdhd")])

;; FR cut: type "mwcut"

(define_insn "mwcut"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:DI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_or_int6_operand" "fI")]
		   UNSPEC_MWCUT))]
  "TARGET_MEDIA"
  "mwcut%i2 %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mwcut")])

;; Dual multiplication (halfword): type "mmulh"

(define_expand "mmulhs"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "=b")
		   (unspec:DI [(match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MMULH))
	      (set (match_operand:HI 3 "accg_operand" "=B")
		   (unspec:HI [(const_int 0)] UNSPEC_MMULH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MMULHS);")

(define_expand "mmulhu"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "=b")
		   (unspec:DI [(match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MMULH))
	      (set (match_operand:HI 3 "accg_operand" "=B")
		   (unspec:HI [(const_int 0)] UNSPEC_MMULH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MMULHU);")

(define_insn "*mmulh"
  [(set (match_operand:DI 0 "even_acc_operand" "=b")
        (unspec:DI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_operand:SI 3 "const_int_operand" "n")]
		   UNSPEC_MMULH))
   (set (match_operand:HI 4 "accg_operand" "=B")
	(unspec:HI [(const_int 0)] UNSPEC_MMULH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		    break;
  case FRV_BUILTIN_MMULHS:  return \"mmulhs %1, %2, %0\";
  case FRV_BUILTIN_MMULHU:  return \"mmulhu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mmulh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mmulh")])

(define_insn "*cond_exec_mmulh"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (parallel [(set (match_operand:DI 2 "even_acc_operand" "=b")
		    (unspec:DI [(match_operand:SI 3 "fpr_operand" "f")
				(match_operand:SI 4 "fpr_operand" "f")
				(match_operand:SI 5 "const_int_operand" "n")]
			       UNSPEC_MMULH))
	       (set (match_operand:HI 6 "accg_operand" "=B")
		    (unspec:HI [(const_int 0)] UNSPEC_MMULH))]))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[5]))
  {
  default:		    break;
  case FRV_BUILTIN_MMULHS:  return \"cmmulhs %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MMULHU:  return \"cmmulhu %3, %4, %2, %1, %e0\";
  }

  fatal_insn (\"Bad media insn, cond_exec_mmulh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mmulh")])

;; Dual cross multiplication (halfword): type "mmulxh"

(define_expand "mmulxhs"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "=b")
		   (unspec:DI [(match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MMULXH))
	      (set (match_operand:HI 3 "accg_operand" "=B")
		   (unspec:HI [(const_int 0)] UNSPEC_MMULXH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MMULXHS);")

(define_expand "mmulxhu"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "=b")
		   (unspec:DI [(match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MMULXH))
	      (set (match_operand:HI 3 "accg_operand" "=B")
		   (unspec:HI [(const_int 0)] UNSPEC_MMULXH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MMULXHU);")

(define_insn "*mmulxh"
  [(set (match_operand:DI 0 "even_acc_operand" "=b")
        (unspec:DI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_operand:SI 3 "const_int_operand" "n")]
		   UNSPEC_MMULXH))
   (set (match_operand:HI 4 "accg_operand" "=B")
	(unspec:HI [(const_int 0)] UNSPEC_MMULXH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		    break;
  case FRV_BUILTIN_MMULXHS: return \"mmulxhs %1, %2, %0\";
  case FRV_BUILTIN_MMULXHU: return \"mmulxhu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mmulxh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mmulxh")])

;; Dual product-sum (halfword): type "mmach"

(define_expand "mmachs"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "+b")
		   (unspec:DI [(match_dup 0)
			       (match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_operand:HI 3 "accg_operand" "+B")
			       (match_dup 4)]
			      UNSPEC_MMACH))
	      (set (match_dup 3)
		   (unspec:HI [(const_int 0)] UNSPEC_MMACH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MMACHS);")

(define_expand "mmachu"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "+b")
		   (unspec:DI [(match_dup 0)
			       (match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_operand:HI 3 "accg_operand" "+B")
			       (match_dup 4)]
			      UNSPEC_MMACH))
	      (set (match_dup 3)
		   (unspec:HI [(const_int 0)] UNSPEC_MMACH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MMACHU);")

(define_insn "*mmach"
  [(set (match_operand:DI 0 "even_acc_operand" "+b")
        (unspec:DI [(match_dup 0)
		    (match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_operand:HI 3 "accg_operand" "+B")
		    (match_operand:SI 4 "const_int_operand" "n")]
		   UNSPEC_MMACH))
   (set (match_dup 3) (unspec:HI [(const_int 0)] UNSPEC_MMACH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[4]))
  {
  default:		   break;
  case FRV_BUILTIN_MMACHS: return \"mmachs %1, %2, %0\";
  case FRV_BUILTIN_MMACHU: return \"mmachu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mmach\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mmach")])

(define_insn "*cond_exec_mmach"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (parallel [(set (match_operand:DI 2 "even_acc_operand" "+b")
		    (unspec:DI [(match_dup 2)
				(match_operand:SI 3 "fpr_operand" "f")
				(match_operand:SI 4 "fpr_operand" "f")
				(match_operand:HI 5 "accg_operand" "+B")
				(match_operand:SI 6 "const_int_operand" "n")]
			       UNSPEC_MMACH))
	       (set (match_dup 5)
		    (unspec:HI [(const_int 0)] UNSPEC_MMACH))]))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[6]))
  {
  default:		   break;
  case FRV_BUILTIN_MMACHS: return \"cmmachs %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MMACHU: return \"cmmachu %3, %4, %2, %1, %e0\";
  }

  fatal_insn (\"Bad media insn, cond_exec_mmach\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mmach")])

;; Dual product-difference: type "mmrdh"

(define_expand "mmrdhs"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "+b")
		   (unspec:DI [(match_dup 0)
			       (match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_operand:HI 3 "accg_operand" "+B")
			       (match_dup 4)]
			      UNSPEC_MMRDH))
	      (set (match_dup 3)
		   (unspec:HI [(const_int 0)] UNSPEC_MMRDH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MMRDHS);")

(define_expand "mmrdhu"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "+b")
		   (unspec:DI [(match_dup 0)
			       (match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_operand:HI 3 "accg_operand" "+B")
			       (match_dup 4)]
			      UNSPEC_MMRDH))
	      (set (match_dup 3)
		   (unspec:HI [(const_int 0)] UNSPEC_MMRDH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MMRDHU);")

(define_insn "*mmrdh"
  [(set (match_operand:DI 0 "even_acc_operand" "+b")
        (unspec:DI [(match_dup 0)
		    (match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")
		    (match_operand:HI 3 "accg_operand" "+B")
		    (match_operand:SI 4 "const_int_operand" "n")]
		   UNSPEC_MMRDH))
   (set (match_dup 3)
	(unspec:HI [(const_int 0)] UNSPEC_MMRDH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[4]))
  {
  default:		   break;
  case FRV_BUILTIN_MMRDHS: return \"mmrdhs %1, %2, %0\";
  case FRV_BUILTIN_MMRDHU: return \"mmrdhu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mrdh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mmrdh")])

;; Quad multiply (halfword): type "mqmulh"

(define_expand "mqmulhs"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "=A")
		   (unspec:V4SI [(match_operand:DI 1 "even_fpr_operand" "h")
				 (match_operand:DI 2 "even_fpr_operand" "h")
				 (match_dup 4)]
				UNSPEC_MQMULH))
	      (set (match_operand:V4QI 3 "accg_operand" "=B")
		   (unspec:V4QI [(const_int 0)] UNSPEC_MQMULH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQMULHS);")

(define_expand "mqmulhu"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "=A")
		   (unspec:V4SI [(match_operand:DI 1 "even_fpr_operand" "h")
				 (match_operand:DI 2 "even_fpr_operand" "h")
				 (match_dup 4)]
				UNSPEC_MQMULH))
	      (set (match_operand:V4QI 3 "accg_operand" "=B")
		   (unspec:V4QI [(const_int 0)] UNSPEC_MQMULH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQMULHU);")

(define_insn "*mqmulh"
  [(set (match_operand:V4SI 0 "quad_acc_operand" "=A")
        (unspec:V4SI [(match_operand:DI 1 "even_fpr_operand" "h")
		      (match_operand:DI 2 "even_fpr_operand" "h")
		      (match_operand:SI 3 "const_int_operand" "n")]
		     UNSPEC_MQMULH))
   (set (match_operand:V4QI 4 "accg_operand" "=B")
	(unspec:V4QI [(const_int 0)] UNSPEC_MQMULH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		     break;
  case FRV_BUILTIN_MQMULHS:  return \"mqmulhs %1, %2, %0\";
  case FRV_BUILTIN_MQMULHU:  return \"mqmulhu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mqmulh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mqmulh")])

(define_insn "*cond_exec_mqmulh"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (parallel [(set (match_operand:V4SI 2 "quad_acc_operand" "=A")
		    (unspec:V4SI [(match_operand:DI 3 "even_fpr_operand" "h")
				  (match_operand:DI 4 "even_fpr_operand" "h")
				  (match_operand:SI 5 "const_int_operand" "n")]
				 UNSPEC_MQMULH))
	       (set (match_operand:V4QI 6 "accg_operand" "=B")
		    (unspec:V4QI [(const_int 0)] UNSPEC_MQMULH))]))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[5]))
  {
  default:		     break;
  case FRV_BUILTIN_MQMULHS:  return \"cmqmulhs %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MQMULHU:  return \"cmqmulhu %3, %4, %2, %1, %e0\";
  }

  fatal_insn (\"Bad media insn, cond_exec_mqmulh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mqmulh")])

;; Quad cross multiply (halfword): type "mqmulxh"

(define_expand "mqmulxhs"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "=A")
		   (unspec:V4SI [(match_operand:DI 1 "even_fpr_operand" "h")
				 (match_operand:DI 2 "even_fpr_operand" "h")
				 (match_dup 4)]
				UNSPEC_MQMULXH))
	      (set (match_operand:V4QI 3 "accg_operand" "=B")
		   (unspec:V4QI [(const_int 0)] UNSPEC_MQMULXH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQMULXHS);")

(define_expand "mqmulxhu"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "=A")
		   (unspec:V4SI [(match_operand:DI 1 "even_fpr_operand" "h")
				 (match_operand:DI 2 "even_fpr_operand" "h")
				 (match_dup 4)]
				UNSPEC_MQMULXH))
	      (set (match_operand:V4QI 3 "accg_operand" "=B")
		   (unspec:V4QI [(const_int 0)] UNSPEC_MQMULXH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQMULXHU);")

(define_insn "*mqmulxh"
  [(set (match_operand:V4SI 0 "quad_acc_operand" "=A")
        (unspec:V4SI [(match_operand:DI 1 "even_fpr_operand" "h")
		      (match_operand:DI 2 "even_fpr_operand" "h")
		      (match_operand:SI 3 "const_int_operand" "n")]
		     UNSPEC_MQMULXH))
   (set (match_operand:V4QI 4 "accg_operand" "=B")
	(unspec:V4QI [(const_int 0)] UNSPEC_MQMULXH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		     break;
  case FRV_BUILTIN_MQMULXHS: return \"mqmulxhs %1, %2, %0\";
  case FRV_BUILTIN_MQMULXHU: return \"mqmulxhu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mqmulxh\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mqmulxh")])

;; Quad product-sum (halfword): type "mqmach"

(define_expand "mqmachs"
  [(parallel [(set (match_operand:V4SI 0 "even_acc_operand" "+A")
		   (unspec:V4SI [(match_dup 0)
				 (match_operand:DI 1 "even_fpr_operand" "h")
				 (match_operand:DI 2 "even_fpr_operand" "h")
				 (match_operand:V4QI 3 "accg_operand" "+B")
				 (match_dup 4)]
				UNSPEC_MQMACH))
	      (set (match_dup 3)
		   (unspec:V4QI [(const_int 0)] UNSPEC_MQMACH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQMACHS);")

(define_expand "mqmachu"
  [(parallel [(set (match_operand:V4SI 0 "even_acc_operand" "+A")
		   (unspec:V4SI [(match_dup 0)
				 (match_operand:DI 1 "even_fpr_operand" "h")
				 (match_operand:DI 2 "even_fpr_operand" "h")
				 (match_operand:V4QI 3 "accg_operand" "+B")
				 (match_dup 4)]
				UNSPEC_MQMACH))
	      (set (match_dup 3)
		   (unspec:V4QI [(const_int 0)] UNSPEC_MQMACH))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQMACHU);")

(define_insn "*mqmach"
  [(set (match_operand:V4SI 0 "even_acc_operand" "+A")
        (unspec:V4SI [(match_dup 0)
		      (match_operand:DI 1 "even_fpr_operand" "h")
		      (match_operand:DI 2 "even_fpr_operand" "h")
		      (match_operand:V4QI 3 "accg_operand" "+B")
		      (match_operand:SI 4 "const_int_operand" "n")]
		     UNSPEC_MQMACH))
   (set (match_dup 3)
	(unspec:V4QI [(const_int 0)] UNSPEC_MQMACH))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[4]))
  {
  default:		    break;
  case FRV_BUILTIN_MQMACHS: return \"mqmachs %1, %2, %0\";
  case FRV_BUILTIN_MQMACHU: return \"mqmachu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mqmach\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mqmach")])

(define_insn "*cond_exec_mqmach"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (parallel [(set (match_operand:V4SI 2 "even_acc_operand" "+A")
		    (unspec:V4SI [(match_dup 2)
				  (match_operand:DI 3 "even_fpr_operand" "h")
				  (match_operand:DI 4 "even_fpr_operand" "h")
				  (match_operand:V4QI 5 "accg_operand" "+B")
				  (match_operand:SI 6 "const_int_operand" "n")]
				 UNSPEC_MQMACH))
	       (set (match_dup 5)
		    (unspec:V4QI [(const_int 0)] UNSPEC_MQMACH))]))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[6]))
  {
  default:		    break;
  case FRV_BUILTIN_MQMACHS: return \"cmqmachs %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MQMACHU: return \"cmqmachu %3, %4, %2, %1, %e0\";
  }

  fatal_insn (\"Bad media insn, cond_exec_mqmach\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mqmach")])

;; Dual complex number product-sum (halfword)

(define_expand "mcpxrs"
  [(parallel [(set (match_operand:SI 0 "acc_operand" "=a")
		   (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MCPX))
	      (set (match_operand:QI 3 "accg_operand" "=B")
		   (unspec:QI [(const_int 0)] UNSPEC_MCPX))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MCPXRS);")

(define_expand "mcpxru"
  [(parallel [(set (match_operand:SI 0 "acc_operand" "=a")
		   (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MCPX))
	      (set (match_operand:QI 3 "accg_operand" "=B")
		   (unspec:QI [(const_int 0)] UNSPEC_MCPX))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MCPXRU);")

(define_expand "mcpxis"
  [(parallel [(set (match_operand:SI 0 "acc_operand" "=a")
		   (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MCPX))
	      (set (match_operand:QI 3 "accg_operand" "=B")
		   (unspec:QI [(const_int 0)] UNSPEC_MCPX))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MCPXIS);")

(define_expand "mcpxiu"
  [(parallel [(set (match_operand:SI 0 "acc_operand" "=a")
		   (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MCPX))
	      (set (match_operand:QI 3 "accg_operand" "=B")
		   (unspec:QI [(const_int 0)] UNSPEC_MCPX))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MCPXIU);")

(define_insn "*mcpx"
  [(parallel [(set (match_operand:SI 0 "acc_operand" "=a")
		   (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
			       (match_operand:SI 2 "fpr_operand" "f")
			       (match_operand:SI 3 "const_int_operand" "n")]
			      UNSPEC_MCPX))
	      (set (match_operand:QI 4 "accg_operand" "=B")
		   (unspec:QI [(const_int 0)] UNSPEC_MCPX))])]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		   break;
  case FRV_BUILTIN_MCPXRS: return \"mcpxrs %1, %2, %0\";
  case FRV_BUILTIN_MCPXRU: return \"mcpxru %1, %2, %0\";
  case FRV_BUILTIN_MCPXIS: return \"mcpxis %1, %2, %0\";
  case FRV_BUILTIN_MCPXIU: return \"mcpxiu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mcpx\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mcpx")])

(define_insn "*cond_exec_mcpx"
  [(cond_exec
    (match_operator 0 "ccr_eqne_operator"
		    [(match_operand 1 "cr_operand" "C")
		     (const_int 0)])
    (parallel [(set (match_operand:SI 2 "acc_operand" "=a")
		    (unspec:SI [(match_operand:SI 3 "fpr_operand" "f")
				(match_operand:SI 4 "fpr_operand" "f")
				(match_operand:SI 5 "const_int_operand" "n")]
			       UNSPEC_MCPX))
	       (set (match_operand:QI 6 "accg_operand" "=B")
		    (unspec:QI [(const_int 0)] UNSPEC_MCPX))]))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[5]))
  {
  default:		   break;
  case FRV_BUILTIN_MCPXRS: return \"cmcpxrs %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MCPXRU: return \"cmcpxru %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MCPXIS: return \"cmcpxis %3, %4, %2, %1, %e0\";
  case FRV_BUILTIN_MCPXIU: return \"cmcpxiu %3, %4, %2, %1, %e0\";
  }

  fatal_insn (\"Bad media insn, cond_exec_mcpx\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mcpx")])

;; Quad complex number product-sum (halfword): type "mqcpx"

(define_expand "mqcpxrs"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "=b")
		   (unspec:DI [(match_operand:DI 1 "fpr_operand" "f")
			       (match_operand:DI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MQCPX))
	      (set (match_operand:HI 3 "accg_operand" "=B")
		   (unspec:HI [(const_int 0)] UNSPEC_MQCPX))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQCPXRS);")

(define_expand "mqcpxru"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "=b")
		   (unspec:DI [(match_operand:DI 1 "fpr_operand" "f")
			       (match_operand:DI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MQCPX))
	      (set (match_operand:HI 3 "accg_operand" "=B")
		   (unspec:HI [(const_int 0)] UNSPEC_MQCPX))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQCPXRU);")

(define_expand "mqcpxis"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "=b")
		   (unspec:DI [(match_operand:DI 1 "fpr_operand" "f")
			       (match_operand:DI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MQCPX))
	      (set (match_operand:HI 3 "accg_operand" "=B")
		   (unspec:HI [(const_int 0)] UNSPEC_MQCPX))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQCPXIS);")

(define_expand "mqcpxiu"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "=b")
		   (unspec:DI [(match_operand:DI 1 "fpr_operand" "f")
			       (match_operand:DI 2 "fpr_operand" "f")
			       (match_dup 4)]
			      UNSPEC_MQCPX))
	      (set (match_operand:HI 3 "accg_operand" "=B")
		   (unspec:HI [(const_int 0)] UNSPEC_MQCPX))])]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQCPXIU);")

(define_insn "*mqcpx"
  [(set (match_operand:DI 0 "even_acc_operand" "=b")
        (unspec:DI [(match_operand:DI 1 "fpr_operand" "f")
                    (match_operand:DI 2 "fpr_operand" "f")
		    (match_operand:SI 3 "const_int_operand" "n")]
		   UNSPEC_MQCPX))
   (set (match_operand:HI 4 "accg_operand" "=B")
	(unspec:HI [(const_int 0)] UNSPEC_MQCPX))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[3]))
  {
  default:		    break;
  case FRV_BUILTIN_MQCPXRS: return \"mqcpxrs %1, %2, %0\";
  case FRV_BUILTIN_MQCPXRU: return \"mqcpxru %1, %2, %0\";
  case FRV_BUILTIN_MQCPXIS: return \"mqcpxis %1, %2, %0\";
  case FRV_BUILTIN_MQCPXIU: return \"mqcpxiu %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mqcpx\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mqcpx")])

;; Cut: type "mcut"

(define_expand "mcut"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "acc_operand" "a")
                    (match_operand:SI 2 "fpr_or_int6_operand" "fI")
		    (match_operand:QI 3 "accg_operand" "B")
		    (match_dup 4)]
		   UNSPEC_MCUT))]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MCUT);")

(define_expand "mcutss"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "acc_operand" "a")
                    (match_operand:SI 2 "fpr_or_int6_operand" "fI")
		    (match_operand:QI 3 "accg_operand" "B")
		    (match_dup 4)]
		   UNSPEC_MCUT))]
  "TARGET_MEDIA"
  "operands[4] = GEN_INT (FRV_BUILTIN_MCUTSS);")

(define_insn "*mcut"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "acc_operand" "a")
                    (match_operand:SI 2 "fpr_or_int6_operand" "fI")
		    (match_operand:QI 3 "accg_operand" "B")
		    (match_operand:SI 4 "const_int_operand" "n")]
		   UNSPEC_MCUT))]
  "TARGET_MEDIA"
  "*
{
  switch (INTVAL (operands[4]))
  {
  default:		   break;
  case FRV_BUILTIN_MCUT:   return \"mcut%i2 %1, %2, %0\";
  case FRV_BUILTIN_MCUTSS: return \"mcutss%i2 %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mcut\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mcut")])

;; Accumulator read: type "mrdacc"

(define_insn "mrdacc"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(unspec:SI [(match_operand:SI 1 "acc_operand" "a")] UNSPEC_MRDACC))]
  "TARGET_MEDIA"
  "mrdacc %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mrdacc")])

(define_insn "mrdaccg"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(unspec:SI [(match_operand:QI 1 "accg_operand" "B")] UNSPEC_MRDACCG))]
  "TARGET_MEDIA"
  "mrdaccg %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mrdacc")])

;; Accumulator write: type "mwtacc"

(define_insn "mwtacc"
  [(set (match_operand:SI 0 "acc_operand" "=a")
	(unspec:SI [(match_operand:SI 1 "fpr_operand" "f")] UNSPEC_MWTACC))]
  "TARGET_MEDIA"
  "mwtacc %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mwtacc")])

(define_insn "mwtaccg"
  [(set (match_operand:QI 0 "accg_operand" "=B")
	(unspec:QI [(match_operand:SI 1 "fpr_operand" "f")] UNSPEC_MWTACCG))]
  "TARGET_MEDIA"
  "mwtaccg %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mwtacc")])

;; Trap: This one executes on the control unit, not the media units.

(define_insn "mtrap"
  [(unspec_volatile [(const_int 0)] UNSPEC_MTRAP)]
  "TARGET_MEDIA"
  "mtrap"
  [(set_attr "length" "4")
   (set_attr "type" "trap")])

;; Clear single accumulator: type "mclracc"

(define_insn "mclracc_internal"
  [(set (match_operand:SI 0 "acc_operand" "=a")
	(unspec:SI [(const_int 0)] UNSPEC_MCLRACC))
   (set (match_operand:QI 1 "accg_operand" "=B")
	(unspec:QI [(const_int 0)] UNSPEC_MCLRACC))]
  "TARGET_MEDIA"
  "mclracc %0,#0"
  [(set_attr "length" "4")
   (set_attr "type" "mclracc")])

(define_expand "mclracc"
  [(parallel [(set (match_operand:SI 0 "acc_operand" "=a")
		   (unspec:SI [(const_int 0)] UNSPEC_MCLRACC))
	      (set (match_dup 1)
		   (unspec:QI [(const_int 0)] UNSPEC_MCLRACC))])]
  "TARGET_MEDIA"
  "
{
  if (GET_CODE (operands[0]) != REG || !ACC_P (REGNO (operands[0])))
    FAIL;

  operands[1] = frv_matching_accg_for_acc (operands[0]);
}")

;; Clear all accumulators: type "mclracca"

(define_insn "mclracca8_internal"
  [(set (match_operand:V4SI 0 "quad_acc_operand" "=b")
	(unspec:V4SI [(const_int 0)] UNSPEC_MCLRACCA))
   (set (match_operand:V4SI 1 "quad_acc_operand" "=b")
	(unspec:V4SI [(const_int 0)] UNSPEC_MCLRACCA))
   (set (match_operand:V4QI 2 "accg_operand" "=B")
	(unspec:V4QI [(const_int 0)] UNSPEC_MCLRACCA))
   (set (match_operand:V4QI 3 "accg_operand" "=B")
	(unspec:V4QI [(const_int 0)] UNSPEC_MCLRACCA))]
  "TARGET_MEDIA && TARGET_ACC_8"
  "mclracc acc0,#1"
  [(set_attr "length" "4")
   (set_attr "type" "mclracca")])

(define_insn "mclracca4_internal"
  [(set (match_operand:V4SI 0 "quad_acc_operand" "=b")
	(unspec:V4SI [(const_int 0)] UNSPEC_MCLRACCA))
   (set (match_operand:V4QI 1 "accg_operand" "=B")
	(unspec:V4QI [(const_int 0)] UNSPEC_MCLRACCA))]
  "TARGET_MEDIA && TARGET_ACC_4"
  "mclracc acc0,#1"
  [(set_attr "length" "4")
   (set_attr "type" "mclracca")])

(define_expand "mclracca8"
  [(parallel [(set (match_dup 0) (unspec:V4SI [(const_int 0)] UNSPEC_MCLRACCA))
	      (set (match_dup 1) (unspec:V4SI [(const_int 0)] UNSPEC_MCLRACCA))
	      (set (match_dup 2) (unspec:V4QI [(const_int 0)] UNSPEC_MCLRACCA))
	      (set (match_dup 3) (unspec:V4QI [(const_int 0)] UNSPEC_MCLRACCA))])]
  "TARGET_MEDIA && TARGET_ACC_8"
  "
{
  operands[0] = gen_rtx_REG (V4SImode, ACC_FIRST);
  operands[1] = gen_rtx_REG (V4SImode, ACC_FIRST + 4);
  operands[2] = gen_rtx_REG (V4QImode, ACCG_FIRST);
  operands[3] = gen_rtx_REG (V4QImode, ACCG_FIRST + 4);
}")

(define_expand "mclracca4"
  [(parallel [(set (match_dup 0) (unspec:V4SI [(const_int 0)] UNSPEC_MCLRACCA))
	      (set (match_dup 1) (unspec:V4QI [(const_int 0)] UNSPEC_MCLRACCA))])]
  "TARGET_MEDIA && TARGET_ACC_4"
  "
{
  operands[0] = gen_rtx_REG (V4SImode, ACC_FIRST);
  operands[1] = gen_rtx_REG (V4QImode, ACCG_FIRST);
}")

(define_insn "mcop1"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")] UNSPEC_MCOP1))]
  "TARGET_MEDIA_REV1"
  "mcop1 %1, %2, %0"
  [(set_attr "length" "4")
;; What is the class of the insn ???
   (set_attr "type" "multi")])

(define_insn "mcop2"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")
                    (match_operand:SI 2 "fpr_operand" "f")] UNSPEC_MCOP2))]
  "TARGET_MEDIA_REV1"
  "mcop2 %1, %2, %0"
  [(set_attr "length" "4")
;; What is the class of the insn ???
   (set_attr "type" "multi")])

(define_insn "*mdunpackh_internal"
  [(set (match_operand:V4SI 0 "quad_fpr_operand" "=x")
        (unspec:V4SI [(match_operand:DI 1 "even_fpr_operand" "h")]
		     UNSPEC_MDUNPACKH_INTERNAL))]
  "TARGET_MEDIA_REV1"
  "mdunpackh %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mdunpackh")])

(define_insn_and_split "mdunpackh"
  [(set (match_operand:V4SI 0 "memory_operand" "=o")
        (unspec:V4SI [(match_operand:DI 1 "even_fpr_operand" "h")]
		     UNSPEC_MDUNPACKH))
   (clobber (match_scratch:V4SI 2 "=x"))]
  "TARGET_MEDIA_REV1"
  "#"
  "reload_completed"
  [(set (match_dup 2)
	(unspec:V4SI [(match_dup 1)] UNSPEC_MDUNPACKH_INTERNAL))
   (set (match_dup 3)
	(match_dup 4))
   (set (match_dup 5)
	(match_dup 6))]
  "
{
  operands[3] = change_address (operands[0], DImode, NULL_RTX);
  operands[4] = gen_rtx_REG (DImode, REGNO (operands[2]));
  operands[5] = frv_index_memory (operands[0], DImode, 1);
  operands[6] = gen_rtx_REG (DImode, REGNO (operands[2])+2);
}"
  [(set_attr "length" "20")
   (set_attr "type" "multi")])

(define_insn "*mbtohe_internal"
  [(set (match_operand:V4SI 0 "quad_fpr_operand" "=x")
        (unspec:V4SI [(match_operand:SI 1 "fpr_operand" "f")]
		     UNSPEC_MBTOHE_INTERNAL))]
  "TARGET_MEDIA_REV1"
  "mbtohe %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mbhconve")])

(define_insn_and_split "mbtohe"
  [(set (match_operand:V4SI 0 "memory_operand" "=o")
        (unspec:V4SI [(match_operand:SI 1 "fpr_operand" "f")]
		     UNSPEC_MBTOHE))
   (clobber (match_scratch:V4SI 2 "=x"))]
  "TARGET_MEDIA_REV1"
  "#"
  "reload_completed"
  [(set (match_dup 2)
	(unspec:V4SI [(match_dup 1)] UNSPEC_MBTOHE_INTERNAL))
   (set (match_dup 3)
	(match_dup 4))
   (set (match_dup 5)
	(match_dup 6))]
  "
{
  operands[3] = change_address (operands[0], DImode, NULL_RTX);
  operands[4] = gen_rtx_REG (DImode, REGNO (operands[2]));
  operands[5] = frv_index_memory (operands[0], DImode, 1);
  operands[6] = gen_rtx_REG (DImode, REGNO (operands[2])+2);
}"
  [(set_attr "length" "20")
   (set_attr "type" "multi")])

;; Quad product-sum (halfword) instructions only found on the FR400.
;; type "mqmach"

(define_expand "mqxmachs"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "")
	           (unspec:V4SI [(match_dup 0)
		   	         (match_operand:DI 1 "even_fpr_operand" "")
			         (match_operand:DI 2 "even_fpr_operand" "")
				 (match_operand:V4QI 3 "accg_operand" "")
				 (match_dup 4)]
				UNSPEC_MQMACH2))
		(set (match_dup 3)
		     (unspec:V4QI [(const_int 0)] UNSPEC_MQMACH2))])]
  "TARGET_MEDIA_REV2"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQXMACHS);")

(define_expand "mqxmacxhs"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "")
		   (unspec:V4SI [(match_dup 0)
				 (match_operand:DI 1 "even_fpr_operand" "")
				 (match_operand:DI 2 "even_fpr_operand" "")
				 (match_operand:V4QI 3 "accg_operand" "")
				 (match_dup 4)]
				UNSPEC_MQMACH2))
	      (set (match_dup 3)
		   (unspec:V4QI [(const_int 0)] UNSPEC_MQMACH2))])]
  "TARGET_MEDIA_REV2"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQXMACXHS);")

(define_expand "mqmacxhs"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "")
		   (unspec:V4SI [(match_dup 0)
				 (match_operand:DI 1 "even_fpr_operand" "")
				 (match_operand:DI 2 "even_fpr_operand" "")
				 (match_operand:V4QI 3 "accg_operand" "")
				 (match_dup 4)]
				UNSPEC_MQMACH2))
	      (set (match_dup 3)
		   (unspec:V4QI [(const_int 0)] UNSPEC_MQMACH2))])]
  "TARGET_MEDIA_REV2"
  "operands[4] = GEN_INT (FRV_BUILTIN_MQMACXHS);")

(define_insn "*mqmach2"
  [(set (match_operand:V4SI 0 "quad_acc_operand" "+A")
        (unspec:V4SI [(match_dup 0)
		      (match_operand:DI 1 "even_fpr_operand" "h")
		      (match_operand:DI 2 "even_fpr_operand" "h")
		      (match_operand:V4QI 3 "accg_operand" "+B")
		      (match_operand:SI 4 "const_int_operand" "n")]
		     UNSPEC_MQMACH2))
   (set (match_dup 3)
	(unspec:V4QI [(const_int 0)] UNSPEC_MQMACH2))]
  "TARGET_MEDIA_REV2"
  "*
{
  switch (INTVAL (operands[4]))
  {
  default:		      break;
  case FRV_BUILTIN_MQXMACHS:  return \"mqxmachs %1, %2, %0\";
  case FRV_BUILTIN_MQXMACXHS: return \"mqxmacxhs %1, %2, %0\";
  case FRV_BUILTIN_MQMACXHS:  return \"mqmacxhs %1, %2, %0\";
  }

  fatal_insn (\"Bad media insn, mqmach2\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mqmach")])

;; Accumulator addition/subtraction: type "maddacc"

(define_expand "maddaccs"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "")
		   (unspec:DI [(match_dup 0)
			       (match_operand:DI 1 "even_acc_operand" "")]
			      UNSPEC_MADDACC))
	      (set (match_operand:HI 2 "accg_operand" "")
		   (unspec:HI [(match_dup 2)
			       (match_operand:HI 3 "accg_operand" "")
			       (match_dup 4)]
			      UNSPEC_MADDACC))])]
  "TARGET_MEDIA_REV2"
  "operands[4] = GEN_INT (FRV_BUILTIN_MADDACCS);")

(define_expand "msubaccs"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "")
		   (unspec:DI [(match_dup 0)
			       (match_operand:DI 1 "even_acc_operand" "")]
			      UNSPEC_MADDACC))
	      (set (match_operand:HI 2 "accg_operand" "")
		   (unspec:HI [(match_dup 2)
			       (match_operand:HI 3 "accg_operand" "")
			       (match_dup 4)]
			      UNSPEC_MADDACC))])]
  "TARGET_MEDIA_REV2"
  "operands[4] = GEN_INT (FRV_BUILTIN_MSUBACCS);")

(define_expand "masaccs"
  [(parallel [(set (match_operand:DI 0 "even_acc_operand" "")
		   (unspec:DI [(match_dup 0)
			       (match_operand:DI 1 "even_acc_operand" "")]
			      UNSPEC_MADDACC))
	      (set (match_operand:HI 2 "accg_operand" "")
		   (unspec:HI [(match_dup 2)
			       (match_operand:HI 3 "accg_operand" "")
			       (match_dup 4)]
			      UNSPEC_MADDACC))])]
  "TARGET_MEDIA_REV2"
  "operands[4] = GEN_INT (FRV_BUILTIN_MASACCS);")

(define_insn "*maddacc"
  [(set (match_operand:DI 0 "even_acc_operand" "+b")
	(unspec:DI [(match_dup 0)
		    (match_operand:DI 1 "even_acc_operand" "b")]
		   UNSPEC_MADDACC))
   (set (match_operand:HI 2 "accg_operand" "+B")
	(unspec:HI [(match_dup 2)
		    (match_operand:HI 3 "accg_operand" "B")
		    (match_operand:SI 4 "const_int_operand" "n")]
		   UNSPEC_MADDACC))]
  "TARGET_MEDIA_REV2"
  "*
{
  switch (INTVAL (operands[4]))
  {
  default:		     break;
  case FRV_BUILTIN_MADDACCS: return \"maddaccs %1, %0\";
  case FRV_BUILTIN_MSUBACCS: return \"msubaccs %1, %0\";
  case FRV_BUILTIN_MASACCS:  return \"masaccs %1, %0\";
  }

  fatal_insn (\"Bad media insn, maddacc\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "maddacc")])

;; Dual accumulator addition/subtraction: type "mdaddacc"

(define_expand "mdaddaccs"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "")
		   (unspec:V4SI [(match_dup 0)
				 (match_operand:V4SI 1 "quad_acc_operand" "")]
				UNSPEC_MDADDACC))
	      (set (match_operand:V4QI 2 "accg_operand" "")
		   (unspec:V4QI [(match_dup 2)
				 (match_operand:V4QI 3 "accg_operand" "")
				 (match_dup 4)]
				UNSPEC_MDADDACC))])]
  "TARGET_MEDIA_REV2"
  "operands[4] = GEN_INT (FRV_BUILTIN_MDADDACCS);")

(define_expand "mdsubaccs"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "")
		   (unspec:V4SI [(match_dup 0)
				 (match_operand:V4SI 1 "quad_acc_operand" "")]
				UNSPEC_MDADDACC))
	      (set (match_operand:V4QI 2 "accg_operand" "")
	      	   (unspec:V4QI [(match_dup 2)
				 (match_operand:V4QI 3 "accg_operand" "")
				 (match_dup 4)]
				UNSPEC_MDADDACC))])]
  "TARGET_MEDIA_REV2"
  "operands[4] = GEN_INT (FRV_BUILTIN_MDSUBACCS);")

(define_expand "mdasaccs"
  [(parallel [(set (match_operand:V4SI 0 "quad_acc_operand" "")
		   (unspec:V4SI [(match_dup 0)
				 (match_operand:V4SI 1 "quad_acc_operand" "")]
				UNSPEC_MDADDACC))
	      (set (match_operand:V4QI 2 "accg_operand" "")
		   (unspec:V4QI [(match_dup 2)
			         (match_operand:V4QI 3 "accg_operand" "")
				 (match_dup 4)]
			        UNSPEC_MDADDACC))])]
  "TARGET_MEDIA_REV2"
  "operands[4] = GEN_INT (FRV_BUILTIN_MDASACCS);")

(define_insn "*mdaddacc"
  [(set (match_operand:V4SI 0 "quad_acc_operand" "+A")
	(unspec:V4SI [(match_dup 0)
		      (match_operand:V4SI 1 "quad_acc_operand" "A")]
		     UNSPEC_MDADDACC))
   (set (match_operand:V4QI 2 "accg_operand" "+B")
	(unspec:V4QI [(match_dup 2)
		      (match_operand:V4QI 3 "accg_operand" "B")
		      (match_operand:SI 4 "const_int_operand" "n")]
		     UNSPEC_MDADDACC))]
  "TARGET_MEDIA_REV2"
  "*
{
  switch (INTVAL (operands[4]))
  {
  default:		      break;
  case FRV_BUILTIN_MDADDACCS: return \"mdaddaccs %1, %0\";
  case FRV_BUILTIN_MDSUBACCS: return \"mdsubaccs %1, %0\";
  case FRV_BUILTIN_MDASACCS:  return \"mdasaccs %1, %0\";
  }

  fatal_insn (\"Bad media insn, mdaddacc\", insn);
}"
  [(set_attr "length" "4")
   (set_attr "type" "mdaddacc")])

;; Dual absolute (halfword): type "mabsh"

(define_insn "mabshs"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:SI 1 "fpr_operand" "f")] UNSPEC_MABSHS))]
  "TARGET_MEDIA_REV2"
  "mabshs %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mabsh")])

;; Dual rotate: type "mdrot"

(define_insn "mdrotli"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:DI 1 "even_fpr_operand" "h")
		    (match_operand:SI 2 "uint5_operand" "I")]
		   UNSPEC_MDROTLI))]
  "TARGET_MEDIA_REV2"
  "mdrotli %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mdrot")])

;; Dual coupling (concatenation): type "mcpl"

(define_insn "mcplhi"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:DI 1 "fpr_operand" "h")
		    (match_operand:SI 2 "uint4_operand" "I")]
		   UNSPEC_MCPLHI))]
  "TARGET_MEDIA_REV2"
  "mcplhi %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mcpl")])

(define_insn "mcpli"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
        (unspec:SI [(match_operand:DI 1 "fpr_operand" "h")
		    (match_operand:SI 2 "uint5_operand" "I")]
		   UNSPEC_MCPLI))]
  "TARGET_MEDIA_REV2"
  "mcpli %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mcpl")])

;; Dual cut: type "mdcut"

(define_insn "mdcutssi"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:DI 1 "even_acc_operand" "b")
		    (match_operand:SI 2 "int6_operand" "I")
		    (match_operand:HI 3 "accg_operand" "B")]
		   UNSPEC_MDCUTSSI))]
  "TARGET_MEDIA_REV2"
  "mdcutssi %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mdcut")])

;; Quad saturate (halfword): type "mqsath"

(define_insn "mqsaths"
  [(set (match_operand:DI 0 "even_fpr_operand" "=h")
        (unspec:DI [(match_operand:DI 1 "even_fpr_operand" "h")
		    (match_operand:DI 2 "even_fpr_operand" "h")]
		   UNSPEC_MQSATHS))]
  "TARGET_MEDIA_REV2"
  "mqsaths %1, %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mqsath")])

;; Set hi/lo instrctions: type "mset"

(define_insn "mhsetlos"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(unspec:SI [(match_operand:SI 1 "fpr_operand" "0")
		    (match_operand:SI 2 "int12_operand" "NOP")]
		   UNSPEC_MHSETLOS))]
  "TARGET_MEDIA_REV2"
  "mhsetlos %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mset")])

(define_insn "mhsetloh"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(unspec:SI [(match_operand:SI 1 "fpr_operand" "0")
		    (match_operand:SI 2 "int5_operand" "I")]
		   UNSPEC_MHSETLOH))]
  "TARGET_MEDIA_REV2"
  "mhsetloh %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mset")])

(define_insn "mhsethis"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(unspec:SI [(match_operand:SI 1 "fpr_operand" "0")
		    (match_operand:SI 2 "int12_operand" "NOP")]
		   UNSPEC_MHSETHIS))]
  "TARGET_MEDIA_REV2"
  "mhsethis %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mset")])

(define_insn "mhsethih"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(unspec:SI [(match_operand:SI 1 "fpr_operand" "0")
		    (match_operand:SI 2 "int5_operand" "I")]
		   UNSPEC_MHSETHIH))]
  "TARGET_MEDIA_REV2"
  "mhsethih %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mset")])

(define_insn "mhdsets"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(unspec:SI [(match_operand:SI 1 "int12_operand" "NOP")]
		   UNSPEC_MHDSETS))]
  "TARGET_MEDIA_REV2"
  "mhdsets %1, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mset")])

(define_insn "mhdseth"
  [(set (match_operand:SI 0 "fpr_operand" "=f")
	(unspec:SI [(match_operand:SI 1 "fpr_operand" "0")
		    (match_operand:SI 2 "int5_operand" "I")]
		   UNSPEC_MHDSETH))]
  "TARGET_MEDIA_REV2"
  "mhdseth %2, %0"
  [(set_attr "length" "4")
   (set_attr "type" "mset")])
