This is ../../gcc-3.4/gcc/doc/gccint.info, produced by makeinfo version
4.2 from ../../gcc-3.4/gcc/doc/gccint.texi.

Copyright (C) 1988, 1989, 1992, 1993, 1994, 1995, 1996, 1997, 1998,
1999, 2000, 2001, 2002, 2003 Free Software Foundation, Inc.

   Permission is granted to copy, distribute and/or modify this document
under the terms of the GNU Free Documentation License, Version 1.2 or
any later version published by the Free Software Foundation; with the
Invariant Sections being "GNU General Public License" and "Funding Free
Software", the Front-Cover texts being (a) (see below), and with the
Back-Cover Texts being (b) (see below).  A copy of the license is
included in the section entitled "GNU Free Documentation License".

   (a) The FSF's Front-Cover Text is:

   A GNU Manual

   (b) The FSF's Back-Cover Text is:

   You have freedom to copy and modify this GNU Manual, like GNU
software.  Copies published by the Free Software Foundation raise
funds for GNU development.
INFO-DIR-SECTION Programming
START-INFO-DIR-ENTRY
* gccint: (gccint).            Internals of the GNU Compiler Collection.
END-INFO-DIR-ENTRY
   This file documents the internals of the GNU compilers.

   Published by the Free Software Foundation
59 Temple Place - Suite 330
Boston, MA 02111-1307 USA

File: gccint.info,  Node: Standard Names,  Next: Pattern Ordering,  Prev: Constraints,  Up: Machine Desc

Standard Pattern Names For Generation
=====================================

   Here is a table of the instruction names that are meaningful in the
RTL generation pass of the compiler.  Giving one of these names to an
instruction pattern tells the RTL generation pass that it can use the
pattern to accomplish a certain task.

`movM'
     Here M stands for a two-letter machine mode name, in lowercase.
     This instruction pattern moves data with that machine mode from
     operand 1 to operand 0.  For example, `movsi' moves full-word data.

     If operand 0 is a `subreg' with mode M of a register whose own
     mode is wider than M, the effect of this instruction is to store
     the specified value in the part of the register that corresponds
     to mode M.  Bits outside of M, but which are within the same
     target word as the `subreg' are undefined.  Bits which are outside
     the target word are left unchanged.

     This class of patterns is special in several ways.  First of all,
     each of these names up to and including full word size _must_ be
     defined, because there is no other way to copy a datum from one
     place to another.  If there are patterns accepting operands in
     larger modes, `movM' must be defined for integer modes of those
     sizes.

     Second, these patterns are not used solely in the RTL generation
     pass.  Even the reload pass can generate move insns to copy values
     from stack slots into temporary registers.  When it does so, one
     of the operands is a hard register and the other is an operand
     that can need to be reloaded into a register.

     Therefore, when given such a pair of operands, the pattern must
     generate RTL which needs no reloading and needs no temporary
     registers--no registers other than the operands.  For example, if
     you support the pattern with a `define_expand', then in such a
     case the `define_expand' mustn't call `force_reg' or any other such
     function which might generate new pseudo registers.

     This requirement exists even for subword modes on a RISC machine
     where fetching those modes from memory normally requires several
     insns and some temporary registers.

     During reload a memory reference with an invalid address may be
     passed as an operand.  Such an address will be replaced with a
     valid address later in the reload pass.  In this case, nothing may
     be done with the address except to use it as it stands.  If it is
     copied, it will not be replaced with a valid address.  No attempt
     should be made to make such an address into a valid address and no
     routine (such as `change_address') that will do so may be called.
     Note that `general_operand' will fail when applied to such an
     address.

     The global variable `reload_in_progress' (which must be explicitly
     declared if required) can be used to determine whether such special
     handling is required.

     The variety of operands that have reloads depends on the rest of
     the machine description, but typically on a RISC machine these can
     only be pseudo registers that did not get hard registers, while on
     other machines explicit memory references will get optional
     reloads.

     If a scratch register is required to move an object to or from
     memory, it can be allocated using `gen_reg_rtx' prior to life
     analysis.

     If there are cases which need scratch registers during or after
     reload, you must define `SECONDARY_INPUT_RELOAD_CLASS' and/or
     `SECONDARY_OUTPUT_RELOAD_CLASS' to detect them, and provide
     patterns `reload_inM' or `reload_outM' to handle them.  *Note
     Register Classes::.

     The global variable `no_new_pseudos' can be used to determine if it
     is unsafe to create new pseudo registers.  If this variable is
     nonzero, then it is unsafe to call `gen_reg_rtx' to allocate a new
     pseudo.

     The constraints on a `movM' must permit moving any hard register
     to any other hard register provided that `HARD_REGNO_MODE_OK'
     permits mode M in both registers and `REGISTER_MOVE_COST' applied
     to their classes returns a value of 2.

     It is obligatory to support floating point `movM' instructions
     into and out of any registers that can hold fixed point values,
     because unions and structures (which have modes `SImode' or
     `DImode') can be in those registers and they may have floating
     point members.

     There may also be a need to support fixed point `movM'
     instructions in and out of floating point registers.
     Unfortunately, I have forgotten why this was so, and I don't know
     whether it is still true.  If `HARD_REGNO_MODE_OK' rejects fixed
     point values in floating point registers, then the constraints of
     the fixed point `movM' instructions must be designed to avoid ever
     trying to reload into a floating point register.

`reload_inM'
`reload_outM'
     Like `movM', but used when a scratch register is required to move
     between operand 0 and operand 1.  Operand 2 describes the scratch
     register.  See the discussion of the `SECONDARY_RELOAD_CLASS'
     macro in *note Register Classes::.

     There are special restrictions on the form of the `match_operand's
     used in these patterns.  First, only the predicate for the reload
     operand is examined, i.e., `reload_in' examines operand 1, but not
     the predicates for operand 0 or 2.  Second, there may be only one
     alternative in the constraints.  Third, only a single register
     class letter may be used for the constraint; subsequent constraint
     letters are ignored.  As a special exception, an empty constraint
     string matches the `ALL_REGS' register class.  This may relieve
     ports of the burden of defining an `ALL_REGS' constraint letter
     just for these patterns.

`movstrictM'
     Like `movM' except that if operand 0 is a `subreg' with mode M of
     a register whose natural mode is wider, the `movstrictM'
     instruction is guaranteed not to alter any of the register except
     the part which belongs to mode M.

`load_multiple'
     Load several consecutive memory locations into consecutive
     registers.  Operand 0 is the first of the consecutive registers,
     operand 1 is the first memory location, and operand 2 is a
     constant: the number of consecutive registers.

     Define this only if the target machine really has such an
     instruction; do not define this if the most efficient way of
     loading consecutive registers from memory is to do them one at a
     time.

     On some machines, there are restrictions as to which consecutive
     registers can be stored into memory, such as particular starting or
     ending register numbers or only a range of valid counts.  For those
     machines, use a `define_expand' (*note Expander Definitions::) and
     make the pattern fail if the restrictions are not met.

     Write the generated insn as a `parallel' with elements being a
     `set' of one register from the appropriate memory location (you may
     also need `use' or `clobber' elements).  Use a `match_parallel'
     (*note RTL Template::) to recognize the insn.  See `rs6000.md' for
     examples of the use of this insn pattern.

`store_multiple'
     Similar to `load_multiple', but store several consecutive registers
     into consecutive memory locations.  Operand 0 is the first of the
     consecutive memory locations, operand 1 is the first register, and
     operand 2 is a constant: the number of consecutive registers.

`pushM'
     Output a push instruction.  Operand 0 is value to push.  Used only
     when `PUSH_ROUNDING' is defined.  For historical reason, this
     pattern may be missing and in such case an `mov' expander is used
     instead, with a `MEM' expression forming the push operation.  The
     `mov' expander method is deprecated.

`addM3'
     Add operand 2 and operand 1, storing the result in operand 0.  All
     operands must have mode M.  This can be used even on two-address
     machines, by means of constraints requiring operands 1 and 0 to be
     the same location.

`subM3', `mulM3'
`divM3', `udivM3', `modM3', `umodM3'
`sminM3', `smaxM3', `uminM3', `umaxM3'
`andM3', `iorM3', `xorM3'
     Similar, for other arithmetic operations.

`minM3', `maxM3'
     Floating point min and max operations.  If both operands are zeros,
     or if either operand is NaN, then it is unspecified which of the
     two operands is returned as the result.

`mulhisi3'
     Multiply operands 1 and 2, which have mode `HImode', and store a
     `SImode' product in operand 0.

`mulqihi3', `mulsidi3'
     Similar widening-multiplication instructions of other widths.

`umulqihi3', `umulhisi3', `umulsidi3'
     Similar widening-multiplication instructions that do unsigned
     multiplication.

`smulM3_highpart'
     Perform a signed multiplication of operands 1 and 2, which have
     mode M, and store the most significant half of the product in
     operand 0.  The least significant half of the product is discarded.

`umulM3_highpart'
     Similar, but the multiplication is unsigned.

`divmodM4'
     Signed division that produces both a quotient and a remainder.
     Operand 1 is divided by operand 2 to produce a quotient stored in
     operand 0 and a remainder stored in operand 3.

     For machines with an instruction that produces both a quotient and
     a remainder, provide a pattern for `divmodM4' but do not provide
     patterns for `divM3' and `modM3'.  This allows optimization in the
     relatively common case when both the quotient and remainder are
     computed.

     If an instruction that just produces a quotient or just a remainder
     exists and is more efficient than the instruction that produces
     both, write the output routine of `divmodM4' to call
     `find_reg_note' and look for a `REG_UNUSED' note on the quotient
     or remainder and generate the appropriate instruction.

`udivmodM4'
     Similar, but does unsigned division.

`ashlM3'
     Arithmetic-shift operand 1 left by a number of bits specified by
     operand 2, and store the result in operand 0.  Here M is the mode
     of operand 0 and operand 1; operand 2's mode is specified by the
     instruction pattern, and the compiler will convert the operand to
     that mode before generating the instruction.

`ashrM3', `lshrM3', `rotlM3', `rotrM3'
     Other shift and rotate instructions, analogous to the `ashlM3'
     instructions.

`negM2'
     Negate operand 1 and store the result in operand 0.

`absM2'
     Store the absolute value of operand 1 into operand 0.

`sqrtM2'
     Store the square root of operand 1 into operand 0.

     The `sqrt' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `sqrtf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`cosM2'
     Store the cosine of operand 1 into operand 0.

     The `cos' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `cosf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`sinM2'
     Store the sine of operand 1 into operand 0.

     The `sin' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `sinf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`expM2'
     Store the exponential of operand 1 into operand 0.

     The `exp' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `expf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`logM2'
     Store the natural logarithm of operand 1 into operand 0.

     The `log' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `logf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`powM3'
     Store the value of operand 1 raised to the exponent operand 2 into
     operand 0.

     The `pow' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `powf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`atan2M3'
     Store the arc tangent (inverse tangent) of operand 1 divided by
     operand 2 into operand 0, using the signs of both arguments to
     determine the quadrant of the result.

     The `atan2' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `atan2f' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`floorM2'
     Store the largest integral value not greater than argument.

     The `floor' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `floorf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`truncM2'
     Store the argument rounded to integer towards zero.

     The `trunc' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `truncf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`roundM2'
     Store the argument rounded to integer away from zero.

     The `round' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `roundf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`ceilM2'
     Store the argument rounded to integer away from zero.

     The `ceil' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `ceilf' built-in
     function uses the mode which corresponds to the C data type
     `float'.

`nearbyintM2'
     Store the argument rounded according to the default rounding mode

     The `nearbyint' built-in function of C always uses the mode which
     corresponds to the C data type `double' and the `nearbyintf'
     built-in function uses the mode which corresponds to the C data
     type `float'.

`ffsM2'
     Store into operand 0 one plus the index of the least significant
     1-bit of operand 1.  If operand 1 is zero, store zero.  M is the
     mode of operand 0; operand 1's mode is specified by the instruction
     pattern, and the compiler will convert the operand to that mode
     before generating the instruction.

     The `ffs' built-in function of C always uses the mode which
     corresponds to the C data type `int'.

`clzM2'
     Store into operand 0 the number of leading 0-bits in X, starting
     at the most significant bit position.  If X is 0, the result is
     undefined.  M is the mode of operand 0; operand 1's mode is
     specified by the instruction pattern, and the compiler will
     convert the operand to that mode before generating the instruction.

`ctzM2'
     Store into operand 0 the number of trailing 0-bits in X, starting
     at the least significant bit position.  If X is 0, the result is
     undefined.  M is the mode of operand 0; operand 1's mode is
     specified by the instruction pattern, and the compiler will
     convert the operand to that mode before generating the instruction.

`popcountM2'
     Store into operand 0 the number of 1-bits in X.  M is the mode of
     operand 0; operand 1's mode is specified by the instruction
     pattern, and the compiler will convert the operand to that mode
     before generating the instruction.

`parityM2'
     Store into operand 0 the parity of X, i.e. the number of 1-bits in
     X modulo 2.  M is the mode of operand 0; operand 1's mode is
     specified by the instruction pattern, and the compiler will convert
     the operand to that mode before generating the instruction.

`one_cmplM2'
     Store the bitwise-complement of operand 1 into operand 0.

`cmpM'
     Compare operand 0 and operand 1, and set the condition codes.  The
     RTL pattern should look like this:

          (set (cc0) (compare (match_operand:M 0 ...)
                              (match_operand:M 1 ...)))

`tstM'
     Compare operand 0 against zero, and set the condition codes.  The
     RTL pattern should look like this:

          (set (cc0) (match_operand:M 0 ...))

     `tstM' patterns should not be defined for machines that do not use
     `(cc0)'.  Doing so would confuse the optimizer since it would no
     longer be clear which `set' operations were comparisons.  The
     `cmpM' patterns should be used instead.

`movstrM'
     Block move instruction.  The addresses of the destination and
     source strings are the first two operands, and both are in mode
     `Pmode'.

     The number of bytes to move is the third operand, in mode M.
     Usually, you specify `word_mode' for M.  However, if you can
     generate better code knowing the range of valid lengths is smaller
     than those representable in a full word, you should provide a
     pattern with a mode corresponding to the range of values you can
     handle efficiently (e.g., `QImode' for values in the range 0-127;
     note we avoid numbers that appear negative) and also a pattern
     with `word_mode'.

     The fourth operand is the known shared alignment of the source and
     destination, in the form of a `const_int' rtx.  Thus, if the
     compiler knows that both source and destination are word-aligned,
     it may provide the value 4 for this operand.

     Descriptions of multiple `movstrM' patterns can only be beneficial
     if the patterns for smaller modes have fewer restrictions on their
     first, second and fourth operands.  Note that the mode M in
     `movstrM' does not impose any restriction on the mode of
     individually moved data units in the block.

     These patterns need not give special consideration to the
     possibility that the source and destination strings might overlap.

`clrstrM'
     Block clear instruction.  The addresses of the destination string
     is the first operand, in mode `Pmode'.  The number of bytes to
     clear is the second operand, in mode M.  See `movstrM' for a
     discussion of the choice of mode.

     The third operand is the known alignment of the destination, in
     the form of a `const_int' rtx.  Thus, if the compiler knows that
     the destination is word-aligned, it may provide the value 4 for
     this operand.

     The use for multiple `clrstrM' is as for `movstrM'.

`cmpstrM'
     String compare instruction, with five operands.  Operand 0 is the
     output; it has mode M.  The remaining four operands are like the
     operands of `movstrM'.  The two memory blocks specified are
     compared byte by byte in lexicographic order starting at the
     beginning of each string.  The instruction is not allowed to
     prefetch more than one byte at a time since either string may end
     in the first byte and reading past that may access an invalid page
     or segment and cause a fault.  The effect of the instruction is to
     store a value in operand 0 whose sign indicates the result of the
     comparison.

`cmpmemM'
     Block compare instruction, with five operands like the operands of
     `cmpstrM'.  The two memory blocks specified are compared byte by
     byte in lexicographic order starting at the beginning of each
     block.  Unlike `cmpstrM' the instruction can prefetch any bytes in
     the two memory blocks.  The effect of the instruction is to store
     a value in operand 0 whose sign indicates the result of the
     comparison.

`strlenM'
     Compute the length of a string, with three operands.  Operand 0 is
     the result (of mode M), operand 1 is a `mem' referring to the
     first character of the string, operand 2 is the character to
     search for (normally zero), and operand 3 is a constant describing
     the known alignment of the beginning of the string.

`floatMN2'
     Convert signed integer operand 1 (valid for fixed point mode M) to
     floating point mode N and store in operand 0 (which has mode N).

`floatunsMN2'
     Convert unsigned integer operand 1 (valid for fixed point mode M)
     to floating point mode N and store in operand 0 (which has mode N).

`fixMN2'
     Convert operand 1 (valid for floating point mode M) to fixed point
     mode N as a signed number and store in operand 0 (which has mode
     N).  This instruction's result is defined only when the value of
     operand 1 is an integer.

`fixunsMN2'
     Convert operand 1 (valid for floating point mode M) to fixed point
     mode N as an unsigned number and store in operand 0 (which has
     mode N).  This instruction's result is defined only when the value
     of operand 1 is an integer.

`ftruncM2'
     Convert operand 1 (valid for floating point mode M) to an integer
     value, still represented in floating point mode M, and store it in
     operand 0 (valid for floating point mode M).

`fix_truncMN2'
     Like `fixMN2' but works for any floating point value of mode M by
     converting the value to an integer.

`fixuns_truncMN2'
     Like `fixunsMN2' but works for any floating point value of mode M
     by converting the value to an integer.

`truncMN2'
     Truncate operand 1 (valid for mode M) to mode N and store in
     operand 0 (which has mode N).  Both modes must be fixed point or
     both floating point.

`extendMN2'
     Sign-extend operand 1 (valid for mode M) to mode N and store in
     operand 0 (which has mode N).  Both modes must be fixed point or
     both floating point.

`zero_extendMN2'
     Zero-extend operand 1 (valid for mode M) to mode N and store in
     operand 0 (which has mode N).  Both modes must be fixed point.

`extv'
     Extract a bit-field from operand 1 (a register or memory operand),
     where operand 2 specifies the width in bits and operand 3 the
     starting bit, and store it in operand 0.  Operand 0 must have mode
     `word_mode'.  Operand 1 may have mode `byte_mode' or `word_mode';
     often `word_mode' is allowed only for registers.  Operands 2 and 3
     must be valid for `word_mode'.

     The RTL generation pass generates this instruction only with
     constants for operands 2 and 3.

     The bit-field value is sign-extended to a full word integer before
     it is stored in operand 0.

`extzv'
     Like `extv' except that the bit-field value is zero-extended.

`insv'
     Store operand 3 (which must be valid for `word_mode') into a
     bit-field in operand 0, where operand 1 specifies the width in
     bits and operand 2 the starting bit.  Operand 0 may have mode
     `byte_mode' or `word_mode'; often `word_mode' is allowed only for
     registers.  Operands 1 and 2 must be valid for `word_mode'.

     The RTL generation pass generates this instruction only with
     constants for operands 1 and 2.

`movMODEcc'
     Conditionally move operand 2 or operand 3 into operand 0 according
     to the comparison in operand 1.  If the comparison is true,
     operand 2 is moved into operand 0, otherwise operand 3 is moved.

     The mode of the operands being compared need not be the same as
     the operands being moved.  Some machines, sparc64 for example,
     have instructions that conditionally move an integer value based
     on the floating point condition codes and vice versa.

     If the machine does not have conditional move instructions, do not
     define these patterns.

`addMODEcc'
     Similar to `movMODEcc' but for conditional addition.  Conditionally
     move operand 2 or (operands 2 + operand 3) into operand 0
     according to the comparison in operand 1.  If the comparison is
     true, operand 2 is moved into operand 0, otherwise (operand 2 +
     operand 3) is moved.

`sCOND'
     Store zero or nonzero in the operand according to the condition
     codes.  Value stored is nonzero iff the condition COND is true.
     COND is the name of a comparison operation expression code, such
     as `eq', `lt' or `leu'.

     You specify the mode that the operand must have when you write the
     `match_operand' expression.  The compiler automatically sees which
     mode you have used and supplies an operand of that mode.

     The value stored for a true condition must have 1 as its low bit,
     or else must be negative.  Otherwise the instruction is not
     suitable and you should omit it from the machine description.  You
     describe to the compiler exactly which value is stored by defining
     the macro `STORE_FLAG_VALUE' (*note Misc::).  If a description
     cannot be found that can be used for all the `sCOND' patterns, you
     should omit those operations from the machine description.

     These operations may fail, but should do so only in relatively
     uncommon cases; if they would fail for common cases involving
     integer comparisons, it is best to omit these patterns.

     If these operations are omitted, the compiler will usually
     generate code that copies the constant one to the target and
     branches around an assignment of zero to the target.  If this code
     is more efficient than the potential instructions used for the
     `sCOND' pattern followed by those required to convert the result
     into a 1 or a zero in `SImode', you should omit the `sCOND'
     operations from the machine description.

`bCOND'
     Conditional branch instruction.  Operand 0 is a `label_ref' that
     refers to the label to jump to.  Jump if the condition codes meet
     condition COND.

     Some machines do not follow the model assumed here where a
     comparison instruction is followed by a conditional branch
     instruction.  In that case, the `cmpM' (and `tstM') patterns should
     simply store the operands away and generate all the required insns
     in a `define_expand' (*note Expander Definitions::) for the
     conditional branch operations.  All calls to expand `bCOND'
     patterns are immediately preceded by calls to expand either a
     `cmpM' pattern or a `tstM' pattern.

     Machines that use a pseudo register for the condition code value,
     or where the mode used for the comparison depends on the condition
     being tested, should also use the above mechanism.  *Note Jump
     Patterns::.

     The above discussion also applies to the `movMODEcc' and `sCOND'
     patterns.

`jump'
     A jump inside a function; an unconditional branch.  Operand 0 is
     the `label_ref' of the label to jump to.  This pattern name is
     mandatory on all machines.

`call'
     Subroutine call instruction returning no value.  Operand 0 is the
     function to call; operand 1 is the number of bytes of arguments
     pushed as a `const_int'; operand 2 is the number of registers used
     as operands.

     On most machines, operand 2 is not actually stored into the RTL
     pattern.  It is supplied for the sake of some RISC machines which
     need to put this information into the assembler code; they can put
     it in the RTL instead of operand 1.

     Operand 0 should be a `mem' RTX whose address is the address of the
     function.  Note, however, that this address can be a `symbol_ref'
     expression even if it would not be a legitimate memory address on
     the target machine.  If it is also not a valid argument for a call
     instruction, the pattern for this operation should be a
     `define_expand' (*note Expander Definitions::) that places the
     address into a register and uses that register in the call
     instruction.

`call_value'
     Subroutine call instruction returning a value.  Operand 0 is the
     hard register in which the value is returned.  There are three more
     operands, the same as the three operands of the `call' instruction
     (but with numbers increased by one).

     Subroutines that return `BLKmode' objects use the `call' insn.

`call_pop', `call_value_pop'
     Similar to `call' and `call_value', except used if defined and if
     `RETURN_POPS_ARGS' is nonzero.  They should emit a `parallel' that
     contains both the function call and a `set' to indicate the
     adjustment made to the frame pointer.

     For machines where `RETURN_POPS_ARGS' can be nonzero, the use of
     these patterns increases the number of functions for which the
     frame pointer can be eliminated, if desired.

`untyped_call'
     Subroutine call instruction returning a value of any type.
     Operand 0 is the function to call; operand 1 is a memory location
     where the result of calling the function is to be stored; operand
     2 is a `parallel' expression where each element is a `set'
     expression that indicates the saving of a function return value
     into the result block.

     This instruction pattern should be defined to support
     `__builtin_apply' on machines where special instructions are needed
     to call a subroutine with arbitrary arguments or to save the value
     returned.  This instruction pattern is required on machines that
     have multiple registers that can hold a return value (i.e.
     `FUNCTION_VALUE_REGNO_P' is true for more than one register).

`return'
     Subroutine return instruction.  This instruction pattern name
     should be defined only if a single instruction can do all the work
     of returning from a function.

     Like the `movM' patterns, this pattern is also used after the RTL
     generation phase.  In this case it is to support machines where
     multiple instructions are usually needed to return from a
     function, but some class of functions only requires one
     instruction to implement a return.  Normally, the applicable
     functions are those which do not need to save any registers or
     allocate stack space.

     For such machines, the condition specified in this pattern should
     only be true when `reload_completed' is nonzero and the function's
     epilogue would only be a single instruction.  For machines with
     register windows, the routine `leaf_function_p' may be used to
     determine if a register window push is required.

     Machines that have conditional return instructions should define
     patterns such as

          (define_insn ""
            [(set (pc)
                  (if_then_else (match_operator
                                   0 "comparison_operator"
                                   [(cc0) (const_int 0)])
                                (return)
                                (pc)))]
            "CONDITION"
            "...")

     where CONDITION would normally be the same condition specified on
     the named `return' pattern.

`untyped_return'
     Untyped subroutine return instruction.  This instruction pattern
     should be defined to support `__builtin_return' on machines where
     special instructions are needed to return a value of any type.

     Operand 0 is a memory location where the result of calling a
     function with `__builtin_apply' is stored; operand 1 is a
     `parallel' expression where each element is a `set' expression
     that indicates the restoring of a function return value from the
     result block.

`nop'
     No-op instruction.  This instruction pattern name should always be
     defined to output a no-op in assembler code.  `(const_int 0)' will
     do as an RTL pattern.

`indirect_jump'
     An instruction to jump to an address which is operand zero.  This
     pattern name is mandatory on all machines.

`casesi'
     Instruction to jump through a dispatch table, including bounds
     checking.  This instruction takes five operands:

       1. The index to dispatch on, which has mode `SImode'.

       2. The lower bound for indices in the table, an integer constant.

       3. The total range of indices in the table--the largest index
          minus the smallest one (both inclusive).

       4. A label that precedes the table itself.

       5. A label to jump to if the index has a value outside the
          bounds.  (If the machine-description macro
          `CASE_DROPS_THROUGH' is defined, then an out-of-bounds index
          drops through to the code following the jump table instead of
          jumping to this label.  In that case, this label is not
          actually used by the `casesi' instruction, but it is always
          provided as an operand.)

     The table is a `addr_vec' or `addr_diff_vec' inside of a
     `jump_insn'.  The number of elements in the table is one plus the
     difference between the upper bound and the lower bound.

`tablejump'
     Instruction to jump to a variable address.  This is a low-level
     capability which can be used to implement a dispatch table when
     there is no `casesi' pattern.

     This pattern requires two operands: the address or offset, and a
     label which should immediately precede the jump table.  If the
     macro `CASE_VECTOR_PC_RELATIVE' evaluates to a nonzero value then
     the first operand is an offset which counts from the address of
     the table; otherwise, it is an absolute address to jump to.  In
     either case, the first operand has mode `Pmode'.

     The `tablejump' insn is always the last insn before the jump table
     it uses.  Its assembler code normally has no need to use the
     second operand, but you should incorporate it in the RTL pattern so
     that the jump optimizer will not delete the table as unreachable
     code.

`decrement_and_branch_until_zero'
     Conditional branch instruction that decrements a register and
     jumps if the register is nonzero.  Operand 0 is the register to
     decrement and test; operand 1 is the label to jump to if the
     register is nonzero.  *Note Looping Patterns::.

     This optional instruction pattern is only used by the combiner,
     typically for loops reversed by the loop optimizer when strength
     reduction is enabled.

`doloop_end'
     Conditional branch instruction that decrements a register and
     jumps if the register is nonzero.  This instruction takes five
     operands: Operand 0 is the register to decrement and test; operand
     1 is the number of loop iterations as a `const_int' or
     `const0_rtx' if this cannot be determined until run-time; operand
     2 is the actual or estimated maximum number of iterations as a
     `const_int'; operand 3 is the number of enclosed loops as a
     `const_int' (an innermost loop has a value of 1); operand 4 is the
     label to jump to if the register is nonzero.  *Note Looping
     Patterns::.

     This optional instruction pattern should be defined for machines
     with low-overhead looping instructions as the loop optimizer will
     try to modify suitable loops to utilize it.  If nested
     low-overhead looping is not supported, use a `define_expand'
     (*note Expander Definitions::) and make the pattern fail if
     operand 3 is not `const1_rtx'.  Similarly, if the actual or
     estimated maximum number of iterations is too large for this
     instruction, make it fail.

`doloop_begin'
     Companion instruction to `doloop_end' required for machines that
     need to perform some initialization, such as loading special
     registers used by a low-overhead looping instruction.  If
     initialization insns do not always need to be emitted, use a
     `define_expand' (*note Expander Definitions::) and make it fail.

`canonicalize_funcptr_for_compare'
     Canonicalize the function pointer in operand 1 and store the result
     into operand 0.

     Operand 0 is always a `reg' and has mode `Pmode'; operand 1 may be
     a `reg', `mem', `symbol_ref', `const_int', etc and also has mode
     `Pmode'.

     Canonicalization of a function pointer usually involves computing
     the address of the function which would be called if the function
     pointer were used in an indirect call.

     Only define this pattern if function pointers on the target machine
     can have different values but still call the same function when
     used in an indirect call.

`save_stack_block'
`save_stack_function'
`save_stack_nonlocal'
`restore_stack_block'
`restore_stack_function'
`restore_stack_nonlocal'
     Most machines save and restore the stack pointer by copying it to
     or from an object of mode `Pmode'.  Do not define these patterns on
     such machines.

     Some machines require special handling for stack pointer saves and
     restores.  On those machines, define the patterns corresponding to
     the non-standard cases by using a `define_expand' (*note Expander
     Definitions::) that produces the required insns.  The three types
     of saves and restores are:

       1. `save_stack_block' saves the stack pointer at the start of a
          block that allocates a variable-sized object, and
          `restore_stack_block' restores the stack pointer when the
          block is exited.

       2. `save_stack_function' and `restore_stack_function' do a
          similar job for the outermost block of a function and are
          used when the function allocates variable-sized objects or
          calls `alloca'.  Only the epilogue uses the restored stack
          pointer, allowing a simpler save or restore sequence on some
          machines.

       3. `save_stack_nonlocal' is used in functions that contain labels
          branched to by nested functions.  It saves the stack pointer
          in such a way that the inner function can use
          `restore_stack_nonlocal' to restore the stack pointer.  The
          compiler generates code to restore the frame and argument
          pointer registers, but some machines require saving and
          restoring additional data such as register window information
          or stack backchains.  Place insns in these patterns to save
          and restore any such required data.

     When saving the stack pointer, operand 0 is the save area and
     operand 1 is the stack pointer.  The mode used to allocate the
     save area defaults to `Pmode' but you can override that choice by
     defining the `STACK_SAVEAREA_MODE' macro (*note Storage Layout::).
     You must specify an integral mode, or `VOIDmode' if no save area
     is needed for a particular type of save (either because no save is
     needed or because a machine-specific save area can be used).
     Operand 0 is the stack pointer and operand 1 is the save area for
     restore operations.  If `save_stack_block' is defined, operand 0
     must not be `VOIDmode' since these saves can be arbitrarily nested.

     A save area is a `mem' that is at a constant offset from
     `virtual_stack_vars_rtx' when the stack pointer is saved for use by
     nonlocal gotos and a `reg' in the other two cases.

`allocate_stack'
     Subtract (or add if `STACK_GROWS_DOWNWARD' is undefined) operand 1
     from the stack pointer to create space for dynamically allocated
     data.

     Store the resultant pointer to this space into operand 0.  If you
     are allocating space from the main stack, do this by emitting a
     move insn to copy `virtual_stack_dynamic_rtx' to operand 0.  If
     you are allocating the space elsewhere, generate code to copy the
     location of the space to operand 0.  In the latter case, you must
     ensure this space gets freed when the corresponding space on the
     main stack is free.

     Do not define this pattern if all that must be done is the
     subtraction.  Some machines require other operations such as stack
     probes or maintaining the back chain.  Define this pattern to emit
     those operations in addition to updating the stack pointer.

`check_stack'
     If stack checking cannot be done on your system by probing the
     stack with a load or store instruction (*note Stack Checking::),
     define this pattern to perform the needed check and signaling an
     error if the stack has overflowed.  The single operand is the
     location in the stack furthest from the current stack pointer that
     you need to validate.  Normally, on machines where this pattern is
     needed, you would obtain the stack limit from a global or
     thread-specific variable or register.

`nonlocal_goto'
     Emit code to generate a non-local goto, e.g., a jump from one
     function to a label in an outer function.  This pattern has four
     arguments, each representing a value to be used in the jump.  The
     first argument is to be loaded into the frame pointer, the second
     is the address to branch to (code to dispatch to the actual label),
     the third is the address of a location where the stack is saved,
     and the last is the address of the label, to be placed in the
     location for the incoming static chain.

     On most machines you need not define this pattern, since GCC will
     already generate the correct code, which is to load the frame
     pointer and static chain, restore the stack (using the
     `restore_stack_nonlocal' pattern, if defined), and jump indirectly
     to the dispatcher.  You need only define this pattern if this code
     will not work on your machine.

`nonlocal_goto_receiver'
     This pattern, if defined, contains code needed at the target of a
     nonlocal goto after the code already generated by GCC.  You will
     not normally need to define this pattern.  A typical reason why
     you might need this pattern is if some value, such as a pointer to
     a global table, must be restored when the frame pointer is
     restored.  Note that a nonlocal goto only occurs within a
     unit-of-translation, so a global table pointer that is shared by
     all functions of a given module need not be restored.  There are
     no arguments.

`exception_receiver'
     This pattern, if defined, contains code needed at the site of an
     exception handler that isn't needed at the site of a nonlocal
     goto.  You will not normally need to define this pattern.  A
     typical reason why you might need this pattern is if some value,
     such as a pointer to a global table, must be restored after
     control flow is branched to the handler of an exception.  There
     are no arguments.

`builtin_setjmp_setup'
     This pattern, if defined, contains additional code needed to
     initialize the `jmp_buf'.  You will not normally need to define
     this pattern.  A typical reason why you might need this pattern is
     if some value, such as a pointer to a global table, must be
     restored.  Though it is preferred that the pointer value be
     recalculated if possible (given the address of a label for
     instance).  The single argument is a pointer to the `jmp_buf'.
     Note that the buffer is five words long and that the first three
     are normally used by the generic mechanism.

`builtin_setjmp_receiver'
     This pattern, if defined, contains code needed at the site of an
     built-in setjmp that isn't needed at the site of a nonlocal goto.
     You will not normally need to define this pattern.  A typical
     reason why you might need this pattern is if some value, such as a
     pointer to a global table, must be restored.  It takes one
     argument, which is the label to which builtin_longjmp transfered
     control; this pattern may be emitted at a small offset from that
     label.

`builtin_longjmp'
     This pattern, if defined, performs the entire action of the
     longjmp.  You will not normally need to define this pattern unless
     you also define `builtin_setjmp_setup'.  The single argument is a
     pointer to the `jmp_buf'.

`eh_return'
     This pattern, if defined, affects the way `__builtin_eh_return',
     and thence the call frame exception handling library routines, are
     built.  It is intended to handle non-trivial actions needed along
     the abnormal return path.

     The address of the exception handler to which the function should
     return is passed as operand to this pattern.  It will normally
     need to copied by the pattern to some special register or memory
     location.  If the pattern needs to determine the location of the
     target call frame in order to do so, it may use
     `EH_RETURN_STACKADJ_RTX', if defined; it will have already been
     assigned.

     If this pattern is not defined, the default action will be to
     simply copy the return address to `EH_RETURN_HANDLER_RTX'.  Either
     that macro or this pattern needs to be defined if call frame
     exception handling is to be used.

`prologue'
     This pattern, if defined, emits RTL for entry to a function.  The
     function entry is responsible for setting up the stack frame,
     initializing the frame pointer register, saving callee saved
     registers, etc.

     Using a prologue pattern is generally preferred over defining
     `TARGET_ASM_FUNCTION_PROLOGUE' to emit assembly code for the
     prologue.

     The `prologue' pattern is particularly useful for targets which
     perform instruction scheduling.

`epilogue'
     This pattern emits RTL for exit from a function.  The function
     exit is responsible for deallocating the stack frame, restoring
     callee saved registers and emitting the return instruction.

     Using an epilogue pattern is generally preferred over defining
     `TARGET_ASM_FUNCTION_EPILOGUE' to emit assembly code for the
     epilogue.

     The `epilogue' pattern is particularly useful for targets which
     perform instruction scheduling or which have delay slots for their
     return instruction.

`sibcall_epilogue'
     This pattern, if defined, emits RTL for exit from a function
     without the final branch back to the calling function.  This
     pattern will be emitted before any sibling call (aka tail call)
     sites.

     The `sibcall_epilogue' pattern must not clobber any arguments used
     for parameter passing or any stack slots for arguments passed to
     the current function.

`trap'
     This pattern, if defined, signals an error, typically by causing
     some kind of signal to be raised.  Among other places, it is used
     by the Java front end to signal `invalid array index' exceptions.

`conditional_trap'
     Conditional trap instruction.  Operand 0 is a piece of RTL which
     performs a comparison.  Operand 1 is the trap code, an integer.

     A typical `conditional_trap' pattern looks like

          (define_insn "conditional_trap"
            [(trap_if (match_operator 0 "trap_operator"
                       [(cc0) (const_int 0)])
                      (match_operand 1 "const_int_operand" "i"))]
            ""
            "...")

`prefetch'
     This pattern, if defined, emits code for a non-faulting data
     prefetch instruction.  Operand 0 is the address of the memory to
     prefetch.  Operand 1 is a constant 1 if the prefetch is preparing
     for a write to the memory address, or a constant 0 otherwise.
     Operand 2 is the expected degree of temporal locality of the data
     and is a value between 0 and 3, inclusive; 0 means that the data
     has no temporal locality, so it need not be left in the cache
     after the access; 3 means that the data has a high degree of
     temporal locality and should be left in all levels of cache
     possible;  1 and 2 mean, respectively, a low or moderate degree of
     temporal locality.

     Targets that do not support write prefetches or locality hints can
     ignore the values of operands 1 and 2.


File: gccint.info,  Node: Pattern Ordering,  Next: Dependent Patterns,  Prev: Standard Names,  Up: Machine Desc

When the Order of Patterns Matters
==================================

   Sometimes an insn can match more than one instruction pattern.  Then
the pattern that appears first in the machine description is the one
used.  Therefore, more specific patterns (patterns that will match
fewer things) and faster instructions (those that will produce better
code when they do match) should usually go first in the description.

   In some cases the effect of ordering the patterns can be used to hide
a pattern when it is not valid.  For example, the 68000 has an
instruction for converting a fullword to floating point and another for
converting a byte to floating point.  An instruction converting an
integer to floating point could match either one.  We put the pattern
to convert the fullword first to make sure that one will be used rather
than the other.  (Otherwise a large integer might be generated as a
single-byte immediate quantity, which would not work.)  Instead of
using this pattern ordering it would be possible to make the pattern
for convert-a-byte smart enough to deal properly with any constant
value.

