## evc_wait

System Trap - Wait for a kernel (device) signalled event.

### SYNOPSIS

    kern_return_t	evc_wait
    		(unsigned int	event);

### PARAMETERS

event
  [in scalar] The task local event ID of the kernel event object.

### DESCRIPTION

The evc_wait function causes the invoking thread to wait until the specified kernel (device) generated event occurs. Device drivers (typically mapped devices intended to be supported by user space drivers) may supply an event service. The event service defines one or more event objects, named by task local event IDs. Each of these event objects has an associated event count, initially zero. Whenever the associated event occurs (typically a device interrupt), the event count is incremented. If this count is zero when evc_wait is called, the calling thread waits for the next event to occur. Only one thread may be waiting for the event to occur. If the count is non-zero when evc_wait is called, the count is simply decremented without causing the thread to wait. The event count guarantees that no events are lost.

### NOTES

The typical use of this service is within user space device drivers. When a device interrupt occurs, the (in this case, simple) kernel device driver would place device status in a shared (with the user device driver) memory window (established by device_map) and signal the associated event. The user space device driver would normally be waiting with evc_wait. The user thread then wakes, processes the device status, typically interacting with the device via its shared memory window, then waits for the next interrupt.

### RETURN VALUES

KERN_NO_SPACE
  There is already a thread waiting for this event.

### RELATED INFORMATION

Functions: device_map.