From: Chris Renshaw <osm0sis@outlook.com>
Date: Wed, 11 Jan 2017 15:34:44 -0400
Subject: [PATCH] ipneigh/iproute/iprule: add missing headers

Imported from dorimanx's combined ported header toolchain:
https://github.com/dorimanx/android-busybox-ndk
---
 include/linux/if_addr.h   |  59 +++++
 include/linux/if_link.h   | 380 +++++++++++++++++++++++++++++
 include/linux/neighbour.h | 156 ++++++++++++
 include/linux/rtnetlink.h | 610 ++++++++++++++++++++++++++++++++++++++++++++++
 4 files changed, 1205 insertions(+)
 create mode 100644 include/linux/if_addr.h
 create mode 100644 include/linux/if_link.h
 create mode 100644 include/linux/neighbour.h
 create mode 100644 include/linux/rtnetlink.h

diff --git a/include/linux/if_addr.h b/include/linux/if_addr.h
new file mode 100644
index 0000000..58b39f4
--- /dev/null
+++ b/include/linux/if_addr.h
@@ -0,0 +1,59 @@
+#ifndef __LINUX_IF_ADDR_H
+#define __LINUX_IF_ADDR_H
+
+#include <linux/types.h>
+#include <linux/netlink.h>
+
+struct ifaddrmsg {
+	__u8		ifa_family;
+	__u8		ifa_prefixlen;	/* The prefix length		*/
+	__u8		ifa_flags;	/* Flags			*/
+	__u8		ifa_scope;	/* Address scope		*/
+	__u32		ifa_index;	/* Link index			*/
+};
+
+/*
+ * Important comment:
+ * IFA_ADDRESS is prefix address, rather than local interface address.
+ * It makes no difference for normally configured broadcast interfaces,
+ * but for point-to-point IFA_ADDRESS is DESTINATION address,
+ * local address is supplied in IFA_LOCAL attribute.
+ */
+enum {
+	IFA_UNSPEC,
+	IFA_ADDRESS,
+	IFA_LOCAL,
+	IFA_LABEL,
+	IFA_BROADCAST,
+	IFA_ANYCAST,
+	IFA_CACHEINFO,
+	IFA_MULTICAST,
+	__IFA_MAX,
+};
+
+#define IFA_MAX (__IFA_MAX - 1)
+
+/* ifa_flags */
+#define IFA_F_SECONDARY		0x01
+#define IFA_F_TEMPORARY		IFA_F_SECONDARY
+
+#define	IFA_F_NODAD		0x02
+#define IFA_F_OPTIMISTIC	0x04
+#define IFA_F_DADFAILED		0x08
+#define	IFA_F_HOMEADDRESS	0x10
+#define IFA_F_DEPRECATED	0x20
+#define IFA_F_TENTATIVE		0x40
+#define IFA_F_PERMANENT		0x80
+
+struct ifa_cacheinfo {
+	__u32	ifa_prefered;
+	__u32	ifa_valid;
+	__u32	cstamp; /* created timestamp, hundredths of seconds */
+	__u32	tstamp; /* updated timestamp, hundredths of seconds */
+};
+
+/* backwards compatibility for userspace */
+#define IFA_RTA(r)  ((struct rtattr*)(((char*)(r)) + NLMSG_ALIGN(sizeof(struct ifaddrmsg))))
+#define IFA_PAYLOAD(n) NLMSG_PAYLOAD(n,sizeof(struct ifaddrmsg))
+
+#endif
diff --git a/include/linux/if_link.h b/include/linux/if_link.h
new file mode 100644
index 0000000..06a3a47
--- /dev/null
+++ b/include/linux/if_link.h
@@ -0,0 +1,380 @@
+#ifndef _LINUX_IF_LINK_H
+#define _LINUX_IF_LINK_H
+
+#include <linux/types.h>
+#include <linux/netlink.h>
+
+/* This struct should be in sync with struct rtnl_link_stats64 */
+struct rtnl_link_stats {
+	__u32	rx_packets;		/* total packets received	*/
+	__u32	tx_packets;		/* total packets transmitted	*/
+	__u32	rx_bytes;		/* total bytes received 	*/
+	__u32	tx_bytes;		/* total bytes transmitted	*/
+	__u32	rx_errors;		/* bad packets received		*/
+	__u32	tx_errors;		/* packet transmit problems	*/
+	__u32	rx_dropped;		/* no space in linux buffers	*/
+	__u32	tx_dropped;		/* no space available in linux	*/
+	__u32	multicast;		/* multicast packets received	*/
+	__u32	collisions;
+
+	/* detailed rx_errors: */
+	__u32	rx_length_errors;
+	__u32	rx_over_errors;		/* receiver ring buff overflow	*/
+	__u32	rx_crc_errors;		/* recved pkt with crc error	*/
+	__u32	rx_frame_errors;	/* recv'd frame alignment error */
+	__u32	rx_fifo_errors;		/* recv'r fifo overrun		*/
+	__u32	rx_missed_errors;	/* receiver missed packet	*/
+
+	/* detailed tx_errors */
+	__u32	tx_aborted_errors;
+	__u32	tx_carrier_errors;
+	__u32	tx_fifo_errors;
+	__u32	tx_heartbeat_errors;
+	__u32	tx_window_errors;
+
+	/* for cslip etc */
+	__u32	rx_compressed;
+	__u32	tx_compressed;
+};
+
+/* The main device statistics structure */
+struct rtnl_link_stats64 {
+	__u64	rx_packets;		/* total packets received	*/
+	__u64	tx_packets;		/* total packets transmitted	*/
+	__u64	rx_bytes;		/* total bytes received 	*/
+	__u64	tx_bytes;		/* total bytes transmitted	*/
+	__u64	rx_errors;		/* bad packets received		*/
+	__u64	tx_errors;		/* packet transmit problems	*/
+	__u64	rx_dropped;		/* no space in linux buffers	*/
+	__u64	tx_dropped;		/* no space available in linux	*/
+	__u64	multicast;		/* multicast packets received	*/
+	__u64	collisions;
+
+	/* detailed rx_errors: */
+	__u64	rx_length_errors;
+	__u64	rx_over_errors;		/* receiver ring buff overflow	*/
+	__u64	rx_crc_errors;		/* recved pkt with crc error	*/
+	__u64	rx_frame_errors;	/* recv'd frame alignment error */
+	__u64	rx_fifo_errors;		/* recv'r fifo overrun		*/
+	__u64	rx_missed_errors;	/* receiver missed packet	*/
+
+	/* detailed tx_errors */
+	__u64	tx_aborted_errors;
+	__u64	tx_carrier_errors;
+	__u64	tx_fifo_errors;
+	__u64	tx_heartbeat_errors;
+	__u64	tx_window_errors;
+
+	/* for cslip etc */
+	__u64	rx_compressed;
+	__u64	tx_compressed;
+};
+
+/* The struct should be in sync with struct ifmap */
+struct rtnl_link_ifmap {
+	__u64	mem_start;
+	__u64	mem_end;
+	__u64	base_addr;
+	__u16	irq;
+	__u8	dma;
+	__u8	port;
+};
+
+/*
+ * IFLA_AF_SPEC
+ *   Contains nested attributes for address family specific attributes.
+ *   Each address family may create a attribute with the address family
+ *   number as type and create its own attribute structure in it.
+ *
+ *   Example:
+ *   [IFLA_AF_SPEC] = {
+ *       [AF_INET] = {
+ *           [IFLA_INET_CONF] = ...,
+ *       },
+ *       [AF_INET6] = {
+ *           [IFLA_INET6_FLAGS] = ...,
+ *           [IFLA_INET6_CONF] = ...,
+ *       }
+ *   }
+ */
+
+enum {
+	IFLA_UNSPEC,
+	IFLA_ADDRESS,
+	IFLA_BROADCAST,
+	IFLA_IFNAME,
+	IFLA_MTU,
+	IFLA_LINK,
+	IFLA_QDISC,
+	IFLA_STATS,
+	IFLA_COST,
+#define IFLA_COST IFLA_COST
+	IFLA_PRIORITY,
+#define IFLA_PRIORITY IFLA_PRIORITY
+	IFLA_MASTER,
+#define IFLA_MASTER IFLA_MASTER
+	IFLA_WIRELESS,		/* Wireless Extension event - see wireless.h */
+#define IFLA_WIRELESS IFLA_WIRELESS
+	IFLA_PROTINFO,		/* Protocol specific information for a link */
+#define IFLA_PROTINFO IFLA_PROTINFO
+	IFLA_TXQLEN,
+#define IFLA_TXQLEN IFLA_TXQLEN
+	IFLA_MAP,
+#define IFLA_MAP IFLA_MAP
+	IFLA_WEIGHT,
+#define IFLA_WEIGHT IFLA_WEIGHT
+	IFLA_OPERSTATE,
+	IFLA_LINKMODE,
+	IFLA_LINKINFO,
+#define IFLA_LINKINFO IFLA_LINKINFO
+	IFLA_NET_NS_PID,
+	IFLA_IFALIAS,
+	IFLA_NUM_VF,		/* Number of VFs if device is SR-IOV PF */
+	IFLA_VFINFO_LIST,
+	IFLA_STATS64,
+	IFLA_VF_PORTS,
+	IFLA_PORT_SELF,
+	IFLA_AF_SPEC,
+	IFLA_GROUP,		/* Group the device belongs to */
+	IFLA_NET_NS_FD,
+	IFLA_EXT_MASK,		/* Extended info mask, VFs, etc */
+	__IFLA_MAX
+};
+
+
+#define IFLA_MAX (__IFLA_MAX - 1)
+
+/* backwards compatibility for userspace */
+#define IFLA_RTA(r)  ((struct rtattr*)(((char*)(r)) + NLMSG_ALIGN(sizeof(struct ifinfomsg))))
+#define IFLA_PAYLOAD(n) NLMSG_PAYLOAD(n,sizeof(struct ifinfomsg))
+
+enum {
+	IFLA_INET_UNSPEC,
+	IFLA_INET_CONF,
+	__IFLA_INET_MAX,
+};
+
+#define IFLA_INET_MAX (__IFLA_INET_MAX - 1)
+
+/* ifi_flags.
+
+   IFF_* flags.
+
+   The only change is:
+   IFF_LOOPBACK, IFF_BROADCAST and IFF_POINTOPOINT are
+   more not changeable by user. They describe link media
+   characteristics and set by device driver.
+
+   Comments:
+   - Combination IFF_BROADCAST|IFF_POINTOPOINT is invalid
+   - If neither of these three flags are set;
+     the interface is NBMA.
+
+   - IFF_MULTICAST does not mean anything special:
+   multicasts can be used on all not-NBMA links.
+   IFF_MULTICAST means that this media uses special encapsulation
+   for multicast frames. Apparently, all IFF_POINTOPOINT and
+   IFF_BROADCAST devices are able to use multicasts too.
+ */
+
+/* IFLA_LINK.
+   For usual devices it is equal ifi_index.
+   If it is a "virtual interface" (f.e. tunnel), ifi_link
+   can point to real physical interface (f.e. for bandwidth calculations),
+   or maybe 0, what means, that real media is unknown (usual
+   for IPIP tunnels, when route to endpoint is allowed to change)
+ */
+
+/* Subtype attributes for IFLA_PROTINFO */
+enum {
+	IFLA_INET6_UNSPEC,
+	IFLA_INET6_FLAGS,	/* link flags			*/
+	IFLA_INET6_CONF,	/* sysctl parameters		*/
+	IFLA_INET6_STATS,	/* statistics			*/
+	IFLA_INET6_MCAST,	/* MC things. What of them?	*/
+	IFLA_INET6_CACHEINFO,	/* time values and max reasm size */
+	IFLA_INET6_ICMP6STATS,	/* statistics (icmpv6)		*/
+	__IFLA_INET6_MAX
+};
+
+#define IFLA_INET6_MAX	(__IFLA_INET6_MAX - 1)
+
+struct ifla_cacheinfo {
+	__u32	max_reasm_len;
+	__u32	tstamp;		/* ipv6InterfaceTable updated timestamp */
+	__u32	reachable_time;
+	__u32	retrans_time;
+};
+
+enum {
+	IFLA_INFO_UNSPEC,
+	IFLA_INFO_KIND,
+	IFLA_INFO_DATA,
+	IFLA_INFO_XSTATS,
+	__IFLA_INFO_MAX,
+};
+
+#define IFLA_INFO_MAX	(__IFLA_INFO_MAX - 1)
+
+/* VLAN section */
+
+enum {
+	IFLA_VLAN_UNSPEC,
+	IFLA_VLAN_ID,
+	IFLA_VLAN_FLAGS,
+	IFLA_VLAN_EGRESS_QOS,
+	IFLA_VLAN_INGRESS_QOS,
+	__IFLA_VLAN_MAX,
+};
+
+#define IFLA_VLAN_MAX	(__IFLA_VLAN_MAX - 1)
+
+struct ifla_vlan_flags {
+	__u32	flags;
+	__u32	mask;
+};
+
+enum {
+	IFLA_VLAN_QOS_UNSPEC,
+	IFLA_VLAN_QOS_MAPPING,
+	__IFLA_VLAN_QOS_MAX
+};
+
+#define IFLA_VLAN_QOS_MAX	(__IFLA_VLAN_QOS_MAX - 1)
+
+struct ifla_vlan_qos_mapping {
+	__u32 from;
+	__u32 to;
+};
+
+/* MACVLAN section */
+enum {
+	IFLA_MACVLAN_UNSPEC,
+	IFLA_MACVLAN_MODE,
+	__IFLA_MACVLAN_MAX,
+};
+
+#define IFLA_MACVLAN_MAX (__IFLA_MACVLAN_MAX - 1)
+
+enum macvlan_mode {
+	MACVLAN_MODE_PRIVATE = 1, /* don't talk to other macvlans */
+	MACVLAN_MODE_VEPA    = 2, /* talk to other ports through ext bridge */
+	MACVLAN_MODE_BRIDGE  = 4, /* talk to bridge ports directly */
+	MACVLAN_MODE_PASSTHRU = 8,/* take over the underlying device */
+};
+
+/* SR-IOV virtual function management section */
+
+enum {
+	IFLA_VF_INFO_UNSPEC,
+	IFLA_VF_INFO,
+	__IFLA_VF_INFO_MAX,
+};
+
+#define IFLA_VF_INFO_MAX (__IFLA_VF_INFO_MAX - 1)
+
+enum {
+	IFLA_VF_UNSPEC,
+	IFLA_VF_MAC,		/* Hardware queue specific attributes */
+	IFLA_VF_VLAN,
+	IFLA_VF_TX_RATE,	/* TX Bandwidth Allocation */
+	IFLA_VF_SPOOFCHK,	/* Spoof Checking on/off switch */
+	__IFLA_VF_MAX,
+};
+
+#define IFLA_VF_MAX (__IFLA_VF_MAX - 1)
+
+struct ifla_vf_mac {
+	__u32 vf;
+	__u8 mac[32]; /* MAX_ADDR_LEN */
+};
+
+struct ifla_vf_vlan {
+	__u32 vf;
+	__u32 vlan; /* 0 - 4095, 0 disables VLAN filter */
+	__u32 qos;
+};
+
+struct ifla_vf_tx_rate {
+	__u32 vf;
+	__u32 rate; /* Max TX bandwidth in Mbps, 0 disables throttling */
+};
+
+struct ifla_vf_spoofchk {
+	__u32 vf;
+	__u32 setting;
+};
+
+/* VF ports management section
+ *
+ *	Nested layout of set/get msg is:
+ *
+ *		[IFLA_NUM_VF]
+ *		[IFLA_VF_PORTS]
+ *			[IFLA_VF_PORT]
+ *				[IFLA_PORT_*], ...
+ *			[IFLA_VF_PORT]
+ *				[IFLA_PORT_*], ...
+ *			...
+ *		[IFLA_PORT_SELF]
+ *			[IFLA_PORT_*], ...
+ */
+
+enum {
+	IFLA_VF_PORT_UNSPEC,
+	IFLA_VF_PORT,			/* nest */
+	__IFLA_VF_PORT_MAX,
+};
+
+#define IFLA_VF_PORT_MAX (__IFLA_VF_PORT_MAX - 1)
+
+enum {
+	IFLA_PORT_UNSPEC,
+	IFLA_PORT_VF,			/* __u32 */
+	IFLA_PORT_PROFILE,		/* string */
+	IFLA_PORT_VSI_TYPE,		/* 802.1Qbg (pre-)standard VDP */
+	IFLA_PORT_INSTANCE_UUID,	/* binary UUID */
+	IFLA_PORT_HOST_UUID,		/* binary UUID */
+	IFLA_PORT_REQUEST,		/* __u8 */
+	IFLA_PORT_RESPONSE,		/* __u16, output only */
+	__IFLA_PORT_MAX,
+};
+
+#define IFLA_PORT_MAX (__IFLA_PORT_MAX - 1)
+
+#define PORT_PROFILE_MAX	40
+#define PORT_UUID_MAX		16
+#define PORT_SELF_VF		-1
+
+enum {
+	PORT_REQUEST_PREASSOCIATE = 0,
+	PORT_REQUEST_PREASSOCIATE_RR,
+	PORT_REQUEST_ASSOCIATE,
+	PORT_REQUEST_DISASSOCIATE,
+};
+
+enum {
+	PORT_VDP_RESPONSE_SUCCESS = 0,
+	PORT_VDP_RESPONSE_INVALID_FORMAT,
+	PORT_VDP_RESPONSE_INSUFFICIENT_RESOURCES,
+	PORT_VDP_RESPONSE_UNUSED_VTID,
+	PORT_VDP_RESPONSE_VTID_VIOLATION,
+	PORT_VDP_RESPONSE_VTID_VERSION_VIOALTION,
+	PORT_VDP_RESPONSE_OUT_OF_SYNC,
+	/* 0x08-0xFF reserved for future VDP use */
+	PORT_PROFILE_RESPONSE_SUCCESS = 0x100,
+	PORT_PROFILE_RESPONSE_INPROGRESS,
+	PORT_PROFILE_RESPONSE_INVALID,
+	PORT_PROFILE_RESPONSE_BADSTATE,
+	PORT_PROFILE_RESPONSE_INSUFFICIENT_RESOURCES,
+	PORT_PROFILE_RESPONSE_ERROR,
+};
+
+struct ifla_port_vsi {
+	__u8 vsi_mgr_id;
+	__u8 vsi_type_id[3];
+	__u8 vsi_type_version;
+	__u8 pad[3];
+};
+
+#endif /* _LINUX_IF_LINK_H */
diff --git a/include/linux/neighbour.h b/include/linux/neighbour.h
new file mode 100644
index 0000000..b188f68
--- /dev/null
+++ b/include/linux/neighbour.h
@@ -0,0 +1,156 @@
+#ifndef __LINUX_NEIGHBOUR_H
+#define __LINUX_NEIGHBOUR_H
+
+#include <linux/types.h>
+#include <linux/netlink.h>
+
+struct ndmsg {
+	__u8		ndm_family;
+	__u8		ndm_pad1;
+	__u16		ndm_pad2;
+	__s32		ndm_ifindex;
+	__u16		ndm_state;
+	__u8		ndm_flags;
+	__u8		ndm_type;
+};
+
+enum {
+	NDA_UNSPEC,
+	NDA_DST,
+	NDA_LLADDR,
+	NDA_CACHEINFO,
+	NDA_PROBES,
+	__NDA_MAX
+};
+
+#define NDA_MAX (__NDA_MAX - 1)
+
+/*
+ *	Neighbor Cache Entry Flags
+ */
+
+#define NTF_USE		0x01
+#define NTF_PROXY	0x08	/* == ATF_PUBL */
+#define NTF_ROUTER	0x80
+
+/*
+ *	Neighbor Cache Entry States.
+ */
+
+#define NUD_INCOMPLETE	0x01
+#define NUD_REACHABLE	0x02
+#define NUD_STALE	0x04
+#define NUD_DELAY	0x08
+#define NUD_PROBE	0x10
+#define NUD_FAILED	0x20
+
+/* Dummy states */
+#define NUD_NOARP	0x40
+#define NUD_PERMANENT	0x80
+#define NUD_NONE	0x00
+
+/* NUD_NOARP & NUD_PERMANENT are pseudostates, they never change
+   and make no address resolution or NUD.
+   NUD_PERMANENT is also cannot be deleted by garbage collectors.
+ */
+
+struct nda_cacheinfo {
+	__u32		ndm_confirmed;
+	__u32		ndm_used;
+	__u32		ndm_updated;
+	__u32		ndm_refcnt;
+};
+
+/*****************************************************************
+ *		Neighbour tables specific messages.
+ *
+ * To retrieve the neighbour tables send RTM_GETNEIGHTBL with the
+ * NLM_F_DUMP flag set. Every neighbour table configuration is
+ * spread over multiple messages to avoid running into message
+ * size limits on systems with many interfaces. The first message
+ * in the sequence transports all not device specific data such as
+ * statistics, configuration, and the default parameter set.
+ * This message is followed by 0..n messages carrying device
+ * specific parameter sets.
+ * Although the ordering should be sufficient, NDTA_NAME can be
+ * used to identify sequences. The initial message can be identified
+ * by checking for NDTA_CONFIG. The device specific messages do
+ * not contain this TLV but have NDTPA_IFINDEX set to the
+ * corresponding interface index.
+ *
+ * To change neighbour table attributes, send RTM_SETNEIGHTBL
+ * with NDTA_NAME set. Changeable attribute include NDTA_THRESH[1-3],
+ * NDTA_GC_INTERVAL, and all TLVs in NDTA_PARMS unless marked
+ * otherwise. Device specific parameter sets can be changed by
+ * setting NDTPA_IFINDEX to the interface index of the corresponding
+ * device.
+ ****/
+
+struct ndt_stats {
+	__u64		ndts_allocs;
+	__u64		ndts_destroys;
+	__u64		ndts_hash_grows;
+	__u64		ndts_res_failed;
+	__u64		ndts_lookups;
+	__u64		ndts_hits;
+	__u64		ndts_rcv_probes_mcast;
+	__u64		ndts_rcv_probes_ucast;
+	__u64		ndts_periodic_gc_runs;
+	__u64		ndts_forced_gc_runs;
+};
+
+enum {
+	NDTPA_UNSPEC,
+	NDTPA_IFINDEX,			/* u32, unchangeable */
+	NDTPA_REFCNT,			/* u32, read-only */
+	NDTPA_REACHABLE_TIME,		/* u64, read-only, msecs */
+	NDTPA_BASE_REACHABLE_TIME,	/* u64, msecs */
+	NDTPA_RETRANS_TIME,		/* u64, msecs */
+	NDTPA_GC_STALETIME,		/* u64, msecs */
+	NDTPA_DELAY_PROBE_TIME,		/* u64, msecs */
+	NDTPA_QUEUE_LEN,		/* u32 */
+	NDTPA_APP_PROBES,		/* u32 */
+	NDTPA_UCAST_PROBES,		/* u32 */
+	NDTPA_MCAST_PROBES,		/* u32 */
+	NDTPA_ANYCAST_DELAY,		/* u64, msecs */
+	NDTPA_PROXY_DELAY,		/* u64, msecs */
+	NDTPA_PROXY_QLEN,		/* u32 */
+	NDTPA_LOCKTIME,			/* u64, msecs */
+	NDTPA_QUEUE_LENBYTES,		/* u32 */
+	__NDTPA_MAX
+};
+#define NDTPA_MAX (__NDTPA_MAX - 1)
+
+struct ndtmsg {
+	__u8		ndtm_family;
+	__u8		ndtm_pad1;
+	__u16		ndtm_pad2;
+};
+
+struct ndt_config {
+	__u16		ndtc_key_len;
+	__u16		ndtc_entry_size;
+	__u32		ndtc_entries;
+	__u32		ndtc_last_flush;	/* delta to now in msecs */
+	__u32		ndtc_last_rand;		/* delta to now in msecs */
+	__u32		ndtc_hash_rnd;
+	__u32		ndtc_hash_mask;
+	__u32		ndtc_hash_chain_gc;
+	__u32		ndtc_proxy_qlen;
+};
+
+enum {
+	NDTA_UNSPEC,
+	NDTA_NAME,			/* char *, unchangeable */
+	NDTA_THRESH1,			/* u32 */
+	NDTA_THRESH2,			/* u32 */
+	NDTA_THRESH3,			/* u32 */
+	NDTA_CONFIG,			/* struct ndt_config, read-only */
+	NDTA_PARMS,			/* nested TLV NDTPA_* */
+	NDTA_STATS,			/* struct ndt_stats, read-only */
+	NDTA_GC_INTERVAL,		/* u64, msecs */
+	__NDTA_MAX
+};
+#define NDTA_MAX (__NDTA_MAX - 1)
+
+#endif
diff --git a/include/linux/rtnetlink.h b/include/linux/rtnetlink.h
new file mode 100644
index 0000000..d5b7fdd
--- /dev/null
+++ b/include/linux/rtnetlink.h
@@ -0,0 +1,610 @@
+#ifndef __LINUX_RTNETLINK_H
+#define __LINUX_RTNETLINK_H
+
+#include <linux/types.h>
+#include <linux/netlink.h>
+#include <linux/if_link.h>
+#include <linux/if_addr.h>
+#include <linux/neighbour.h>
+
+/* rtnetlink families. Values up to 127 are reserved for real address
+ * families, values above 128 may be used arbitrarily.
+ */
+#define RTNL_FAMILY_IPMR		128
+#define RTNL_FAMILY_IP6MR		129
+#define RTNL_FAMILY_MAX			129
+
+/****
+ *		Routing/neighbour discovery messages.
+ ****/
+
+/* Types of messages */
+
+enum {
+	RTM_BASE	= 16,
+#define RTM_BASE	RTM_BASE
+
+	RTM_NEWLINK	= 16,
+#define RTM_NEWLINK	RTM_NEWLINK
+	RTM_DELLINK,
+#define RTM_DELLINK	RTM_DELLINK
+	RTM_GETLINK,
+#define RTM_GETLINK	RTM_GETLINK
+	RTM_SETLINK,
+#define RTM_SETLINK	RTM_SETLINK
+
+	RTM_NEWADDR	= 20,
+#define RTM_NEWADDR	RTM_NEWADDR
+	RTM_DELADDR,
+#define RTM_DELADDR	RTM_DELADDR
+	RTM_GETADDR,
+#define RTM_GETADDR	RTM_GETADDR
+
+	RTM_NEWROUTE	= 24,
+#define RTM_NEWROUTE	RTM_NEWROUTE
+	RTM_DELROUTE,
+#define RTM_DELROUTE	RTM_DELROUTE
+	RTM_GETROUTE,
+#define RTM_GETROUTE	RTM_GETROUTE
+
+	RTM_NEWNEIGH	= 28,
+#define RTM_NEWNEIGH	RTM_NEWNEIGH
+	RTM_DELNEIGH,
+#define RTM_DELNEIGH	RTM_DELNEIGH
+	RTM_GETNEIGH,
+#define RTM_GETNEIGH	RTM_GETNEIGH
+
+	RTM_NEWRULE	= 32,
+#define RTM_NEWRULE	RTM_NEWRULE
+	RTM_DELRULE,
+#define RTM_DELRULE	RTM_DELRULE
+	RTM_GETRULE,
+#define RTM_GETRULE	RTM_GETRULE
+
+	RTM_NEWQDISC	= 36,
+#define RTM_NEWQDISC	RTM_NEWQDISC
+	RTM_DELQDISC,
+#define RTM_DELQDISC	RTM_DELQDISC
+	RTM_GETQDISC,
+#define RTM_GETQDISC	RTM_GETQDISC
+
+	RTM_NEWTCLASS	= 40,
+#define RTM_NEWTCLASS	RTM_NEWTCLASS
+	RTM_DELTCLASS,
+#define RTM_DELTCLASS	RTM_DELTCLASS
+	RTM_GETTCLASS,
+#define RTM_GETTCLASS	RTM_GETTCLASS
+
+	RTM_NEWTFILTER	= 44,
+#define RTM_NEWTFILTER	RTM_NEWTFILTER
+	RTM_DELTFILTER,
+#define RTM_DELTFILTER	RTM_DELTFILTER
+	RTM_GETTFILTER,
+#define RTM_GETTFILTER	RTM_GETTFILTER
+
+	RTM_NEWACTION	= 48,
+#define RTM_NEWACTION   RTM_NEWACTION
+	RTM_DELACTION,
+#define RTM_DELACTION   RTM_DELACTION
+	RTM_GETACTION,
+#define RTM_GETACTION   RTM_GETACTION
+
+	RTM_NEWPREFIX	= 52,
+#define RTM_NEWPREFIX	RTM_NEWPREFIX
+
+	RTM_GETMULTICAST = 58,
+#define RTM_GETMULTICAST RTM_GETMULTICAST
+
+	RTM_GETANYCAST	= 62,
+#define RTM_GETANYCAST	RTM_GETANYCAST
+
+	RTM_NEWNEIGHTBL	= 64,
+#define RTM_NEWNEIGHTBL	RTM_NEWNEIGHTBL
+	RTM_GETNEIGHTBL	= 66,
+#define RTM_GETNEIGHTBL	RTM_GETNEIGHTBL
+	RTM_SETNEIGHTBL,
+#define RTM_SETNEIGHTBL	RTM_SETNEIGHTBL
+
+	RTM_NEWNDUSEROPT = 68,
+#define RTM_NEWNDUSEROPT RTM_NEWNDUSEROPT
+
+	RTM_NEWADDRLABEL = 72,
+#define RTM_NEWADDRLABEL RTM_NEWADDRLABEL
+	RTM_DELADDRLABEL,
+#define RTM_DELADDRLABEL RTM_DELADDRLABEL
+	RTM_GETADDRLABEL,
+#define RTM_GETADDRLABEL RTM_GETADDRLABEL
+
+	RTM_GETDCB = 78,
+#define RTM_GETDCB RTM_GETDCB
+	RTM_SETDCB,
+#define RTM_SETDCB RTM_SETDCB
+
+	__RTM_MAX,
+#define RTM_MAX		(((__RTM_MAX + 3) & ~3) - 1)
+};
+
+#define RTM_NR_MSGTYPES	(RTM_MAX + 1 - RTM_BASE)
+#define RTM_NR_FAMILIES	(RTM_NR_MSGTYPES >> 2)
+#define RTM_FAM(cmd)	(((cmd) - RTM_BASE) >> 2)
+
+/* 
+   Generic structure for encapsulation of optional route information.
+   It is reminiscent of sockaddr, but with sa_family replaced
+   with attribute type.
+ */
+
+struct rtattr {
+	unsigned short	rta_len;
+	unsigned short	rta_type;
+};
+
+/* Macros to handle rtattributes */
+
+#define RTA_ALIGNTO	4
+#define RTA_ALIGN(len) ( ((len)+RTA_ALIGNTO-1) & ~(RTA_ALIGNTO-1) )
+#define RTA_OK(rta,len) ((len) >= (int)sizeof(struct rtattr) && \
+			 (rta)->rta_len >= sizeof(struct rtattr) && \
+			 (rta)->rta_len <= (len))
+#define RTA_NEXT(rta,attrlen)	((attrlen) -= RTA_ALIGN((rta)->rta_len), \
+				 (struct rtattr*)(((char*)(rta)) + RTA_ALIGN((rta)->rta_len)))
+#define RTA_LENGTH(len)	(RTA_ALIGN(sizeof(struct rtattr)) + (len))
+#define RTA_SPACE(len)	RTA_ALIGN(RTA_LENGTH(len))
+#define RTA_DATA(rta)   ((void*)(((char*)(rta)) + RTA_LENGTH(0)))
+#define RTA_PAYLOAD(rta) ((int)((rta)->rta_len) - RTA_LENGTH(0))
+
+
+
+
+/******************************************************************************
+ *		Definitions used in routing table administration.
+ ****/
+
+struct rtmsg {
+	unsigned char		rtm_family;
+	unsigned char		rtm_dst_len;
+	unsigned char		rtm_src_len;
+	unsigned char		rtm_tos;
+
+	unsigned char		rtm_table;	/* Routing table id */
+	unsigned char		rtm_protocol;	/* Routing protocol; see below	*/
+	unsigned char		rtm_scope;	/* See below */	
+	unsigned char		rtm_type;	/* See below	*/
+
+	unsigned		rtm_flags;
+};
+
+/* rtm_type */
+
+enum {
+	RTN_UNSPEC,
+	RTN_UNICAST,		/* Gateway or direct route	*/
+	RTN_LOCAL,		/* Accept locally		*/
+	RTN_BROADCAST,		/* Accept locally as broadcast,
+				   send as broadcast */
+	RTN_ANYCAST,		/* Accept locally as broadcast,
+				   but send as unicast */
+	RTN_MULTICAST,		/* Multicast route		*/
+	RTN_BLACKHOLE,		/* Drop				*/
+	RTN_UNREACHABLE,	/* Destination is unreachable   */
+	RTN_PROHIBIT,		/* Administratively prohibited	*/
+	RTN_THROW,		/* Not in this table		*/
+	RTN_NAT,		/* Translate this address	*/
+	RTN_XRESOLVE,		/* Use external resolver	*/
+	__RTN_MAX
+};
+
+#define RTN_MAX (__RTN_MAX - 1)
+
+
+/* rtm_protocol */
+
+#define RTPROT_UNSPEC	0
+#define RTPROT_REDIRECT	1	/* Route installed by ICMP redirects;
+				   not used by current IPv4 */
+#define RTPROT_KERNEL	2	/* Route installed by kernel		*/
+#define RTPROT_BOOT	3	/* Route installed during boot		*/
+#define RTPROT_STATIC	4	/* Route installed by administrator	*/
+
+/* Values of protocol >= RTPROT_STATIC are not interpreted by kernel;
+   they are just passed from user and back as is.
+   It will be used by hypothetical multiple routing daemons.
+   Note that protocol values should be standardized in order to
+   avoid conflicts.
+ */
+
+#define RTPROT_GATED	8	/* Apparently, GateD */
+#define RTPROT_RA	9	/* RDISC/ND router advertisements */
+#define RTPROT_MRT	10	/* Merit MRT */
+#define RTPROT_ZEBRA	11	/* Zebra */
+#define RTPROT_BIRD	12	/* BIRD */
+#define RTPROT_DNROUTED	13	/* DECnet routing daemon */
+#define RTPROT_XORP	14	/* XORP */
+#define RTPROT_NTK	15	/* Netsukuku */
+#define RTPROT_DHCP	16      /* DHCP client */
+
+/* rtm_scope
+
+   Really it is not scope, but sort of distance to the destination.
+   NOWHERE are reserved for not existing destinations, HOST is our
+   local addresses, LINK are destinations, located on directly attached
+   link and UNIVERSE is everywhere in the Universe.
+
+   Intermediate values are also possible f.e. interior routes
+   could be assigned a value between UNIVERSE and LINK.
+*/
+
+enum rt_scope_t {
+	RT_SCOPE_UNIVERSE=0,
+/* User defined values  */
+	RT_SCOPE_SITE=200,
+	RT_SCOPE_LINK=253,
+	RT_SCOPE_HOST=254,
+	RT_SCOPE_NOWHERE=255
+};
+
+/* rtm_flags */
+
+#define RTM_F_NOTIFY		0x100	/* Notify user of route change	*/
+#define RTM_F_CLONED		0x200	/* This route is cloned		*/
+#define RTM_F_EQUALIZE		0x400	/* Multipath equalizer: NI	*/
+#define RTM_F_PREFIX		0x800	/* Prefix addresses		*/
+
+/* Reserved table identifiers */
+
+enum rt_class_t {
+	RT_TABLE_UNSPEC=0,
+/* User defined values */
+	RT_TABLE_COMPAT=252,
+	RT_TABLE_DEFAULT=253,
+	RT_TABLE_MAIN=254,
+	RT_TABLE_LOCAL=255,
+	RT_TABLE_MAX=0xFFFFFFFF
+};
+
+
+/* Routing message attributes */
+
+enum rtattr_type_t {
+	RTA_UNSPEC,
+	RTA_DST,
+	RTA_SRC,
+	RTA_IIF,
+	RTA_OIF,
+	RTA_GATEWAY,
+	RTA_PRIORITY,
+	RTA_PREFSRC,
+	RTA_METRICS,
+	RTA_MULTIPATH,
+	RTA_PROTOINFO, /* no longer used */
+	RTA_FLOW,
+	RTA_CACHEINFO,
+	RTA_SESSION, /* no longer used */
+	RTA_MP_ALGO, /* no longer used */
+	RTA_TABLE,
+	RTA_MARK,
+	__RTA_MAX
+};
+
+#define RTA_MAX (__RTA_MAX - 1)
+
+#define RTM_RTA(r)  ((struct rtattr*)(((char*)(r)) + NLMSG_ALIGN(sizeof(struct rtmsg))))
+#define RTM_PAYLOAD(n) NLMSG_PAYLOAD(n,sizeof(struct rtmsg))
+
+/* RTM_MULTIPATH --- array of struct rtnexthop.
+ *
+ * "struct rtnexthop" describes all necessary nexthop information,
+ * i.e. parameters of path to a destination via this nexthop.
+ *
+ * At the moment it is impossible to set different prefsrc, mtu, window
+ * and rtt for different paths from multipath.
+ */
+
+struct rtnexthop {
+	unsigned short		rtnh_len;
+	unsigned char		rtnh_flags;
+	unsigned char		rtnh_hops;
+	int			rtnh_ifindex;
+};
+
+/* rtnh_flags */
+
+#define RTNH_F_DEAD		1	/* Nexthop is dead (used by multipath)	*/
+#define RTNH_F_PERVASIVE	2	/* Do recursive gateway lookup	*/
+#define RTNH_F_ONLINK		4	/* Gateway is forced on link	*/
+
+/* Macros to handle hexthops */
+
+#define RTNH_ALIGNTO	4
+#define RTNH_ALIGN(len) ( ((len)+RTNH_ALIGNTO-1) & ~(RTNH_ALIGNTO-1) )
+#define RTNH_OK(rtnh,len) ((rtnh)->rtnh_len >= sizeof(struct rtnexthop) && \
+			   ((int)(rtnh)->rtnh_len) <= (len))
+#define RTNH_NEXT(rtnh)	((struct rtnexthop*)(((char*)(rtnh)) + RTNH_ALIGN((rtnh)->rtnh_len)))
+#define RTNH_LENGTH(len) (RTNH_ALIGN(sizeof(struct rtnexthop)) + (len))
+#define RTNH_SPACE(len)	RTNH_ALIGN(RTNH_LENGTH(len))
+#define RTNH_DATA(rtnh)   ((struct rtattr*)(((char*)(rtnh)) + RTNH_LENGTH(0)))
+
+/* RTM_CACHEINFO */
+
+struct rta_cacheinfo {
+	__u32	rta_clntref;
+	__u32	rta_lastuse;
+	__s32	rta_expires;
+	__u32	rta_error;
+	__u32	rta_used;
+
+#define RTNETLINK_HAVE_PEERINFO 1
+	__u32	rta_id;
+	__u32	rta_ts;
+	__u32	rta_tsage;
+};
+
+/* RTM_METRICS --- array of struct rtattr with types of RTAX_* */
+
+enum {
+	RTAX_UNSPEC,
+#define RTAX_UNSPEC RTAX_UNSPEC
+	RTAX_LOCK,
+#define RTAX_LOCK RTAX_LOCK
+	RTAX_MTU,
+#define RTAX_MTU RTAX_MTU
+	RTAX_WINDOW,
+#define RTAX_WINDOW RTAX_WINDOW
+	RTAX_RTT,
+#define RTAX_RTT RTAX_RTT
+	RTAX_RTTVAR,
+#define RTAX_RTTVAR RTAX_RTTVAR
+	RTAX_SSTHRESH,
+#define RTAX_SSTHRESH RTAX_SSTHRESH
+	RTAX_CWND,
+#define RTAX_CWND RTAX_CWND
+	RTAX_ADVMSS,
+#define RTAX_ADVMSS RTAX_ADVMSS
+	RTAX_REORDERING,
+#define RTAX_REORDERING RTAX_REORDERING
+	RTAX_HOPLIMIT,
+#define RTAX_HOPLIMIT RTAX_HOPLIMIT
+	RTAX_INITCWND,
+#define RTAX_INITCWND RTAX_INITCWND
+	RTAX_FEATURES,
+#define RTAX_FEATURES RTAX_FEATURES
+	RTAX_RTO_MIN,
+#define RTAX_RTO_MIN RTAX_RTO_MIN
+	RTAX_INITRWND,
+#define RTAX_INITRWND RTAX_INITRWND
+	__RTAX_MAX
+};
+
+#define RTAX_MAX (__RTAX_MAX - 1)
+
+#define RTAX_FEATURE_ECN	0x00000001
+#define RTAX_FEATURE_SACK	0x00000002
+#define RTAX_FEATURE_TIMESTAMP	0x00000004
+#define RTAX_FEATURE_ALLFRAG	0x00000008
+
+struct rta_session {
+	__u8	proto;
+	__u8	pad1;
+	__u16	pad2;
+
+	union {
+		struct {
+			__u16	sport;
+			__u16	dport;
+		} ports;
+
+		struct {
+			__u8	type;
+			__u8	code;
+			__u16	ident;
+		} icmpt;
+
+		__u32		spi;
+	} u;
+};
+
+/****
+ *		General form of address family dependent message.
+ ****/
+
+struct rtgenmsg {
+	unsigned char		rtgen_family;
+};
+
+/*****************************************************************
+ *		Link layer specific messages.
+ ****/
+
+/* struct ifinfomsg
+ * passes link level specific information, not dependent
+ * on network protocol.
+ */
+
+struct ifinfomsg {
+	unsigned char	ifi_family;
+	unsigned char	__ifi_pad;
+	unsigned short	ifi_type;		/* ARPHRD_* */
+	int		ifi_index;		/* Link index	*/
+	unsigned	ifi_flags;		/* IFF_* flags	*/
+	unsigned	ifi_change;		/* IFF_* change mask */
+};
+
+/********************************************************************
+ *		prefix information 
+ ****/
+
+struct prefixmsg {
+	unsigned char	prefix_family;
+	unsigned char	prefix_pad1;
+	unsigned short	prefix_pad2;
+	int		prefix_ifindex;
+	unsigned char	prefix_type;
+	unsigned char	prefix_len;
+	unsigned char	prefix_flags;
+	unsigned char	prefix_pad3;
+};
+
+enum 
+{
+	PREFIX_UNSPEC,
+	PREFIX_ADDRESS,
+	PREFIX_CACHEINFO,
+	__PREFIX_MAX
+};
+
+#define PREFIX_MAX	(__PREFIX_MAX - 1)
+
+struct prefix_cacheinfo {
+	__u32	preferred_time;
+	__u32	valid_time;
+};
+
+
+/*****************************************************************
+ *		Traffic control messages.
+ ****/
+
+struct tcmsg {
+	unsigned char	tcm_family;
+	unsigned char	tcm__pad1;
+	unsigned short	tcm__pad2;
+	int		tcm_ifindex;
+	__u32		tcm_handle;
+	__u32		tcm_parent;
+	__u32		tcm_info;
+};
+
+enum {
+	TCA_UNSPEC,
+	TCA_KIND,
+	TCA_OPTIONS,
+	TCA_STATS,
+	TCA_XSTATS,
+	TCA_RATE,
+	TCA_FCNT,
+	TCA_STATS2,
+	TCA_STAB,
+	__TCA_MAX
+};
+
+#define TCA_MAX (__TCA_MAX - 1)
+
+#define TCA_RTA(r)  ((struct rtattr*)(((char*)(r)) + NLMSG_ALIGN(sizeof(struct tcmsg))))
+#define TCA_PAYLOAD(n) NLMSG_PAYLOAD(n,sizeof(struct tcmsg))
+
+/********************************************************************
+ *		Neighbor Discovery userland options
+ ****/
+
+struct nduseroptmsg {
+	unsigned char	nduseropt_family;
+	unsigned char	nduseropt_pad1;
+	unsigned short	nduseropt_opts_len;	/* Total length of options */
+	int		nduseropt_ifindex;
+	__u8		nduseropt_icmp_type;
+	__u8		nduseropt_icmp_code;
+	unsigned short	nduseropt_pad2;
+	unsigned int	nduseropt_pad3;
+	/* Followed by one or more ND options */
+};
+
+enum {
+	NDUSEROPT_UNSPEC,
+	NDUSEROPT_SRCADDR,
+	__NDUSEROPT_MAX
+};
+
+#define NDUSEROPT_MAX	(__NDUSEROPT_MAX - 1)
+
+/* RTnetlink multicast groups - backwards compatibility for userspace */
+#define RTMGRP_LINK		1
+#define RTMGRP_NOTIFY		2
+#define RTMGRP_NEIGH		4
+#define RTMGRP_TC		8
+
+#define RTMGRP_IPV4_IFADDR	0x10
+#define RTMGRP_IPV4_MROUTE	0x20
+#define RTMGRP_IPV4_ROUTE	0x40
+#define RTMGRP_IPV4_RULE	0x80
+
+#define RTMGRP_IPV6_IFADDR	0x100
+#define RTMGRP_IPV6_MROUTE	0x200
+#define RTMGRP_IPV6_ROUTE	0x400
+#define RTMGRP_IPV6_IFINFO	0x800
+
+#define RTMGRP_DECnet_IFADDR    0x1000
+#define RTMGRP_DECnet_ROUTE     0x4000
+
+#define RTMGRP_IPV6_PREFIX	0x20000
+
+/* RTnetlink multicast groups */
+enum rtnetlink_groups {
+	RTNLGRP_NONE,
+#define RTNLGRP_NONE		RTNLGRP_NONE
+	RTNLGRP_LINK,
+#define RTNLGRP_LINK		RTNLGRP_LINK
+	RTNLGRP_NOTIFY,
+#define RTNLGRP_NOTIFY		RTNLGRP_NOTIFY
+	RTNLGRP_NEIGH,
+#define RTNLGRP_NEIGH		RTNLGRP_NEIGH
+	RTNLGRP_TC,
+#define RTNLGRP_TC		RTNLGRP_TC
+	RTNLGRP_IPV4_IFADDR,
+#define RTNLGRP_IPV4_IFADDR	RTNLGRP_IPV4_IFADDR
+	RTNLGRP_IPV4_MROUTE,
+#define	RTNLGRP_IPV4_MROUTE	RTNLGRP_IPV4_MROUTE
+	RTNLGRP_IPV4_ROUTE,
+#define RTNLGRP_IPV4_ROUTE	RTNLGRP_IPV4_ROUTE
+	RTNLGRP_IPV4_RULE,
+#define RTNLGRP_IPV4_RULE	RTNLGRP_IPV4_RULE
+	RTNLGRP_IPV6_IFADDR,
+#define RTNLGRP_IPV6_IFADDR	RTNLGRP_IPV6_IFADDR
+	RTNLGRP_IPV6_MROUTE,
+#define RTNLGRP_IPV6_MROUTE	RTNLGRP_IPV6_MROUTE
+	RTNLGRP_IPV6_ROUTE,
+#define RTNLGRP_IPV6_ROUTE	RTNLGRP_IPV6_ROUTE
+	RTNLGRP_IPV6_IFINFO,
+#define RTNLGRP_IPV6_IFINFO	RTNLGRP_IPV6_IFINFO
+	RTNLGRP_DECnet_IFADDR,
+#define RTNLGRP_DECnet_IFADDR	RTNLGRP_DECnet_IFADDR
+	RTNLGRP_NOP2,
+	RTNLGRP_DECnet_ROUTE,
+#define RTNLGRP_DECnet_ROUTE	RTNLGRP_DECnet_ROUTE
+	RTNLGRP_DECnet_RULE,
+#define RTNLGRP_DECnet_RULE	RTNLGRP_DECnet_RULE
+	RTNLGRP_NOP4,
+	RTNLGRP_IPV6_PREFIX,
+#define RTNLGRP_IPV6_PREFIX	RTNLGRP_IPV6_PREFIX
+	RTNLGRP_IPV6_RULE,
+#define RTNLGRP_IPV6_RULE	RTNLGRP_IPV6_RULE
+	RTNLGRP_ND_USEROPT,
+#define RTNLGRP_ND_USEROPT	RTNLGRP_ND_USEROPT
+	RTNLGRP_PHONET_IFADDR,
+#define RTNLGRP_PHONET_IFADDR	RTNLGRP_PHONET_IFADDR
+	RTNLGRP_PHONET_ROUTE,
+#define RTNLGRP_PHONET_ROUTE	RTNLGRP_PHONET_ROUTE
+	RTNLGRP_DCB,
+#define RTNLGRP_DCB		RTNLGRP_DCB
+	__RTNLGRP_MAX
+};
+#define RTNLGRP_MAX	(__RTNLGRP_MAX - 1)
+
+/* TC action piece */
+struct tcamsg {
+	unsigned char	tca_family;
+	unsigned char	tca__pad1;
+	unsigned short	tca__pad2;
+};
+#define TA_RTA(r)  ((struct rtattr*)(((char*)(r)) + NLMSG_ALIGN(sizeof(struct tcamsg))))
+#define TA_PAYLOAD(n) NLMSG_PAYLOAD(n,sizeof(struct tcamsg))
+#define TCA_ACT_TAB 1 /* attr type must be >=1 */	
+#define TCAA_MAX 1
+
+/* New extended info filters for IFLA_EXT_MASK */
+#define RTEXT_FILTER_VF		(1 << 0)
+
+/* End of information exported to user level */
+
+
+
+#endif	/* __LINUX_RTNETLINK_H */
-- 
2.8.3

