Nap protocol specification
==========================

By cyberalien@users.sourceforge.net
14 Dec 2001

Original by drscholl@users.sourceforge.net
April 7, 2001

0.  Foreward by Dr. Scholl

This is meant to be an open specification.  If you find errors or know of
additional functionality not described hereafter, please send me email.
It benefits the entire community to have a complete and accurate protocol
specification. Not only does it allow for clients to be developed for any
platform, but also decreases the strain on the server having to parse out
bad client messages.

0.1  Foreward by CyberAlien

Original document is created by Dr.Scholl. I have fixed some messages,
added OpenNap and SlavaNap messages and extentions to messages, added
Napigator protocol specification.
If you have any comments please mail me at mailto:cyberalien@users.sourceforge.net

1.  Recent Changes

* Fixed napigator protocol (12 October 2001)
* Fixed commands 100, 110 (12 October 2001)
* Updated to match opennap 0.44 and slavanap 2.0.0 capabilities (14 Dec 2001)

2.  Client-Server protocol

Nap protocol uses TCP for client to server communication.  Typically the
servers run on ports 8888 and 7777.  Note that this is different from the
`metaserver' (or redirector) which runs on port 8875.
Note: Napster 10.3 and older use port 8876 instead of 8875.

each message to/from the server is in the form of
	<length><type><data>
where <length> and <type> are 2 bytes each.  <length> specifies the length in
bytes of the <data> portion of the message.  Be aware that <length> and <type>
appear to be in little-endian format (least significant byte goes first).  For
example, in the C language you would encode the number 1 as
	const unsigned char num[2] = { 0x01, 0x00 };
and 256 would be encoded as
	const unsigned char num[2] = { 0x00, 0x01 };
[The above is for illustrative purposes only, there are much quicker ways to
actually encode a number. -ed]
The <data> portion of the message is a plain ASCII string.

Napster Beta 10.3+ use big-endian format instead of little-endian.
This means that 256 would be encoded as { 0x01, 0x00 }
and 1 as { 0x00, 0x01 };

Note that in many cases, strings are passed as double-quoted entries.  For
example, filenames and client id strings are always sent as
	"random band - generic cowboy song.mp3"
or
	"nap v0.8"
Where required, double quotes are used in the description of the messages
below.

Some additional information about use of quotes inside of quotes:
> The answer is, no, it doesn't do escaping of quotes.  If you try searching
> for the phrase 'a "quoted" string' on the windows client, you get no songs
> found, and "invalid search request" printed in yellow in your console
> window.  (don't know what code that is, sorry.)
>
> and no wonder-- a little birdie told me that the client sends this:
>
> FILENAME CONTAINS "a "quoted" string" MAX_RESULTS 100

[contributed by Ben Byer <bbyer@rice.edu>.  -ed]

Note that unlike the IRC protocol, each line does NOT end in \r\n.  The
<length> field specifies exactly how much data you should read.

3.  Message Types

The following section describes the format of the <data> section for each
specific message type.  Each field is denoted with <>.  The fields in a
message are separated by a single space character (ASCII 32).  Where
appropriate, examples of the <data> section for each message are given.

[SERVER] means that message is sent by server
[CLIENT] means that message is send by client
[NAPSTER] means that Napster client or server uses this message
[OPENNAP] means that this message is supported by OpenNap 0.44
[SLAVANAP] means that this message is supported by SlavaNap 2.0.0

Detecting server type is easy. When user logs in server sends MOTD
and OpenNap and SlavaNap sends string "VERSION opennap 0.44" or
"VERSION SlavaNap 2.0.0" among other MOTD strings.

<type> can be one of the following (converted to big-endian):

0	error message [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <message>

2	login [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <nick> <password> <port> "<client-info>" <link-type> [ <num> ]

	<port> is the port the client is listening on for data transfer.  if
		this value is 0, it means that the client is behind a firewall
		and can only push files outward.  it is expected that requests
		for downloads be made using the 500 message (see below)
	<client-info> is a string containing the client version info
	<link-type> is an integer indicating the client's bandwidth
		0  unknown
		1  14.4 kbps
		2  28.8 kpbs
		3  33.6 kbps
		4  56.7 kbps
		5  64K ISDN
		6  128K ISDN
		7  Cable
		8  DSL
		9  T1
		10 T3 or greater
	<num> build number for the windows client [optional]
		
	Example:

	foo badpass 6699 "nap v0.8" 3

3	login ack [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <email> [<number>]

	the server sends this message to the client after a succesful
	login (2).  If the nick is registered, the <email> address given at
	registration time is returned.  If the nick is not registered, a
	dummy value is returned.

	<number> is added by Napster server.
		This is probably user's number.

4	version check [CLIENT] [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

        Format: <version>

	Server sends [5] if an update is needed and [4] if not.

	<version> = string, version 2.0b5a sends "2.0"

5       "auto-upgrade" [SERVER]

	[NAPSTER]

        Format: <version>
        Beta5 Format: <version> <hostname:filename>

        Napster is out of date, get a new version.
        Used to be gaping security hole in Beta5.

        <version>  = string, the new version number.
        <hostname> = string, hostname of upgrade (http) server
        <filename> = string, filename

	<hostname> and <filename> are used only by Beta5
	Later versions ignore these values.

6	new user login [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <nick> <pass> <port> "<client-info>" <speed> <email-address>

	This message is used when logging in for the first time to register
	a new nickname.  The client normally checks for an unused nick using
	the "check nickname" (7) message and upon receipt of a "nickname not
	registered" (8) from the server will proceceed to log in with this
	command.

	note: this message is similar to the 0x02 message, with the addition	
	of <email-address> on the end

	Example:

	foo foo 6699 "nap v0.8" 3 email@here.com

7	nick check [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <nick>

	Queries the server to see if <nick> is already registered.  This
	message is typically used prior to logging in for the first time to
	check for a valid nickname.

	Response to this message is one of 8, 9 or 10

8	nickname not registered [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: (empty)

	The server sends this message in response to the "nick check" (7)
	message to indicate that the specified nickname is not already
	registered and is ok to use.

9	nickname already registered [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: (empty)

	The server sends this message when the nickname the client has
	requested has already been registered by another user

10 (0x0a)	invalid nickname [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: (empty)

	This server sends this message in response to the "check nickname"
	(7) messages when the specified nickname is invalid, usually due to
	bad characters such as spaces or other non-printable characters.

        The Napster, Inc. servers only accept (upper- and lower-case) nicks
        comprised of the following:
               abcdefghijklmnopqrstuvwxyz1234567890_[]{}-@^!$

11	password check [CLIENT]

	[NAPSTER,SLAVANAP]

	Format: <nick> <pass>

	This command is used by Napster only during setup sequence.
	If password is correct server replies with message 12. If not
	server sends message 0.

12	password OK [SERVER]

	[NAPSTER,SLAVANAP]

	Format: (empty)

	this message is returned in response to message 11 from the client

13	echo??? [SERVER]

	[NAPSTER]

	Format: <numeric>: [args]

	Prior to issuing a login (2) command, the server will echo back the
	received numeric and any arguments of any commands it receives.

14	login options [CLIENT]

	[NAPSTER]

	NAME:%s ADDRESS:%s CITY:%s STATE:%s PHONE:%s AGE:%s INCOME:%s EDUCATION:%s

	Example:

	NAME: kev  ADDRESS:  CITY: ephrata  STATE: pa  PHONE:  AGE: 60 or older INCOME: $100,000 or more        EDUCATION: Graduate Degree

	No reply is required.

15	Same as 14. Used by Beta7+ (I don't know if previous versions used command 15 or not)

	[NAPSTER]

100 (0x64)	client notification of shared file [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: "<filename>" <md5> <size> <bitrate> <frequency> <time>

	<md5> see section "MD5"
	<size> is bytes
	<bitrate> is kbps
	<frequency> is hz
	<time> is seconds
	
	Example:

	"generic band - generic song.mp3" b92870e0d41bc8e698cf2f0a1ddfeac7-443008 443332 128 44100 60

	For sharing non-mp3 files there is a command 10300 that is supported
	by OpenNap and SlavaNap, but most clients use command 100 (or 870)
	and just set bitrate=24 freq=16000 time=600.

102 (0x66)	remove file [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <filename>

	client requests to remove file from shared library

110		unshare all files [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: (empty)
	server: <num>

	Notifies the server that the client is no longer sharing any of the
	files previously shared. Server replies with 110 containing number
	of files that client shared before.

200 (0xc8)	client search request [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format:

	[FILENAME CONTAINS "artist name"] MAX_RESULTS <max> [FILENAME CONTAINS
	"song"] [LINESPEED <compare> <link-type>] [BITRATE <compare> "<br>"] [FREQ
	<compare> "<freq>"] [WMA-FILE] [LOCAL_ONLY]

	For OpenNap and SlavaNap only:

	[TYPE <mime-type>] [FILENAME EXCLUDES "exclude string"] [SIZE <compare>
	<filesize_in_bytes>] [DURATION <compare> <song_duration_in_seconds>]

	For SlavaNap 2.x only:

	[SHOW_QUEUE] [SHOW_SOFTWARE]	



        The artist name and the song name are strings filename should include.
	There is no difference between artist name and song name.

        <max> is a number; if it is greater than 100, Napster server will only return
	100 results. With OpenNap and SlavaNap <max> can be greater than 100.

        <compare> is one of the following:
                "AT LEAST" "AT BEST" "EQUAL TO"

        <link-type> integer ranging from 1 to 10. see 0x02 (client login) for a description.

        <br> is a number, in kbps

        <freq> is a sample frequency, in Hz

	<mime-type> OpenNap and SlavaNap support other media types besides mp3.
		By default, searches will only match mp3 files.  A client can
		however search for other media types by specifying a partial
		MIME content-type (audio, video, text, application, image, mp3).
		(See message 10300 for adding media to the database).
		The special keyword `any' will match any media type in the
		database.

		The results of the search are returned as with mp3, except
		the fields for bitrate, sample frequency and length are
		meaningless. The client can then download as they would any
		other mp3 file.

	FILENAME EXCLUDES "..."

		allows filtering search results by excluded all files which
		match words in an exclude list.  this must be used in
		conjunction with FILENAME CONTAINS "...".
		(NOTE: as of Napster 2.0 BETA 8, words in the
		FILENAME CONTAINS string which are prefixed with a minus
		sign (-) are considered to be exclusive.)
		Can be used only with OpenNap and SlavaNap servers.

	SIZE, DURATION

		allows matching on the file size and song length in addition
		to the other file attributes. Can be used only with OpenNap
		and SlavaNap servers.

	LOCAL_ONLY causes the server to only search for files from users on
		the same server rather than all linked servers.

	SHOW_QUEUE this works only with SlavaNap 2.x servers. if causes server
		to add number of queued items for remote user to each search result.
		if remote user's software doesn't show queue server will add "n/a"
		instead of queue. otherwise server will return number counted
		with the following simple algorythm:
		 current_uploads + queued_uploads - max_uploads;
		so, if you can download from remote user without entering queue
		server will return any negative number, if user has maximum
		uploads right now server will return number of queued items.
		To set number of queued items use SlavaNap's command 8112. You
		can also retreive number of queued items using SlavaNap's command
		8113 instead of adding "SHOW_QUEUE" to search request.
		See also "readme.txt" in SlavaNap.

	SHOW_SOFTWARE this works only with SlavaNap 2.x servers. if causes server
		to add client's software signature to search result. This might
		be used if your client has its own special protocol and you
		don't want to disturb other clients with messages that other
		client wouldn't understand.
		If you use both "SHOW_QUEUE" and "SHOW_SOFTWARE" in search
		request, server will add queue first and software second to
		search result.
		See also "readme.txt" in SlavaNap.
		

        The windows client filters by ping time inside the client.
                It pretty much has to, and it's easy to see the
                result by setting ping time to at best 100 ms or
                so, and max search terms to 50.  You'll get back
                like 3 results, but the client will still tell you
                that it found "50 results".

        Examples:
                FILENAME CONTAINS "Sneaker Pimps" MAX_RESULTS 75 FILENAME
                         CONTAINS "tesko suicide" BITRATE "AT LEAST" "128"

                MAX_RESULTS 100 FILENAME CONTAINS "Ventolin" LINESPEED
                        "EQUAL TO" 10

	[Thanks to Ben Byer <bbyer@rice.edu> for this contribution.  -ed]


	SEE ALSO: 10300 share non-mp3 file.

201 (0xc9)	search response [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	"<filename>" <md5> <size> <bitrate> <frequency> <length> <nick> <ip>
	<link-type> [ [weight] | [queue] "[software]" ]

	<md5> see secton "MD5"
	<size> is file size in bytes
	<bitrate> is mp3 bit rate in kbps
	<frequency> is sample rate in hz
	<length> is the play length of the mp3 in seconds
	<nick> the person sharing the file
	<ip> is an unsigned long integer representing the ip address of the
		user with this file
	<link-type> see message client login (2) message for a description
	[weight]	a weighting factor to allow the client to sort the
	                list of results.  positive values indicate a "better"
			match, negative values indicate a "worse" match.
			If not present, the weight should be considered to be
			0.
	[queue]		for SlavaNap 2.x only. queued items number for remote
			user. server will return it if you have added
			"SHOW_QUEUE" to search request. parameter [weight]
			is not returned by slavanap server.
			
	[software]	for SlavaNap 2.x only. this parameter shows software
			that is used by remote client. parameter [weight]
			is not returned by slavanap server.

	Example:

	"random band - random song.mp3" 7d733c1e7419674744768db71bff8bcd-2557521 2558199 128 44100 159 lefty 3437166285 4

	SlavaNap examples:

	request: FILENAME CONTAINS "sunshine"
	possible reply: "c:\MP3\Emma Bunton - Sunshine On A Rainy Day.mp3" 00000000000000000000000000000000 4118494 128 44100 257 CyberAlien 3437166285 6

	request: FILENAME CONTAINS "sunshine" SHOW_QUEUE
	possible reply: "c:\MP3\Emma Bunton - Sunshine On A Rainy Day.mp3" 00000000000000000000000000000000 4118494 128 44100 257 CyberAlien 3437166285 6 n/a
	possible reply: "c:\MP3\Emma Bunton - Sunshine On A Rainy Day.mp3" 00000000000000000000000000000000 4118494 128 44100 257 CyberAlien 3437166285 6 2
	possible reply: "c:\MP3\Emma Bunton - Sunshine On A Rainy Day.mp3" 00000000000000000000000000000000 4118494 128 44100 257 CyberAlien 3437166285 6 -1

	request: FILENAME CONTAINS "sunshine" SHOW_SOFTWARE
	possible reply: "c:\MP3\Emma Bunton - Sunshine On A Rainy Day.mp3" 00000000000000000000000000000000 4118494 128 44100 257 CyberAlien 3437166285 6 "v2.0 BETA 10.4"
	possible reply: "c:\MP3\Emma Bunton - Sunshine On A Rainy Day.mp3" 00000000000000000000000000000000 4118494 128 44100 257 CyberAlien 3437166285 6 CQ_EX

	request: FILENAME CONTAINS "sunshine" SHOW_SOFTWARE SHOW_QUEUE
	possible reply: "c:\MP3\Emma Bunton - Sunshine On A Rainy Day.mp3" 00000000000000000000000000000000 4118494 128 44100 257 CyberAlien 3437166285 6 n/a "v2.0 BETA 10.4"
	possible reply: "c:\MP3\Emma Bunton - Sunshine On A Rainy Day.mp3" 00000000000000000000000000000000 4118494 128 44100 257 CyberAlien 3437166285 6 0 CQ_EX

202 (0xca)	end of search response from server [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: (empty)

203 (0xcb)	download request [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <nick> "<filename>"

	client requests to download <filename> from <nick>.  client expects
	to make an outgoing connection to <nick> on their specified data
	port.

	Example:

	mred "C:\Program Files\Napster\generic cowboy song.mp3"

	SEE ALSO: 500 alternate download request

204 (0xcc)	download ack [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> <ip> <port> "<filename>" <md5> <linespeed>

	server sends this message in response to a 203 request.

	<nick> is the user who has the file
	<ip> is an unsigned long integer representing the ip address
	<port> is the port <nick> is listening on
	<filename> is the file to retrieve
	<md5> is the md5 sum
	<linespeed> is the user's connection speed (see login(2))

	Example:

	lefty 4877911892 6699 "generic band - generic song.mp3" 10fe9e623b1962da85eea61df7ac1f69 3

205 (0xcd)	private message to/from another user [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> <message>

	note the same type is used for a client sending a msg or recieving one

206 (0xce)	get error [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> "<filename>"

	the server sends this message when the file that the user has
	requested to download is unavailable (such as the user is not logged
	in).

207 (0xcf)	add hotlist entry [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <user>

	This message is used to add additional entries to the client's
	hotlist.  The server will send 209 and 210 messages when a user
	on the hotlist has logged in or out, respectively.

208 (0xd0)	hotlist [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <user>

	This message is used to send the initial list of hotlist entries
	during the initial login process.  It is normally send prior to
	to the add file (100) commands.  To add more entries to the hotlist
	after the initial list is sent, clients should use the 207 message
	instead.

209 (0xd1)	user signon [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user> <speed>

	server is notifying client that a user in their hotlist, <user>,
	has signed on the server with link <speed>

210 (0xd2)	user signoff [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user>

	server is notifying client that a user on their hotlist, <user>, has
	signed off the server.

	this message is also sent by the server when the client attempts to
	browse a nonexistent client.

211 (0xd3)	browse a user's files [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick>

	the client sends this message when it wants to get a list of the files
	shared by a specific client

212 (0xd4)	browse response [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> "<filename>" <md5> <size> <bitrate> <frequency> <time>

	<nick> is the user contributing the file
	<filename> is the mp3 file contributed
	<md5> is the has of the mp3 file
	<size> is the file size in bytes
	<bitrate> is the mp3 bitrate in kbps
	<frequence> is the sampling frequency in Hz
	<time> is the play time in seconds

	Example:

	foouser "generic band - generic song.mp3" b92870e0d41bc8e698cf2f0a1ddfeac7 443332 128 44100 60

213 (0xd5)	end of browse list [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> [ip]

	indicates no more entries in the browse list for <user>.  <ip> gives
	the client's IP address.

214 (0xd6)	server stats [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: no data
	server: <users> <# files> <size> ["GB" <myfiles>]

	<size> is approximate total library size in gigabytes
	this message is sent by the server occasionaly without request
	"GB" text is added by Napster server since version 10.3
	<myfiles> is number of files shared by user.

	Example:

	old:  553 64692 254
	new:  553 64692 254 GB 102

215 (0xd7)	request resume [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<checksum> <filesize>

	client is requesting a list of all users which have the file with
	the characteristics.  the server responds with a list of 216 messages
	for each match, followed by a 217 message to terminate the list

216 (0xd8)	resume search response [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user> <ip> <port> <filename> <checksum> <size> <speed>

	this message contains the matches for the resume request (215).  the
	list is terminated by a 217 message.

217 (0xd9)	end of resume search list [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	no data.

	this messag terminates a list of 216 messages initiated by a 215
	client request

218 (0xda)	downloading file [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	no body.

	client sends this message to the server to indicate they are in the
	process of downloading a file.  this adds 1 to the download count
	which the server maintains.

219 (0xdb)	download complete [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	no body.

	client sends this message to the server to indicate they have
	completed the file for which a prior 218 message was sent.  this
	subtracts one from the download count the server maintains

220 (0xdc)	uploading file [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	no body.

	client sends this message to indicate they are uploading a file.
	this adds one to the upload count maintained by the server.

221 (0xdd)	upload complete [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	no body.

	client sends this message when they are finished uploading a file.
	this subtracts one from the upload count maintained by the server.

300 (0x12c)	optional ports [CLIENT]

	[NAPSTER]

	<port>

	This command allows the client to specify optional ports to try for
	data connections if the one currently in use is unreachable by other
	parties. Ignored by OpenNap and SlavaNap.

301 (0x12d)	hotlist ack [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <user>

	server is notifying client that <user> has successfully be added to
	their hotlist

302 (0x12e)	hotlist error [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <user>

	server is notifying client that it was unable to add <user> to their
	hotlist.  [can you only add registered nicks to your hotlist? -ed]

303 (0x12f)	remove user from hotlist [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <user>

	client is notifying the server that it no longer wishes to request
	notifications about <user> when they sign on or off the server.  no
	response is sent in return.

310	??? [CLIENT, SERVER]

	[NAPSTER]

	client: no data
	server: 0

	unknown command.  server returns 0 regardless of any parameters

316	client disconnect??? [CLIENT, SERVER]

	[NAPSTER,OPENNAP]

	client: no data
	server: 0

	The server sends this message with a value of `0' when the client is
	about to be disconnected.

	It is unkonwn what this command does when issued by the client.  The
	server appears to send the 316 message without disconnected the client
	in this case.

	[the server seems to send this message if you send it a numeric
	greater than 1000.  the server will also disconnect you after
	sending this message.  -ed]

320 (0x140)	user ignore list [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: no data
	server: <count>

	client request to display the list of ignored users.
	server returns the number of users being ignored

321 (0x141)	user ignore list entry [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user>

	server sends each ignored nick in response to a 320 request.  the
	list is terminated by a 320 message with the number of ignored users.

322 (0x142)	add user to ignore list [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user>

	server acks the request by returning the nick

323 (0x143)	remove user from ignore list [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user>

	server acks the request by returning the nick to be removed from
	the ignore list.

324 (0x144)	user is not ignored [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user>

	server indicates that <user> is not currently ignored in response to
	a 323 request.

325 (0x145)	user is already ignored [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user>

	server indicates the specified user is already on the user's ignore
	list

326 (0x146)	clear ignore list [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: no data.
	server: <count>

	client requests the server clear its ignore list.  server returns the
	number of entries removed from the ignore list.

330 (0x14a)	blocked ip list [CLIENT]
	[NAPSTER]

332 (0x14c)	block ip [CLIENT]
	[NAPSTER]

333 (0x14d)	unblock ip [CLIENT]
	[NAPSTER]

400 (0x190)	join channel [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel-name>

	the client sends this command to join a channel

401 (0x191)	part channel [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel-name>

	The client sends this command to part a channel.  Server sends this
	message to indicate that the client has parted the channel.  Note
	that this is sometimes sent even when the client has not requested,
	so a client _must_ be prepared to accept it at any time.

402 (0x192)	send public message [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <message>

403 (0x193)	public message [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <nick> <text>

	this message is sent by the server when a client sends a public message
	to a channel.

	Example:

	80's espinozaf hello...hola

404 (0x194)	error message [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<text>

	This message is used to send general error messages to a client that
	is logged in.  Note: Message 0 is only sent during the login process.

	Examples:

	User nosuchuser is not currently online.
	Channel #nosuchchannel does not exist!
	permission denied
	ping failed, blah is not online

405 (0x195)	join acknowledge [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel>

	the server sends this message to the client to acknowlege that it
	has joined the requested channel (400)
	Note: <channel> in this message can be different from one sent in 400
	and client must be ready to join another channel instead of requested.
	
406 (0x196)	join message [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <user> <sharing> <link-type>

	<user> has joined <channel>

	Example:

	80's WilmaFlinstone 12 2

407 (0x197)	user parted channel [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <nick> <sharing> <linespeed>

	Example:

	80's DLongley 23 7

408 (0x198)	channel user list entry [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <user> <sharing> <link-type>

	this message is identical to the join (406) message.  the server will
	send the list of users in the channel prior to the client join command
	in this message.  joins that occur after the client has joined will
	be noted by a 406 message.

409 (0x199)	end of channel user list [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel>

	this message is sent by the server to indicate it has sent all information
	about the users in a channel

410 (0x19a)	channel topic [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <topic>

	sent when joining a channel or a new topic is set.  a client requesting
	topic change also uses this message.

	[why didn't they put a field to indicate WHO changed the topic?  as
	it is now you can only tell that it was changed.  -ed]

420 (0x1a4)	channel ban list [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <channel>

	This command is used by clients to request the list of channel bans,
	and by the server to indicate the end of the channel ban list for
	a channel (also see 421).

421 (0x1a5)	channel ban list entry [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

422 (0x1a6)	channel ban [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <user|ip> [ "<reason>" ]

423 (0x1a7)	channel unban [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <user|ip> [ "<reason>" ]

424 (0x1a8)	channel ban clear [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <channel>

425	channel motd (alternate topic (?)) [SERVER]

	[NAPSTER]

	Format: <message>

	[The server sends this command when a user joins one of the
	predefined channels.  It seems to send a default message if the
	topic for the channel is the default, otherwise it sends the current
	channel topic.  -ed]

430	invite a user [CLIENT, SERVER]                                                 

	[NAPSTER,SLAVANAP]

	Client: <nick> <channel>                                               
        Server: <nick> <channel> "<topic>" <unknown> <unknown>       
                                                                                
        This command is used by Napster 2.0 BETA 9.6+ to invite a user to
        a channel. The funniest thing about this command is that it is
	supported by Napster clients but not supported by Napster servers ;)
	Napster implementation of this command is a little bit buggy.

        client:                                                                 
                <nick> - nick of invited user                                   
                <channel> - channel user <nick> was invited to                  
        server:                                                                 
                <nick> - nick of user who was inviting                          
                <channel> - channel                                             
                <topic> - channel's topic                                       
                <unknown> - ??? ("0" works fine)                          
                                                                                
        When user receives 430 message user should reply with 431 or 432
	and, if invitation accepted, user should join channel with 400.
                                                                                
        Client example:                                                         
                                                                                
        CyberAlien2 #test_channel                                               
                                                                                
        Server  example:                                                        
                                                                                
        CyberAlien3 #test_channel "Welcome to the #test_channel." 0 0      
                                                                                
431	invitation accepted [CLIENT]                                                    

	[NAPSTER,SLAVANAP]

	Format: <user> <channel>                                                        
                                                                                
        <user> - user who was inviting                                          
                                                                                
432	invitation declined [CLIENT]

	[NAPSTER,SLAVANAP]

        Format: copy of command received in 430 message works fine.

500 (0x1f4)	alternate download request [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> "<filename>"

	requests that <nick> make an outgoing connection to the requesters
	client and send <filename>.  this message is for use when the
	person sharing the file can only make an outgoing tcp connection
	because of firewalls blocking incoming messages.  this message should
	be used to request files from users who have specified their data
	port as 0 in their login message

501 (0x1f5)	alternate download ack [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> <ip> <port> "<filename>" <md5> <speed>

	this message is sent to the uploader when their data port is set to
	0 to indicate they are behind a firewall and need to push all data
	outware.  the uploader is responsible for connecting to the
	downloader to transfer the file.

600 (0x258)	request user's link speed [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick>

601 (0x259)	link speed response [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> <linespeed>

602 (0x25a)	??? [CLIENT]

	[NAPSTER]

	<?>

	server returns a 404 with "*gulp* Drink milk, it does a body good!"

603 (0x25b)	whois request [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick>

604 (0x25c)	whois response [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> "<user-level>" <time> "<channels>" "<status>" <shared>
	<downloads> <uploads> <link-type> "<client-info>" [ <total downloads>
	<total_uploads> <ip> <connecting port> <data port> <email> [<server>]]

	<user-level> is one of "User", "Moderator", "Admin" or "Elite"
	<time> is seconds this user has been connected
	<channels> is the list of channels the client is a member of, each
		separated by a space (ASCII 32)
	<status> is one of "Active", "Inactive" (offline) or "Remote" (on a
		different server)
	<shared> is number of files user has available for download
	<downloads> is the current number of downloads in progress
	<uploads> is the current number of uploads in progress
	<link-type> see 0x02 (client login) above
	<client-info> see 0x02 (client login) above

	The following fields are displayed for user level moderator and
	above:

	<total uploads>
	<total downloads>
	<ip>			note: can be "unavailable"
	<connecting port>
	<data port>
	<email>			note: can be unavailable
	<server> used only by SlavaNap and opennap servers. It shows
		which server client is connected to.

	Example:

	lefty "User" 1203 "80's " "Active" 0 0 0 3 "nap v0.8"

605 (0x25d)	whowas response [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user> <level> <last-seen>

	if the user listed in a 603 request is not currently online, the
	server sends this message.

	<user> is the user for which information was requested
	<level> is the user's last known userlevel (user/mod/admin)
	<last-seen> is the last time at which this user was seen, measured
		as seconds since 12:00am on January 1, 1970 (UNIX time_t).

606 (0x25e)	change user level [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> <level>

	changes the privileges for <nick> to <level>.  client must be admin
	level to execute this request

	[I have not verified this message since I don't have admin status
	on any of Napster servers.  -ed]

607 (0x25f)	upload request [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> "<filename>" <speed>

	this message is used to notify the client that user <nick> has
	requested upload of <filename>

	Example:

	lefty "generic band - generic song.mp3" 7

608 (0x260)	accept upload request [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> "<filename>"

	client is notifying server that upload of <filename> to <nick> is
	accepted, and that the requesting client may begin download

	Example:

	lefty "generic band - generic song.mp3"

609 (0x261)     accept failed [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

        <nick> "<filename>"

	This message is sent by the server when the client that the file was
	requested from does not accept the upload request.

	This message also used by AudioGnome to notify other user that upload
	or download was canceled.

610 (0x262)	kill (disconnect) a user [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> [ "<reason>" ]

	client request to disconnect a user.

611 (0x263)	nuke a user [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick>

	client request to delete account for <nick>

612 (0x264)	ban user [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick | ip> [ "<reason>" ]

	client request to place a ban on either a specific nickname or
	an ip address

613 (0x265)	set data port for user [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: <user> <port>
	server: <port>

	This command is used by administrators to request that another
	client set the port used for data transfers to <port>.  The server
	sends a message with the requested port number to the target
	client.  NOTE: the target client can change its port number to
	whatever it wishes using the 703 command.

614 (0x266)	unban user [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <nick | ip> [ "<reason>" ]

615 (0x267)	show bans for server [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: (empty)

	client requests the list of banned ips for the current server

616 (0x268)	(ip?) ban list entry [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <ip> <nick> "<reason>" <time> <n>

	<ip> is the string version of the ip banned
	<nick> is the user setting the ban
	<reason> is the reason given
	<time> is the time_t when the ban was set
	<n> is ???.  value is either 0 or 1

	This message is sent in response to the 615 client request, one
	for each ban.  The list is terminated with a 0 length 615 message
	from the server.

	Example:
	
	207.172.245. valkyrie "DoS exploit" 947304224 0

617 (0x269)	list channels [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: (empty)

	client requests a list of channels on the server.  server responds
	with 618/617

	server indicates end of channel list using this message.

618 (0x26a)	channel list entry [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <channel-name> <number-of-users> <topic>

	this is the server response to a 617 client request, one for each
	channel.

	Example:

	Help 50 OpenNap help channel

619 (0x26b)	queue limit [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <nick> "<filename>" <n>

	a client may limit the number of downloads from a particular client.
	once the limit for a particular user has been reached, the uploading
	client can send this message to notify the downloader that they
	have hit the limit and can't have any more simultaneous downloads.
	<nick> is the user who hit the limit, <filename> is the file they
	were trying to download when they hit the limit, and <n> is the
	number of simultaneous downloads allowed.

	Example:

	joebob "C:\MP3\Generic Band - Generic Song.mp3" 3

620 (0x26c)	queue limit [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> "<filename>" <filesize> <digit>

	This message is sent by the server in response to the 619 client
	request, when one user needs to notify another that they have
	reached the maximum allowed simultaneous downloads.  When the server
	recieves the 619 request from the uploading client, it sends the 620
	message to the downloading client.  The only difference in format is
	the addition of the <nick> field in the 620 message which specifies
	the username of the uploading agent which is notifying the
	downloader that the queue is full.

	Example:

	joebob "C:\MP3\Generic Band - Generic Song.mp3" 1234567 3

621 (0x26d)	message of the day [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <text>

	Server: each 621 message contains a single line of text.
		OpenNap and SlavaNap servers send string
		"VERSION opennap 0.41" or "VERSION SlavaNap 1.1.3"
		among other MOTD strings. This might be used to
		detect server version.

	Client: client sends a 621 command with no data to request the
		motd be sent.  The server will usually send this
		automatically after a user logs in, so this command
		allows a user to reread it upon	request.

622 (0x26e)	muzzle a user [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> [ "<reason>" ]

	client requests that <nick> not be allowed to send public messages

623 (0x26f)	unmuzzle a user [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> [ "<reason>" ]

	client requests that the enforced silence on <nick> be lifted

624 (0x270)	un-nuke a user [CLIENT]

	[NAPSTER]

	<user>

625 (0x271)	change user's linespeed [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user> <speed>

626 (0x272)	data port error [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user>

	When a downloading client detects that the uploader's data port
	is unreachable, it should send a 626 message to the server with
	the nick of the user for which the connection failed.  The server
	then relays the message to the uploader, substituing the
	downloader's nickname in the message.

627 (0x273)	operator message [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: <text>
	server: <nick> <text>

	client request to send a message to all admins/moderators

628 (0x274)	global message [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: <text>
	server: <nick> <text>

	client request send a message to all users

629 (0x275)	banned users [SERVER]

	[NAPSTER]

	Format: <nick>

	when displaying the ban list for the server, this message is used
	to indicate banned nicknames.

630-639 missing

640	direct browse request [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Client: <nick>
	Server: <nick> [ip port]

	Client: request files for <nick>
	Server: <nick> is requesting your files.  optionally, <ip> and
		<port> are given if the client getting browsed is firewalled

	This message is sent to initiate a direct client to client browsing of
	shared files.

	See section 5.3.

641	direct browse accept [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	Client: <nick>
	Server: <nick> <ip> <port>

	The client to be browsed sends this message back to the server to
	indicate it is willing to accept a direct browse from <nick>.

	The server sends this message to the requestor of the browse to
	indicate where it should connect in order to do a direct browse from
	<nick>.

	See section 5.3

642	direct browse error [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<nick> "message"

	Server sends this messags in response to a 640 request if there is an
	error (eg. both clients are firewalled, or the browsee is not sharing
	any files).

	See section 5.3

643-649	missing

650-651	??? [CLIENT]
	[NAPSTER]

	permission denied.

652 (0x28c)	cloak user [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	sets the current user to "invisible"

653-699	missing.

700	change link speed [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<speed>

	client is notifying server that its correct link speed is <speed>,
	in the range 0-10 (see the login message for details).

701	change user password [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<password>

	client wishes to change their password

702	change email address [CLIENT]

	[NAPSTER,OPENNAP]

	<email address>

	client wishes to change their email address

703	change data port [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<port>

	client is changing the data port being listened on for file
	transfers

704-747	missing.

748	login attempt [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	the server sends this message to a logged in client when another
	client attempts to log in with the same nickname.

749	missing.

750 (0x2ee)	server ping [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

        Format: <time>

        Client pings server. Server replies with 750. <time> is in time_t
	format. Napster console command: "/sping"

	OpenNap uses <server> instead of <time> where <server> is server
	name to ping.

751 (0x2ef)	ping user [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user>

	client is attempting to determine if <user>'s connection is alive

752 (0x2f0)	pong response [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user>

	this message is sent in response to the the 751 (PING) requeset

753 (0x2f1)	change password for another user [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<user> <password> "<reason>"

	allows an administrator to change the password for another user

754-769	missing.

770	??? [CLIENT]
	[NAPSTER]

	permission denied.

771	??? [CLIENT]
	[NAPSTER]

	permission denied.

772-799	missing.

800 (0x320)	reload config [CLIENT]

	[NAPSTER,OPENNAP]

	<config variable>

	resets configuration parameter to its default value

801 (0x321)	server version [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	no data.

	client request's a server's version

802-804	missing.

805	???
	[NAPSTER]

	[returns permission denied. -ed]

810 (0x32a)	set config [CLIENT]
	[NAPSTER,OPENNAP]

	<config string>

	request a change in server configuration variables

811 (0x32b)	???	[CLIENT]
	[NAPSTER]

	[returns permission denied. -ed]

820 (0x334)	clear channel [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel>

	remove all users from the specified channel

821 (0x335)	redirect client to another server [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: <user> <server> <port>
	server: <server> <port>
	
	This command allows an administrator to redirect clients to another
	server.

822 (0x336)	cycle client [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: <user> <metaserver>
	server: <metaserver>

	This commands allows an administrator to make a client restart the
	login process by first connecting to the metaserver (redirector) at
	<host>.

823 (0x337)	set channel level [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <level>

	Sets <channel> such that users must be at least <level> in order to
	enter the channel

824 (0x338)	emote [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	client: <channel> "<text>"
	server: <channel> <user> "<text>"

	A variation of the public message command to indicate an action by
	the user.  Often implemented as the "/me" command in IRC clients.

825 (0x339)	user list entry [SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <user> <files shared> <speed>

	an 825 message is sent for each user in the channel specified by the
	830 message

	Example:

	Help testor3 0 3

	[This appears to be exactly the same format as the 408 message.  -ed]

826 (0x33a)	channel limit [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <limit>

	sets the maximum number of users that may enter a channel.  <limit>
	is an integer value between 0 and 999999999.  setting it higher that
	this results in the limit being set to -1.  by default, created
	channels have a limit of 200.  there appears to be no restriction on
	any channel member changing the limit, and no notification is given

827 (0x33b)	show all channels [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	no data.

	client request to show all channels, including "hidden" channels.
	the server also sends this message to terminate

828 (0x33c)	channel list [SERVER]
	
	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <users> <n1> <level> <limit> "<topic>"

	the server sends a list of 828 commands, one for each channel,
	including "hidden" channels that don't show up in the normal channel
	list.

	<level> is the mimimum user level required for entry into a channel
	<limit> is the max number of users allowed in a channel

	<n1> is either 0 or 1.  seems to be 1 if the channel was user
	created, or 0 if a predefined channel???

829 (0x33d)	kick user from channel [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel> <user> [ "<reason>" ]

830 (0x33e)	list users in channel [CLIENT, SERVER]

	[NAPSTER,OPENNAP,SLAVANAP]

	<channel>

	client requests a list of all users in <channel>.  server responds
	with a 825 response for each user, followed by an 830 response with
	no data [why didn't they just use the 409 message? -ed]

831 (0x33f)	global user list [CLIENT, SERVER]

	[NAPSTER?,OPENNAP,SLAVANAP]

	no data.

	Napster returns "premission denied."
	OpenNap and SlavaNap return sequence of 832 command. List of users
	is terminated with empty 831 command.

832 (0x340)	global user list entry [SERVER]

	[OPENNAP,SLAVANAP]

	<nick> <ip>

	Response to message 831.

833-869	missing.

870	add files by directory [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: "<directory>" "<file>" <md5> <size> <bitrate> <freq> <duration>
	[ ... ]

	This command allows a client to share multiple files in the same
	directory as a shortcut to multiple 100 (share file) commands.
	<directory> is the path which should be prepended to all the given
	filenames in the rest of the command.  <file> is the name of the file
	to share *without* its directory component.  When other clients do a
	browse/share, the real path will be reported as <directory>/<file>.

	The portion of this command after the <directory> may be repeated as
	many times as necessary for files in the same directory. NOTE: most
	servers will not accept commands of length longer than 2048 bytes
	so you still may need to break up the files into multiple commands
	if there are many files in a single directory.

871-899	missing.

900     connection test [SERVER]

	[NAPSTER]

        <ip> <port> <data>

        <ip>   - string,  ip address to connect to.
        <port> - integer, port to connect to
        <data> - string,  data to send to server.

        Try to connect to <ip> on <port> for atmost 1000 seconds.  If the
        connection succeeds send the <data> to target.

	[reported by Thomas van der Heijden <thom@bart.nl>]

901     listen test [SERVER]

	[NAPSTER]

        <port> <timeout> <data>

        <port>    - integer, port to listen on
        <timeout> - integer, time to wait for connection in seconds
        <data>    - string,  data to send after connection has been made.

        Listen on <port> for <timeout> seconds. If a connection arrives,
        return <data> to sender.

	[reported by Thomas van der Heijden <thom@bart.nl>]

920	socket test [CLIENT]

	[NAPSTER,OPENNAP,SLAVANAP]

	Format: <some_digit>

	This is sent by the Beta8+ client prior to login.
	
	SlavaNap server uses this command to detect byte order for big-endian
	clients (SlavaNap supports clients with big-endian and little-endian).

	OpenNap just ignores this command.

931	blocked file [SERVER]

	[NAPSTER,SLAVANAP]

	Format: <md5>

	This message is used by server to inform client
	that file is blocked.
	Used as reply to commands 100, 870, 10300

932	new share [CLIENT]

	[NAPSTER]

	Format: <binary data>

	This message is used by Napster 10.2+ to share
	files that have ID3v2 tags. Format of binary data:
	(C language, int = 4 bytes)

	struct{
		int    real_size; // file size without ID3 tags
		char   unknown1[4];
		char   unknown2[4];
		char   unknown3[4];
		char   unknown4[4];
		int    bitrate;
		int    frequency;
		char   unknown5[4];
		char   unknown6[4];
		char   MD5[32]; // 36-67
		char   unknown7[4];
	};

	If you want napster to share files using 720 instead of 932
	change "1" to "0" at the end of each line in "shared.dat" file.

995	blocked file [SERVER]

	[NAPSTER]

	Format: <binary data>

	This message is used by Napster 10.2+ server to inform
	client that file is blocked. This message is sent in reply
	to command 932.
	Length of data in reply may vary.

3.1  OpenNap and SlavaNap Message Types

The following messages are supported by both OpenNap and SlavaNap servers.
For complete list of OpenNap and SlavaNap commands see "README" file
for OpenNap or SlavaNap.


10112	show server links [CLIENT, SERVER]

	[OPENNAP,SLAVANAP]

	client: no data
	server: <host> <host> <hops>

	This command is used to show information about the links a
	server has to other servers.  The list is terminated by a 10112
	message with no data (0 length).

	Current version of SlavaNap do not support this command completely
	and replies with empty 10112 message. This command is implemented
	by SlavaNap only because AudioGnome uses it.

10115	show server stats [CLIENT, SERVER]

	[OPENNAP,SLAVANAP]

	client: no data
	server: <clients> <servers> <files> <gigs> <channels> <time>
	<uptime> <memory> <numusers>

	This command is used by administrators to get information about the
	state of the server.

	<clients>	number of locally connected clients
	<servers>	number of locally connected servers
	<users>		total number of global users
	<files>		number of files in the db
	<gigs>		total size of all files shared
	<channels>	number of active channels
	<time>		time at which the server was started
	<uptime>	number of seconds of uptime
	<memory>	if debugging is enabled, this will show the memory
			currently in use, otherwise it will be -1
	<numusers>	number of registered users		

10118	display client information statistics [CLIENT, SERVER]

	[OPENNAP,SLAVANAP]

	Available only if OpenNap was compiled with --enable-version-stats or
	"Enable version stats" was enabled in SlavaNap settings menu.

	The server will dump its lists of known clients and the number
	of logins for each.  It does not keep track of unique ips, so this
	just gives a rough estimate on the popularity of various clients.

	(client): empty
	(server): "<version>" <count>

	The server's list is terminated by an empty 10118 message.

10121	who was [CLIENT]

	[OPENNAP,SLAVANAP]

	Format: <nick>

	Displays info about a user that has recently logged out.

10200 	Register user [CLIENT]

	[OPENNAP, SLAVANAP]

	Format: <user> <pass> <email> [ <level> ]

	admin command to force registration of a nickname.
	Note: for SlavaNap <level> is required and shouldn't be "user"

10204	set channel op [CLIENT]

	[OPENNAP,SLAVANAP]

	Format: <channel> <user> [user ...]

	enable <user> to kick/ban users on <channel>

10205	remove channel op [CLIENT]

	[OPENNAP,SLAVANAP]

	Format: <channel> <user> [user ...]

	remove <user> as operator on <channel>

10207	drop channel [CLIENT]

	[OPENNAP,SLAVANAP]

	Format: <channel> [ "<reason>" ]

	marks the specified channel as being user created such that its
	state is not stored in the persistent channels file and will
	disappear once all users part from it.

10208	send message to channel ops [CLIENT, SERVER]

	[OPENNAP,SLAVANAP]

	client: <channel> <message>
	server: <channel> <code> <text>

	client: sends <message> to all operators and mods+ on <channel>
	server: sends message with code <code> and <text> to all operators
		(can be used only by another server) (n/a yet)

10209	change channel mode [CLIENT, SERVER]

	[OPENNAP,SLAVANAP]

	Format: <channel> [mode [mode ...]]

	if specified, [mode] is of the form

		(+|-)STRING

	where STRING is one of

		PRIVATE		- makes the channel not show up in the list
		MODERATED	- only ops and mods+ can speak in public
		TOPIC		- if set, any user may change the topic

		OpenNap only:
		INVITE		- channel is invite only

		SlavaNap only:
		REGISTERED	- if set, channel will not be destroyed after
				  all users will part from it.

	if [mode] is not specified servers returns current mode.

10210	invite user to a channel [CLIENT] (depreciated. use 430 instead)

	[OPENNAP,SLAVANAP]

	Format: <channel> <user>

	This message is OpenNap version of 430 message.

10211	give voice to speak in moderated channel [CLIENT]

	[OPENNAP,SLAVANAP]

	Format: <channel> [user [user ...]]

10212	remove voice to speak in moderated channel [CLIENT]

	[OPENNAP,SLAVANAP]

	Format: <channel> [user [user ...]]

10300	share generic media file [CLIENT]

	[OPENNAP,SLAVANAP]

	Format: "<filename>" <size> <md5> <major-content-type>

	<content-type> is the major MIME type defined for what the data is.
			should be one of:
				audio, video, text, image, application, mp3
			NOTE: mp3 is a separate type here since the original
			nap protocol was designed for sharing only mp3 files.
			"audio" refers to other types of audio files

	MD5 is counted the same way as for command 100.

	Examples:

	"C:\IMAGES\Grand Canyon.jpg" 54187 bc938fdc0ef63772bfbdbf57aabb0860-54187 image
	"\home\drscholl\src\opennap-0.11.tar.gz" 102161 51c07734811a26853b1a2a87b67c68a1-102161 application


3.  MD5

All MP3 files are hashed using the first 300,032 bytes of the file.
WMA files are not hashed and Napster sends "WMA-FILE" instead of MD5 for .wma

The current method seems to be: skip id3v2, seek to frame sync and hash.

Note: the linux nap client (versions 0.7 - 0.9) hash exactly 300,000
bytes, which is NOT what the official windows client does.

Correct format for MD5 is something like "58dc354f81bf37b050799ead7ca8d3bc-5333975"
where "58dc354f81bf37b050799ead7ca8d3bc" is MD5 hash and "5333975" is file
length - length of ID3 tags (v1 and v2).

Some clients ignore MD5 or send incorrect values. For example, WinMX sends MD5
without file size and FileNavigator sends "AAAAAA" (32 "A" characters) instead
of MD5. OpenNap and SlavaNap ignore md5 and do not support it by default
unless recompiled using special options.


5.  Client-Client Protocol

File transfer occur directly between clients without passing through the
server.  There are four transfer modes, upload, download, firewalled upload,
firewalled download.  The normal method of transfer is that the client
wishing to download a file makes a TCP connection to the client holding the
file on their data port.  However, in the case where the client sharing the
file is behind a firewall, it is necessary for them to "push" the data by
making a TCP connection to the downloader's data port.


5.1  Normal Downloading

Regardless of which mode, the downloading client will first issue either a 
search(200) or browse(211) command to the server.  This returns a list of
files and information on the client sharin the file.  To request a download,
a get(203) request is sent to the server.  The server will respond with
a get ack(204) containing more detailed information.

This is the point at which the different methods diverge.  If the 204 get
ack says that the remote clients data port is 0, you must send a 500 request
to the server requesting that the remote client send the data to you.  In
this case you wait for the remote client to connect to your own data port.

In the case where the sharing client is not firewalled, you make a TCP
connection to the data port specified in the 204 message from the server.
The remote client should accept the connection and immediately send one
ASCII char, `1' (ASCII 49).  Once you read this char, you send a request
for the file you wish to download.  First send the string "GET" in a single
packet, then send
	<mynick> "<filename>" <offset>
where <mynick> is your napster user name, <filename> is the file you wish to
download, and <offset> if the byte offst in the file to begin the transfer
at (if you are downloading for the first time, and not resuming a prior
transfer, you should uses 0 to start at the beginning of the file).

The remote client will then return the file size, or an error message such
as "INVALID REQUEST" or "FILE NOT SHARED".  Note that the file size is not
terminated in any special way, and the best way to figure out the size is to
keep reading until you hit a character that is not a digit (it will usually
be 0xff which is the start of the MP3 frame sync header, but if a ID3v2
tag is present it might look different).  Immediately following the file
size is where the data stream for the file begins.

Once the data transfer is initiated, the downloader should notify the server
that they are downloading a file by sending the 218 message.  Once the
transfer is complete, you send a 219 message to indicate you have finished
the download.  Note that this is cummalitive, so that if you are downloading
multiple files, you send one 218/219 pair for EACH concurrent download--this
is how the server knows how many transfers you have going on.  Likewise,
the uploader should send one 220 messge for each upload, and one 221 when
each upload has finished.


5.2  Firwalled Downloading

As described above, when the file needs to be pushed from a client behind a
firewall, the downloader sends a 500 message to the server.  This causes a
501 message to be sent to the uploader, which is similar to the 204 message
for a normal download.

Once the uploader receives the 501 message from the server, they should make
a TCP connection to the downloader's data port (given in the 501 message).
Upon connection, the downloader's client will sent one byte, the ASCII
character `1'.  The uploader should then send the string "SEND" in a single
packet, and then the information:
	<mynick> "<filename>" <size>
where <mynick> is the uploader's napster user name, <filename> is the file
being sent, and <size> is the size of the file in bytes.

Upon receipt, the downloading client will either send the byte offset at
whcih the transfer should start, or an error message such as
"INVALID REQUEST".  The byte offset should be sent as a single packet
in plain ASCII digits.  Just as with above in section 5.1, a 0 byte offset
indicates the transfer should begin at the start of the file. If you are
writing a nap client and have trouble with firewalled downloading first
check if you are sending offset in ASCII (this is the most common error)

Each client should notify the server that they are uploading or downloading
with the 218/219 (downloading) or 220/221 (uploading) command pairs (see
section 5.1 for more detailed information).


5.3 Client to Client Browsing

Napster 2.0 Beta 8 adds a feature which allows direct client-to-client
browsing of file lists. Direct browsing is supported by Napster Beta 8-9.6
From Napster 2.0 Beta 10 direct browsing is disabled. To request a browse,
a client uses the
	640 <nick>
command.  The server then sends a
	640 <requester>
to the client which is getting browsed with the nick of the client that is
requesting the browse.  If the client accepts the browse request, it sends
back a
	641 <requestor>
to the server with the nick of the client requesting the browse.  The
server then sends a
	641 <nick> <ip> <port>
to the requesting client.  In the case of an error, the server will send a 642
command in response to the 640 command.

The browsing client then makes a TCP conection to the remote client's data
port.  After getting the "1" character, the browsing client sends a
	GETLIST
At which point the remote client sends its nick followed by a linefeed (\n)
by itself in a single packet (ie, one write() call)
	<nick> LF
followed by the list of files being shared (the format being the same as
the data of the "share" command).  Each line is terminated by a linefeed char.
At the end of the list, an additional linefeed char is sent and then the
client closes the connection.

In the case that the remote client is firewalled, the browse list will have to
be pushed to the requesting client.  The remote client makes a TCP connection
to the requesting client, then sends
	SENDLIST <nick>\n
followed by the list of files, as with the "GETLIST" command response.


6.  Napigator protocol specification

Napigator server runs on "stat.napigator.com" port 8890.

In this section when I use word "client" it means OpenNap or SlavaNap
server and when I use word "server" it means Napigator server.

Message format for server: 

    <id> [<text>] \r\n

    <id> is message code in ASCII
    <text> is message text. There is a space (" ") chacter between <id> and <text>.
    Every line is terminated with \r\n (0x0D,0x0A) sequence. Strings should NOT be
    quoted.

Message format for client:

   <command> [<text>] \r\n

   <command> is text command (like USER or PASS)
   Every line is terminated with \r\n (0x0D,0x0A) sequence. String should NOT be
   quoted.

When client connects to server, server should send command 220. Client replies
with "USER". Then server sends command 300. Client replies with "PASS". If name
and password are correct server replies with 201.

Connection should be kept alive. Every 60 seconds (or any other period) client
sends "STATS" message.

Server messages:

	200	stats updated.

		No reply required.

	201	login ok.

		Format: 201 <message>

		Login sequence is complete.
		Client should reply with "IPPORT".

	220	request user name.
		
		Format: 220 <salt_string>

		Salt string used by client to encode password.
		Client should reply with "USER" message.

	221	login error.

		Format: 221 <error>

		Client should disconnect after receiving this message.

	300	password request.

		Client should reply with "PASS" command.

	other messages: something is wrong and client should disconnect.

Client messages:

	USER	send user name

		Format: USER <user_name>

	PASS	send user pass

		Format: PASS <encoded_password>

		password is encoded with MD5. Before encoding password you should
		add salt string (that you have received with 220 message) to password.

		Example:

		If your password is "qwerty" and you have received "1234" as salt string,
		encoded password will be MD5("qwerty1234");.

		Note: MD5 letters should be in upper case.

	IPPORT	send server address.

		Format: <hostname> <ip> <port>

		Note: this command should be sent only when login sequence is completed.
		
	STATS	update server stats.

		Format: <hostname> <users> <files> 0 <size> 0

		<hostname> is name of your server (ex. cyberalien.servemp3.com)
		<users> is number of connected users (ASCII)
		<files> is number of shared files (ASCII)
		<size> is size of files in Gb (ASCII)

		Note: this command cannot be used before login sequence is completed.

If you have created Napigator-compatible server mail me at mailto:cyberalien@users.sourceforge.net
and I'll add support for your server to SlavaNap.
To add you server support to OpenNap mail Dr.Scholl at mailto:drscholl@users.sourceforge.net


7.  Where to get more help?

Join the napdev mailing list by sending email to mailto:napdev-subscribe@onelist.com
or by visiting the community page http://www.onelist.com/community/napdev/.
This list is designed for open source nap developers to share information
about the specification or applications.

Latest version of this document is available at http://slavanap2.sourceforge.net/nap.txt
Original document is available at http://opennap.sourceforge.net/napster.txt

Some implementations of this protocol (servers and clients) come with
source code. Visit http://slavanap2.sourceforge.net or http://opennap.sourceforge.net
for more information.


8.  Servers compatible with this protocol:

	For Linux:  OpenNap      http://opennap.sourceforge.net
	For Win32:  SlavaNap	 http://slavanap2.sourceforge.net
	Java:	    JNerve	 http://jnerve.sourceforge.net (outdated)

9.  Acknowledgements

A big THANKS goes to the following people who contributed valuable information
to this specification:

Ben Byer <bbyer@rice.edu>
JT <jtraub@dragoncat.net>
Evan Martin <eeyem@u.washington.edu>
Colten Edwards (aka panasync@efnet) <edwards@bitchx.dimension6.com>
Thomas van der Heijden <thom@bart.nl>
