<AVRStudio><MANAGEMENT><ProjectName>USBtoRS232</ProjectName><Created>02-Nov-2002 09:38:01</Created><LastEdit>01-Feb-2004 16:22:09</LastEdit><ICON>AVRAssembler.bmp</ICON><ProjectType>0</ProjectType><Created>02-Nov-2002 09:38:01</Created><Version>4</Version><Build>135</Build><ProjectTypeName>Atmel AVR Assembler</ProjectTypeName></MANAGEMENT><CODE_CREATION><ObjectFile>X:\USERS\IGOR\DOC\WORD\Atmel\USB to RS232 Application Note\Firmware\USBtoRS232_ATmega8\AVR Studio 4 project\usbtors232.obj</ObjectFile><EntryFile>X:\USERS\IGOR\DOC\WORD\Atmel\USB to RS232 Application Note\Firmware\USBtoRS232_ATmega8\AVR Studio 4 project\USBtoRS232.asm</EntryFile><SaveFolder>X:\USERS\IGOR\DOC\WORD\Atmel\USB to RS232 Application Note\Firmware\USBtoRS232_ATmega8\AVR Studio 4 project\</SaveFolder></CODE_CREATION><DEBUG_TARGET><CURRENT_TARGET>AVR Simulator</CURRENT_TARGET><CURRENT_PART>ATmega8</CURRENT_PART><BREAKPOINTS></BREAKPOINTS><IO_EXPAND><Item>43</Item><Item>222</Item><Item>17</Item><Item>44</Item><Item>0</Item><Item>241</Item><Item>223</Item><Item>213</Item><Item>214</Item><Item>179</Item><Item>34</Item><Item>276</Item><Item>295</Item><Item>189</Item><Item>195</Item><Item>173</Item><Item>72</Item><Item>56</Item><Item>66</Item><Item>70</Item><Item>252</Item><Item>262</Item><Item>271</Item><Item>280</Item><Item>442</Item><Item>351</Item><Item>352</Item><Item>79</Item><HIDE>false</HIDE></IO_EXPAND><REGISTERNAMES><Register>R0</Register><Register>R1</Register><Register>R2</Register><Register>R3</Register><Register>R4</Register><Register>R5</Register><Register>R6</Register><Register>R7</Register><Register>R8</Register><Register>R9</Register><Register>R10</Register><Register>R11</Register><Register>R12</Register><Register>R13</Register><Register>R14</Register><Register>R15</Register><Register>R16</Register><Register>R17</Register><Register>R18</Register><Register>R19</Register><Register>R20</Register><Register>R21</Register><Register>R22</Register><Register>R23</Register><Register>R24</Register><Register>R25</Register><Register>R26</Register><Register>R27</Register><Register>R28</Register><Register>R29</Register><Register>R30</Register><Register>R31</Register></REGISTERNAMES><COM>Auto</COM><COMType>0</COMType><WATCHNUM>0</WATCHNUM><WATCHNAMES><Pane0><Variables>NoFirstBitsTimerOffset</Variables><Variables>RAMEND</Variables></Pane0><Pane1></Pane1><Pane2></Pane2><Pane3></Pane3></WATCHNAMES></DEBUG_TARGET><FilesInProject><Assembler><OpenString>Assembler File (*.asm)|*.asm;|AllFiles(*.*)|*.*</OpenString></Assembler></FilesInProject><Files><File00000><FileId>00000</FileId><Path>X:\USERS\IGOR\DOC\WORD\Atmel\USB to RS232 Application Note\Firmware\USBtoRS232_ATmega8\AVR Studio 4 project\</Path><Name>USBtoRS232.asm</Name><Status>262</Status></File00000><File00001><FileId>00001</FileId><Path>X:\USERS\IGOR\DOC\WORD\Atmel\USB to RS232 Application Note\Firmware\USBtoRS232_ATmega8\AVR Studio 4 project\</Path><Name>USBtoRS232.lst</Name><Status>96</Status></File00001><File00002><FileId>00002</FileId><Path>X:\USERS\IGOR\DOC\WORD\Atmel\USB to RS232 Application Note\Firmware\USBtoRS232_ATmega8\AVR Studio 4 project\</Path><Name>USBtoRS232.asm</Name><Status>7</Status></File00002><File00003><FileId>00003</FileId><Path>X:\USERS\IGOR\DOC\WORD\Atmel\USB to RS232 Application Note\Firmware\USBtoRS232_ATmega8\AVR Studio 4 project\</Path><Name>USBtoRS232.lst</Name><Status>96</Status></File00003></Files><Workspace><File00002><Position>214 106 1024 544</Position><LineCol>9 9</LineCol><State>Maximized</State></File00002></Workspace><Events><Breakpoints></Breakpoints><Tracepoints><File00000></File00000><File00002></File00002></Tracepoints></Events></AVRStudio>
