[Version]
Signature="$CHICAGO$"
Class=USB
provider=%MB%
LayoutFile=layout.inf

[Manufacturer]
%MfgName%=IgorCeskoCompany

[IgorCeskoCompany]
%USB\VID_03EB&PID_21FF.DeviceDesc%=AVR309Prj.Dev, USB\VID_03EB&PID_21FF
%USB\VID_03EB&PID_21FE.DeviceDesc%=AVR309Prj.Dev, USB\VID_03EB&PID_21FE

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
AVR309Prj.Files.Ext = 10,System32\Drivers
AVR309Prj.Files.Inf = 10,INF
AVR309Prj.Files.Dll = 25

[AVR309Prj.Dev]
CopyFiles=AVR309Prj.Files.Ext, AVR309Prj.Files.Inf, AVR309Prj.Files.Dll
AddReg=AVR309Prj.AddReg

[AVR309Prj.Dev.NT]
CopyFiles=AVR309Prj.Files.Ext, AVR309Prj.Files.Inf, AVR309Prj.Files.Dll
AddReg=AVR309Prj.AddReg

[AVR309Prj.Dev.NT.Services]
Addservice = AVR309Prj, 0x00000002, AVR309Prj.AddService

[AVR309Prj.AddService]
DisplayName    = %AVR309Prj.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\AVR309.sys
LoadOrderGroup = Base

[AVR309Prj.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,AVR309.sys
HKLM,"System\Currentcontrolset\Services\AVR309Prj\Parameters","MaximumTransferSize",0x10001,256
HKLM,"System\Currentcontrolset\Services\AVR309Prj\Parameters","DebugLevel",0x10001,2


[AVR309Prj.Files.Ext]
AVR309.sys

[AVR309Prj.Files.Inf]
AVR309.inf

[AVR309Prj.Files.Dll]
AVR309.dll

;---------------------------------------------------------------;

[Strings]
MB="Ing. Igor Cesko and Atmel corporation"
MfgName="Ing. Igor Cesko Company, Slovakia"
USB\VID_03EB&PID_21FF.DeviceDesc="AVR309:USB to UART protocol converter"
USB\VID_03EB&PID_21FE.DeviceDesc="AVR309:USB to UART protocol converter (simple)"
AVR309Prj.SvcDesc="AVR309:USB to UART device driver"
