# TCP/IP Daemon

Daemon is the control centre, which simultaneously handles the dynamic creation and shutting down of TCP/IP lines, controlling outgoing polls and incoming connections.

When an incoming TCP/IP connection is detected, Daemon creates a new TCP/IP mailer line and initiates high-level file transfer protocol corresponding to the port where the connection is detected. Protocols and ports are defined in TCP/IP Daemon configuration dialogue

There are three FTN file transfer protocols implemented in Argus for working with TCP/IP:

- Raw
- Telnet
- BinkP