# Connection Information Panel

This panel appears when a file transfer session is established. It contains the information about the remote system:

Connect - is the exact response received from the modem at the time of connection. If a connection is made using the TCP/IP transport protocol, this section contains the IP address and the port number of the remote system.

All other parameters are taken from EMSI packet data:

- Station - the name of remote system.
- Address - Address List of remote system.
- Sysop - the name of remote System Operator (SysOp).
- Location - geographical location of remote system.
- Phone - remote system's telephone number.
- Flags - additional flags.
- Mailer - the name and version of mailing system used by remote.

See also: Mailer Widnow and Extended Graphical User Interface Elements.