


                                ==Phrack Inc.==
                    Volume One, Issue Three, Phile 8 of 10

        ***************************************************************
        *                                                             *
        *                      Making a Shock Rod                     *
        *                                                             *
        *                             By                              *
        *                                                             *
        *                        Circle Lord                          *
        *                                                             *
        ***************************************************************


This handy little circuit is the key to generating THOUSANDS of volts of
electricity for warding off attackers (notice the plural).   It generates it
all from a hefty 6-volt source and is easily fit into a tubular casing.
Originally used as a fence charger, this circuit can be put to other uses such
as: charging a whole row of lockers at school, a row of theater seats, or a
metal bleacher set in the gym. More on this later.

To build this, all you need is a GE-3 transistor, a 6.3-volt transformer, and a
handful of spare parts from old radios.   The ammount of shock you wish to
generate is determined by the setting of potentiometer R1, a 15,000 ohm
variable resistor.   Hint: for maximum shock, set R1 at maximum!


***************************************************************
Item    *  Description
***************************************************************
 C1      * 500uF, 10-WVDC electrolytic capacitor
 C2      * 2000uF, 15-WVDC electrolytic capacitor
 M1      * 6-VDC battery
 M2,M3   * Leads
 Q1      * GE-3 transistor (2n555 will also do)
 R1      * 15K potentiometer
 R2      * 160-ohm resistor
 S1      * Spst switch
 T1      * 6.3-VAC filament transformer (Triad F-14x or equiv.)
 X1      * 1N540 diode

***************************************************************


                        Schematics:

                            +---C1--------------+
                            1                   1   HOT
                            1     +-----+       1  LEAD
                            +---1<Q1    1        )(-->
                          R1*     +     1   +--->)(
                        +-->*     1     1   1    )(
                        1   *  +--+     1   1    )(-->
                        1   1  1  1     1   1    1 TO
                        1   1  1  1     1   1    1 GND
                        1   *  C2 1     +---1----+
                        1  R2  1  1         1    1
                        1   *  1  1         1 X1 1
                        +---+--+--1---------1-->-+
                                  1 +/-     1    1
                                  +*M1*-*S1*+   GND    -


         ----         /
        /            /
       /            /
      /    ircle   /    ord
      ----         ----
